<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<text>5V</text>
<text>I2C</text>
<text>3V3</text>
<text>GND</text>
<text>SCL</text>
<text>SDA</text>
<wire x1="67.91325" y1="25.527" x2="9.2075" y2="25.527" width="0.0254" layer="20"/>
<wire x1="0.508" y1="16.1925" x2="0.508" y2="9.2075" width="0.0254" layer="20"/>
<wire x1="9.2075" y1="-0.127" x2="68.0085" y2="-0.127" width="0.0254" layer="20"/>
<wire x1="68.0085" y1="-0.127" x2="69.342" y2="1.27" width="0.0254" layer="20" curve="90"/>
<wire x1="69.342" y1="1.27" x2="69.342" y2="24.13" width="0.0254" layer="20"/>
<wire x1="69.342" y1="24.13" x2="67.91325" y2="25.527" width="0.0254" layer="20" curve="90"/>
<text>SDA</text>
<text>SCL</text>
<text>GND</text>
<text>3V3</text>
<text>Mini-Lora V1.3</text>
<text>Mini-Lora</text>
<text>RFM95</text>
<text>RST</text>
<wire x1="1.905" y1="17.5895" x2="0.508" y2="16.1925" width="0.0254" layer="20" curve="90"/>
<wire x1="8.4455" y1="17.5895" x2="1.905" y2="17.5895" width="0.0254" layer="20"/>
<wire x1="9.2075" y1="25.527" x2="8.4455" y2="24.765" width="0.0254" layer="20" curve="90"/>
<wire x1="8.4455" y1="24.765" x2="8.4455" y2="17.5895" width="0.0254" layer="20"/>
<text>GND</text>
<text>DIO0</text>
<text>BTN</text>
<text>drvn</text>
<text>BLU</text>
<text>GRN</text>
<text>DIO1</text>
<text>DIO2</text>
<text>RED</text>
<text>RAW</text>
<text>GND</text>
<text>RST</text>
<text>3V3</text>
<text>A3</text>
<text>A2</text>
<text>done</text>
<text>RES</text>
<text>SCK</text>
<text>MIS</text>
<text>MOS</text>
<text>SS</text>
<text>BTN</text>
<wire x1="8.4455" y1="6.6675" x2="8.4455" y2="0.635" width="0.0254" layer="20"/>
<wire x1="8.4455" y1="0.635" x2="9.2075" y2="-0.127" width="0.0254" layer="20" curve="90"/>
<wire x1="8.4455" y1="6.6675" x2="7.239" y2="7.8105" width="0.0254" layer="20" curve="90"/>
<wire x1="7.239" y1="7.8105" x2="1.905" y2="7.8105" width="0.0254" layer="20"/>
<wire x1="0.508" y1="9.2075" x2="1.905" y2="7.8105" width="0.0254" layer="20" curve="90"/>
<text>3V3</text>
<text>GND</text>
<text>GND</text>
<text>3V3</text>
<text>V1.3</text>
<text>GND</text>
<text>3V3</text>
<text>GND</text>
<text>3V3</text>
<text>D9/R</text>
<text>D6/G</text>
<text>D5/B</text>
<text>3V3</text>
<text>+</text>
<text>+</text>
<text>+</text>
<text>+</text>
<text>-</text>
<text>-</text>
<text>-</text>
<text>-</text>
<text>D3</text>
<text>24AA02</text>
<text>TPL</text>
<text>RX</text>
<text>PWR
BAT</text>
<text>PWR</text>
</plain>
<libraries>
<library name="_c2h">
<packages>
<package name="1X04_NO_LOCK">
</package>
<package name="1206-RES">
</package>
<package name="0805-RES">
</package>
<package name="LOGO_CH2I_75MM">
</package>
<package name="0805-CAP">
</package>
<package name="PAD">
</package>
<package name="0805-CAP-LARGEPADS">
</package>
<package name="RFM95">
</package>
<package name="SMA_UFL_PAD_TINY">
</package>
<package name="BATTERY_18650-HOLDER">
<description>Works with 18650 clips PRT-13113.</description>
</package>
<package name="PAD-JUMPER-SWAP">
</package>
<package name="ARDUINO_PRO_MINI">
</package>
<package name="LED5MMRGB_ST">
</package>
<package name="LOGO_C2I_015">
</package>
</packages>
</library>
<library name="Switch-2016">
<packages>
<package name="SW4-SMD-4.2X3.2X2.5MM">
</package>
</packages>
</library>
<library name="Microchip-24AA02E64T">
<description>&lt;b&gt; Developed By element14 &lt;/b&gt;&lt;p&gt; 

For feedback and Technical support please contact reach from below:
&lt;br&gt; Tech Support e-mail  : &lt;a href="mailto:CAD_Tech@element14.com"&gt;CAD_Tech@element14.com&lt;/a&gt;
&lt;br&gt;Community website: &lt;a href=http://www.element14.com/community/community/knode/cadsoft_eagle/eagle_cad_libraries&gt;
EAGLE CAD Libraries on element14&lt;/a&gt;</description>
<packages>
<package name="SOT95P270X145-5N">
</package>
</packages>
</library>
<library name="JeeLabs.rpt">
<packages>
<package name="BATTERY-AA">
</package>
</packages>
</library>
<library name="edeca.net-v5">
<description>A simple Eagle library, by David Cannings (david@edeca.net)

This is v1 and is licensed under the Creative Commons (Attribution-Non-Commercial-Share Alike 2.0 UK)

For more information, see http://edeca.net/</description>
<packages>
<package name="KEYSTONE-2/3A">
<description>Keystone Electronics 2/3A battery holder</description>
</package>
</packages>
</library>
<library name="microbuilder">
<packages>
<package name="SOT23-6">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt; - 6 Pin</description>
</package>
</packages>
</library>
<library name="_c2h-MacBook Pro de Charles-Henri">
<packages>
<package name="PAD">
</package>
</packages>
</library>
<library name="OPL_Discrete_Semiconductor">
<description>&lt;b&gt;Seeed Open Parts Library (OPL) for the Seeed Fusion PCB Assembly Service
&lt;br&gt;&lt;br&gt;
&lt;a href="https://www.seeedstudio.com/opl.html" title="https://www.seeedstudio.com/opl.html"&gt;Seeed Fusion PCBA OPL&lt;/a&gt;&lt;br&gt;
&lt;a href="https://www.seeedstudio.com/fusion_pcb.html"&gt;Order PCB/PCBA&lt;/a&gt;&lt;br&gt;&lt;br&gt;
&lt;a href="https://www.seeedstudio.com"&gt;www.seeedstudio.com&lt;/a&gt;
&lt;br&gt;&lt;/b&gt;</description>
<packages>
<package name="SOT-23">
<description>&lt;b&gt;SOT23&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Jumpers">
<description>&lt;h3&gt;SparkFun Jumpers&lt;/h3&gt;
In this library you'll find jumpers, or other semipermanent means of changing current paths. The least permanent form is the solder jumper. These can be changed by adding, removing, or moving solder. In cases that are less likely to be changed we have jumpers that are connected with traces. These can be cut with a razor, or reconnected with solder. Reference designator JP.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SMT-JUMPER_2_NO_NO-SILK">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="R1" library="_c2h" package="0805-RES" value="4.7K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="_c2h" package="0805-RES" value="4.7K">
<attribute name="NAME"/>
</element>
<element name="I2C" library="_c2h" package="1X04_NO_LOCK" value="CON_HEADER_1X04'NO_LOCK'"/>
<element name="C2" library="_c2h" package="0805-CAP-LARGEPADS" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$4" library="_c2h" package="LOGO_CH2I_75MM" value=""/>
<element name="BTN" library="Switch-2016" package="SW4-SMD-4.2X3.2X2.5MM" value="DHT-4235A">
<attribute name="MPN" value="DHT-4235A"/>
</element>
<element name="U$5" library="_c2h" package="RFM95" value="RFM95"/>
<element name="P4" library="_c2h" package="PAD" value="PADNORMAL"/>
<element name="U1" library="Microchip-24AA02E64T" package="SOT95P270X145-5N" value="24AA02E64T">
<attribute name="MPN" value="24AA02E64T-I/OT"/>
<attribute name="OC_NEWARK" value="01X0461"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="OC_FARNELL" value="2345567"/>
<attribute name="SUPPLIER" value="Microchip"/>
<attribute name="NAME"/>
</element>
<element name="J$2" library="_c2h" package="SMA_UFL_PAD_TINY" value="ANTENNATINY"/>
<element name="C1" library="_c2h" package="0805-CAP" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="BAT1" library="JeeLabs.rpt" package="BATTERY-AA" value="AA"/>
<element name="BAT3" library="_c2h" package="BATTERY_18650-HOLDER" value="18650"/>
<element name="R3" library="_c2h" package="0805-RES" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="_c2h" package="0805-RES" value="470">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="_c2h" package="0805-RES" value="1.5K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="_c2h" package="0805-RES" value="680">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="P1" library="_c2h" package="PAD" value="GND"/>
<element name="BAT2" library="edeca.net-v5" package="KEYSTONE-2/3A" value="CR123A"/>
<element name="U$1" library="_c2h" package="PAD-JUMPER-SWAP" value="PAD-JUMPER-SWAPSWAP"/>
<element name="U$6" library="_c2h" package="ARDUINO_PRO_MINI" value="ARDUINO MINI 3.3V 8Mhz"/>
<element name="RGB" library="_c2h" package="LED5MMRGB_ST" value="RGBLED">
<attribute name="NAME"/>
</element>
<element name="U2" library="microbuilder" package="SOT23-6" value="TPL5110">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="WAKE" library="Switch-2016" package="SW4-SMD-4.2X3.2X2.5MM" value="WAKE">
<attribute name="MPN" value="DHT-4235A"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="_c2h" package="0805-RES" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="_c2h" package="1206-RES" value="47K">
<attribute name="NAME"/>
</element>
<element name="C3" library="_c2h" package="0805-CAP" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$2" library="_c2h" package="LOGO_C2I_015" value=""/>
<element name="P2" library="_c2h-MacBook Pro de Charles-Henri" package="PAD" value="PADNORMAL"/>
<element name="P3" library="_c2h-MacBook Pro de Charles-Henri" package="PAD" value="PADNORMAL"/>
<element name="Q1" library="OPL_Discrete_Semiconductor" package="SOT-23" value="CJ2305">
<attribute name="MPN" value="CJ2305"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="_c2h" package="0805-RES" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="P5" library="_c2h-MacBook Pro de Charles-Henri" package="PAD" value="PADNORMAL"/>
<element name="P6" library="_c2h-MacBook Pro de Charles-Henri" package="PAD" value="PADNORMAL"/>
<element name="JP1" library="SparkFun-Jumpers" package="SMT-JUMPER_2_NO_NO-SILK" value="NO_TPL"/>
</elements>
<signals>
<signal name="S$2">
</signal>
<signal name="GND">
<contactref element="C2" pad="1"/>
<contactref element="U$5" pad="GND1"/>
<contactref element="U$5" pad="GND"/>
<contactref element="U$5" pad="GND2"/>
<contactref element="U1" pad="2"/>
<contactref element="J$2" pad="GND1"/>
<contactref element="J$2" pad="GND2"/>
<contactref element="J$2" pad="GND3"/>
<contactref element="J$2" pad="GND4"/>
<contactref element="C1" pad="2"/>
<contactref element="BAT3" pad="GND@1"/>
<contactref element="BAT1" pad="GND@1"/>
<contactref element="P1" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="BAT2" pad="-VE"/>
<contactref element="U$1" pad="1"/>
<contactref element="U$1" pad="11"/>
<contactref element="U$6" pad="23"/>
<contactref element="U$6" pad="4"/>
<contactref element="U2" pad="2"/>
<contactref element="R7" pad="1"/>
<contactref element="C3" pad="2"/>
<contactref element="R9" pad="1"/>
<contactref element="P3" pad="1"/>
<contactref element="P6" pad="1"/>
</signal>
<signal name="SCL">
<contactref element="R2" pad="1"/>
<contactref element="I2C" pad="3"/>
<contactref element="U1" pad="1"/>
<contactref element="U$6" pad="A5-0"/>
<contactref element="U$6" pad="A5-1"/>
</signal>
<signal name="SDA">
<contactref element="R1" pad="1"/>
<contactref element="I2C" pad="4"/>
<contactref element="U1" pad="3"/>
<contactref element="U$6" pad="A4-0"/>
<contactref element="U$6" pad="A4-1"/>
</signal>
<signal name="SCK">
<contactref element="U$5" pad="SCK"/>
<contactref element="U$6" pad="16"/>
</signal>
<signal name="MISO">
<contactref element="U$5" pad="MISO"/>
<contactref element="U$6" pad="15"/>
</signal>
<signal name="MOSI">
<contactref element="U$5" pad="MOSI"/>
<contactref element="U$6" pad="14"/>
</signal>
<signal name="3V3">
<contactref element="R2" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="P4" pad="1"/>
<contactref element="U1" pad="4"/>
<contactref element="C1" pad="1"/>
<contactref element="BAT3" pad="PWR@1"/>
<contactref element="BAT1" pad="PWR@1"/>
<contactref element="BTN" pad="1"/>
<contactref element="BAT2" pad="+VE"/>
<contactref element="U$1" pad="4"/>
<contactref element="U$1" pad="44"/>
<contactref element="U$6" pad="21"/>
<contactref element="RGB" pad="2"/>
<contactref element="U2" pad="1"/>
<contactref element="U2" pad="6"/>
<contactref element="C3" pad="1"/>
<contactref element="WAKE" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="U$5" pad="VDD"/>
<contactref element="Q1" pad="2"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="SS">
<contactref element="U$5" pad="NSS"/>
<contactref element="U$6" pad="13"/>
</signal>
<signal name="ANT">
<contactref element="U$5" pad="ANT"/>
<contactref element="J$2" pad="ANT1"/>
<contactref element="J$2" pad="ANT2"/>
<contactref element="J$2" pad="ANT3"/>
</signal>
<signal name="DIO0">
<contactref element="U$5" pad="DIO0"/>
<contactref element="U$6" pad="5"/>
</signal>
<signal name="DIO1">
<contactref element="U$5" pad="DIO1"/>
<contactref element="U$6" pad="10"/>
</signal>
<signal name="DIO2">
<contactref element="U$5" pad="DIO2"/>
<contactref element="U$6" pad="11"/>
</signal>
<signal name="GREEN">
<contactref element="R6" pad="1"/>
<contactref element="U$6" pad="9"/>
</signal>
<signal name="A1">
<contactref element="U$6" pad="18"/>
<contactref element="U2" pad="4"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="A3">
<contactref element="U$6" pad="20"/>
</signal>
<signal name="RAW">
<contactref element="U$6" pad="24"/>
</signal>
<signal name="TX">
<contactref element="U$6" pad="1"/>
</signal>
<signal name="RX">
<contactref element="U$6" pad="2"/>
</signal>
<signal name="RED">
<contactref element="R4" pad="1"/>
<contactref element="U$6" pad="12"/>
</signal>
<signal name="BLUE">
<contactref element="R5" pad="1"/>
<contactref element="U$6" pad="8"/>
</signal>
<signal name="LB">
<contactref element="R5" pad="2"/>
<contactref element="RGB" pad="4"/>
</signal>
<signal name="LG">
<contactref element="R6" pad="2"/>
<contactref element="RGB" pad="3"/>
</signal>
<signal name="LR">
<contactref element="R4" pad="2"/>
<contactref element="RGB" pad="1"/>
</signal>
<signal name="D3">
<contactref element="U$6" pad="6"/>
<contactref element="R8" pad="1"/>
<contactref element="Q1" pad="1"/>
</signal>
<signal name="RESET">
<contactref element="U$5" pad="RST"/>
<contactref element="U$6" pad="17"/>
</signal>
<signal name="D4">
<contactref element="U$6" pad="7"/>
<contactref element="BTN" pad="3"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="I2C" pad="1"/>
<contactref element="U$1" pad="3"/>
</signal>
<signal name="N$2">
<contactref element="U$1" pad="2"/>
<contactref element="I2C" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="U$6" pad="3"/>
</signal>
<signal name="RST">
<contactref element="U$6" pad="22"/>
</signal>
<signal name="DELAY">
<contactref element="U2" pad="3"/>
<contactref element="WAKE" pad="3"/>
<contactref element="R9" pad="2"/>
<contactref element="P2" pad="1"/>
</signal>
<signal name="PW-3V3">
<contactref element="P5" pad="1"/>
<contactref element="Q1" pad="3"/>
</signal>
<signal name="A2">
<contactref element="U$6" pad="19"/>
</signal>
<signal name="N$4">
<contactref element="U2" pad="5"/>
<contactref element="R8" pad="2"/>
<contactref element="JP1" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
