(kicad_pcb (version 20171130) (host pcbnew "(5.0.2)-1")
  (general
    (thickness 1.6)
    (drawings 26)
    (tracks 22)
    (zones 0)
    (modules 6)
    (nets 1)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.3 2.3)
    (pad_drill 1.3)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 101.6 106.68)
    (grid_origin 101.6 106.68)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module "User - Switch:D2HW_A201D" (layer F.Cu) (tedit 64079F3C)
    (at 118.28 78.043)
    (fp_text reference SW2C (at -10.4 3.8) (layer F.SilkS))
    (fp_text value D2HW (at -11.68 5.337) (layer F.Fab))
    (fp_text user NC (at 5.08 2.286) (layer F.SilkS) hide)
    (fp_text user NO (at 0 2.286) (layer F.SilkS) hide)
    (fp_text user COM (at -5.08 2.286) (layer F.SilkS) hide)
    (pad 3 thru_hole circle (at 5.08 3.937) (size 2 2) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 0 3.937) (size 2 2) (drill 1) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at -5.08 3.937) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )
  (module "User - Switch:D2HW_A201D" (layer F.Cu) (tedit 6407A4CA)
    (at 118.18 60.843)
    (fp_text reference SW1 (at -10.4 3.8) (layer F.SilkS))
    (fp_text value D2HW (at -11.68 5.337) (layer F.Fab))
    (fp_text user COM (at -5.08 2.286) (layer B.SilkS))
    (fp_text user NO (at 0 2.286) (layer B.SilkS))
    (fp_text user NC (at 5.08 2.286) (layer B.SilkS))
    (pad 1 thru_hole rect (at -5.08 3.937) (size 2 2) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 0 3.937) (size 2 2) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 5.08 3.937) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )
  (module "User - Switch:D2HW_A201D" (layer F.Cu) (tedit 6407A4E6)
    (at 118.28 71.843)
    (fp_text reference SW2A (at -10.4 3.8) (layer F.SilkS))
    (fp_text value D2HW (at -11.68 5.337) (layer F.Fab))
    (fp_text user COM (at -5.08 2.286) (layer B.SilkS))
    (fp_text user NO (at 0 2.286) (layer B.SilkS))
    (fp_text user NC (at 5.08 2.286) (layer B.SilkS))
    (pad 1 thru_hole rect (at -5.08 3.937) (size 2 2) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 0 3.937) (size 2 2) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 5.08 3.937) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )
  (module "User - Switch:D2HW_A201D" (layer F.Cu) (tedit 64079F07)
    (at 118.28 74.943)
    (fp_text reference SW2B (at -10.4 3.8) (layer F.SilkS))
    (fp_text value D2HW (at -11.68 5.337) (layer F.Fab))
    (fp_text user COM (at -5.08 2.286) (layer F.SilkS) hide)
    (fp_text user NO (at 0 2.286) (layer F.SilkS) hide)
    (fp_text user NC (at 5.08 2.286) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -5.08 3.937) (size 2 2) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 0 3.937) (size 2 2) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 5.08 3.937) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )
  (module "User - Switch:99-3431-202-04" (layer F.Cu) (tedit 64077F91)
    (at 118.278 51.828 180)
    (fp_text reference REF** (at 0 0.5 180) (layer F.SilkS) hide)
    (fp_text value 99-3431-202-04 (at 0 -0.5 180) (layer F.Fab))
    (fp_circle (center 1.778 -7.112) (end 2.428 -7.112) (layer Edge.Cuts) (width 0.2))
    (fp_circle (center -1.762 -7.112) (end -1.112 -7.112) (layer Edge.Cuts) (width 0.2))
    (fp_circle (center -7.492 -3.112) (end -6.092 -3.112) (layer Edge.Cuts) (width 0.2))
    (fp_circle (center 7.508 -3.112) (end 8.908 -3.112) (layer Edge.Cuts) (width 0.2))
    (fp_circle (center 7.508 -7.112) (end 8.708 -7.112) (layer Edge.Cuts) (width 0.2))
    (fp_circle (center -1.762 -9.652) (end -1.112 -9.652) (layer Edge.Cuts) (width 0.2))
    (fp_circle (center -7.492 -7.112) (end -6.292 -7.112) (layer Edge.Cuts) (width 0.2))
    (fp_circle (center 1.778 -9.652) (end 2.428 -9.652) (layer Edge.Cuts) (width 0.2))
    (pad 4 thru_hole circle (at 1.778 -7.112 180) (size 2.3 2.3) (drill 1.3) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at -1.778 -7.112 180) (size 2.3 2.3) (drill 1.3) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at -1.778 -9.652 180) (size 2.3 2.3) (drill 1.3) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 1.778 -9.652 180) (size 2.3 2.3) (drill 1.3) (layers *.Cu *.Mask))
  )
  (module "User - Switch:D2HW_A201D" (layer F.Cu) (tedit 6407A51B)
    (at 118.28 90.843)
    (fp_text reference SW3 (at -10.4 3.8) (layer F.SilkS))
    (fp_text value D2HW (at -11.68 5.337) (layer F.Fab))
    (fp_text user NC (at 5.08 2.286) (layer B.SilkS))
    (fp_text user NO (at 0 2.286) (layer B.SilkS))
    (fp_text user COM (at -5.08 2.286) (layer B.SilkS))
    (pad 3 thru_hole circle (at 5.08 3.937) (size 2 2) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 0 3.937) (size 2 2) (drill 1) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at -5.08 3.937) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )
  (gr_text Fill (at 127.2 94.78) (layer F.SilkS))
  (gr_text Full (at 127.8 78.78) (layer F.SilkS))
  (gr_text Overfill (at 129.7 64.78) (layer F.SilkS))
  (gr_text "Sub-zero Appliance \nPot Monitor Board" (at 102.5 78.58 270) (layer F.SilkS))
  (gr_text OUTSIDE (at 119.3 100.58) (layer F.SilkS))
  (gr_text INSIDE (at 119.6 100.58) (layer B.SilkS))
  (gr_line (start 100 50) (end 138.1 50) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 103.175 100.625) (end 105.715 100.625) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 134.925 100.625) (end 137.465 100.625) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 134.925 56.35) (end 137.465 56.35) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 100 103.8) (end 100 50) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 138.1 103.8) (end 100 103.8) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 138.1 50) (end 138.1 103.8) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 103.175 56.35) (end 105.715 56.35) (layer Edge.Cuts) (width 0.15))
)
