<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<text>BBBLUE2FTDI</text>
<wire x1="-1.27" y1="4.953" x2="-1.27" y2="21.209" width="0" layer="20"/>
<wire x1="-1.27" y1="21.209" x2="10.668" y2="21.209" width="0" layer="20"/>
<wire x1="-1.27" y1="4.953" x2="10.668" y2="4.953" width="0" layer="20"/>
<wire x1="10.668" y1="4.953" x2="10.668" y2="21.209" width="0" layer="20"/>
<text>GND</text>
<text>NC</text>
<text>NC</text>
<text>NC</text>
<text>GND</text>
<text>TX</text>
<text>RX</text>
<text>NC</text>
</plain>
<libraries>
<library name="dp_devices">
<description>Dangerous Prototypes Standard PCB sizes
http://dangerousprototypes.com</description>
<packages>
<package name="M1X6">
</package>
</packages>
</library>
<library name="Seeed-Connector">
<packages>
<package name="HW4-2.0">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J2" library="dp_devices" package="M1X6" value="CON_HEADER_1X06-PTH"/>
<element name="J1" library="Seeed-Connector" package="HW4-2.0" value="4P-2.0"/>
</elements>
<signals>
<signal name="GND">
<contactref element="J2" pad="1"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="RXD-BB">
<contactref element="J2" pad="4"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="TXD-BB">
<contactref element="J2" pad="5"/>
<contactref element="J1" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
