(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen") (color "White"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (color "Purple") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (color "Purple") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen") (color "White"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (footprint "CJC_Footprint_Library:Turret_terminal_Harwin_H2071ZS1" (layer "F.Cu")
    (tedit 0)
    (at 120 97.5)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Turret_terminal_Harwin_H2071ZS1" (at 0 4.5 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -4 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0) (size 5 5) (drill 2.73) (layers F&B.Cu *.Mask))
  )
  (footprint "CJC_Footprint_Library:Turret_terminal_Harwin_H2071ZS1" (layer "F.Cu")
    (tedit 0)
    (at 135 97.5)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Turret_terminal_Harwin_H2071ZS1" (at 0 4.5 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -4 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0) (size 5 5) (drill 2.73) (layers F&B.Cu *.Mask))
  )
  (footprint "CJC_Footprint_Library:Turret_terminal_Harwin_H2071ZS1" (layer "F.Cu")
    (tedit 0)
    (at 195 52.5)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Turret_terminal_Harwin_H2071ZS1" (at 0 4.5 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -4 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0) (size 5 5) (drill 2.73) (layers F&B.Cu *.Mask))
  )
  (footprint "CJC_Footprint_Library:Turret_terminal_Harwin_H2071ZS1" (layer "F.Cu")
    (tedit 0)
    (at 165 52.5)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Turret_terminal_Harwin_H2071ZS1" (at 0 4.5 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -4 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0) (size 5 5) (drill 2.73) (layers F&B.Cu *.Mask))
  )
  (footprint "CJC_Footprint_Library:Turret_terminal_Harwin_H2071ZS1" (layer "F.Cu")
    (tedit 0)
    (at 120 52.5)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Turret_terminal_Harwin_H2071ZS1" (at 0 4.5 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -4 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0) (size 5 5) (drill 2.73) (layers F&B.Cu *.Mask))
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2_DIN965" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 52.5 75)
    (descr "Mounting Hole 2.2mm, no annular, M2, DIN965")
    (tags "mounting hole 2.2mm no annular m2 din965")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -2.9) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_2.2mm_M2_DIN965" (at 0 2.9) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (footprint "CJC_Footprint_Library:Turret_terminal_Harwin_H2071ZS1" (layer "F.Cu")
    (tedit 0)
    (at 90 52.5)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Turret_terminal_Harwin_H2071ZS1" (at 0 4.5 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -4 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0) (size 5 5) (drill 2.73) (layers F&B.Cu *.Mask))
  )
  (footprint "CJC_Footprint_Library:Turret_terminal_Harwin_H2071ZS1" (layer "F.Cu")
    (tedit 0)
    (at 150 97.5)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Turret_terminal_Harwin_H2071ZS1" (at 0 4.5 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -4 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0) (size 5 5) (drill 2.73) (layers F&B.Cu *.Mask))
  )
  (footprint "CJC_Footprint_Library:Turret_terminal_Harwin_H2071ZS1" (layer "F.Cu")
    (tedit 0)
    (at 150 52.5)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Turret_terminal_Harwin_H2071ZS1" (at 0 4.5 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -4 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0) (size 5 5) (drill 2.73) (layers F&B.Cu *.Mask))
  )
  (footprint "CJC_Footprint_Library:Turret_terminal_Harwin_H2071ZS1" (layer "F.Cu")
    (tedit 0)
    (at 180 52.5)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Turret_terminal_Harwin_H2071ZS1" (at 0 4.5 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -4 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0) (size 5 5) (drill 2.73) (layers F&B.Cu *.Mask))
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2_DIN965" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 202.5 75)
    (descr "Mounting Hole 2.2mm, no annular, M2, DIN965")
    (tags "mounting hole 2.2mm no annular m2 din965")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -2.9) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_2.2mm_M2_DIN965" (at 0 2.9) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (footprint "CJC_Footprint_Library:Turret_terminal_Harwin_H2071ZS1" (layer "F.Cu")
    (tedit 0)
    (at 105 97.5)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Turret_terminal_Harwin_H2071ZS1" (at 0 4.5 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -4 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0) (size 5 5) (drill 2.73) (layers F&B.Cu *.Mask))
  )
  (footprint "CJC_Footprint_Library:Turret_terminal_Harwin_H2071ZS1" (layer "F.Cu")
    (tedit 0)
    (at 135 52.5)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Turret_terminal_Harwin_H2071ZS1" (at 0 4.5 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -4 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0) (size 5 5) (drill 2.73) (layers F&B.Cu *.Mask))
  )
  (footprint "CJC_Footprint_Library:Turret_terminal_Harwin_H2071ZS1" (layer "F.Cu")
    (tedit 0)
    (at 75 52.5)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Turret_terminal_Harwin_H2071ZS1" (at 0 4.5 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -4 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0) (size 5 5) (drill 2.73) (layers F&B.Cu *.Mask))
  )
  (footprint "CJC_Footprint_Library:Turret_terminal_Harwin_H2071ZS1" (layer "F.Cu")
    (tedit 0)
    (at 105 52.5)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Turret_terminal_Harwin_H2071ZS1" (at 0 4.5 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -4 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0) (size 5 5) (drill 2.73) (layers F&B.Cu *.Mask))
  )
  (footprint "CJC_Footprint_Library:Turret_terminal_Harwin_H2071ZS1" (layer "F.Cu")
    (tedit 0)
    (at 60 52.5)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Turret_terminal_Harwin_H2071ZS1" (at 0 4.5 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -4 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0) (size 5 5) (drill 2.73) (layers F&B.Cu *.Mask))
  )
  (footprint "CJC_Footprint_Library:Turret_terminal_Harwin_H2071ZS1" (layer "F.Cu")
    (tedit 0)
    (at 90 97.5)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Turret_terminal_Harwin_H2071ZS1" (at 0 4.5 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -4 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0) (size 5 5) (drill 2.73) (layers F&B.Cu *.Mask))
  )
  (footprint "CJC_Footprint_Library:Turret_terminal_Harwin_H2071ZS1" (layer "F.Cu")
    (tedit 0)
    (at 75 97.5)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Turret_terminal_Harwin_H2071ZS1" (at 0 4.5 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -4 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0) (size 5 5) (drill 2.73) (layers F&B.Cu *.Mask))
  )
  (footprint "CJC_Footprint_Library:Turret_terminal_Harwin_H2071ZS1" (layer "F.Cu")
    (tedit 0)
    (at 165 97.5)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Turret_terminal_Harwin_H2071ZS1" (at 0 4.5 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -4 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0) (size 5 5) (drill 2.73) (layers F&B.Cu *.Mask))
  )
  (footprint "CJC_Footprint_Library:Turret_terminal_Harwin_H2071ZS1" (layer "F.Cu")
    (tedit 0)
    (at 60 97.5)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Turret_terminal_Harwin_H2071ZS1" (at 0 4.5 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -4 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0) (size 5 5) (drill 2.73) (layers F&B.Cu *.Mask))
  )
  (footprint "CJC_Footprint_Library:Turret_terminal_Harwin_H2071ZS1" (layer "F.Cu")
    (tedit 0)
    (at 180 97.5)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Turret_terminal_Harwin_H2071ZS1" (at 0 4.5 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -4 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0) (size 5 5) (drill 2.73) (layers F&B.Cu *.Mask))
  )
  (footprint "CJC_Footprint_Library:Turret_terminal_Harwin_H2071ZS1" (layer "F.Cu")
    (tedit 0)
    (at 195 97.5)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Turret_terminal_Harwin_H2071ZS1" (at 0 4.5 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -4 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0) (size 5 5) (drill 2.73) (layers F&B.Cu *.Mask))
  )
  (gr_arc (start 45 47.5) (mid 45.732233 45.732233) (end 47.5 45) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 47.5 105) (mid 45.732233 104.267767) (end 45 102.5) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 207.5 45) (end 47.5 45) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 47.5 105) (end 207.5 105) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 45 47.5) (end 45 102.5) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 207.5 45) (mid 209.267767 45.732233) (end 210 47.5) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 210 102.5) (mid 209.267767 104.267767) (end 207.5 105) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 210 102.5) (end 210 47.5) (layer "Edge.Cuts") (width 0.1))
  (gr_text "10" (at 195 60 180) (layer "B.SilkS"))
  (gr_text "8" (at 165 60 180) (layer "B.SilkS"))
  (gr_text "13" (at 90 90 180) (layer "B.SilkS"))
  (gr_text "9" (at 180 60 180) (layer "B.SilkS"))
  (gr_text "4" (at 105 60 180) (layer "B.SilkS"))
  (gr_text "11" (at 60 90 180) (layer "B.SilkS"))
  (gr_text "14" (at 105 90 180) (layer "B.SilkS"))
  (gr_text "1" (at 60 60 180) (layer "B.SilkS"))
  (gr_text "18" (at 165 90 180) (layer "B.SilkS"))
  (gr_text "6" (at 135 60 180) (layer "B.SilkS"))
  (gr_text "20" (at 195 90 180) (layer "B.SilkS"))
  (gr_text "2" (at 75 60 180) (layer "B.SilkS"))
  (gr_text "19" (at 180 90 180) (layer "B.SilkS"))
  (gr_text "12" (at 75 90 180) (layer "B.SilkS"))
  (gr_text "16" (at 135 90 180) (layer "B.SilkS"))
  (gr_text "15" (at 120 90 180) (layer "B.SilkS"))
  (gr_text "5" (at 120 60 180) (layer "B.SilkS"))
  (gr_text "7" (at 150 60 180) (layer "B.SilkS"))
  (gr_text "3" (at 90 60 180) (layer "B.SilkS"))
  (gr_text "chris.carter.iee@protonmail.com: September 2022" (at 127.5 72.5 180) (layer "B.SilkS"))
  (gr_text "Turret Tag Board - Type 01" (at 127.5 77.5 180) (layer "B.SilkS"))
  (gr_text "17" (at 150 90 180) (layer "B.SilkS"))
  (gr_text "17" (at 150 90) (layer "F.SilkS"))
  (gr_text "9" (at 180 60) (layer "F.SilkS"))
  (gr_text "2" (at 75 60) (layer "F.SilkS"))
  (gr_text "6" (at 135 60) (layer "F.SilkS"))
  (gr_text "14" (at 105 90) (layer "F.SilkS"))
  (gr_text "13" (at 90 90) (layer "F.SilkS"))
  (gr_text "18" (at 165 90) (layer "F.SilkS"))
  (gr_text "16" (at 135 90) (layer "F.SilkS"))
  (gr_text "11" (at 60 90) (layer "F.SilkS"))
  (gr_text "3" (at 90 60) (layer "F.SilkS"))
  (gr_text "8" (at 165 60) (layer "F.SilkS"))
  (gr_text "12" (at 75 90) (layer "F.SilkS"))
  (gr_text "7" (at 150 60) (layer "F.SilkS"))
  (gr_text "20" (at 195 90) (layer "F.SilkS"))
  (gr_text "10" (at 195 60) (layer "F.SilkS"))
  (gr_text "15" (at 120 90) (layer "F.SilkS"))
  (gr_text "4" (at 105 60) (layer "F.SilkS"))
  (gr_text "19" (at 180 90) (layer "F.SilkS"))
  (gr_text "5" (at 120 60) (layer "F.SilkS"))
  (gr_text "1" (at 60 60) (layer "F.SilkS"))
)
