(kicad_pcb (version 20171130) (host pcbnew "(5.1.5-0-10_14)")
  (general
    (thickness 1.6)
    (drawings 29)
    (tracks 405)
    (zones 0)
    (modules 14)
    (nets 10)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (1 In1.Cu power)
    (2 In2.Cu power)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.346)
    (trace_clearance 0.346)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(FL1-Pad2)")
  (net 2 "Net-(FL1-Pad1)")
  (net 3 "Net-(FL2-Pad1)")
  (net 4 GND)
  (net 5 "Net-(J3-Pad1)")
  (net 6 "Net-(J10-Pad1)")
  (net 7 "Net-(J11-Pad1)")
  (net 8 "Net-(J12-Pad1)")
  (net 9 "Net-(FL2-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.346)
    (trace_width 0.346)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(FL1-Pad1)")
    (add_net "Net-(FL1-Pad2)")
    (add_net "Net-(FL2-Pad1)")
    (add_net "Net-(FL2-Pad2)")
    (add_net "Net-(J10-Pad1)")
    (add_net "Net-(J11-Pad1)")
    (add_net "Net-(J12-Pad1)")
    (add_net "Net-(J3-Pad1)")
  )
  (module aps_radar_lib:SMA_Molex_73251-1153_EdgeMount_Horizontal (layer F.Cu) (tedit 5E3860C7)
    (at 69.088 53.34)
    (descr "Molex SMA RF Connectors, Edge Mount, (http://www.molex.com/pdm_docs/sd/732511150_sd.pdf)")
    (tags "sma edge")
    (attr smd)
    (fp_text reference J2 (at -1.5 7) (layer F.SilkS) hide)
    (fp_text value 2.9G-P1 (at -1.72 -7.11) (layer F.SilkS))
    (fp_text user %R (at -1.5 7) (layer F.Fab))
    (pad 2 smd rect (at 1.27 4.38) (size 0.95 0.46) (layers B.Cu)
      (net 4 GND))
    (pad 2 smd rect (at 1.27 -4.38) (size 0.95 0.46) (layers B.Cu)
      (net 4 GND))
    (pad 2 smd rect (at 1.27 4.38) (size 0.95 0.46) (layers F.Cu)
      (net 4 GND))
    (pad 2 smd rect (at 1.27 -4.38) (size 0.95 0.46) (layers F.Cu)
      (net 4 GND))
    (pad 2 thru_hole circle (at 1.72 4.38) (size 0.97 0.97) (drill 0.46) (layers *.Cu)
      (net 4 GND))
    (pad 2 thru_hole circle (at 1.72 -4.38) (size 0.97 0.97) (drill 0.46) (layers *.Cu)
      (net 4 GND))
    (pad 2 smd rect (at -1.72 4.38) (size 5.08 2.42) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 2 smd rect (at -1.72 -4.38) (size 5.08 2.42) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 2 smd rect (at -1.72 4.38) (size 5.08 2.42) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at -1.72 -4.38) (size 5.08 2.42) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 1 smd rect (at -1.72 0) (size 5.08 1.5) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(FL2-Pad1)"))
    (model ${KISYS3DMOD}/Connector_Coaxial.3dshapes/SMA_Molex_73251-1153_EdgeMount_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module aps_radar_lib:SMA_Molex_73251-1153_EdgeMount_Horizontal (layer F.Cu) (tedit 5E3860C7)
    (at 83.82 137.16 180)
    (descr "Molex SMA RF Connectors, Edge Mount, (http://www.molex.com/pdm_docs/sd/732511150_sd.pdf)")
    (tags "sma edge")
    (attr smd)
    (fp_text reference J12 (at -1.5 7) (layer F.SilkS) hide)
    (fp_text value L2F-P2 (at -1.778 7.112) (layer F.SilkS))
    (fp_text user %R (at -1.5 7) (layer F.Fab))
    (pad 2 smd rect (at 1.27 4.38 180) (size 0.95 0.46) (layers B.Cu)
      (net 4 GND))
    (pad 2 smd rect (at 1.27 -4.38 180) (size 0.95 0.46) (layers B.Cu)
      (net 4 GND))
    (pad 2 smd rect (at 1.27 4.38 180) (size 0.95 0.46) (layers F.Cu)
      (net 4 GND))
    (pad 2 smd rect (at 1.27 -4.38 180) (size 0.95 0.46) (layers F.Cu)
      (net 4 GND))
    (pad 2 thru_hole circle (at 1.72 4.38 180) (size 0.97 0.97) (drill 0.46) (layers *.Cu)
      (net 4 GND))
    (pad 2 thru_hole circle (at 1.72 -4.38 180) (size 0.97 0.97) (drill 0.46) (layers *.Cu)
      (net 4 GND))
    (pad 2 smd rect (at -1.72 4.38 180) (size 5.08 2.42) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 2 smd rect (at -1.72 -4.38 180) (size 5.08 2.42) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 2 smd rect (at -1.72 4.38 180) (size 5.08 2.42) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at -1.72 -4.38 180) (size 5.08 2.42) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 1 smd rect (at -1.72 0 180) (size 5.08 1.5) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J12-Pad1)"))
    (model ${KISYS3DMOD}/Connector_Coaxial.3dshapes/SMA_Molex_73251-1153_EdgeMount_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module aps_radar_lib:SMA_Molex_73251-1153_EdgeMount_Horizontal (layer F.Cu) (tedit 5E3860C7)
    (at 119.957 105.664 180)
    (descr "Molex SMA RF Connectors, Edge Mount, (http://www.molex.com/pdm_docs/sd/732511150_sd.pdf)")
    (tags "sma edge")
    (attr smd)
    (fp_text reference J11 (at -1.5 7) (layer F.SilkS) hide)
    (fp_text value L1F-P2 (at -1.72 -7.11) (layer F.SilkS))
    (fp_text user %R (at -1.5 7) (layer F.Fab))
    (pad 2 smd rect (at 1.27 4.38 180) (size 0.95 0.46) (layers B.Cu)
      (net 4 GND))
    (pad 2 smd rect (at 1.27 -4.38 180) (size 0.95 0.46) (layers B.Cu)
      (net 4 GND))
    (pad 2 smd rect (at 1.27 4.38 180) (size 0.95 0.46) (layers F.Cu)
      (net 4 GND))
    (pad 2 smd rect (at 1.27 -4.38 180) (size 0.95 0.46) (layers F.Cu)
      (net 4 GND))
    (pad 2 thru_hole circle (at 1.72 4.38 180) (size 0.97 0.97) (drill 0.46) (layers *.Cu)
      (net 4 GND))
    (pad 2 thru_hole circle (at 1.72 -4.38 180) (size 0.97 0.97) (drill 0.46) (layers *.Cu)
      (net 4 GND))
    (pad 2 smd rect (at -1.72 4.38 180) (size 5.08 2.42) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 2 smd rect (at -1.72 -4.38 180) (size 5.08 2.42) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 2 smd rect (at -1.72 4.38 180) (size 5.08 2.42) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at -1.72 -4.38 180) (size 5.08 2.42) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 1 smd rect (at -1.72 0 180) (size 5.08 1.5) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J11-Pad1)"))
    (model ${KISYS3DMOD}/Connector_Coaxial.3dshapes/SMA_Molex_73251-1153_EdgeMount_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module aps_radar_lib:SMA_Molex_73251-1153_EdgeMount_Horizontal (layer F.Cu) (tedit 5E3860C7)
    (at 83.82 121.412 180)
    (descr "Molex SMA RF Connectors, Edge Mount, (http://www.molex.com/pdm_docs/sd/732511150_sd.pdf)")
    (tags "sma edge")
    (attr smd)
    (fp_text reference J10 (at -1.5 7) (layer F.SilkS) hide)
    (fp_text value L2-P2 (at -1.524 6.985) (layer F.SilkS))
    (fp_text user %R (at -1.5 7) (layer F.Fab))
    (pad 2 smd rect (at 1.27 4.38 180) (size 0.95 0.46) (layers B.Cu)
      (net 4 GND))
    (pad 2 smd rect (at 1.27 -4.38 180) (size 0.95 0.46) (layers B.Cu)
      (net 4 GND))
    (pad 2 smd rect (at 1.27 4.38 180) (size 0.95 0.46) (layers F.Cu)
      (net 4 GND))
    (pad 2 smd rect (at 1.27 -4.38 180) (size 0.95 0.46) (layers F.Cu)
      (net 4 GND))
    (pad 2 thru_hole circle (at 1.72 4.38 180) (size 0.97 0.97) (drill 0.46) (layers *.Cu)
      (net 4 GND))
    (pad 2 thru_hole circle (at 1.72 -4.38 180) (size 0.97 0.97) (drill 0.46) (layers *.Cu)
      (net 4 GND))
    (pad 2 smd rect (at -1.72 4.38 180) (size 5.08 2.42) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 2 smd rect (at -1.72 -4.38 180) (size 5.08 2.42) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 2 smd rect (at -1.72 4.38 180) (size 5.08 2.42) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at -1.72 -4.38 180) (size 5.08 2.42) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 1 smd rect (at -1.72 0 180) (size 5.08 1.5) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J10-Pad1)"))
    (model ${KISYS3DMOD}/Connector_Coaxial.3dshapes/SMA_Molex_73251-1153_EdgeMount_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module aps_radar_lib:SMA_Molex_73251-1153_EdgeMount_Horizontal (layer F.Cu) (tedit 5E3860C7)
    (at 119.957 90.043 180)
    (descr "Molex SMA RF Connectors, Edge Mount, (http://www.molex.com/pdm_docs/sd/732511150_sd.pdf)")
    (tags "sma edge")
    (attr smd)
    (fp_text reference J9 (at -1.5 7) (layer F.SilkS) hide)
    (fp_text value L1-P2 (at -1.836 -7.366 180) (layer F.SilkS))
    (fp_text user %R (at -1.5 7) (layer F.Fab))
    (pad 2 smd rect (at 1.27 4.38 180) (size 0.95 0.46) (layers B.Cu)
      (net 4 GND))
    (pad 2 smd rect (at 1.27 -4.38 180) (size 0.95 0.46) (layers B.Cu)
      (net 4 GND))
    (pad 2 smd rect (at 1.27 4.38 180) (size 0.95 0.46) (layers F.Cu)
      (net 4 GND))
    (pad 2 smd rect (at 1.27 -4.38 180) (size 0.95 0.46) (layers F.Cu)
      (net 4 GND))
    (pad 2 thru_hole circle (at 1.72 4.38 180) (size 0.97 0.97) (drill 0.46) (layers *.Cu)
      (net 4 GND))
    (pad 2 thru_hole circle (at 1.72 -4.38 180) (size 0.97 0.97) (drill 0.46) (layers *.Cu)
      (net 4 GND))
    (pad 2 smd rect (at -1.72 4.38 180) (size 5.08 2.42) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 2 smd rect (at -1.72 -4.38 180) (size 5.08 2.42) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 2 smd rect (at -1.72 4.38 180) (size 5.08 2.42) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at -1.72 -4.38 180) (size 5.08 2.42) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 1 smd rect (at -1.72 0 180) (size 5.08 1.5) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J3-Pad1)"))
    (model ${KISYS3DMOD}/Connector_Coaxial.3dshapes/SMA_Molex_73251-1153_EdgeMount_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module aps_radar_lib:SMA_Molex_73251-1153_EdgeMount_Horizontal (layer F.Cu) (tedit 5E3860C7)
    (at 120.142 53.34 180)
    (descr "Molex SMA RF Connectors, Edge Mount, (http://www.molex.com/pdm_docs/sd/732511150_sd.pdf)")
    (tags "sma edge")
    (attr smd)
    (fp_text reference J8 (at -1.5 7) (layer F.SilkS) hide)
    (fp_text value 2.9G-P2 (at -1.651 7.112) (layer F.SilkS))
    (fp_text user %R (at -1.5 7) (layer F.Fab))
    (pad 2 smd rect (at 1.27 4.38 180) (size 0.95 0.46) (layers B.Cu)
      (net 4 GND))
    (pad 2 smd rect (at 1.27 -4.38 180) (size 0.95 0.46) (layers B.Cu)
      (net 4 GND))
    (pad 2 smd rect (at 1.27 4.38 180) (size 0.95 0.46) (layers F.Cu)
      (net 4 GND))
    (pad 2 smd rect (at 1.27 -4.38 180) (size 0.95 0.46) (layers F.Cu)
      (net 4 GND))
    (pad 2 thru_hole circle (at 1.72 4.38 180) (size 0.97 0.97) (drill 0.46) (layers *.Cu)
      (net 4 GND))
    (pad 2 thru_hole circle (at 1.72 -4.38 180) (size 0.97 0.97) (drill 0.46) (layers *.Cu)
      (net 4 GND))
    (pad 2 smd rect (at -1.72 4.38 180) (size 5.08 2.42) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 2 smd rect (at -1.72 -4.38 180) (size 5.08 2.42) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 2 smd rect (at -1.72 4.38 180) (size 5.08 2.42) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at -1.72 -4.38 180) (size 5.08 2.42) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 1 smd rect (at -1.72 0 180) (size 5.08 1.5) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(FL2-Pad2)"))
    (model ${KISYS3DMOD}/Connector_Coaxial.3dshapes/SMA_Molex_73251-1153_EdgeMount_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module aps_radar_lib:SMA_Molex_73251-1153_EdgeMount_Horizontal (layer F.Cu) (tedit 5E3860C7)
    (at 109.982 74.422 180)
    (descr "Molex SMA RF Connectors, Edge Mount, (http://www.molex.com/pdm_docs/sd/732511150_sd.pdf)")
    (tags "sma edge")
    (attr smd)
    (fp_text reference J7 (at -1.5 7) (layer F.SilkS) hide)
    (fp_text value 5.8G-P2 (at -1.651 7.112) (layer F.SilkS))
    (fp_text user %R (at -1.5 7) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.27 4.38 180) (size 0.95 0.46) (layers B.Cu)
      (net 4 GND))
    (pad 2 smd rect (at 1.27 -4.38 180) (size 0.95 0.46) (layers B.Cu)
      (net 4 GND))
    (pad 2 smd rect (at 1.27 4.38 180) (size 0.95 0.46) (layers F.Cu)
      (net 4 GND))
    (pad 2 smd rect (at 1.27 -4.38 180) (size 0.95 0.46) (layers F.Cu)
      (net 4 GND))
    (pad 2 thru_hole circle (at 1.72 4.38 180) (size 0.97 0.97) (drill 0.46) (layers *.Cu)
      (net 4 GND))
    (pad 2 thru_hole circle (at 1.72 -4.38 180) (size 0.97 0.97) (drill 0.46) (layers *.Cu)
      (net 4 GND))
    (pad 2 smd rect (at -1.72 4.38 180) (size 5.08 2.42) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 2 smd rect (at -1.72 -4.38 180) (size 5.08 2.42) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 2 smd rect (at -1.72 4.38 180) (size 5.08 2.42) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at -1.72 -4.38 180) (size 5.08 2.42) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 1 smd rect (at -1.72 0 180) (size 5.08 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(FL1-Pad2)"))
    (model ${KISYS3DMOD}/Connector_Coaxial.3dshapes/SMA_Molex_73251-1153_EdgeMount_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module aps_radar_lib:SMA_Molex_73251-1153_EdgeMount_Horizontal (layer F.Cu) (tedit 5E3860C7)
    (at 69.088 137.16)
    (descr "Molex SMA RF Connectors, Edge Mount, (http://www.molex.com/pdm_docs/sd/732511150_sd.pdf)")
    (tags "sma edge")
    (attr smd)
    (fp_text reference J6 (at -1.5 7) (layer F.SilkS) hide)
    (fp_text value L2F-P1 (at -1.72 -7.11) (layer F.SilkS))
    (fp_text user %R (at -1.5 7) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.27 4.38) (size 0.95 0.46) (layers B.Cu)
      (net 4 GND))
    (pad 2 smd rect (at 1.27 -4.38) (size 0.95 0.46) (layers B.Cu)
      (net 4 GND))
    (pad 2 smd rect (at 1.27 4.38) (size 0.95 0.46) (layers F.Cu)
      (net 4 GND))
    (pad 2 smd rect (at 1.27 -4.38) (size 0.95 0.46) (layers F.Cu)
      (net 4 GND))
    (pad 2 thru_hole circle (at 1.72 4.38) (size 0.97 0.97) (drill 0.46) (layers *.Cu)
      (net 4 GND))
    (pad 2 thru_hole circle (at 1.72 -4.38) (size 0.97 0.97) (drill 0.46) (layers *.Cu)
      (net 4 GND))
    (pad 2 smd rect (at -1.72 4.38) (size 5.08 2.42) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 2 smd rect (at -1.72 -4.38) (size 5.08 2.42) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 2 smd rect (at -1.72 4.38) (size 5.08 2.42) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at -1.72 -4.38) (size 5.08 2.42) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 1 smd rect (at -1.72 0) (size 5.08 1.5) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J12-Pad1)"))
    (model ${KISYS3DMOD}/Connector_Coaxial.3dshapes/SMA_Molex_73251-1153_EdgeMount_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module aps_radar_lib:SMA_Molex_73251-1153_EdgeMount_Horizontal (layer F.Cu) (tedit 5E3860C7)
    (at 69.088 105.664)
    (descr "Molex SMA RF Connectors, Edge Mount, (http://www.molex.com/pdm_docs/sd/732511150_sd.pdf)")
    (tags "sma edge")
    (attr smd)
    (fp_text reference J5 (at -1.5 7) (layer F.SilkS) hide)
    (fp_text value L1F-P1 (at -1.72 -7.11) (layer F.SilkS))
    (fp_text user %R (at -1.5 7) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.27 4.38) (size 0.95 0.46) (layers B.Cu)
      (net 4 GND))
    (pad 2 smd rect (at 1.27 -4.38) (size 0.95 0.46) (layers B.Cu)
      (net 4 GND))
    (pad 2 smd rect (at 1.27 4.38) (size 0.95 0.46) (layers F.Cu)
      (net 4 GND))
    (pad 2 smd rect (at 1.27 -4.38) (size 0.95 0.46) (layers F.Cu)
      (net 4 GND))
    (pad 2 thru_hole circle (at 1.72 4.38) (size 0.97 0.97) (drill 0.46) (layers *.Cu)
      (net 4 GND))
    (pad 2 thru_hole circle (at 1.72 -4.38) (size 0.97 0.97) (drill 0.46) (layers *.Cu)
      (net 4 GND))
    (pad 2 smd rect (at -1.72 4.38) (size 5.08 2.42) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 2 smd rect (at -1.72 -4.38) (size 5.08 2.42) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 2 smd rect (at -1.72 4.38) (size 5.08 2.42) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at -1.72 -4.38) (size 5.08 2.42) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 1 smd rect (at -1.72 0) (size 5.08 1.5) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J11-Pad1)"))
    (model ${KISYS3DMOD}/Connector_Coaxial.3dshapes/SMA_Molex_73251-1153_EdgeMount_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module aps_radar_lib:SMA_Molex_73251-1153_EdgeMount_Horizontal (layer F.Cu) (tedit 5E3860C7)
    (at 69.088 121.412)
    (descr "Molex SMA RF Connectors, Edge Mount, (http://www.molex.com/pdm_docs/sd/732511150_sd.pdf)")
    (tags "sma edge")
    (attr smd)
    (fp_text reference J4 (at -1.5 7) (layer F.SilkS) hide)
    (fp_text value L2-P1 (at -1.72 -7.11) (layer F.SilkS))
    (fp_text user %R (at -1.5 7) (layer F.Fab))
    (pad 2 smd rect (at 1.27 4.38) (size 0.95 0.46) (layers B.Cu)
      (net 4 GND))
    (pad 2 smd rect (at 1.27 -4.38) (size 0.95 0.46) (layers B.Cu)
      (net 4 GND))
    (pad 2 smd rect (at 1.27 4.38) (size 0.95 0.46) (layers F.Cu)
      (net 4 GND))
    (pad 2 smd rect (at 1.27 -4.38) (size 0.95 0.46) (layers F.Cu)
      (net 4 GND))
    (pad 2 thru_hole circle (at 1.72 4.38) (size 0.97 0.97) (drill 0.46) (layers *.Cu)
      (net 4 GND))
    (pad 2 thru_hole circle (at 1.72 -4.38) (size 0.97 0.97) (drill 0.46) (layers *.Cu)
      (net 4 GND))
    (pad 2 smd rect (at -1.72 4.38) (size 5.08 2.42) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 2 smd rect (at -1.72 -4.38) (size 5.08 2.42) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 2 smd rect (at -1.72 4.38) (size 5.08 2.42) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at -1.72 -4.38) (size 5.08 2.42) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 1 smd rect (at -1.72 0) (size 5.08 1.5) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J10-Pad1)"))
    (model ${KISYS3DMOD}/Connector_Coaxial.3dshapes/SMA_Molex_73251-1153_EdgeMount_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module aps_radar_lib:SMA_Molex_73251-1153_EdgeMount_Horizontal (layer F.Cu) (tedit 5E3860C7)
    (at 69.088 90.043)
    (descr "Molex SMA RF Connectors, Edge Mount, (http://www.molex.com/pdm_docs/sd/732511150_sd.pdf)")
    (tags "sma edge")
    (attr smd)
    (fp_text reference J3 (at -1.5 7) (layer F.SilkS) hide)
    (fp_text value L1-P1 (at -1.72 -7.11) (layer F.SilkS))
    (fp_text user %R (at -1.5 7) (layer F.Fab))
    (pad 2 smd rect (at 1.27 4.38) (size 0.95 0.46) (layers B.Cu)
      (net 4 GND))
    (pad 2 smd rect (at 1.27 -4.38) (size 0.95 0.46) (layers B.Cu)
      (net 4 GND))
    (pad 2 smd rect (at 1.27 4.38) (size 0.95 0.46) (layers F.Cu)
      (net 4 GND))
    (pad 2 smd rect (at 1.27 -4.38) (size 0.95 0.46) (layers F.Cu)
      (net 4 GND))
    (pad 2 thru_hole circle (at 1.72 4.38) (size 0.97 0.97) (drill 0.46) (layers *.Cu)
      (net 4 GND))
    (pad 2 thru_hole circle (at 1.72 -4.38) (size 0.97 0.97) (drill 0.46) (layers *.Cu)
      (net 4 GND))
    (pad 2 smd rect (at -1.72 4.38) (size 5.08 2.42) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 2 smd rect (at -1.72 -4.38) (size 5.08 2.42) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 2 smd rect (at -1.72 4.38) (size 5.08 2.42) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at -1.72 -4.38) (size 5.08 2.42) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 1 smd rect (at -1.72 0) (size 5.08 1.5) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J3-Pad1)"))
    (model ${KISYS3DMOD}/Connector_Coaxial.3dshapes/SMA_Molex_73251-1153_EdgeMount_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module aps_radar_lib:SMA_Molex_73251-1153_EdgeMount_Horizontal (layer F.Cu) (tedit 5E3860C7)
    (at 69.088 74.422)
    (descr "Molex SMA RF Connectors, Edge Mount, (http://www.molex.com/pdm_docs/sd/732511150_sd.pdf)")
    (tags "sma edge")
    (attr smd)
    (fp_text reference J1 (at -1.5 7) (layer F.SilkS) hide)
    (fp_text value 5.8G-P1 (at -1.72 -7.11) (layer F.SilkS))
    (fp_text user %R (at -1.5 7) (layer F.Fab))
    (pad 2 smd rect (at 1.27 4.38) (size 0.95 0.46) (layers B.Cu)
      (net 4 GND))
    (pad 2 smd rect (at 1.27 -4.38) (size 0.95 0.46) (layers B.Cu)
      (net 4 GND))
    (pad 2 smd rect (at 1.27 4.38) (size 0.95 0.46) (layers F.Cu)
      (net 4 GND))
    (pad 2 smd rect (at 1.27 -4.38) (size 0.95 0.46) (layers F.Cu)
      (net 4 GND))
    (pad 2 thru_hole circle (at 1.72 4.38) (size 0.97 0.97) (drill 0.46) (layers *.Cu)
      (net 4 GND))
    (pad 2 thru_hole circle (at 1.72 -4.38) (size 0.97 0.97) (drill 0.46) (layers *.Cu)
      (net 4 GND))
    (pad 2 smd rect (at -1.72 4.38) (size 5.08 2.42) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 2 smd rect (at -1.72 -4.38) (size 5.08 2.42) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 2 smd rect (at -1.72 4.38) (size 5.08 2.42) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at -1.72 -4.38) (size 5.08 2.42) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 1 smd rect (at -1.72 0) (size 5.08 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(FL1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_Coaxial.3dshapes/SMA_Molex_73251-1153_EdgeMount_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module aps_radar_lib:2.9G_ring_resonator_2mm (layer F.Cu) (tedit 5E384915)
    (at 94.615 53.34)
    (fp_text reference FL2 (at -0.04 -11.7) (layer F.SilkS) hide)
    (fp_text value 2.9GHz (at -0.01 12.55) (layer F.SilkS) hide)
    (pad 2 smd rect (at 11.98 0) (size 0.346 0.346) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(FL2-Pad2)"))
    (pad 1 smd rect (at -11.98 0) (size 0.346 0.346) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(FL2-Pad1)"))
  )
  (module aps_radar_lib:5.8G_ring_resonator_2mm (layer F.Cu) (tedit 5E378548)
    (at 89.535 74.422)
    (fp_text reference FL1 (at 0.02 -6.57) (layer F.SilkS) hide)
    (fp_text value 5.8GHz (at -0.06 6.94) (layer F.SilkS) hide)
    (pad 2 smd rect (at 7.02 0) (size 0.346 0.346) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(FL1-Pad2)"))
    (pad 1 smd rect (at -7.02 0) (size 0.346 0.346) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(FL1-Pad1)"))
  )
  (gr_arc (start 64.135 144.272) (end 63.246 144.272) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 124.841 39.116) (end 125.73 39.116) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 124.841 60.706) (end 124.841 61.595) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 116.332 62.484) (end 116.332 61.595) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 116.332 82.296) (end 115.443 82.296) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 124.841 84.074) (end 125.73 84.074) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 124.841 112.903) (end 124.841 113.792) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 90.424 114.681) (end 90.424 113.792) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 88.646 144.272) (end 88.646 145.161) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 64.135 39.116) (end 64.135 38.227) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 124.841 38.227) (end 64.135 38.227) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 125.73 60.706) (end 125.73 39.116) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 116.332 61.595) (end 124.841 61.595) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 115.443 82.296) (end 115.443 62.484) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 124.841 83.185) (end 116.332 83.185) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 125.73 112.903) (end 125.73 84.074) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 90.424 113.792) (end 124.841 113.792) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 89.535 144.272) (end 89.535 114.681) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 64.135 145.161) (end 88.646 145.161) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 63.246 39.116) (end 63.246 144.272) (layer Edge.Cuts) (width 0.05))
  (zone (net 4) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.127)
    (fill yes (arc_segments 32) (thermal_gap 0.25) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 125.73 61.595) (xy 115.443 61.595) (xy 115.443 83.185) (xy 125.73 83.185) (xy 125.73 113.792)
        (xy 89.535 113.792) (xy 89.535 145.161) (xy 63.246 145.161) (xy 63.246 38.227) (xy 125.73 38.227)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 107.061 66.802) (xy 99.441 66.802) (xy 97.155 69.088) (xy 97.155 82.296) (xy 82.169 82.296)
        (xy 82.169 41.021) (xy 107.061 41.021)
      )
    )
  )
  (zone (net 4) (net_name GND) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.127)
    (fill yes (arc_segments 32) (thermal_gap 0.25) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 125.73 61.595) (xy 115.443 61.595) (xy 115.443 83.185) (xy 125.73 83.185) (xy 125.73 113.792)
        (xy 89.535 113.792) (xy 89.535 145.161) (xy 63.246 145.161) (xy 63.246 38.227) (xy 125.73 38.227)
      )
    )
  )
  (zone (net 4) (net_name GND) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.127)
    (fill yes (arc_segments 32) (thermal_gap 0.25) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 125.73 61.595) (xy 115.443 61.595) (xy 115.443 83.185) (xy 125.73 83.185) (xy 125.73 113.792)
        (xy 89.535 113.792) (xy 89.535 145.161) (xy 63.246 145.161) (xy 63.246 38.227) (xy 125.73 38.227)
      )
    )
  )
  (zone (net 4) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.127)
    (fill yes (arc_segments 32) (thermal_gap 0.25) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 125.73 61.595) (xy 115.443 61.595) (xy 115.443 83.185) (xy 125.73 83.185) (xy 125.73 113.792)
        (xy 89.535 113.792) (xy 89.535 145.161) (xy 63.246 145.161) (xy 63.246 38.227) (xy 125.73 38.227)
      )
    )
  )
)
