(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 16)
    (no_connects 16)
    (area 165.124429 102.908404 200.866829 137.193325)
    (thickness 1.6002)
    (drawings 17)
    (tracks 58)
    (zones 0)
    (modules 5)
    (nets 15)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.1524)
    (user_trace_width 0.2)
    (user_trace_width 0.25)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (user_trace_width 0.8)
    (trace_clearance 0.254)
    (zone_clearance 0.1524)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.127)
    (edge_width 0.127)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.127)
    (pcb_text_size 0.6 0.6)
    (mod_edge_width 0.127)
    (mod_text_size 0.6 0.6)
    (mod_text_width 0.127)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.05)
    (pad_to_paste_clearance -0.04)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x3ffff_80000001)
      (usegerberextensions true)
      (usegerberattributes true)
      (excludeedgelayer true)
      (linewidth 0.127000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory CAM/))
  )
  (net 0 "")
  (net 1 "Net-(JN1-Pad1)")
  (net 2 "Net-(JN1-Pad2)")
  (net 3 "Net-(JN1-Pad3)")
  (net 4 "Net-(JN1-Pad4)")
  (net 5 "Net-(JN1-Pad5)")
  (net 6 "Net-(JN1-Pad6)")
  (net 7 "Net-(JN1-Pad7)")
  (net 8 "Net-(JN1-Pad8)")
  (net 9 "Net-(JN1-Pad9)")
  (net 10 "Net-(JN1-Pad10)")
  (net 11 "Net-(JN1-Pad11)")
  (net 12 "Net-(JN1-Pad12)")
  (net 13 "Net-(JR1-Pad1)")
  (net 14 "Net-(N1-PadPR)")
  (net_class Default "Imperial - this is the standard class"
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net "Net-(JN1-Pad1)")
    (add_net "Net-(JN1-Pad10)")
    (add_net "Net-(JN1-Pad11)")
    (add_net "Net-(JN1-Pad12)")
    (add_net "Net-(JN1-Pad2)")
    (add_net "Net-(JN1-Pad3)")
    (add_net "Net-(JN1-Pad4)")
    (add_net "Net-(JN1-Pad5)")
    (add_net "Net-(JN1-Pad6)")
    (add_net "Net-(JN1-Pad7)")
    (add_net "Net-(JN1-Pad8)")
    (add_net "Net-(JN1-Pad9)")
    (add_net "Net-(JR1-Pad1)")
    (add_net "Net-(N1-PadPR)")
  )
  (net_class 0.2mm ""
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
  )
  (net_class Minimal ""
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 168.99793 114.269824 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0 -1.7 180) (layer F.SilkS))
    (fp_text value R (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(JR1-Pad1)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(JN1-Pad12)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module logos:mermaid_l (layer F.Cu) (tedit 0)
    (at 193.17496 132.09315)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module SparkFun-Connectors:SparkFun-Connectors-1X12_NO_SILK (layer F.Cu) (tedit 59737949)
    (at 195.66793 105.379824 180)
    (descr "PLATED THROUGH HOLE -12 PIN NO SILK")
    (tags "PLATED THROUGH HOLE -12 PIN NO SILK")
    (attr virtual)
    (fp_text reference JN1 (at -4.10307 -0.157176 180) (layer F.SilkS) hide)
    (fp_text value nixie (at 0.5588 1.7272 180) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 1 "Net-(JN1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 2 "Net-(JN1-Pad2)"))
    (pad 3 thru_hole circle (at 5.08 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 3 "Net-(JN1-Pad3)"))
    (pad 4 thru_hole circle (at 7.62 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 4 "Net-(JN1-Pad4)"))
    (pad 5 thru_hole circle (at 10.16 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 5 "Net-(JN1-Pad5)"))
    (pad 6 thru_hole circle (at 12.7 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 6 "Net-(JN1-Pad6)"))
    (pad 7 thru_hole circle (at 15.24 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 7 "Net-(JN1-Pad7)"))
    (pad 8 thru_hole circle (at 17.78 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 8 "Net-(JN1-Pad8)"))
    (pad 9 thru_hole circle (at 20.32 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 9 "Net-(JN1-Pad9)"))
    (pad 10 thru_hole circle (at 22.86 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 10 "Net-(JN1-Pad10)"))
    (pad 11 thru_hole circle (at 25.4 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 11 "Net-(JN1-Pad11)"))
    (pad 12 thru_hole circle (at 27.94 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 12 "Net-(JN1-Pad12)"))
  )
  (module SparkFun-Connectors:SparkFun-Connectors-1X02_NO_SILK (layer F.Cu) (tedit 59737923)
    (at 170.26793 110.459824 180)
    (descr "PLATED THROUGH HOLE - NO SILK OUTLINE")
    (tags "PLATED THROUGH HOLE - NO SILK OUTLINE")
    (attr virtual)
    (fp_text reference JR1 (at 0.254 -1.7018 180) (layer F.SilkS) hide)
    (fp_text value jumper (at 1.23093 -1.554176 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 13 "Net-(JR1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 12 "Net-(JN1-Pad12)"))
  )
  (module mynixies:mynixies-ZM1000-DSUB (layer F.Cu) (tedit 59780A39)
    (at 181.737 121.89968)
    (attr virtual)
    (fp_text reference N1 (at 0 0) (layer F.SilkS) hide)
    (fp_text value NX1 (at -9.144 9.16432) (layer F.SilkS))
    (pad 0 thru_hole circle (at -1.27 0.39878) (size 2.09804 2.09804) (drill 1.39954) (layers *.Cu *.Paste *.Mask)
      (net 11 "Net-(JN1-Pad11)"))
    (pad 1 thru_hole circle (at 1.27 5.47878) (size 2.09804 2.09804) (drill 1.39954) (layers *.Cu *.Paste *.Mask)
      (net 2 "Net-(JN1-Pad2)"))
    (pad 2 thru_hole circle (at 1.27 2.93878) (size 2.09804 2.09804) (drill 1.39954) (layers *.Cu *.Paste *.Mask)
      (net 3 "Net-(JN1-Pad3)"))
    (pad 3 thru_hole circle (at 1.27 0.39878) (size 2.09804 2.09804) (drill 1.39954) (layers *.Cu *.Paste *.Mask)
      (net 4 "Net-(JN1-Pad4)"))
    (pad 4 thru_hole circle (at 1.27 -2.13868) (size 2.09804 2.09804) (drill 1.39954) (layers *.Cu *.Paste *.Mask)
      (net 5 "Net-(JN1-Pad5)"))
    (pad 5 thru_hole circle (at 1.27 -4.67868) (size 2.09804 2.09804) (drill 1.39954) (layers *.Cu *.Paste *.Mask)
      (net 6 "Net-(JN1-Pad6)"))
    (pad 6 thru_hole circle (at -1.27 -4.67868) (size 2.09804 2.09804) (drill 1.39954) (layers *.Cu *.Paste *.Mask)
      (net 7 "Net-(JN1-Pad7)"))
    (pad 7 thru_hole circle (at -1.27 -2.13868) (size 2.09804 2.09804) (drill 1.39954) (layers *.Cu *.Paste *.Mask)
      (net 8 "Net-(JN1-Pad8)"))
    (pad 8 thru_hole circle (at -1.27 5.47878) (size 2.09804 2.09804) (drill 1.39954) (layers *.Cu *.Paste *.Mask)
      (net 9 "Net-(JN1-Pad9)"))
    (pad 9 thru_hole circle (at -1.27 2.93878) (size 2.09804 2.09804) (drill 1.39954) (layers *.Cu *.Paste *.Mask)
      (net 10 "Net-(JN1-Pad10)"))
    (pad A1 thru_hole circle (at 3.81 -2.13868) (size 2.09804 2.09804) (drill 1.39954) (layers *.Cu *.Paste *.Mask)
      (net 13 "Net-(JR1-Pad1)"))
    (pad A2 thru_hole circle (at -3.81 -2.13868) (size 2.09804 2.09804) (drill 1.39954) (layers *.Cu *.Paste *.Mask)
      (net 13 "Net-(JR1-Pad1)"))
    (pad PL thru_hole circle (at -3.81 0.39878) (size 2.09804 2.09804) (drill 1.39954) (layers *.Cu *.Paste *.Mask)
      (net 1 "Net-(JN1-Pad1)"))
    (pad PR thru_hole circle (at 3.81 0.39878) (size 2.09804 2.09804) (drill 1.39954) (layers *.Cu *.Paste *.Mask)
      (net 14 "Net-(N1-PadPR)"))
  )
  (gr_text DL (at 195.58 107.442) (layer F.SilkS))
  (gr_text 1 (at 193.103695 107.430229) (layer F.SilkS))
  (gr_text 2 (at 190.563695 107.430229) (layer F.SilkS))
  (gr_text 3 (at 188.023695 107.430229) (layer F.SilkS))
  (gr_text 4 (at 185.483695 107.430229) (layer F.SilkS))
  (gr_text 5 (at 182.943695 107.430229) (layer F.SilkS))
  (gr_text 6 (at 180.403695 107.430229) (layer F.SilkS))
  (gr_text 7 (at 177.863695 107.430229) (layer F.SilkS))
  (gr_text 8 (at 175.323695 107.430229) (layer F.SilkS))
  (gr_text 9 (at 172.783695 107.430229) (layer F.SilkS))
  (gr_text 0 (at 170.243695 107.430229) (layer F.SilkS))
  (gr_text A (at 167.72793 107.284824) (layer F.SilkS))
  (gr_line (start 198.20793 104.109824) (end 198.20793 137.129824) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 165.18793 137.129824) (end 165.18793 104.109824) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 198.20793 137.129824) (end 165.18793 137.129824) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 165.18793 104.109824) (end 198.20793 104.109824) (layer Edge.Cuts) (width 0.127))
  (gr_text nixies.us (at 196.34996 132.09315 90) (layer F.Mask))
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 190.63496 127.64815) (xy 190.63496 136.53815) (xy 197.61996 136.53815) (xy 197.61996 127.64815)
      )
    )
  )
)
