(kicad_pcb (version 4) (host pcbnew 4.0.7-e2-6376~58~ubuntu17.04.1)
  (general
    (links 60)
    (no_connects 0)
    (area 82.474999 69.139999 130.885001 117.550001)
    (thickness 1.6)
    (drawings 55)
    (tracks 143)
    (zones 0)
    (modules 35)
    (nets 25)
  )
  (page A4)
  (layers
    (0 F.Cu signal hide)
    (31 B.Cu signal hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.508)
    (trace_clearance 0.254)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.254)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.762)
    (via_drill 0.3048)
    (via_min_size 0.762)
    (via_min_drill 0.3048)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2 2)
    (pad_drill 1)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFCE69)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask true)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory grbr/))
  )
  (net 0 "")
  (net 1 IN)
  (net 2 "Net-(C1-Pad2)")
  (net 3 "Net-(C2-Pad2)")
  (net 4 "Net-(C3-Pad1)")
  (net 5 "Net-(C3-Pad2)")
  (net 6 +9V)
  (net 7 GND)
  (net 8 "Net-(C5-Pad1)")
  (net 9 "Net-(C6-Pad1)")
  (net 10 "Net-(C6-Pad2)")
  (net 11 "Net-(C7-Pad2)")
  (net 12 "Net-(C8-Pad2)")
  (net 13 "Net-(D1-Pad2)")
  (net 14 "Net-(IO1-Pad-)")
  (net 15 "Net-(IO1-Pad+)")
  (net 16 OUT)
  (net 17 "Net-(POT1-Pad1)")
  (net 18 "Net-(POT1-Pad3)")
  (net 19 "Net-(POT2-Pad2)")
  (net 20 "Net-(Q1-Pad1)")
  (net 21 "Net-(Q2-Pad1)")
  (net 22 "Net-(Q2-Pad3)")
  (net 23 "Net-(Q3-Pad3)")
  (net 24 "Net-(POT2-Pad1)")
  (net_class Default "Ceci est la Netclass par défaut"
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.762)
    (via_drill 0.3048)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +9V)
    (add_net GND)
    (add_net IN)
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C6-Pad2)")
    (add_net "Net-(C7-Pad2)")
    (add_net "Net-(C8-Pad2)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(IO1-Pad+)")
    (add_net "Net-(IO1-Pad-)")
    (add_net "Net-(POT1-Pad1)")
    (add_net "Net-(POT1-Pad3)")
    (add_net "Net-(POT2-Pad1)")
    (add_net "Net-(POT2-Pad2)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(Q2-Pad1)")
    (add_net "Net-(Q2-Pad3)")
    (add_net "Net-(Q3-Pad3)")
    (add_net OUT)
  )
  (module transistors-BJT:TO92 (layer F.Cu) (tedit 5B26A999)
    (at 123.19 90.805 90)
    (fp_text reference Q4 (at -3.937 1.016 180) (layer F.SilkS))
    (fp_text value B109C (at 0 0 90) (layer F.SilkS) hide)
    (fp_text user E (at -2.54 -1.397 180) (layer F.SilkS))
    (fp_text user C (at 2.54 -1.397 180) (layer F.SilkS))
    (fp_text user B (at 0 -1.397 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at -2.54 0 270) (size 1.9304 1.9304) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(C6-Pad1)"))
    (pad 2 thru_hole circle (at 0 0 270) (size 1.9304 1.9304) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(Q3-Pad3)"))
    (pad 3 thru_hole circle (at 2.54 0 270) (size 1.9304 1.9304) (drill 1) (layers *.Cu *.Mask)
      (net 6 +9V))
  )
  (module transistors-BJT:TO92 (layer F.Cu) (tedit 5B26A98F)
    (at 118.745 90.805 270)
    (fp_text reference Q3 (at 3.937 -1.016 360) (layer F.SilkS))
    (fp_text value B109C (at 0 0 270) (layer F.SilkS) hide)
    (fp_text user E (at -2.54 -1.397 360) (layer F.SilkS))
    (fp_text user C (at 2.54 -1.397 360) (layer F.SilkS))
    (fp_text user B (at 0 -1.397 360) (layer F.SilkS))
    (pad 1 thru_hole rect (at -2.54 0 90) (size 1.9304 1.9304) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(POT1-Pad3)"))
    (pad 2 thru_hole circle (at 0 0 90) (size 1.9304 1.9304) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(Q2-Pad3)"))
    (pad 3 thru_hole circle (at 2.54 0 90) (size 1.9304 1.9304) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(Q3-Pad3)"))
  )
  (module transistors-BJT:TO92 (layer F.Cu) (tedit 5B26A983)
    (at 107.315 90.805 90)
    (fp_text reference Q2 (at -3.937 1.016 180) (layer F.SilkS))
    (fp_text value B109C (at 0 0 90) (layer F.SilkS) hide)
    (fp_text user C (at 2.54 -1.27 180) (layer F.SilkS))
    (fp_text user E (at -2.54 -1.27 180) (layer F.SilkS))
    (fp_text user B (at 0 -1.27 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at -2.54 0 270) (size 1.9304 1.9304) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(Q2-Pad1)"))
    (pad 2 thru_hole circle (at 0 0 270) (size 1.9304 1.9304) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(C3-Pad2)"))
    (pad 3 thru_hole circle (at 2.54 0 270) (size 1.9304 1.9304) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(Q2-Pad3)"))
  )
  (module transistors-BJT:TO92 (layer F.Cu) (tedit 5B26A977)
    (at 92.71 90.805 90)
    (fp_text reference Q1 (at -3.937 1.016 180) (layer F.SilkS))
    (fp_text value B109C (at 0 0 90) (layer F.SilkS) hide)
    (fp_text user C (at 2.54 -1.27 180) (layer F.SilkS))
    (fp_text user E (at -2.54 -1.27 180) (layer F.SilkS))
    (fp_text user B (at 0 -1.27 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at -2.54 0 270) (size 1.9304 1.9304) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(Q1-Pad1)"))
    (pad 2 thru_hole circle (at 0 0 270) (size 1.9304 1.9304) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad2)"))
    (pad 3 thru_hole circle (at 2.54 0 270) (size 1.9304 1.9304) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(C3-Pad1)"))
  )
  (module potentiometers:16MM_B.MOUNT (layer F.Cu) (tedit 5A391D9E)
    (at 122.555 71.755 180)
    (descr "<b>16mm / Right-Angle /  PC Mount / Short Pin</b>\n<p>\nFor bottom-mount potentiometers\n<p>\n<a href=\"http://smallbear-electronics.mybigcommerce.com/alpha-single-gang-16mm-right-angle-pc-mount/\">http://smallbear-electronics.mybigcommerce.com/alpha-single-gang-16mm-right-angle-pc-mount/</a>")
    (fp_text reference POT2 (at 0 -2.413 180) (layer B.SilkS) hide)
    (fp_text value "SPARKLE B50K" (at 0 -2.3495 180) (layer B.SilkS))
    (fp_text user 1 (at 6.35 -2.159 180) (layer B.SilkS))
    (pad 1 thru_hole rect (at 5.08 0) (size 2.54 2.54) (drill 1.4) (layers *.Cu *.Mask)
      (net 24 "Net-(POT2-Pad1)"))
    (pad 2 thru_hole circle (at 0 0) (size 2.54 2.54) (drill 1.4) (layers *.Cu *.Mask)
      (net 19 "Net-(POT2-Pad2)"))
    (pad 3 thru_hole circle (at -5.08 0) (size 2.54 2.54) (drill 1.4) (layers *.Cu *.Mask)
      (net 11 "Net-(C7-Pad2)"))
  )
  (module potentiometers:16MM_B.MOUNT (layer F.Cu) (tedit 5B26A9DD)
    (at 90.805 71.755 180)
    (descr "<b>16mm / Right-Angle /  PC Mount / Short Pin</b>\n<p>\nFor bottom-mount potentiometers\n<p>\n<a href=\"http://smallbear-electronics.mybigcommerce.com/alpha-single-gang-16mm-right-angle-pc-mount/\">http://smallbear-electronics.mybigcommerce.com/alpha-single-gang-16mm-right-angle-pc-mount/</a>")
    (fp_text reference POT1 (at 0 -2.413 180) (layer B.SilkS) hide)
    (fp_text value "ABUSE C1K" (at 0 -2.3495 180) (layer B.SilkS))
    (fp_text user 1 (at 6.35 -2.159 180) (layer B.SilkS))
    (pad 1 thru_hole rect (at 5.08 0) (size 2.54 2.54) (drill 1.4) (layers *.Cu *.Mask)
      (net 17 "Net-(POT1-Pad1)"))
    (pad 2 thru_hole circle (at 0 0) (size 2.54 2.54) (drill 1.4) (layers *.Cu *.Mask)
      (net 8 "Net-(C5-Pad1)"))
    (pad 3 thru_hole circle (at -5.08 0) (size 2.54 2.54) (drill 1.4) (layers *.Cu *.Mask)
      (net 18 "Net-(POT1-Pad3)"))
  )
  (module potentiometers:16MM_B.MOUNT (layer F.Cu) (tedit 5A391D97)
    (at 107.95 104.775 270)
    (descr "<b>16mm / Right-Angle /  PC Mount / Short Pin</b>\n<p>\nFor bottom-mount potentiometers\n<p>\n<a href=\"http://smallbear-electronics.mybigcommerce.com/alpha-single-gang-16mm-right-angle-pc-mount/\">http://smallbear-electronics.mybigcommerce.com/alpha-single-gang-16mm-right-angle-pc-mount/</a>")
    (fp_text reference POT3 (at 0 -2.413 270) (layer B.SilkS) hide)
    (fp_text value "VOL A100K" (at 0 -2.3495 270) (layer B.SilkS))
    (fp_text user 1 (at 6.35 -2.159 270) (layer B.SilkS))
    (pad 1 thru_hole rect (at 5.08 0 90) (size 2.54 2.54) (drill 1.4) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 2 thru_hole circle (at 0 0 90) (size 2.54 2.54) (drill 1.4) (layers *.Cu *.Mask)
      (net 16 OUT))
    (pad 3 thru_hole circle (at -5.08 0 90) (size 2.54 2.54) (drill 1.4) (layers *.Cu *.Mask)
      (net 19 "Net-(POT2-Pad2)"))
  )
  (module jacks:DC_TS (layer B.Cu) (tedit 5A391CD2)
    (at 106.68 76.835 180)
    (fp_text reference DC1 (at 0 1.905 180) (layer F.SilkS) hide)
    (fp_text value DC (at 0 1.905 180) (layer F.SilkS))
    (fp_text user DC (at 0 1.905 180) (layer B.SilkS))
    (fp_text user + (at -2.032 1.905 180) (layer B.SilkS))
    (fp_text user + (at -2.032 1.905 180) (layer F.SilkS))
    (fp_text user - (at 2.032 1.905 180) (layer F.SilkS))
    (fp_text user - (at 2.032 1.905 180) (layer B.SilkS))
    (pad 2 thru_hole oval (at 1.27 0 180) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 1 thru_hole rect (at -1.27 0 180) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 13 "Net-(D1-Pad2)"))
  )
  (module potentiometers:TRIM1 (layer F.Cu) (tedit 5B26A958)
    (at 89.535 80.645)
    (descr "<b>Bourns 3362p</b>\n<p>\n<a href=\"http://www.taydaelectronics.com/potentiometer-variable-resistors/cermet-potentiometers/3362p.html\">http://www.taydaelectronics.com/potentiometer-variable-resistors/cermet-potentiometers/3362p.html</a>")
    (fp_text reference TRIM1 (at 0 2.794) (layer F.SilkS))
    (fp_text value 5K (at 0 2.7305) (layer F.SilkS) hide)
    (fp_text user 1 (at -3.302 -2.159) (layer F.SilkS))
    (pad 3 thru_hole circle (at 2.54 2.54) (size 1.9304 1.9304) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(POT1-Pad1)"))
    (pad 1 thru_hole oval (at -2.54 2.54) (size 1.9304 1.9304) (drill 1) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 1 thru_hole oval (at -2.54 0) (size 1.9304 1.9304) (drill 1) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 2 thru_hole circle (at 0 -2.54) (size 1.9304 1.9304) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(POT1-Pad1)"))
    (pad 3 thru_hole circle (at 2.54 0) (size 1.9304 1.9304) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(POT1-Pad1)"))
  )
  (module caps-elec:0502 (layer F.Cu) (tedit 5994B2B9)
    (at 114.3 104.775 90)
    (descr "0.1\" (2.54mm) spacing")
    (fp_text reference C1 (at 0 1.778 90) (layer F.SilkS))
    (fp_text value 10µ (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0 90) (size 1.9304 1.9304) (drill 1) (layers *.Cu *.Mask)
      (net 1 IN))
    (pad 2 thru_hole circle (at 1.27 0 90) (size 1.9304 1.9304) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad2)"))
  )
  (module caps-film:0.2_22.SML (layer F.Cu) (tedit 59787A64)
    (at 103.505 106.045 90)
    (descr "0.2\" (5.08mm) spacing\n<p>\n<b> \n10pf - 180n</b>")
    (fp_text reference C2 (at 0 0 90) (layer F.SilkS))
    (fp_text value 10n (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -2.54 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 IN))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad2)"))
  )
  (module caps-film:0.2_22.SML (layer F.Cu) (tedit 59787A64)
    (at 97.155 92.075 270)
    (descr "0.2\" (5.08mm) spacing\n<p>\n<b> \n10pf - 180n</b>")
    (fp_text reference C3 (at 0 0 270) (layer F.SilkS))
    (fp_text value 100n (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -2.54 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(C3-Pad2)"))
  )
  (module caps-elec:0502 (layer F.Cu) (tedit 5A356BD4)
    (at 105.41 81.915 90)
    (descr "0.1\" (2.54mm) spacing")
    (fp_text reference C4 (at 0 1.778 90) (layer F.SilkS))
    (fp_text value 47µ (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0 90) (size 1.9304 1.9304) (drill 1) (layers *.Cu *.Mask)
      (net 6 +9V))
    (pad 2 thru_hole oval (at 1.27 0 90) (size 1.9304 1.9304) (drill 1) (layers *.Cu *.Mask)
      (net 7 GND))
  )
  (module caps-elec:0502 (layer F.Cu) (tedit 5A356BD9)
    (at 97.79 81.915 270)
    (descr "0.1\" (2.54mm) spacing")
    (fp_text reference C5 (at 0 1.778 270) (layer F.SilkS))
    (fp_text value 4µ7 (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0 270) (size 1.9304 1.9304) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(C5-Pad1)"))
    (pad 2 thru_hole oval (at 1.27 0 270) (size 1.9304 1.9304) (drill 1) (layers *.Cu *.Mask)
      (net 7 GND))
  )
  (module caps-film:0.2_22.SML (layer F.Cu) (tedit 59787A64)
    (at 127.635 92.075 90)
    (descr "0.2\" (5.08mm) spacing\n<p>\n<b> \n10pf - 180n</b>")
    (fp_text reference C6 (at 0 0 90) (layer F.SilkS))
    (fp_text value 100n (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -2.54 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(C6-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(C6-Pad2)"))
  )
  (module caps-film:0.2_22.SML (layer F.Cu) (tedit 5A356BCE)
    (at 124.46 78.74 90)
    (descr "0.2\" (5.08mm) spacing\n<p>\n<b> \n10pf - 180n</b>")
    (fp_text reference C7 (at 0 0 90) (layer F.SilkS))
    (fp_text value 8n2 (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 thru_hole oval (at -2.54 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(C7-Pad2)"))
  )
  (module caps-film:0.2_22.SML (layer F.Cu) (tedit 5A356BC8)
    (at 127.635 78.74 90)
    (descr "0.2\" (5.08mm) spacing\n<p>\n<b> \n10pf - 180n</b>")
    (fp_text reference C8 (at 0 0 90) (layer F.SilkS))
    (fp_text value 100n (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 thru_hole oval (at -2.54 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(C8-Pad2)"))
  )
  (module diodes:DO41-3 (layer F.Cu) (tedit 5978792E)
    (at 111.125 80.01 90)
    (descr "<b>DO-41 0.3\" pad spacing</b>")
    (fp_text reference D1 (at 0.3175 0 90) (layer F.SilkS))
    (fp_text value 1N5817 (at 0 0 90) (layer F.SilkS) hide)
    (pad 2 thru_hole oval (at 3.81 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(D1-Pad2)"))
    (pad 1 thru_hole rect (at -3.81 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 6 +9V))
  )
  (module supply_pins:IO.2 (layer F.Cu) (tedit 5A356C0A)
    (at 106.68 114.3)
    (fp_text reference IO1 (at 0 0) (layer F.SilkS) hide)
    (fp_text value Supply_Pins (at 0 0) (layer F.SilkS) hide)
    (fp_text user GND (at -6.35 1.905) (layer F.SilkS))
    (fp_text user IN (at 3.81 1.905) (layer F.SilkS))
    (fp_text user OUT (at 6.35 1.905) (layer F.SilkS))
    (fp_text user + (at -1.905 1.905) (layer F.SilkS))
    (fp_text user - (at 1.905 1.905) (layer F.SilkS))
    (fp_text user L (at -3.81 1.905) (layer B.SilkS))
    (fp_text user GND (at -6.35 1.905) (layer B.SilkS))
    (fp_text user IN (at 3.81 1.905) (layer B.SilkS))
    (fp_text user OUT (at 6.35 1.905) (layer B.SilkS))
    (fp_text user + (at -1.905 1.905) (layer B.SilkS))
    (fp_text user - (at 1.905 1.905) (layer B.SilkS))
    (fp_text user LED (at 0 2.0955) (layer B.SilkS))
    (fp_text user L (at -3.81 1.905) (layer F.SilkS))
    (fp_text user LED (at 0 2.0955) (layer F.SilkS))
    (pad G thru_hole oval (at -6.35 0) (size 2.1844 2.1844) (drill 1.2) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad SW thru_hole circle (at -3.81 0) (size 2.1844 2.1844) (drill 1.2) (layers *.Cu *.Mask)
      (net 14 "Net-(IO1-Pad-)"))
    (pad + thru_hole rect (at -1.27 0) (size 2.1844 2.1844) (drill 1.2) (layers *.Cu *.Mask)
      (net 15 "Net-(IO1-Pad+)"))
    (pad IN thru_hole rect (at 3.81 0) (size 2.1844 2.1844) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 IN))
    (pad OUT thru_hole rect (at 6.35 0) (size 2.1844 2.1844) (drill 1.2) (layers *.Cu *.Mask)
      (net 16 OUT))
    (pad - thru_hole circle (at 1.27 0) (size 2.1844 2.1844) (drill 1.2) (layers *.Cu *.Mask)
      (net 14 "Net-(IO1-Pad-)"))
  )
  (module resistors:0.3_22.B (layer F.Cu) (tedit 5A356BF9)
    (at 118.745 104.775 90)
    (descr "0.3\"  (7.62mm) lead spacing, 1/4W (flat)")
    (fp_text reference R1 (at 0 0 90) (layer F.SilkS))
    (fp_text value 1M (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -3.81 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 IN))
    (pad 2 thru_hole oval (at 3.81 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 7 GND))
  )
  (module resistors:0.3_22.B (layer F.Cu) (tedit 59787A05)
    (at 88.9 90.805 270)
    (descr "0.3\"  (7.62mm) lead spacing, 1/4W (flat)")
    (fp_text reference R2 (at 0 0 270) (layer F.SilkS))
    (fp_text value 150k (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -3.81 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 6 +9V))
    (pad 2 thru_hole circle (at 3.81 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad2)"))
  )
  (module resistors:0.3_22.B (layer F.Cu) (tedit 5A356BF1)
    (at 99.695 104.775 270)
    (descr "0.3\"  (7.62mm) lead spacing, 1/4W (flat)")
    (fp_text reference R3 (at 0 0 270) (layer F.SilkS))
    (fp_text value 22k (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -3.81 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad2)"))
    (pad 2 thru_hole oval (at 3.81 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 7 GND))
  )
  (module resistors:0.3_22.B (layer F.Cu) (tedit 59787A05)
    (at 85.725 90.805 270)
    (descr "0.3\"  (7.62mm) lead spacing, 1/4W (flat)")
    (fp_text reference R4 (at 0 0 270) (layer F.SilkS))
    (fp_text value 10k (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -3.81 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 6 +9V))
    (pad 2 thru_hole circle (at 3.81 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(C3-Pad1)"))
  )
  (module resistors:0.3_22.B (layer F.Cu) (tedit 5A356BED)
    (at 95.885 104.775 270)
    (descr "0.3\"  (7.62mm) lead spacing, 1/4W (flat)")
    (fp_text reference R5 (at 0 0 270) (layer F.SilkS))
    (fp_text value 1k (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -3.81 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(Q1-Pad1)"))
    (pad 2 thru_hole oval (at 3.81 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 7 GND))
  )
  (module resistors:0.3_22.B (layer F.Cu) (tedit 59787A05)
    (at 100.33 90.805 270)
    (descr "0.3\"  (7.62mm) lead spacing, 1/4W (flat)")
    (fp_text reference R6 (at 0 0 270) (layer F.SilkS))
    (fp_text value 10k (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -3.81 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 6 +9V))
    (pad 2 thru_hole circle (at 3.81 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(Q2-Pad3)"))
  )
  (module resistors:0.3_22.B (layer F.Cu) (tedit 5A356BE6)
    (at 103.505 90.805 90)
    (descr "0.3\"  (7.62mm) lead spacing, 1/4W (flat)")
    (fp_text reference R7 (at 0 0 90) (layer F.SilkS))
    (fp_text value 100R (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -3.81 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(Q2-Pad1)"))
    (pad 2 thru_hole oval (at 3.81 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 7 GND))
  )
  (module resistors:0.3_22.B (layer F.Cu) (tedit 59787A05)
    (at 111.76 90.805 90)
    (descr "0.3\"  (7.62mm) lead spacing, 1/4W (flat)")
    (fp_text reference R8 (at 0 0 90) (layer F.SilkS))
    (fp_text value 47k (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -3.81 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(C3-Pad2)"))
    (pad 2 thru_hole circle (at 3.81 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(POT1-Pad3)"))
  )
  (module resistors:0.3_22.B (layer F.Cu) (tedit 59787A05)
    (at 114.935 90.805 270)
    (descr "0.3\"  (7.62mm) lead spacing, 1/4W (flat)")
    (fp_text reference R9 (at 0 0 270) (layer F.SilkS))
    (fp_text value 10k (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -3.81 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 6 +9V))
    (pad 2 thru_hole circle (at 3.81 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(Q3-Pad3)"))
  )
  (module resistors:0.3_22.B (layer F.Cu) (tedit 5A356BFE)
    (at 127.635 104.775 270)
    (descr "0.3\"  (7.62mm) lead spacing, 1/4W (flat)")
    (fp_text reference R10 (at 0 0 270) (layer F.SilkS))
    (fp_text value 10k (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -3.81 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(C6-Pad1)"))
    (pad 2 thru_hole oval (at 3.81 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 7 GND))
  )
  (module resistors:0.3_22.B (layer F.Cu) (tedit 59787A05)
    (at 121.285 80.01 90)
    (descr "0.3\"  (7.62mm) lead spacing, 1/4W (flat)")
    (fp_text reference R11 (at 0 0 90) (layer F.SilkS))
    (fp_text value 10k (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -3.81 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(C6-Pad2)"))
    (pad 2 thru_hole circle (at 3.81 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(C7-Pad2)"))
  )
  (module resistors:0.3_22.B (layer F.Cu) (tedit 59787A05)
    (at 114.935 80.01 270)
    (descr "0.3\"  (7.62mm) lead spacing, 1/4W (flat)")
    (fp_text reference R12 (at 0 0 270) (layer F.SilkS))
    (fp_text value 10k (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -3.81 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(POT2-Pad1)"))
    (pad 2 thru_hole circle (at 3.81 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(C6-Pad2)"))
  )
  (module resistors:0.3_22.B (layer F.Cu) (tedit 59787A05)
    (at 118.11 80.01 90)
    (descr "0.3\"  (7.62mm) lead spacing, 1/4W (flat)")
    (fp_text reference R13 (at 0 0 90) (layer F.SilkS))
    (fp_text value 2k2 (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -3.81 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(C8-Pad2)"))
    (pad 2 thru_hole circle (at 3.81 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(POT2-Pad1)"))
  )
  (module resistors:0.3_22.B (layer F.Cu) (tedit 5A358650)
    (at 123.19 104.775 90)
    (descr "0.3\"  (7.62mm) lead spacing, 1/4W (flat)")
    (fp_text reference R14 (at 0 0 90) (layer F.SilkS))
    (fp_text value 100k (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -3.81 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 16 OUT))
    (pad 2 thru_hole oval (at 3.81 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 7 GND))
  )
  (module resistors:0.3_22.B (layer F.Cu) (tedit 59787A05)
    (at 85.725 104.775 270)
    (descr "0.3\"  (7.62mm) lead spacing, 1/4W (flat)")
    (fp_text reference R15 (at 0 0 270) (layer F.SilkS))
    (fp_text value CLR (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -3.81 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 6 +9V))
    (pad 2 thru_hole circle (at 3.81 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(IO1-Pad+)"))
  )
  (module switches:SPDT.LUGS (layer F.Cu) (tedit 5A391D8D)
    (at 90.805 104.775 180)
    (descr "<b>Toggle Switch, Solder Lugs</b>\n<br>\nTaiway 1MS1T1B1C0M1QE: <a href=\"http://smallbear-electronics.mybigcommerce.com/spdt-on-on/\">http://smallbear-electronics.mybigcommerce.com/spdt-on-on/</a>")
    (fp_text reference SW1 (at -3.048 0 270) (layer B.SilkS) hide)
    (fp_text value Fat/Thin (at -3.175 0 270) (layer B.SilkS))
    (fp_text user SOLDER (at 2.032 0 270) (layer F.SilkS))
    (fp_text user SWITCH (at 2.032 0 450) (layer B.SilkS))
    (pad 1 thru_hole rect (at 0 -4.699 180) (size 3.416 3.416) (drill 2.4) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 2 thru_hole circle (at 0 0 180) (size 3.416 3.416) (drill 2.4) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad2)"))
    (pad 3 thru_hole circle (at 0 4.699 180) (size 3.416 3.416) (drill 2.4) (layers *.Cu *.Mask))
  )
  (gr_text "Zombie Sonore \n2018.06" (at 104.521 97.79) (layer B.SilkS))
  (gr_text "For DIY use only" (at 99.771 111.125) (layer B.SilkS))
  (gr_text "rev 0.2" (at 99.06 104.775) (layer B.SilkS))
  (gr_text "Hot\nSilicon" (at 104.521 90.932) (layer B.SilkS))
  (gr_text "For DIY use only" (at 117.475 110.49) (layer F.SilkS))
  (gr_text "Zombie Sonore 2018.06" (at 93.345 75.565) (layer F.SilkS))
  (gr_text "rev 0.2" (at 125.73 97.79) (layer F.SilkS))
  (gr_text "Hot Silicon" (at 116.84 97.79) (layer F.SilkS))
  (gr_line (start 99.06 72.39) (end 99.06 71.12) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 84.455 71.12) (end 82.55 71.12) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 100.33 72.39) (end 100.33 73.66) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 113.03 73.66) (end 111.76 73.66) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 114.3 71.12) (end 114.3 72.39) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 113.03 72.39) (end 114.3 72.39) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 128.905 71.12) (end 128.905 69.215) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 94.615 114.935) (end 94.615 113.03) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 118.745 114.935) (end 116.84 114.935) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 97.155 71.12) (end 97.155 69.215) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 116.205 71.12) (end 114.3 71.12) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 85.09 113.03) (end 94.615 113.03) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 99.06 114.935) (end 99.06 117.475) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 118.745 113.03) (end 128.27 113.03) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 114.3 114.935) (end 116.84 114.935) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 99.06 117.475) (end 114.3 117.475) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 128.27 110.49) (end 130.81 110.49) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 85.09 110.49) (end 85.09 113.03) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 130.81 71.12) (end 130.81 110.49) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 116.205 69.215) (end 128.905 69.215) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 100.33 73.66) (end 111.76 73.66) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 84.455 69.215) (end 97.155 69.215) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 82.55 71.12) (end 82.55 110.49) (layer Edge.Cuts) (width 0.15))
  (zone (net 7) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.508)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.51))
    (polygon
      (pts
        (xy 82.55 69.215) (xy 130.81 69.215) (xy 130.81 117.475) (xy 82.55 117.475)
      )
    )
  )
)
