<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<text>2</text>
<text>4</text>
<text>5</text>
<text>RX</text>
<text>TX</text>
<text>0</text>
<text>GND</text>
<text>RST</text>
<text>5V</text>
<text>14</text>
<text>12</text>
<text>A0</text>
<text>3V3</text>
<text>15</text>
<text>13</text>
<text>16</text>
<text>3V3</text>
<text>GND</text>
<text>SCL</text>
<text>SDA</text>
<wire x1="34.89325" y1="25.527" x2="4.445" y2="25.527" width="0.0254" layer="20"/>
<wire x1="4.445" y1="25.527" x2="4.41325" y2="25.527" width="0.0254" layer="20"/>
<wire x1="3.048" y1="24.13" x2="3.048" y2="3.1115" width="0.0254" layer="20"/>
<wire x1="3.048" y1="3.1115" x2="3.048" y2="3.048" width="0.0254" layer="20"/>
<wire x1="11.3665" y1="-0.127" x2="34.9885" y2="-0.127" width="0.0254" layer="20"/>
<wire x1="34.9885" y1="-0.127" x2="36.322" y2="1.27" width="0.0254" layer="20" curve="90"/>
<wire x1="36.322" y1="1.27" x2="36.322" y2="24.13" width="0.0254" layer="20"/>
<wire x1="36.322" y1="24.13" x2="34.89325" y2="25.527" width="0.0254" layer="20" curve="90"/>
<text>3V3</text>
<text>5V</text>
<text>SDA</text>
<text>SCL</text>
<text>Lora Node</text>
<text>DO</text>
<text>Lora
Node
V1.3</text>
<text>RFM92/95
RFM96/98</text>
<text>WS2812</text>
<text>GND</text>
<wire x1="11.3665" y1="-0.127" x2="9.4615" y2="1.778" width="0.0254" layer="20"/>
<wire x1="9.4615" y1="1.778" x2="4.3815" y2="1.778" width="0.0254" layer="20"/>
<wire x1="4.3815" y1="1.778" x2="3.048" y2="3.1115" width="0.0254" layer="20" curve="-90"/>
<wire x1="4.445" y1="25.527" x2="3.048" y2="24.13" width="0.0254" layer="20" curve="90"/>
<text>Cut Wire if you put
D1 to avoid LED pb</text>
<text>SEL</text>
<text>GPIO</text>
<text>RST</text>
<text>V1.3</text>
<text>16</text>
<text>24AA02</text>
<text>GND</text>
<text>3V3</text>
</plain>
<libraries>
<library name="_c2h">
<packages>
<package name="1X04_LOCK">
</package>
<package name="0805-RES">
</package>
<package name="LOGO_CH2I_75MM">
</package>
<package name="WS2812B">
</package>
<package name="0805-CAP">
</package>
<package name="PAD">
</package>
<package name="0805-CAP-LARGEPADS">
</package>
<package name="RFM95">
</package>
<package name="SMA_UFL_PAD_TINY">
</package>
<package name="PAD-JUMPER-3-2OF3_NC_BY_TRACE_YES_SILK_FULL_BOX">
</package>
<package name="PAD-JUMPER-SWAP">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X08_NO_SILK">
</package>
</packages>
</library>
<library name="Seeed-Discrete">
<packages>
<package name="SOD123-2.7X1.6">
</package>
</packages>
</library>
<library name="Switch-2016">
<packages>
<package name="SW4-SMD-4.2X3.2X2.5MM">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="PAD-JUMPER-2-NC_BY_TRACE_YES_SILK">
<description>Solder jumper, small, shorted with trace. No paste layer. Trace is cuttable.</description>
</package>
</packages>
</library>
<library name="Microchip-24AA02E64T">
<description>&lt;b&gt; Developed By element14 &lt;/b&gt;&lt;p&gt; 

For feedback and Technical support please contact reach from below:
&lt;br&gt; Tech Support e-mail  : &lt;a href="mailto:CAD_Tech@element14.com"&gt;CAD_Tech@element14.com&lt;/a&gt;
&lt;br&gt;Community website: &lt;a href=http://www.element14.com/community/community/knode/cadsoft_eagle/eagle_cad_libraries&gt;
EAGLE CAD Libraries on element14&lt;/a&gt;</description>
<packages>
<package name="SOT95P270X145-5N">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="R1" library="_c2h" package="0805-RES" value="4.7K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="_c2h" package="0805-RES" value="4.7K">
<attribute name="NAME"/>
</element>
<element name="I2C_OLED" library="_c2h" package="1X04_LOCK" value="CON_HEADER_1X04'LOCK'"/>
<element name="JP2" library="SparkFun-Connectors" package="1X08_NO_SILK" value="">
<attribute name="VALUE"/>
<attribute name="PROD_ID" value="CONN-08438"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="1X08_NO_SILK" value="">
<attribute name="VALUE"/>
<attribute name="PROD_ID" value="CONN-08438"/>
</element>
<element name="WS2812" library="_c2h" package="WS2812B" value="WS2812B">
<attribute name="NAME"/>
</element>
<element name="C3" library="_c2h" package="0805-CAP" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="Seeed-Discrete" package="SOD123-2.7X1.6" value="1N4148">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="P2" library="_c2h" package="PAD" value="PADNORMAL"/>
<element name="P3" library="_c2h" package="PAD" value="PADNORMAL"/>
<element name="C2" library="_c2h" package="0805-CAP-LARGEPADS" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$4" library="_c2h" package="LOGO_CH2I_75MM" value=""/>
<element name="BTN" library="Switch-2016" package="SW4-SMD-4.2X3.2X2.5MM" value="DHT-4235A">
<attribute name="MPN" value="DHT-4235A"/>
<attribute name="NAME"/>
</element>
<element name="U$5" library="_c2h" package="RFM95" value="RFM95"/>
<element name="WS1" library="_c2h" package="WS2812B" value="WS2812B"/>
<element name="C4" library="_c2h" package="0805-CAP" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP4" library="SparkFun-Passives" package="PAD-JUMPER-2-NC_BY_TRACE_YES_SILK" value="JUMPER-PAD-2-NC_BY_TRACE"/>
<element name="C1" library="_c2h" package="0805-CAP-LARGEPADS" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="P1" library="_c2h" package="PAD" value="PADNORMAL"/>
<element name="P4" library="_c2h" package="PAD" value="PADNORMAL"/>
<element name="D2" library="Seeed-Discrete" package="SOD123-2.7X1.6" value="1N4148">
<attribute name="NAME"/>
</element>
<element name="D3" library="Seeed-Discrete" package="SOD123-2.7X1.6" value="1N4148">
<attribute name="NAME"/>
</element>
<element name="D4" library="Seeed-Discrete" package="SOD123-2.7X1.6" value="1N4148">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="Microchip-24AA02E64T" package="SOT95P270X145-5N" value="24AA02E64T">
<attribute name="MPN" value="24AA02E64T-I/OT"/>
<attribute name="OC_NEWARK" value="01X0461"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="OC_FARNELL" value="2345567"/>
<attribute name="SUPPLIER" value="Microchip"/>
<attribute name="NAME"/>
</element>
<element name="J$2" library="_c2h" package="SMA_UFL_PAD_TINY" value="ANTENNATINY"/>
<element name="C5" library="_c2h" package="0805-CAP" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP3" library="_c2h" package="PAD-JUMPER-3-2OF3_NC_BY_TRACE_YES_SILK_FULL_BOX" value="DS"/>
<element name="R3" library="_c2h" package="0805-RES" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$2" library="_c2h" package="PAD-JUMPER-SWAP" value="PAD-JUMPER-SWAPSWAP"/>
</elements>
<signals>
<signal name="S$2">
</signal>
<signal name="GND">
<contactref element="JP1" pad="7"/>
<contactref element="WS2812" pad="3"/>
<contactref element="C3" pad="2"/>
<contactref element="P3" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="BTN" pad="3"/>
<contactref element="U$5" pad="GND1"/>
<contactref element="U$5" pad="GND"/>
<contactref element="U$5" pad="GND2"/>
<contactref element="WS1" pad="3"/>
<contactref element="C4" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="U1" pad="2"/>
<contactref element="J$2" pad="GND1"/>
<contactref element="J$2" pad="GND2"/>
<contactref element="J$2" pad="GND3"/>
<contactref element="J$2" pad="GND4"/>
<contactref element="C5" pad="2"/>
<contactref element="R3" pad="1"/>
<contactref element="U$2" pad="11"/>
<contactref element="U$2" pad="1"/>
</signal>
<signal name="SCL">
<contactref element="R2" pad="1"/>
<contactref element="I2C_OLED" pad="3"/>
<contactref element="JP1" pad="3"/>
<contactref element="U1" pad="1"/>
</signal>
<signal name="SDA">
<contactref element="R1" pad="1"/>
<contactref element="I2C_OLED" pad="4"/>
<contactref element="JP1" pad="4"/>
<contactref element="U1" pad="3"/>
</signal>
<signal name="GPIO14">
<contactref element="JP2" pad="4"/>
<contactref element="U$5" pad="SCK"/>
</signal>
<signal name="GPIO12">
<contactref element="JP2" pad="5"/>
<contactref element="U$5" pad="MISO"/>
</signal>
<signal name="GPIO13">
<contactref element="JP2" pad="6"/>
<contactref element="U$5" pad="MOSI"/>
</signal>
<signal name="GPIO15">
<contactref element="JP2" pad="7"/>
<contactref element="D2" pad="2"/>
<contactref element="D3" pad="2"/>
<contactref element="D4" pad="2"/>
</signal>
<signal name="3V3">
<contactref element="R2" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="JP2" pad="8"/>
<contactref element="U$5" pad="VDD"/>
<contactref element="C1" pad="2"/>
<contactref element="P4" pad="1"/>
<contactref element="U1" pad="4"/>
<contactref element="C5" pad="1"/>
<contactref element="U$2" pad="4"/>
<contactref element="U$2" pad="44"/>
</signal>
<signal name="A0">
<contactref element="JP2" pad="2"/>
</signal>
<signal name="GPIO16">
<contactref element="JP2" pad="3"/>
<contactref element="JP3" pad="2"/>
</signal>
<signal name="GPIO0">
<contactref element="JP1" pad="5"/>
<contactref element="WS2812" pad="4"/>
</signal>
<signal name="GPIO2">
<contactref element="JP1" pad="6"/>
<contactref element="BTN" pad="1"/>
</signal>
<signal name="GPIO3">
<contactref element="JP1" pad="2"/>
</signal>
<signal name="RST">
<contactref element="JP2" pad="1"/>
<contactref element="U$5" pad="RST"/>
<contactref element="JP3" pad="1"/>
</signal>
<signal name="GPIO1">
<contactref element="JP1" pad="1"/>
</signal>
<signal name="5V">
<contactref element="JP1" pad="8"/>
<contactref element="D1" pad="1"/>
<contactref element="JP4" pad="2"/>
<contactref element="WS1" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="P1" pad="1"/>
</signal>
<signal name="DO">
<contactref element="P2" pad="1"/>
<contactref element="WS1" pad="2"/>
</signal>
<signal name="VLED">
<contactref element="WS2812" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="D1" pad="2"/>
<contactref element="JP4" pad="1"/>
</signal>
<signal name="ANT">
<contactref element="U$5" pad="ANT"/>
<contactref element="J$2" pad="ANT1"/>
<contactref element="J$2" pad="ANT2"/>
<contactref element="J$2" pad="ANT3"/>
</signal>
<signal name="N$1">
<contactref element="WS1" pad="4"/>
<contactref element="WS2812" pad="2"/>
</signal>
<signal name="DIO0">
<contactref element="D2" pad="1"/>
<contactref element="U$5" pad="DIO0"/>
</signal>
<signal name="DIO1">
<contactref element="D3" pad="1"/>
<contactref element="U$5" pad="DIO1"/>
</signal>
<signal name="DIO2">
<contactref element="D4" pad="1"/>
<contactref element="U$5" pad="DIO2"/>
</signal>
<signal name="SEL">
<contactref element="JP3" pad="3"/>
<contactref element="R3" pad="2"/>
<contactref element="U$5" pad="NSS"/>
</signal>
<signal name="GD_3V3">
<contactref element="U$2" pad="2"/>
<contactref element="I2C_OLED" pad="2"/>
</signal>
<signal name="3V3_GD">
<contactref element="U$2" pad="3"/>
<contactref element="I2C_OLED" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
