<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<board>
<plain>
<wire x1="0.635" y1="1.27" x2="47.5234" y2="1.27" width="0.1524" layer="20"/>
<wire x1="47.5234" y1="1.27" x2="47.5234" y2="35.55" width="0.1524" layer="20"/>
<wire x1="47.5234" y1="35.55" x2="0.635" y2="35.55" width="0.1524" layer="20"/>
<wire x1="0.635" y1="35.55" x2="0.635" y2="1.27" width="0.1524" layer="20"/>
<text>- Trigger+ </text>
<text>Load-Out-3.3V
</text>
<text>RV-Project.Com
Remote Controlled 
Switch</text>
<text>Use Polycase 
BF-150275</text>
<text>Active</text>
<text>MCS-3 Rev F</text>
<text>Reset</text>
<text>3/25/2022</text>
<text>400mA Max</text>
<text>Trigger</text>
<text>GND  12V</text>
<text>Trigger +</text>
<text>GND</text>
<text>GND</text>
<text>12V</text>
<text>++3.3V --</text>
<text>IN</text>
<text>OUT</text>
<text>Control</text>
<text>Common
GND</text>
<text>Conformal Coat vulnerable
items to prevent potting
intrusion.</text>
<text>Power</text>
<text>Reverse 
Voltage Protection</text>
</plain>
<libraries>
<library name="a-lib">
<description>&lt;b&gt;Al's Components.&lt;/b&gt;
&lt;p&gt;Including:
&lt;ul&gt;
&lt;li&gt;GPS Receivers
&lt;li&gt;ASK Transmitters and Receivers
&lt;li&gt;Specialtiy Switches
&lt;/ul&gt;</description>
<packages>
<package name="RADIAL_ELECTROLYTIC_100MIL(5MM)">
<description>Generic Electrolytic Capacitor.&lt;br&gt;Pitch:0.1&lt;br&gt;
Dia: 0.2"Dia (5.08mm)</description>
</package>
<package name="1206-CAP">
</package>
<package name="DIP08">
<description>&lt;b&gt;Dual In Line&lt;/b&gt;</description>
</package>
<package name="TO-220-MOSFET">
</package>
<package name="LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
<package name="1206-RES">
</package>
<package name="SOD-123">
<description>Suitable for 4148
&lt;br&gt;Pad Size:  0.55"x0.8"</description>
</package>
<package name="6PIN_OPTO">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="SOD-323">
<description>Pad Size: 0.22"x0.8"</description>
</package>
<package name="DIL06">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="GODZILLA_LARGE">
</package>
</packages>
</library>
<library name="a-lib_Switches">
<description>Thru-Hole Switches, Relays</description>
<packages>
<package name="2PINTACT">
</package>
</packages>
</library>
<library name="a-lib_Connectors">
<description>Thru-Hole Connectors (Connectors, Terminals)</description>
<packages>
<package name="MO1-18AWG-SMALL">
</package>
<package name="KEYSTONE4901">
</package>
</packages>
</library>
<library name="a-lib_SMD">
<description>All SMD Devices; Actives, Passives, Connectors</description>
<packages>
<package name="SMD-JUMPER_2">
<description>Pad Size: 0.12"x0.06"&lt;br&gt;Resist remoted between pads for ease of solder bridge.</description>
</package>
<package name="SOD-323">
<description>Pad Size: 0.22"x0.8"</description>
</package>
</packages>
</library>
<library name="a-lib_Actives">
<description>Thru-Hole Actives (Transistors, Diodes, MPUs)</description>
<packages>
<package name="IPAK_VERTICAL(TO251)">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C3" library="a-lib" package="RADIAL_ELECTROLYTIC_100MIL(5MM)" value="10UF">
<attribute name="MARKING" value="106"/>
<attribute name="NAME"/>
<attribute name="VOLTAGE" value="25v"/>
</element>
<element name="C4" library="a-lib" package="1206-CAP" value="0.01uF">
<attribute name="NAME"/>
</element>
<element name="C1" library="a-lib" package="1206-CAP" value=".1uF">
<attribute name="NAME"/>
</element>
<element name="C2" library="a-lib" package="1206-CAP" value="0.33uF">
<attribute name="NAME"/>
</element>
<element name="R5" library="a-lib" package="1206-RES" value="10k">
<attribute name="NAME"/>
</element>
<element name="U2" library="a-lib" package="DIP08" value="TINY85-20-DIP">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="IC-09445"/>
</element>
<element name="Q1" library="a-lib" package="TO-220-MOSFET" value="IRF520">
<attribute name="NAME"/>
</element>
<element name="LED1" library="a-lib" package="LED3MM" value="">
<attribute name="VALUE"/>
</element>
<element name="R6" library="a-lib" package="1206-RES" value="1K">
<attribute name="NAME"/>
</element>
<element name="D1" library="a-lib" package="SOD-123" value="TVS-SSOD123">
<attribute name="NAME"/>
</element>
<element name="OK1" library="a-lib" package="6PIN_OPTO" value="4N35">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="a-lib" package="1206-RES" value="1K">
<attribute name="NAME"/>
</element>
<element name="R3" library="a-lib" package="1206-RES" value="1K">
<attribute name="NAME"/>
</element>
<element name="R1" library="a-lib" package="1206-RES" value="10k">
<attribute name="NAME"/>
</element>
<element name="D3" library="a-lib" package="SOD-123" value="TVS-SSOD123">
<attribute name="NAME"/>
</element>
<element name="D4" library="a-lib" package="SOD-323" value="250mA/100V">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="DIO-09646"/>
</element>
<element name="LED2" library="a-lib" package="LED3MM" value="">
<attribute name="VALUE"/>
</element>
<element name="R8" library="a-lib" package="1206-RES" value="1K">
<attribute name="NAME"/>
</element>
<element name="S2" library="a-lib" package="DIL06" value="DIPSWITCH-3">
<attribute name="NAME"/>
</element>
<element name="R2" library="a-lib" package="1206-RES" value="1K">
<attribute name="NAME"/>
</element>
<element name="R9" library="a-lib" package="1206-RES" value="1K">
<attribute name="NAME"/>
</element>
<element name="R10" library="a-lib" package="1206-RES" value="1K">
<attribute name="NAME"/>
</element>
<element name="U$2" library="a-lib" package="GODZILLA_LARGE" value=""/>
<element name="S3" library="a-lib_Switches" package="2PINTACT" value=""/>
<element name="TB1" library="a-lib_Connectors" package="MO1-18AWG-SMALL" value=""/>
<element name="TB2" library="a-lib_Connectors" package="MO1-18AWG-SMALL" value=""/>
<element name="TB3" library="a-lib_Connectors" package="MO1-18AWG-SMALL" value=""/>
<element name="TB4" library="a-lib_Connectors" package="MO1-18AWG-SMALL" value=""/>
<element name="TB5" library="a-lib_Connectors" package="KEYSTONE4901" value=""/>
<element name="TB6" library="a-lib_Connectors" package="KEYSTONE4901" value=""/>
<element name="J1" library="a-lib_SMD" package="SMD-JUMPER_2" value="M2JUMPER1"/>
<element name="LED3" library="a-lib" package="LED3MM" value="">
<attribute name="VALUE"/>
</element>
<element name="R4" library="a-lib" package="1206-RES" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="a-lib_Actives" package="IPAK_VERTICAL(TO251)" value="">
<attribute name="NAME"/>
</element>
<element name="D2" library="a-lib_SMD" package="SOD-323" value="250mA/100V">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="DIO-09646"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="U2" pad="4"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="1"/>
<contactref element="C3" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="Q1" pad="S"/>
<contactref element="R5" pad="1"/>
<contactref element="D1" pad="A"/>
<contactref element="OK1" pad="4"/>
<contactref element="S2" pad="3"/>
<contactref element="S2" pad="2"/>
<contactref element="S2" pad="1"/>
<contactref element="S3" pad="P$2"/>
<contactref element="TB2" pad="P$1"/>
<contactref element="J1" pad="2"/>
<contactref element="R4" pad="1"/>
<contactref element="U1" pad="G"/>
</signal>
<signal name="12V">
<contactref element="TB1" pad="P$1"/>
<contactref element="LED3" pad="A"/>
<contactref element="D2" pad="A"/>
</signal>
<signal name="N$12">
<contactref element="Q1" pad="G"/>
<contactref element="R5" pad="2"/>
<contactref element="U2" pad="2"/>
</signal>
<signal name="N$14">
</signal>
<signal name="N$15">
</signal>
<signal name="N$18">
<contactref element="Q1" pad="D"/>
<contactref element="R6" pad="1"/>
<contactref element="TB4" pad="P$1"/>
</signal>
<signal name="N$13">
<contactref element="U2" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="S3" pad="P$1"/>
</signal>
<signal name="N$2">
<contactref element="R7" pad="1"/>
<contactref element="OK1" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="OK1" pad="2"/>
<contactref element="D3" pad="A"/>
<contactref element="LED2" pad="K"/>
<contactref element="TB6" pad="P$1"/>
<contactref element="TB6" pad="P$2"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="R7" pad="2"/>
<contactref element="D3" pad="C"/>
<contactref element="D4" pad="C"/>
<contactref element="R8" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="D4" pad="A"/>
<contactref element="TB5" pad="P$1"/>
<contactref element="TB5" pad="P$2"/>
</signal>
<signal name="N$8">
<contactref element="LED2" pad="A"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="N$16">
<contactref element="R3" pad="1"/>
<contactref element="U2" pad="3"/>
<contactref element="OK1" pad="5"/>
</signal>
<signal name="N$5">
<contactref element="U2" pad="5"/>
<contactref element="R10" pad="1"/>
<contactref element="S2" pad="6"/>
</signal>
<signal name="N$9">
<contactref element="R9" pad="1"/>
<contactref element="S2" pad="5"/>
<contactref element="U2" pad="6"/>
</signal>
<signal name="N$11">
<contactref element="U2" pad="7"/>
<contactref element="R2" pad="1"/>
<contactref element="S2" pad="4"/>
</signal>
<signal name="3.3V">
<contactref element="LED1" pad="A"/>
<contactref element="R1" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="R9" pad="2"/>
<contactref element="R10" pad="2"/>
<contactref element="C4" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="U2" pad="8"/>
<contactref element="R3" pad="2"/>
<contactref element="TB3" pad="P$1"/>
<contactref element="U1" pad="O"/>
</signal>
<signal name="N$1">
<contactref element="LED1" pad="K"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="LED3" pad="K"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="C3" pad="1"/>
<contactref element="C2" pad="2"/>
<contactref element="D1" pad="C"/>
<contactref element="U1" pad="I"/>
<contactref element="D2" pad="C"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
