<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<text>SDA</text>
<text>SCL</text>
<text>VCC</text>
<text>GND</text>
<text>A0</text>
<text>A2</text>
<text>A1</text>
<text>C</text>
<text>D</text>
<text>-</text>
<text>+</text>
<hole x="1.905" y="1.905" drill="2"/>
<hole x="99.695" y="1.905" drill="2"/>
<hole x="1.905" y="27.305" drill="2"/>
<hole x="99.695" y="27.305" drill="2"/>
<text>Vi2c</text>
<text>+</text>
<wire x1="0" y1="26.67" x2="2.54" y2="29.21" width="0" layer="20" curve="-90"/>
<wire x1="2.54" y1="0" x2="0" y2="2.54" width="0" layer="20" curve="-90"/>
<wire x1="101.6" y1="2.54" x2="99.06" y2="0" width="0" layer="20" curve="-90"/>
<wire x1="2.54" y1="29.21" x2="99.06" y2="29.21" width="0" layer="20"/>
<wire x1="2.54" y1="0" x2="99.06" y2="0" width="0" layer="20"/>
<wire x1="0" y1="26.67" x2="0" y2="2.54" width="0" layer="20"/>
<wire x1="101.6" y1="2.54" x2="101.6" y2="26.67" width="0" layer="20"/>
<wire x1="99.06" y1="29.21" x2="101.6" y2="26.67" width="0" layer="20" curve="-90"/>
<text>Alphanumeric Backpack</text>
<text>Technoblogy</text>
</plain>
<libraries>
<library name="microbuilder">
<packages>
<package name="SOLDERJUMPER_REFLOW_NOPASTE">
</package>
<package name="SOP28_300MIL">
</package>
<package name="SEGMENT_STARTBUST_DUAL_KWA-541CBB">
</package>
<package name="0805-NO">
</package>
<package name="1X05_ROUND_70">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="SOD-323F">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="R1" library="microbuilder" package="0805-NO" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="microbuilder" package="0805-NO" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="A1" library="microbuilder" package="SOLDERJUMPER_REFLOW_NOPASTE" value="">
<attribute name="VALUE"/>
</element>
<element name="A0" library="microbuilder" package="SOLDERJUMPER_REFLOW_NOPASTE" value="">
<attribute name="VALUE"/>
</element>
<element name="D1" library="adafruit" package="SOD-323F" value="1N4148">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="microbuilder" package="0805-NO" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="microbuilder" package="0805-NO" value="47K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="microbuilder" package="0805-NO" value="47K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U2" library="microbuilder" package="SOP28_300MIL" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="A2" library="microbuilder" package="SOLDERJUMPER_REFLOW_NOPASTE" value="">
<attribute name="VALUE"/>
</element>
<element name="R5" library="microbuilder" package="0805-NO" value="47K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED3" library="microbuilder" package="SEGMENT_STARTBUST_DUAL_KWA-541CBB" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED4" library="microbuilder" package="SEGMENT_STARTBUST_DUAL_KWA-541CBB" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="microbuilder" package="1X05_ROUND_70" value="">
<attribute name="VALUE"/>
</element>
<element name="LED2" library="microbuilder" package="SEGMENT_STARTBUST_DUAL_KWA-541CBB" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="microbuilder" package="SEGMENT_STARTBUST_DUAL_KWA-541CBB" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="VDD">
<contactref element="C1" pad="1"/>
<contactref element="JP1" pad="4"/>
<contactref element="U2" pad="P$28"/>
</signal>
<signal name="GND">
<contactref element="C1" pad="2"/>
<contactref element="U2" pad="P$1"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="N$19">
<contactref element="A1" pad="1"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$20">
<contactref element="A0" pad="1"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="A1">
<contactref element="U2" pad="P$24"/>
<contactref element="A1" pad="2"/>
<contactref element="LED3" pad="10"/>
<contactref element="LED4" pad="10"/>
<contactref element="LED2" pad="10"/>
<contactref element="LED1" pad="10"/>
</signal>
<signal name="COM0">
<contactref element="U2" pad="P$2"/>
<contactref element="D1" pad="A"/>
<contactref element="LED1" pad="16"/>
</signal>
<signal name="N$10">
<contactref element="U2" pad="P$22"/>
<contactref element="LED3" pad="7"/>
<contactref element="LED4" pad="7"/>
<contactref element="LED2" pad="7"/>
<contactref element="LED1" pad="7"/>
</signal>
<signal name="N$11">
<contactref element="U2" pad="P$21"/>
<contactref element="LED3" pad="1"/>
<contactref element="LED4" pad="1"/>
<contactref element="LED2" pad="1"/>
<contactref element="LED1" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="U2" pad="P$20"/>
<contactref element="LED3" pad="18"/>
<contactref element="LED4" pad="18"/>
<contactref element="LED2" pad="18"/>
<contactref element="LED1" pad="18"/>
</signal>
<signal name="N$13">
<contactref element="U2" pad="P$19"/>
<contactref element="LED3" pad="13"/>
<contactref element="LED4" pad="13"/>
<contactref element="LED2" pad="13"/>
<contactref element="LED1" pad="13"/>
</signal>
<signal name="N$16">
<contactref element="U2" pad="P$18"/>
<contactref element="LED3" pad="6"/>
<contactref element="LED4" pad="6"/>
<contactref element="LED2" pad="6"/>
<contactref element="LED1" pad="6"/>
</signal>
<signal name="A0">
<contactref element="U2" pad="P$23"/>
<contactref element="A0" pad="2"/>
<contactref element="LED3" pad="9"/>
<contactref element="LED4" pad="9"/>
<contactref element="LED2" pad="9"/>
<contactref element="LED1" pad="9"/>
</signal>
<signal name="A2">
<contactref element="U2" pad="P$25"/>
<contactref element="A2" pad="2"/>
<contactref element="LED3" pad="12"/>
<contactref element="LED4" pad="12"/>
<contactref element="LED2" pad="12"/>
<contactref element="LED1" pad="12"/>
</signal>
<signal name="SDA">
<contactref element="R2" pad="2"/>
<contactref element="U2" pad="P$27"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="SCL">
<contactref element="R1" pad="2"/>
<contactref element="U2" pad="P$26"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="R5" pad="1"/>
<contactref element="D1" pad="C"/>
<contactref element="R3" pad="1"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="A2" pad="1"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="U2" pad="P$17"/>
<contactref element="LED3" pad="17"/>
<contactref element="LED4" pad="17"/>
<contactref element="LED2" pad="17"/>
<contactref element="LED1" pad="17"/>
</signal>
<signal name="N$5">
<contactref element="U2" pad="P$16"/>
<contactref element="LED3" pad="15"/>
<contactref element="LED4" pad="15"/>
<contactref element="LED2" pad="15"/>
<contactref element="LED1" pad="15"/>
</signal>
<signal name="N$6">
<contactref element="U2" pad="P$15"/>
<contactref element="LED3" pad="14"/>
<contactref element="LED4" pad="14"/>
<contactref element="LED2" pad="14"/>
<contactref element="LED1" pad="14"/>
</signal>
<signal name="N$8">
<contactref element="U2" pad="P$14"/>
<contactref element="LED3" pad="2"/>
<contactref element="LED4" pad="2"/>
<contactref element="LED2" pad="2"/>
<contactref element="LED1" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="U2" pad="P$13"/>
<contactref element="LED3" pad="4"/>
<contactref element="LED4" pad="4"/>
<contactref element="LED2" pad="4"/>
<contactref element="LED1" pad="4"/>
</signal>
<signal name="N$14">
<contactref element="U2" pad="P$12"/>
<contactref element="LED3" pad="5"/>
<contactref element="LED4" pad="5"/>
<contactref element="LED2" pad="5"/>
<contactref element="LED1" pad="5"/>
</signal>
<signal name="N$15">
<contactref element="U2" pad="P$11"/>
<contactref element="LED3" pad="8"/>
<contactref element="LED4" pad="8"/>
<contactref element="LED2" pad="8"/>
<contactref element="LED1" pad="8"/>
</signal>
<signal name="COM1">
<contactref element="U2" pad="P$3"/>
<contactref element="LED1" pad="11"/>
</signal>
<signal name="COM2">
<contactref element="U2" pad="P$4"/>
<contactref element="LED2" pad="16"/>
</signal>
<signal name="COM3">
<contactref element="U2" pad="P$5"/>
<contactref element="LED2" pad="11"/>
</signal>
<signal name="N$2">
<contactref element="R1" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="COM4">
<contactref element="U2" pad="P$6"/>
<contactref element="LED3" pad="16"/>
</signal>
<signal name="COM5">
<contactref element="U2" pad="P$7"/>
<contactref element="LED3" pad="11"/>
</signal>
<signal name="N$23">
<contactref element="U2" pad="P$8"/>
<contactref element="LED4" pad="16"/>
</signal>
<signal name="N$24">
<contactref element="U2" pad="P$9"/>
<contactref element="LED4" pad="11"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
