(kicad_pcb (version 20171130) (host pcbnew "(5.1.2-1)-1")
  (general
    (thickness 1.6)
    (drawings 16)
    (tracks 33)
    (zones 0)
    (modules 20)
    (nets 7)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 1)
    (user_trace_width 1.25)
    (user_trace_width 1.5)
    (user_trace_width 2)
    (user_trace_width 2.5)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.508)
    (via_drill 0.254)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.508)
    (uvia_drill 0.254)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.15)
    (segment_width 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.4 2.4)
    (pad_drill 1.2)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (grid_origin 265.04 97.02)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer false)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers/"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(J2-Pad1)")
  (net 3 "Net-(C75-Pad1)")
  (net 4 "Net-(C76-Pad2)")
  (net 5 "Net-(C79-Pad1)")
  (net 6 "Net-(C80-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
    (add_net GND)
    (add_net "Net-(C75-Pad1)")
    (add_net "Net-(C76-Pad2)")
    (add_net "Net-(C79-Pad1)")
    (add_net "Net-(C80-Pad2)")
    (add_net "Net-(J2-Pad1)")
  )
  (net_class SMD ""
    (clearance 0.1524)
    (trace_width 0.254)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
  )
  (net_class grounds ""
    (clearance 0.254)
    (trace_width 1)
    (via_dia 0.762)
    (via_drill 0.381)
    (uvia_dia 0.762)
    (uvia_drill 0.381)
  )
  (net_class power ""
    (clearance 0.254)
    (trace_width 1)
    (via_dia 0.762)
    (via_drill 0.254)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
  )
  (net_class signal ""
    (clearance 0.2)
    (trace_width 0.6096)
    (via_dia 0.762)
    (via_drill 0.381)
    (uvia_dia 0.762)
    (uvia_drill 0.381)
  )
  (net_class soic ""
    (clearance 0.1524)
    (trace_width 0.4)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
  )
  (module SMC_generic:Bourns_RLB0912 (layer F.Cu) (tedit 5AE59B06)
    (at 253.04 97.32 270)
    (descr "Inductor, Radial series, Radial, pin pitch=5.00mm, , diameter=8.7mm, Fastron, 07HCP, http://cdn-reichelt.de/documents/datenblatt/B400/DS_07HCP.pdf")
    (tags "Inductor Radial series Radial pin pitch 5.00mm  diameter 8.7mm Bourns RLB0912")
    (fp_text reference L2 (at 6.8 -3.8 90) (layer F.SilkS))
    (fp_text value 1000uH (at 2.5 0) (layer F.SilkS))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 270) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 4 "Net-(C76-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 6 "Net-(C80-Pad2)"))
    (model ${KIPRJMOD}/Lib/3D/rlb0912.stp
      (offset (xyz 2.539999961853027 0 0))
      (scale (xyz 0.9 1 0.9))
      (rotate (xyz -90 0 90))
    )
  )
  (module SMC_generic:C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima (layer F.Cu) (tedit 5D53486E)
    (at 236.54 83.62 180)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*5.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 5.5mm Capacitor")
    (fp_text reference C81 (at 2.6 -3.4) (layer F.SilkS))
    (fp_text value 100n (at 2.5 -0.05 90) (layer F.SilkS))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C79-Pad1)"))
    (model ${KIPRJMOD}/Lib/3D/C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1.1 1.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima (layer F.Cu) (tedit 5D53486E)
    (at 264.54 83.62 180)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*5.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 5.5mm Capacitor")
    (fp_text reference C82 (at 2.6 -3.4) (layer F.SilkS))
    (fp_text value 100n (at 2.5 0 90) (layer F.SilkS))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C80-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KIPRJMOD}/Lib/3D/C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1.1 1.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:CP_5x11mm_Silmic (layer F.Cu) (tedit 5D587B39)
    (at 261.34 102.32 90)
    (descr "Capacitor, pol, cyl 5x11mm")
    (fp_text reference C78 (at 0.1 3.7 -90) (layer F.SilkS))
    (fp_text value 10u (at 1.77 0.03) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 1 90) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole circle (at 0 -1 90) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(C76-Pad2)"))
    (model ${KIPRJMOD}/Lib/3D/cp_5x11mm_Silmic.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 226.04 110.22 90)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference H1 (at 0 -4.2 90) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4.2 90) (layer F.Fab))
    (fp_text user %R (at 0.3 0 90) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0 90) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 270.04 110.22 90)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference H2 (at 0 -4.2 90) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4.2 90) (layer F.Fab))
    (fp_text user %R (at 0.3 0 90) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0 90) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 226.04 84.02 90)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference H3 (at 0 -4.2 90) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4.2 90) (layer F.Fab))
    (fp_text user %R (at 0.3 0 90) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0 90) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 270.04 84.02 90)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference H4 (at 0 -4.2 90) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4.2 90) (layer F.Fab))
    (fp_text user %R (at 0.3 0 90) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0 90) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module SMC_generic:CP_8x11.5mm_Silmic (layer F.Cu) (tedit 5D5AE3F7)
    (at 235.54 92.32 90)
    (descr "Capacitor, pol, cyl 8x11.5mm")
    (fp_text reference C79 (at -5.1 -0.1) (layer F.SilkS))
    (fp_text value 47u (at 2.5 0) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 1.75 90) (size 1.8 1.8) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(C79-Pad1)"))
    (pad 2 thru_hole circle (at 0 -1.75 90) (size 1.8 1.8) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model ${KIPRJMOD}/Lib/3D/cp_8x11.5mm_Silmic.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:CP_8x11.5mm_Silmic (layer F.Cu) (tedit 5D5AE3F7)
    (at 260.54 92.32 90)
    (descr "Capacitor, pol, cyl 8x11.5mm")
    (fp_text reference C80 (at -5 0.1) (layer F.SilkS))
    (fp_text value 47u (at 2.5 0 180) (layer F.SilkS))
    (pad 2 thru_hole circle (at 0 -1.75 90) (size 1.8 1.8) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(C80-Pad2)"))
    (pad 1 thru_hole rect (at 0 1.75 90) (size 1.8 1.8) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model ${KIPRJMOD}/Lib/3D/cp_8x11.5mm_Silmic.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:CP_5x11mm_Silmic (layer F.Cu) (tedit 5D587B39)
    (at 234.64 102.32 90)
    (descr "Capacitor, pol, cyl 5x11mm")
    (fp_text reference C77 (at 0 -3.5 90) (layer F.SilkS))
    (fp_text value 10u (at 1.5 0) (layer F.SilkS))
    (pad 2 thru_hole circle (at 0 -1 90) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 1 90) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(C75-Pad1)"))
    (model ${KIPRJMOD}/Lib/3D/cp_5x11mm_Silmic.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima (layer F.Cu) (tedit 5D53486E)
    (at 236.54 110.52 180)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*5.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 5.5mm Capacitor")
    (fp_text reference C75 (at 2.3 3.5 180) (layer F.SilkS))
    (fp_text value 100n (at 2.5 0 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C75-Pad1)"))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KIPRJMOD}/Lib/3D/C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1.1 1.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima (layer F.Cu) (tedit 5D53486E)
    (at 264.54 110.52 180)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*5.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 5.5mm Capacitor")
    (fp_text reference C76 (at 2.6 3.55) (layer F.SilkS))
    (fp_text value 100n (at 2.5 0 90) (layer F.SilkS))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C76-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KIPRJMOD}/Lib/3D/C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1.1 1.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:mkds_1,5-3 (layer F.Cu) (tedit 5F876DC5)
    (at 248.04 85.02 180)
    (descr "3-way 5mm pitch terminal block, Phoenix MKDS series")
    (fp_text reference J1 (at 0 -5.4) (layer F.Fab))
    (fp_text value Power-In (at 0 3.5) (layer F.SilkS))
    (pad 2 thru_hole circle (at 0 0 180) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (thermal_width 1))
    (pad 1 thru_hole circle (at -5 0 180) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(C80-Pad2)"))
    (pad 3 thru_hole circle (at 5 0 180) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(C79-Pad1)"))
    (model ${KIPRJMOD}/Lib/3D/pxc_1935174_03_PT-1-5-3-5-0-H_3D.stp
      (offset (xyz -30.09899954795837 -44.70399932861328 -38.86199941635132))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 180 90))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 246.79 93.87 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J2 (at -2.125 1.2) (layer F.Fab))
    (fp_text value LED (at -2.15 1.225) (layer F.SilkS))
    (fp_text user %R (at 0 1.27) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J2-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(C80-Pad2)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:mkds_1,5-3 (layer F.Cu) (tedit 5F876DB7)
    (at 248.04 109.22)
    (descr "3-way 5mm pitch terminal block, Phoenix MKDS series")
    (fp_text reference J3 (at 0 -5.4) (layer F.Fab))
    (fp_text value Power-Out (at 0 3.5 unlocked) (layer F.SilkS))
    (pad 3 thru_hole circle (at 5 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(C76-Pad2)"))
    (pad 1 thru_hole circle (at -5 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(C75-Pad1)"))
    (pad 2 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (thermal_width 1))
    (model ${KIPRJMOD}/Lib/3D/pxc_1935174_03_PT-1-5-3-5-0-H_3D.stp
      (offset (xyz -30.09899954795837 -44.70399932861328 -38.86199941635132))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 180 90))
    )
  )
  (module SMC_generic:Bourns_RLB0912 (layer F.Cu) (tedit 5AE59B06)
    (at 243.04 97.32 270)
    (descr "Inductor, Radial series, Radial, pin pitch=5.00mm, , diameter=8.7mm, Fastron, 07HCP, http://cdn-reichelt.de/documents/datenblatt/B400/DS_07HCP.pdf")
    (tags "Inductor Radial series Radial pin pitch 5.00mm  diameter 8.7mm Bourns RLB0912")
    (fp_text reference L1 (at 6.6 3.9 90) (layer F.SilkS))
    (fp_text value 1000uH (at 2.5 0) (layer F.SilkS))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 5 "Net-(C79-Pad1)"))
    (pad 2 thru_hole circle (at 5 0 270) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 3 "Net-(C75-Pad1)"))
    (model ${KIPRJMOD}/Lib/3D/rlb0912.stp
      (offset (xyz 2.539999961853027 0 0))
      (scale (xyz 0.9 1 0.9))
      (rotate (xyz -90 0 90))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 242.94 90.72)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R97 (at -1.725 -0.05 -90) (layer F.SilkS))
    (fp_text value 100k (at 5.08 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C79-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(J2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P15.24mm_Horizontal (layer F.Cu) (tedit 5F876DF1)
    (at 227.84 89.52 270)
    (descr "Resistor, Axial_DIN0411 series, Axial, Horizontal, pin pitch=15.24mm, 1W, length*diameter=9.9*3.6mm^2")
    (tags "Resistor Axial_DIN0411 series Axial Horizontal pin pitch 15.24mm 1W length 9.9mm diameter 3.6mm")
    (fp_text reference R95 (at 7.6 -2.8 90) (layer F.SilkS))
    (fp_text value 390 (at 7.62 0.05 90) (layer F.SilkS))
    (fp_text user %R (at 7.62 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 5 "Net-(C79-Pad1)"))
    (pad 2 thru_hole oval (at 15.24 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND) (thermal_width 1))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0411_L9.9mm_D3.6mm_P15.24mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P15.24mm_Horizontal (layer F.Cu) (tedit 5F876DFE)
    (at 268.04 89.52 270)
    (descr "Resistor, Axial_DIN0411 series, Axial, Horizontal, pin pitch=15.24mm, 1W, length*diameter=9.9*3.6mm^2")
    (tags "Resistor Axial_DIN0411 series Axial Horizontal pin pitch 15.24mm 1W length 9.9mm diameter 3.6mm")
    (fp_text reference R96 (at 7.6 2.7 90) (layer F.SilkS))
    (fp_text value 390 (at 7.62 0 90) (layer F.SilkS))
    (fp_text user %R (at 7.62 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 15.24 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND) (thermal_width 1))
    (pad 1 thru_hole circle (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 6 "Net-(C80-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0411_L9.9mm_D3.6mm_P15.24mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text - (at 251.64 93.82 180) (layer F.SilkS))
  (gr_text + (at 244.09 93.82 90) (layer F.SilkS))
  (gr_line (start 222.04 114.22) (end 222.04 80.02) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 274.04 114.22) (end 222.04 114.22) (layer Edge.Cuts) (width 0.05))
  (gr_text "-V in" (at 253.04 81.52 180) (layer B.SilkS))
  (gr_text "+V in" (at 243.04 81.52 180) (layer B.SilkS))
  (gr_text "-V out" (at 253.04 112.52 180) (layer B.SilkS))
  (gr_text "+V out" (at 243.04 112.52 180) (layer B.SilkS))
  (gr_text "+V out" (at 239.79 110.77 90) (layer F.SilkS))
  (gr_text "-V out" (at 256.54 110.77 90) (layer F.SilkS))
  (gr_text "-V in" (at 256.54 83.52 90) (layer F.SilkS))
  (gr_text "+V in" (at 239.79 83.52 90) (layer F.SilkS))
  (gr_line (start 274.04 114.22) (end 274.04 80.02) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 222.04 80.02) (end 274.04 80.02) (layer Edge.Cuts) (width 0.05))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 229.54 85.52) (xy 227.54 87.52) (xy 222.04 87.52) (xy 222.04 106.72) (xy 227.54 106.72)
        (xy 229.54 108.72) (xy 229.54 114.22) (xy 266.54 114.22) (xy 266.54 108.72) (xy 268.54 106.72)
        (xy 274.04 106.72) (xy 274.04 87.52) (xy 268.54 87.52) (xy 266.54 85.52) (xy 266.54 80.02)
        (xy 229.54 80.02)
      )
    )
  )
)
