(kicad_pcb (version 4) (host pcbnew 4.0.7-e2-6376~58~ubuntu16.04.1)
  (general
    (links 22)
    (no_connects 0)
    (area 109.169999 53.289999 146.100001 123.240001)
    (thickness 1.6)
    (drawings 21)
    (tracks 0)
    (zones 0)
    (modules 13)
    (nets 3)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFEFF7F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /GND)
  (net 2 /VCC)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /GND)
    (add_net /VCC)
  )
  (net_class Thick ""
    (clearance 0.2)
    (trace_width 1)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module xt60board:XT60 (layer F.Cu) (tedit 59B749AB)
    (at 140.97 58.42 180)
    (fp_text reference J1 (at 3.556 6.096 180) (layer F.SilkS) hide)
    (fp_text value XT60 (at 3.2 -5.9 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 6 6) (drill 4.5) (layers *.Cu *.Mask F.SilkS)
      (net 1 /GND))
    (pad 2 thru_hole circle (at 7.5 0 180) (size 6 6) (drill 4.5) (layers *.Cu *.Mask F.SilkS)
      (net 2 /VCC))
  )
  (module xt60board:XT60 (layer F.Cu) (tedit 59B749B0)
    (at 140.97 68.58 180)
    (fp_text reference J2 (at 3.556 6.096 180) (layer F.SilkS) hide)
    (fp_text value XT60 (at 3.2 -5.9 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 6 6) (drill 4.5) (layers *.Cu *.Mask F.SilkS)
      (net 1 /GND))
    (pad 2 thru_hole circle (at 7.5 0 180) (size 6 6) (drill 4.5) (layers *.Cu *.Mask F.SilkS)
      (net 2 /VCC))
  )
  (module xt60board:XT60 (layer F.Cu) (tedit 59B749B4)
    (at 140.97 78.74 180)
    (fp_text reference J3 (at 3.556 6.096 180) (layer F.SilkS) hide)
    (fp_text value XT60 (at 3.2 -5.9 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 6 6) (drill 4.5) (layers *.Cu *.Mask F.SilkS)
      (net 1 /GND))
    (pad 2 thru_hole circle (at 7.5 0 180) (size 6 6) (drill 4.5) (layers *.Cu *.Mask F.SilkS)
      (net 2 /VCC))
  )
  (module xt60board:XT60 (layer F.Cu) (tedit 59B749BA)
    (at 140.97 88.9 180)
    (fp_text reference J4 (at 3.556 6.096 180) (layer F.SilkS) hide)
    (fp_text value XT60 (at 3.2 -5.9 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 6 6) (drill 4.5) (layers *.Cu *.Mask F.SilkS)
      (net 1 /GND))
    (pad 2 thru_hole circle (at 7.5 0 180) (size 6 6) (drill 4.5) (layers *.Cu *.Mask F.SilkS)
      (net 2 /VCC))
  )
  (module xt60board:XT60 (layer F.Cu) (tedit 59B749BD)
    (at 140.97 99.06 180)
    (fp_text reference J5 (at 3.556 6.096 180) (layer F.SilkS) hide)
    (fp_text value XT60 (at 3.2 -5.9 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 6 6) (drill 4.5) (layers *.Cu *.Mask F.SilkS)
      (net 1 /GND))
    (pad 2 thru_hole circle (at 7.5 0 180) (size 6 6) (drill 4.5) (layers *.Cu *.Mask F.SilkS)
      (net 2 /VCC))
  )
  (module xt60board:XT60 (layer F.Cu) (tedit 59B749C3)
    (at 140.97 109.22 180)
    (fp_text reference J6 (at 3.556 6.096 180) (layer F.SilkS) hide)
    (fp_text value XT60 (at 3.2 -5.9 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 6 6) (drill 4.5) (layers *.Cu *.Mask F.SilkS)
      (net 1 /GND))
    (pad 2 thru_hole circle (at 7.5 0 180) (size 6 6) (drill 4.5) (layers *.Cu *.Mask F.SilkS)
      (net 2 /VCC))
  )
  (module xt60board:XT60 (layer F.Cu) (tedit 59B7499E)
    (at 114.3 58.42)
    (fp_text reference J7 (at 3.556 6.096) (layer F.SilkS) hide)
    (fp_text value XT60 (at 3.2 -5.9) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 4.5) (layers *.Cu *.Mask F.SilkS)
      (net 1 /GND))
    (pad 2 thru_hole circle (at 7.5 0) (size 6 6) (drill 4.5) (layers *.Cu *.Mask F.SilkS)
      (net 2 /VCC))
  )
  (module xt60board:XT60 (layer F.Cu) (tedit 59B7499A)
    (at 114.3 68.58)
    (fp_text reference J8 (at 3.556 6.096) (layer F.SilkS) hide)
    (fp_text value XT60 (at 3.2 -5.9) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 4.5) (layers *.Cu *.Mask F.SilkS)
      (net 1 /GND))
    (pad 2 thru_hole circle (at 7.5 0) (size 6 6) (drill 4.5) (layers *.Cu *.Mask F.SilkS)
      (net 2 /VCC))
  )
  (module xt60board:XT60 (layer F.Cu) (tedit 59B74993)
    (at 114.3 78.74)
    (fp_text reference J9 (at 3.556 6.096) (layer F.SilkS) hide)
    (fp_text value XT60 (at 3.2 -5.9) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 4.5) (layers *.Cu *.Mask F.SilkS)
      (net 1 /GND))
    (pad 2 thru_hole circle (at 7.5 0) (size 6 6) (drill 4.5) (layers *.Cu *.Mask F.SilkS)
      (net 2 /VCC))
  )
  (module xt60board:XT60 (layer F.Cu) (tedit 59B7498D)
    (at 114.3 88.9)
    (fp_text reference J10 (at 3.556 6.096) (layer F.SilkS) hide)
    (fp_text value XT60 (at 3.2 -5.9) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 4.5) (layers *.Cu *.Mask F.SilkS)
      (net 1 /GND))
    (pad 2 thru_hole circle (at 7.5 0) (size 6 6) (drill 4.5) (layers *.Cu *.Mask F.SilkS)
      (net 2 /VCC))
  )
  (module xt60board:XT60 (layer F.Cu) (tedit 59B74988)
    (at 114.3 99.06)
    (fp_text reference J11 (at 3.556 6.096) (layer F.SilkS) hide)
    (fp_text value XT60 (at 3.2 -5.9) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 4.5) (layers *.Cu *.Mask F.SilkS)
      (net 1 /GND))
    (pad 2 thru_hole circle (at 7.5 0) (size 6 6) (drill 4.5) (layers *.Cu *.Mask F.SilkS)
      (net 2 /VCC))
  )
  (module xt60board:XT60 (layer F.Cu) (tedit 59B74974)
    (at 114.3 109.22)
    (fp_text reference J12 (at 3.556 6.096) (layer F.SilkS) hide)
    (fp_text value XT60 (at 3.2 -5.9) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 4.5) (layers *.Cu *.Mask F.SilkS)
      (net 1 /GND))
    (pad 2 thru_hole circle (at 7.5 0) (size 6 6) (drill 4.5) (layers *.Cu *.Mask F.SilkS)
      (net 2 /VCC))
  )
  (module Symbols:OSHW-Logo_5.7x6mm_SilkScreen (layer F.Cu) (tedit 0)
    (at 140.97 117.475)
    (descr "Open Source Hardware Logo")
    (tags "Logo OSHW")
    (attr virtual)
    (fp_text reference REF*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value OSHW-Logo_5.7x6mm_SilkScreen (at 0.75 0) (layer F.Fab) hide)
  )
  (gr_arc (start 140.97 58.42) (end 140.97 53.34) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 114.3 118.11) (end 114.3 123.19) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 140.97 118.11) (end 146.05 118.11) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 109.22 118.11) (end 109.22 58.42) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 140.97 123.19) (end 114.3 123.19) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.05 58.42) (end 146.05 118.11) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.3 53.34) (end 140.97 53.34) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_text "XT60 Board Version 2" (at 124.46 119.38) (layer F.SilkS))
  (gr_text "Justin Easter 2017" (at 124.46 116.84) (layer F.SilkS))
  (gr_text VCC (at 127.635 63.5) (layer F.SilkS))
  (gr_text GND (at 114.3 63.5) (layer F.SilkS))
  (gr_text GND (at 140.97 63.5) (layer F.SilkS))
  (gr_arc (start 114.3 58.42) (end 109.22 58.42) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 1) (net_name /GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 110.49 57.15) (xy 113.03 54.61) (xy 117.475 54.61) (xy 117.475 114.3) (xy 137.795 114.3)
        (xy 137.795 54.61) (xy 142.875 54.61) (xy 144.78 56.515) (xy 144.78 118.745) (xy 141.605 121.92)
        (xy 113.665 121.92) (xy 110.49 118.745)
      )
    )
  )
  (zone (net 2) (net_name /VCC) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 118.745 54.61) (xy 118.745 113.03) (xy 136.525 113.03) (xy 136.525 54.61)
      )
    )
  )
  (zone (net 1) (net_name /GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 110.49 57.15) (xy 113.03 54.61) (xy 117.475 54.61) (xy 117.475 114.3) (xy 137.795 114.3)
        (xy 137.795 54.61) (xy 142.875 54.61) (xy 144.78 56.515) (xy 144.78 118.745) (xy 141.605 121.92)
        (xy 113.665 121.92) (xy 110.49 118.745)
      )
    )
  )
  (zone (net 2) (net_name /VCC) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 118.745 54.61) (xy 118.745 113.03) (xy 136.525 113.03) (xy 136.525 54.61)
      )
    )
  )
)
