<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<text>SPK_L+</text>
<text>SPK_R+</text>
<text>SPK_L-</text>
<text>SPK_R-</text>
<text>MIC_R-</text>
<text>MIC_L-</text>
<text>MIC_R+</text>
<text>MIC_L+</text>
<text>M_BIAS</text>
<text>GPIO3</text>
<text>GPIO2</text>
<text>ACI0</text>
<text>GPIO4</text>
<text>GPIO5</text>
<text>GPIO12</text>
<text>GPIO13</text>
<text>GPIO11</text>
<text>GPIO10</text>
<text>GPIO9</text>
<text>USBD-</text>
<text>USBD+</text>
<text>GPIO6</text>
<text>GPIO7</text>
<text>PWR_EN</text>
<text>3.3V</text>
<text>UART_RX</text>
<text>UART_TX</text>
<text>UART_CTS</text>
<text>UART_RTS</text>
<text>LED0</text>
<text>LED1</text>
<text>SPI_MOSI</text>
<text>SPI_CLK</text>
<text>SPI_MISO</text>
<text>SPI_SS</text>
<text>PCM_IN</text>
<text>PCM_OUT</text>
<text>PCM_SYNC</text>
<text>PCM_CK</text>
<text>GND</text>
<wire x1="0" y1="51.054" x2="38.1" y2="51.054" width="0.254" layer="20"/>
<wire x1="38.1" y1="51.054" x2="38.1" y2="0" width="0.254" layer="20"/>
<wire x1="38.1" y1="0" x2="0" y2="0" width="0.254" layer="20"/>
<wire x1="0" y1="0" x2="0" y2="51.054" width="0.254" layer="20"/>
<text>RN-52 Breakout</text>
<text>LED1</text>
<text>LED0</text>
<text>V10</text>
<text>SparkFun modified 0.2</text>
</plain>
<libraries>
<library name="SparkFun-RF">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find things that send or receive RF- GPS, cellular modules, Bluetooth, WiFi, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="RN-52">
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CREATIVE_COMMONS">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X20">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-RES">
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="STAND-OFF">
<description>&lt;b&gt;Stand Off&lt;/b&gt;&lt;p&gt;
This is the mechanical footprint for a #4 phillips button head screw. Use the keepout ring to avoid running the screw head into surrounding components. SKU : PRT-00447</description>
</package>
</packages>
</library>
<library name="DougM.LED.LCD">
<packages>
<package name="LED-1206">
</package>
</packages>
</library>
<library name="DougM.capacitor">
<packages>
<package name="0603">
</package>
<package name="PANASONIC_B">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package B&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="SparkFun-RF" package="RN-52" value="BLUETOOTH-RN-52"/>
<element name="FRAME1" library="SparkFun-Aesthetics" package="CREATIVE_COMMONS" value="FRAME-LETTER"/>
<element name="JP1" library="SparkFun-Connectors" package="1X20" value="M20"/>
<element name="JP2" library="SparkFun-Connectors" package="1X20" value="M20"/>
<element name="R1" library="SparkFun-Resistors" package="0603-RES" value="330"/>
<element name="R2" library="SparkFun-Resistors" package="0603-RES" value="330"/>
<element name="STANDOFF1" library="SparkFun-Electromechanical" package="STAND-OFF" value="STAND-OFF"/>
<element name="STANDOFF2" library="SparkFun-Electromechanical" package="STAND-OFF" value="STAND-OFF"/>
<element name="LED1" library="DougM.LED.LCD" package="LED-1206" value="grn"/>
<element name="LED2" library="DougM.LED.LCD" package="LED-1206" value="red"/>
<element name="C1" library="DougM.capacitor" package="0603" value="100n"/>
<element name="C2" library="DougM.capacitor" package="PANASONIC_B" value="10uF"/>
</elements>
<signals>
<signal name="GND">
<contactref element="U1" pad="RFG1"/>
<contactref element="U1" pad="RFG2"/>
<contactref element="U1" pad="RFG3"/>
<contactref element="U1" pad="RFG4"/>
<contactref element="U1" pad="RFG5"/>
<contactref element="U1" pad="RFG6"/>
<contactref element="U1" pad="G4"/>
<contactref element="U1" pad="G3"/>
<contactref element="U1" pad="G2"/>
<contactref element="U1" pad="G1"/>
<contactref element="U1" pad="36"/>
<contactref element="JP2" pad="20"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="-"/>
</signal>
<signal name="3.3V">
<contactref element="U1" pad="20"/>
<contactref element="JP1" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="+"/>
</signal>
<signal name="LED0">
<contactref element="U1" pad="30"/>
<contactref element="JP2" pad="10"/>
<contactref element="LED1" pad="C"/>
</signal>
<signal name="LED1">
<contactref element="U1" pad="29"/>
<contactref element="JP2" pad="11"/>
<contactref element="LED2" pad="C"/>
</signal>
<signal name="SPI_MOSI">
<contactref element="U1" pad="28"/>
<contactref element="JP2" pad="12"/>
</signal>
<signal name="SPI_CLK">
<contactref element="U1" pad="27"/>
<contactref element="JP2" pad="13"/>
</signal>
<signal name="SPI_MISO">
<contactref element="U1" pad="26"/>
<contactref element="JP2" pad="14"/>
</signal>
<signal name="SPI_SS">
<contactref element="U1" pad="25"/>
<contactref element="JP2" pad="15"/>
</signal>
<signal name="MIC_BIAS">
<contactref element="U1" pad="31"/>
<contactref element="JP2" pad="9"/>
</signal>
<signal name="MIC_L+">
<contactref element="U1" pad="32"/>
<contactref element="JP2" pad="8"/>
</signal>
<signal name="MIC_R+">
<contactref element="U1" pad="33"/>
<contactref element="JP2" pad="7"/>
</signal>
<signal name="MIC_L-">
<contactref element="U1" pad="34"/>
<contactref element="JP2" pad="6"/>
</signal>
<signal name="MIC_R-">
<contactref element="U1" pad="35"/>
<contactref element="JP2" pad="5"/>
</signal>
<signal name="PCM_CLK">
<contactref element="U1" pad="24"/>
<contactref element="JP2" pad="16"/>
</signal>
<signal name="PCM_SYNC">
<contactref element="U1" pad="23"/>
<contactref element="JP2" pad="17"/>
</signal>
<signal name="PCM_OUT">
<contactref element="U1" pad="22"/>
<contactref element="JP2" pad="18"/>
</signal>
<signal name="PCM_IN">
<contactref element="U1" pad="21"/>
<contactref element="JP2" pad="19"/>
</signal>
<signal name="SPKR_L+">
<contactref element="U1" pad="40"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="SPKR_R+">
<contactref element="U1" pad="39"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="SPKR_L-">
<contactref element="U1" pad="38"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="SPKR_R-">
<contactref element="U1" pad="37"/>
<contactref element="JP2" pad="4"/>
</signal>
<signal name="PWREN">
<contactref element="U1" pad="19"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="GPIO3">
<contactref element="U1" pad="1"/>
<contactref element="JP1" pad="20"/>
</signal>
<signal name="GPIO2">
<contactref element="U1" pad="2"/>
<contactref element="JP1" pad="19"/>
</signal>
<signal name="AIC0">
<contactref element="U1" pad="3"/>
<contactref element="JP1" pad="18"/>
</signal>
<signal name="GPIO4">
<contactref element="U1" pad="4"/>
<contactref element="JP1" pad="17"/>
</signal>
<signal name="GPIO5">
<contactref element="U1" pad="5"/>
<contactref element="JP1" pad="16"/>
</signal>
<signal name="GPIO12">
<contactref element="U1" pad="6"/>
<contactref element="JP1" pad="15"/>
</signal>
<signal name="GPIO13">
<contactref element="U1" pad="7"/>
<contactref element="JP1" pad="14"/>
</signal>
<signal name="GPIO11">
<contactref element="U1" pad="8"/>
<contactref element="JP1" pad="13"/>
</signal>
<signal name="GPIO10">
<contactref element="U1" pad="9"/>
<contactref element="JP1" pad="12"/>
</signal>
<signal name="GPIO9">
<contactref element="U1" pad="10"/>
<contactref element="JP1" pad="11"/>
</signal>
<signal name="GPIO7">
<contactref element="U1" pad="17"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="GPIO6">
<contactref element="U1" pad="18"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="USBD-">
<contactref element="U1" pad="11"/>
<contactref element="JP1" pad="10"/>
</signal>
<signal name="USBD+">
<contactref element="U1" pad="12"/>
<contactref element="JP1" pad="9"/>
</signal>
<signal name="UART_RTS">
<contactref element="U1" pad="13"/>
<contactref element="JP1" pad="8"/>
</signal>
<signal name="UART_CTS">
<contactref element="U1" pad="14"/>
<contactref element="JP1" pad="7"/>
</signal>
<signal name="UART_TX">
<contactref element="U1" pad="15"/>
<contactref element="JP1" pad="6"/>
</signal>
<signal name="UART_RX">
<contactref element="U1" pad="16"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="N$1">
<contactref element="R2" pad="1"/>
<contactref element="LED2" pad="A"/>
</signal>
<signal name="N$2">
<contactref element="R1" pad="1"/>
<contactref element="LED1" pad="A"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
