(kicad_pcb (version 20171130) (host pcbnew "(5.1.6-87-g1447494bc)")
  (general
    (thickness 1.6)
    (drawings 50)
    (tracks 58)
    (zones 0)
    (modules 4)
    (nets 8)
  )
  (page A4)
  (title_block
    (title "NanoDAP Adapter")
    (date 2021-05-15)
    (rev v1.0)
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (33 F.Adhes user hide)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.254)
    (user_trace_width 0.4)
    (user_trace_width 0.6096)
    (trace_clearance 0.152)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.762)
    (via_drill 0.508)
    (via_min_size 0.6096)
    (via_min_drill 0.3302)
    (user_via 0.6096 0.3302)
    (user_via 1 0.6)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (edge_width 0.15)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.7 1.7)
    (pad_drill 1)
    (pad_to_mask_clearance 0.1)
    (aux_axis_origin 0 0)
    (grid_origin 117.7 136.8)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "../gerbers"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 NRST)
  (net 3 SWCLK)
  (net 4 SWDIO)
  (net 5 3V3)
  (net 6 RX)
  (net 7 TX)
  (net_class Default "This is the default net class."
    (clearance 0.152)
    (trace_width 0.254)
    (via_dia 0.762)
    (via_drill 0.508)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (add_net 3V3)
    (add_net GND)
    (add_net NRST)
    (add_net RX)
    (add_net SWCLK)
    (add_net SWDIO)
    (add_net TX)
  )
  (net_class Large ""
    (clearance 0.254)
    (trace_width 0.61)
    (via_dia 1)
    (via_drill 0.6)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
  )
  (module nanodap-adapter:10-pin-edge-connector-with-soldermask (layer F.Cu) (tedit 62DF4BC5)
    (at 125.32 133.244)
    (fp_text reference J1 (at 0 4.4 180) (layer F.SilkS) hide)
    (fp_text value "10-pin EDGE CONN" (at 0.2 -4.4 180) (layer F.Fab) hide)
    (pad 9 smd oval (at 5.08 0) (size 1.52 6) (layers B.Cu B.Mask))
    (pad 7 smd oval (at 2.54 0) (size 1.52 6) (layers B.Cu B.Mask)
      (net 5 3V3))
    (pad 5 smd oval (at 0 0) (size 1.52 6) (layers B.Cu B.Mask)
      (net 4 SWDIO))
    (pad 3 smd oval (at -2.54 0) (size 1.52 6) (layers B.Cu B.Mask)
      (net 1 GND))
    (pad 10 smd oval (at 5.08 0) (size 1.52 6) (layers F.Cu F.Mask)
      (net 6 RX))
    (pad 8 smd oval (at 2.54 0) (size 1.52 6) (layers F.Cu F.Mask)
      (net 7 TX))
    (pad 6 smd oval (at 0 0) (size 1.52 6) (layers F.Cu F.Mask)
      (net 2 NRST))
    (pad 4 smd oval (at -2.54 0) (size 1.52 6) (layers F.Cu F.Mask))
    (pad 2 smd oval (at -5.08 0) (size 1.52 6) (layers F.Cu F.Mask))
    (pad 1 smd oval (at -5.08 0) (size 1.52 6) (layers B.Cu B.Mask)
      (net 3 SWCLK))
  )
  (module nanodap-adapter:PinHeader_1x03_P2.54mm_Vertical_Odd_Even (layer F.Cu) (tedit 5F55653D)
    (at 119.351 122.068)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J3 (at 2.049 -0.068 180) (layer F.SilkS) hide)
    (fp_text value Conn_01x03 (at 0 7.41 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 2.54 -90) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0.127 0) (size 1.7 1.7) (drill 0.9144 (offset -0.127 0)) (layers *.Cu *.Mask)
      (net 7 TX))
    (pad 2 thru_hole oval (at -0.127 2.54) (size 1.7 1.7) (drill 0.9144 (offset 0.127 0)) (layers *.Cu *.Mask)
      (net 6 RX))
    (pad 3 thru_hole oval (at 0.127 5) (size 1.7 1.7) (drill 0.9144 (offset -0.127 0)) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Symbol:OSHW-Logo_5.7x6mm_SilkScreen locked (layer B.Cu) (tedit 0)
    (at 126.8 123.7 180)
    (descr "Open Source Hardware Logo")
    (tags "Logo OSHW")
    (attr virtual)
    (fp_text reference REF** (at 0 0) (layer B.SilkS) hide)
    (fp_text value OSHW-Logo_5.7x6mm_SilkScreen (at 0.75 0) (layer B.Fab) hide)
  )
  (module nanodap-adapter:CONN5X2_1.27 (layer F.Cu) (tedit 5F36C86B)
    (at 126.844 124.608 180)
    (fp_text reference J2 (at -4.44 1.835) (layer F.SilkS) hide)
    (fp_text value FTSH-105-01-F-DV-K (at 9.85 -0.58) (layer F.Fab))
    (pad 10 smd rect (at 2.54 -2 180) (size 0.7 2.1) (layers F.Cu F.Paste F.Mask)
      (net 2 NRST))
    (pad 9 smd rect (at 2.54 2 180) (size 0.7 2.1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 8 smd rect (at 1.27 -2 180) (size 0.7 2.1) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at 1.27 2 180) (size 0.7 2.1) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at 0 -2 180) (size 0.7 2.1) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 0 2 180) (size 0.7 2.1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at -1.27 -2 180) (size 0.7 2.1) (layers F.Cu F.Paste F.Mask)
      (net 3 SWCLK))
    (pad 3 smd rect (at -1.27 2 180) (size 0.7 2.1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -2.54 -2 180) (size 0.7 2.1) (layers F.Cu F.Paste F.Mask)
      (net 4 SWDIO))
    (pad 1 smd rect (at -2.54 2 180) (size 0.7 2.1) (layers F.Cu F.Paste F.Mask)
      (net 5 3V3))
    (model ${KIPRJMOD}/libs/FTSH-105-01-F-DV-K-TR--3DModel-STEP-56544.STEP
      (offset (xyz 0.64 0 0.4))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (gr_text v1.0 (at 123.45 124.925) (layer B.SilkS))
  (gr_text GND (at 123.825 129.35) (layer B.SilkS))
  (gr_text TX (at 127.5 129.375) (layer F.SilkS))
  (gr_text RX (at 130.025 129.35) (layer F.SilkS))
  (gr_text NRST (at 123.475 129.35) (layer F.SilkS))
  (gr_text "3V3\n" (at 129.735476 129.375) (layer B.SilkS))
  (gr_text IO (at 125.95 129.375) (layer B.SilkS))
  (gr_text TCK (at 120.975 129.375) (layer B.SilkS))
  (gr_arc (start 130.975 121.8) (end 132.975 121.8) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 119.7 121.8) (end 119.7 119.8) (angle -90) (layer Edge.Cuts) (width 0.15))
  (dimension 9 (width 0.15) (layer F.Fab)
    (gr_text "9.000 mm" (at 166.6 83.1 90) (layer F.Fab))
    (feature1 (pts (xy 169.2 78.6) (xy 167.313579 78.6)))
    (feature2 (pts (xy 169.2 87.6) (xy 167.313579 87.6)))
    (crossbar (pts (xy 167.9 87.6) (xy 167.9 78.6)))
    (arrow1a (pts (xy 167.9 78.6) (xy 168.486421 79.726504)))
    (arrow1b (pts (xy 167.9 78.6) (xy 167.313579 79.726504)))
    (arrow2a (pts (xy 167.9 87.6) (xy 168.486421 86.473496)))
    (arrow2b (pts (xy 167.9 87.6) (xy 167.313579 86.473496)))
  )
  (dimension 3 (width 0.15) (layer F.Fab)
    (gr_text "3.000 mm" (at 164.2 65.85) (layer F.Fab))
    (feature1 (pts (xy 162.7 70.7) (xy 162.7 66.563579)))
    (feature2 (pts (xy 165.7 70.7) (xy 165.7 66.563579)))
    (crossbar (pts (xy 165.7 67.15) (xy 162.7 67.15)))
    (arrow1a (pts (xy 162.7 67.15) (xy 163.826504 66.563579)))
    (arrow1b (pts (xy 162.7 67.15) (xy 163.826504 67.736421)))
    (arrow2a (pts (xy 165.7 67.15) (xy 164.573496 66.563579)))
    (arrow2b (pts (xy 165.7 67.15) (xy 164.573496 67.736421)))
  )
  (dimension 12 (width 0.15) (layer F.Fab)
    (gr_text "12.000 mm" (at 159.7 68.35) (layer F.Fab))
    (feature1 (pts (xy 153.7 70.7) (xy 153.7 69.063579)))
    (feature2 (pts (xy 165.7 70.7) (xy 165.7 69.063579)))
    (crossbar (pts (xy 165.7 69.65) (xy 153.7 69.65)))
    (arrow1a (pts (xy 153.7 69.65) (xy 154.826504 69.063579)))
    (arrow1b (pts (xy 153.7 69.65) (xy 154.826504 70.236421)))
    (arrow2a (pts (xy 165.7 69.65) (xy 164.573496 69.063579)))
    (arrow2b (pts (xy 165.7 69.65) (xy 164.573496 70.236421)))
  )
  (gr_text "TX\n\nRX\n\nGND" (at 120.7 124.6) (layer F.SilkS))
  (dimension 7 (width 0.15) (layer F.Fab)
    (gr_text "7.000 mm" (at 170.5 84.1 90) (layer F.Fab))
    (feature1 (pts (xy 169.2 80.6) (xy 169.786421 80.6)))
    (feature2 (pts (xy 169.2 87.6) (xy 169.786421 87.6)))
    (crossbar (pts (xy 169.2 87.6) (xy 169.2 80.6)))
    (arrow1a (pts (xy 169.2 80.6) (xy 169.786421 81.726504)))
    (arrow1b (pts (xy 169.2 80.6) (xy 168.613579 81.726504)))
    (arrow2a (pts (xy 169.2 87.6) (xy 169.786421 86.473496)))
    (arrow2b (pts (xy 169.2 87.6) (xy 168.613579 86.473496)))
  )
  (dimension 24 (width 0.15) (layer F.Fab)
    (gr_text "24.000 mm" (at 153.7 142.999999) (layer F.Fab))
    (feature1 (pts (xy 165.7 137.6) (xy 165.7 142.28642)))
    (feature2 (pts (xy 141.7 137.6) (xy 141.7 142.28642)))
    (crossbar (pts (xy 141.7 141.699999) (xy 165.7 141.699999)))
    (arrow1a (pts (xy 165.7 141.699999) (xy 164.573496 142.28642)))
    (arrow1b (pts (xy 165.7 141.699999) (xy 164.573496 141.113578)))
    (arrow2a (pts (xy 141.7 141.699999) (xy 142.826504 142.28642)))
    (arrow2b (pts (xy 141.7 141.699999) (xy 142.826504 141.113578)))
  )
  (dimension 24 (width 0.15) (layer F.Fab)
    (gr_text "24.000 mm" (at 129.7 143) (layer F.Fab))
    (feature1 (pts (xy 117.7 137.6) (xy 117.7 142.286421)))
    (feature2 (pts (xy 141.7 137.6) (xy 141.7 142.286421)))
    (crossbar (pts (xy 141.7 141.7) (xy 117.7 141.7)))
    (arrow1a (pts (xy 117.7 141.7) (xy 118.826504 141.113579)))
    (arrow1b (pts (xy 117.7 141.7) (xy 118.826504 142.286421)))
    (arrow2a (pts (xy 141.7 141.7) (xy 140.573496 141.113579)))
    (arrow2b (pts (xy 141.7 141.7) (xy 140.573496 142.286421)))
  )
  (dimension 19.2 (width 0.15) (layer F.Fab)
    (gr_text "19.200 mm" (at 176.5 127.2 270) (layer F.Fab))
    (feature1 (pts (xy 161.7 136.8) (xy 175.786421 136.8)))
    (feature2 (pts (xy 161.7 117.6) (xy 175.786421 117.6)))
    (crossbar (pts (xy 175.2 117.6) (xy 175.2 136.8)))
    (arrow1a (pts (xy 175.2 136.8) (xy 174.613579 135.673496)))
    (arrow1b (pts (xy 175.2 136.8) (xy 175.786421 135.673496)))
    (arrow2a (pts (xy 175.2 117.6) (xy 174.613579 118.726504)))
    (arrow2b (pts (xy 175.2 117.6) (xy 175.786421 118.726504)))
  )
  (dimension 18 (width 0.15) (layer F.Fab)
    (gr_text "18.000 mm" (at 173.5 126.6 270) (layer F.Fab))
    (feature1 (pts (xy 161.7 135.6) (xy 172.786421 135.6)))
    (feature2 (pts (xy 161.7 117.6) (xy 172.786421 117.6)))
    (crossbar (pts (xy 172.2 117.6) (xy 172.2 135.6)))
    (arrow1a (pts (xy 172.2 135.6) (xy 171.613579 134.473496)))
    (arrow1b (pts (xy 172.2 135.6) (xy 172.786421 134.473496)))
    (arrow2a (pts (xy 172.2 117.6) (xy 171.613579 118.726504)))
    (arrow2b (pts (xy 172.2 117.6) (xy 172.786421 118.726504)))
  )
  (dimension 13.6 (width 0.15) (layer F.Fab)
    (gr_text "13.600 mm" (at 170.5 124.4 270) (layer F.Fab))
    (feature1 (pts (xy 141.7 131.2) (xy 169.786421 131.2)))
    (feature2 (pts (xy 141.7 117.6) (xy 169.786421 117.6)))
    (crossbar (pts (xy 169.2 117.6) (xy 169.2 131.2)))
    (arrow1a (pts (xy 169.2 131.2) (xy 168.613579 130.073496)))
    (arrow1b (pts (xy 169.2 131.2) (xy 169.786421 130.073496)))
    (arrow2a (pts (xy 169.2 117.6) (xy 168.613579 118.726504)))
    (arrow2b (pts (xy 169.2 117.6) (xy 169.786421 118.726504)))
  )
  (dimension 66.1 (width 0.15) (layer F.Fab)
    (gr_text "66.100 mm" (at 111.3 103.75 270) (layer F.Fab))
    (feature1 (pts (xy 117 136.8) (xy 112.413579 136.8)))
    (feature2 (pts (xy 117 70.7) (xy 112.413579 70.7)))
    (crossbar (pts (xy 113 70.7) (xy 113 136.8)))
    (arrow1a (pts (xy 113 136.8) (xy 112.413579 135.673496)))
    (arrow1b (pts (xy 113 136.8) (xy 113.586421 135.673496)))
    (arrow2a (pts (xy 113 70.7) (xy 112.413579 71.826504)))
    (arrow2b (pts (xy 113 70.7) (xy 113.586421 71.826504)))
  )
  (dimension 12 (width 0.15) (layer F.Fab)
    (gr_text "12.000 mm" (at 147.7 84.700001) (layer F.Fab))
    (feature1 (pts (xy 141.7 87.6) (xy 141.7 85.41358)))
    (feature2 (pts (xy 153.7 87.6) (xy 153.7 85.41358)))
    (crossbar (pts (xy 153.7 86.000001) (xy 141.7 86.000001)))
    (arrow1a (pts (xy 141.7 86.000001) (xy 142.826504 85.41358)))
    (arrow1b (pts (xy 141.7 86.000001) (xy 142.826504 86.586422)))
    (arrow2a (pts (xy 153.7 86.000001) (xy 152.573496 85.41358)))
    (arrow2b (pts (xy 153.7 86.000001) (xy 152.573496 86.586422)))
  )
  (dimension 24 (width 0.15) (layer F.Fab)
    (gr_text "24.000 mm" (at 141.7 82.2) (layer F.Fab))
    (feature1 (pts (xy 153.7 87.6) (xy 153.7 82.913579)))
    (feature2 (pts (xy 129.7 87.6) (xy 129.7 82.913579)))
    (crossbar (pts (xy 129.7 83.5) (xy 153.7 83.5)))
    (arrow1a (pts (xy 153.7 83.5) (xy 152.573496 84.086421)))
    (arrow1b (pts (xy 153.7 83.5) (xy 152.573496 82.913579)))
    (arrow2a (pts (xy 129.7 83.5) (xy 130.826504 84.086421)))
    (arrow2b (pts (xy 129.7 83.5) (xy 130.826504 82.913579)))
  )
  (dimension 30 (width 0.15) (layer F.Fab)
    (gr_text "30.000 mm" (at 170.5 102.6 90) (layer F.Fab))
    (feature1 (pts (xy 161.7 87.6) (xy 169.786421 87.6)))
    (feature2 (pts (xy 161.7 117.6) (xy 169.786421 117.6)))
    (crossbar (pts (xy 169.2 117.6) (xy 169.2 87.6)))
    (arrow1a (pts (xy 169.2 87.6) (xy 169.786421 88.726504)))
    (arrow1b (pts (xy 169.2 87.6) (xy 168.613579 88.726504)))
    (arrow2a (pts (xy 169.2 117.6) (xy 169.786421 116.473496)))
    (arrow2b (pts (xy 169.2 117.6) (xy 168.613579 116.473496)))
  )
  (dimension 20 (width 0.15) (layer F.Fab)
    (gr_text "20.000 mm" (at 151.7 140.5) (layer F.Fab))
    (feature1 (pts (xy 161.7 117.6) (xy 161.7 139.786421)))
    (feature2 (pts (xy 141.7 117.6) (xy 141.7 139.786421)))
    (crossbar (pts (xy 141.7 139.2) (xy 161.7 139.2)))
    (arrow1a (pts (xy 161.7 139.2) (xy 160.573496 139.786421)))
    (arrow1b (pts (xy 161.7 139.2) (xy 160.573496 138.613579)))
    (arrow2a (pts (xy 141.7 139.2) (xy 142.826504 139.786421)))
    (arrow2b (pts (xy 141.7 139.2) (xy 142.826504 138.613579)))
  )
  (dimension 20 (width 0.15) (layer F.Fab)
    (gr_text "20.000 mm" (at 131.7 140.5) (layer F.Fab))
    (feature1 (pts (xy 141.7 117.6) (xy 141.7 139.786421)))
    (feature2 (pts (xy 121.7 117.6) (xy 121.7 139.786421)))
    (crossbar (pts (xy 121.7 139.2) (xy 141.7 139.2)))
    (arrow1a (pts (xy 141.7 139.2) (xy 140.573496 139.786421)))
    (arrow1b (pts (xy 141.7 139.2) (xy 140.573496 138.613579)))
    (arrow2a (pts (xy 121.7 139.2) (xy 122.826504 139.786421)))
    (arrow2b (pts (xy 121.7 139.2) (xy 122.826504 138.613579)))
  )
  (gr_line (start 130.975 119.8) (end 119.7 119.8) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 117.7 121.8) (end 117.7 136.8) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 117.7 136.8) (end 132.975 136.8) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 132.975 136.8) (end 132.975 121.8) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 132.8125 135.46875) (xy 117.5375 135.43125) (xy 117.7 119.8) (xy 132.975 119.8375)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.255))
    (polygon
      (pts
        (xy 133.00625 135.50625) (xy 117.69375 135.44375) (xy 117.7 119.8) (xy 133.0125 119.8625)
      )
    )
  )
)
