<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.4.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="88.9" x2="0" y2="0" width="0.254" layer="20"/>
<wire x1="0" y1="0" x2="190.5" y2="0" width="0.254" layer="20"/>
<wire x1="190.5" y1="88.9" x2="190.5" y2="0" width="0.254" layer="20"/>
<wire x1="0" y1="88.9" x2="190.5" y2="88.9" width="0.254" layer="20"/>
<hole x="5.715" y="5.715" drill="3.81"/>
<hole x="5.715" y="83.185" drill="3.81"/>
<hole x="184.785" y="83.185" drill="3.81"/>
<hole x="184.785" y="5.715" drill="3.81"/>
<text>LED DRIVER</text>
<text>PMT H
CTRL</text>
<text>PMT
HEATER</text>
<text>FAN1</text>
<text>FAN2</text>
<text>INLET T1</text>
<text>INLET T2</text>
<text>3-WAY
VALVE</text>
<text>PUMP SPEED</text>
<text>PUMP
CTRL</text>
<text>PMT AMP
POWER</text>
<text>+24V
SPARE</text>
<text>+5V 
SPARE</text>
<text>HUMIDITY</text>
<text>SIGNAL DP</text>
<text>+24V

GND</text>
<text>ground jumpers</text>
<text>ROZE LED-DP BOARD
September 2019
v 3.0.0</text>
<text>CELL H CTRL</text>
<text>CELL
HEATER</text>
<text>UV LED ASSY</text>
<text>LED TEC</text>
<text>Jumper for voltage ctrl</text>
</plain>
<libraries>
<library name="parts">
<packages>
<package name="IXYX_DIP_6">
<description>6-DIP, 2.54 mm (0.10 in) pitch, 7.60 mm (0.30 in) span, 8.38 X 6.47 X 4.06 mm body
&lt;p&gt;6-pin DIP package with 2.54 mm (0.10 in) pitch, 7.60 mm (0.30 in) span with body size 8.38 X 6.47 X 4.06 mm&lt;/p&gt;</description>
</package>
<package name="COOLCUBE">
</package>
<package name="MINCO_CT335">
</package>
<package name="DIP_08">
<description>8-DIP, 2.54 mm (0.10 in) pitch, 7.87 mm (0.31 in) span, 9.50 X 6.60 X 5.33 mm body
&lt;p&gt;8-pin DIP package with 2.54 mm (0.10 in) pitch, 7.87 mm (0.31 in) span with body size 9.50 X 6.60 X 5.33 mm&lt;/p&gt;</description>
</package>
<package name="RES_1/4_WATT">
<description>Axial Resistor, 10.26 mm pitch, 6.50 mm body length, 2.50 mm body diameter
&lt;p&gt;Axial Resistor package with 10.26 mm pitch, 0.63 mm lead diameter, 6.50 mm body length and 2.50 mm body diameter&lt;/p&gt;</description>
</package>
<package name="BEADC2016X70">
<description>Chip, 2.00 X 1.60 X 0.70 mm body
&lt;p&gt;Chip package with body size 2.00 X 1.60 X 0.70 mm&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="parts">
<description>&lt;h1&gt;ROZE parts&lt;/h1&gt;
&lt;p&gt;This library contains all the parts needed for the ROZE instrument. &lt;/p&gt;</description>
<packages>
<package name="TE_103735-1">
</package>
<package name="TE_103735-2">
</package>
<package name="TE_103735-3">
</package>
<package name="TE_103735-4">
</package>
<package name="TE_103735-5">
</package>
<package name="TE_103735-6">
</package>
<package name="TE_103735-8">
</package>
<package name="MOL_MICROFIT3_16">
</package>
<package name="MOL_MICROFIT3_20">
</package>
<package name="CUI_PDQXX-D">
</package>
<package name="TE_641964">
</package>
<package name="EPCOS_B32529">
<description>this footprint is valid for the .22uF and smaller capacitors. larger ones in this series may require larger tolerances.</description>
</package>
<package name="RECOM_R-78C-1.0">
</package>
<package name="BOURNS_3296">
</package>
<package name="6PINHEADER">
<description>Double-row, 6-pin Pin Header (Male) Straight, 2.54 mm (0.10 in) row pitch, 2.54 mm (0.10 in) col pitch, 6.00 mm mating length, 7.62 X 5.08 X 8.54 mm body
&lt;p&gt;Double-row (2X3), 6-pin Pin Header (Male) Straight package with 2.54 mm (0.10 in) row pitch, 2.54 mm (0.10 in) col pitch, 0.64 mm lead width, 3.00 mm tail length and 6.00 mm mating length with overall size 7.62 X 5.08 X 8.54 mm, pin pattern - counter-clockwise from bottom left&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="mastar_components">
<packages>
<package name="MEATBALL_4IN_SILK">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J70" library="parts" package="MOL_MICROFIT3_16" value="MOLEX_MICROFIT3_16PIN">
<attribute name="NAME"/>
</element>
<element name="J71" library="parts" package="TE_103735-5" value="AMPMODU_MTE_6">
<attribute name="NAME"/>
</element>
<element name="J72" library="parts" package="TE_103735-8" value="AMPMODU_MTE_9">
<attribute name="NAME"/>
</element>
<element name="J73" library="parts" package="TE_103735-6" value="AMPMODU_MTE_7">
<attribute name="NAME"/>
</element>
<element name="J74" library="parts" package="TE_103735-3" value="AMPMODU_MTE_4">
<attribute name="NAME"/>
</element>
<element name="J75" library="parts" package="TE_103735-6" value="AMPMODU_MTE_7">
<attribute name="NAME"/>
</element>
<element name="J76" library="parts" package="TE_103735-3" value="AMPMODU_MTE_4">
<attribute name="NAME"/>
</element>
<element name="J77" library="parts" package="TE_103735-1" value="AMPMODU_MTE_2">
<attribute name="NAME"/>
</element>
<element name="J78" library="parts" package="TE_103735-1" value="AMPMODU_MTE_2">
<attribute name="NAME"/>
</element>
<element name="J79" library="parts" package="TE_103735-5" value="AMPMODU_MTE_6">
<attribute name="NAME"/>
</element>
<element name="J80" library="parts" package="TE_103735-5" value="AMPMODU_MTE_6">
<attribute name="NAME"/>
</element>
<element name="J81" library="parts" package="TE_103735-1" value="AMPMODU_MTE_2">
<attribute name="NAME"/>
</element>
<element name="J82" library="parts" package="TE_103735-3" value="AMPMODU_MTE_4">
<attribute name="NAME"/>
</element>
<element name="J83" library="parts" package="TE_103735-1" value="AMPMODU_MTE_2">
<attribute name="NAME"/>
</element>
<element name="J84" library="parts" package="TE_103735-2" value="AMPMODU_MTE_3">
<attribute name="NAME"/>
</element>
<element name="J85" library="parts" package="TE_103735-1" value="AMPMODU_MTE_2">
<attribute name="NAME"/>
</element>
<element name="J86" library="parts" package="TE_103735-1" value="AMPMODU_MTE_2">
<attribute name="NAME"/>
</element>
<element name="J87" library="parts" package="TE_103735-4" value="AMPMODU_MTE_5">
<attribute name="NAME"/>
</element>
<element name="J88" library="parts" package="MOL_MICROFIT3_20" value="MOLEX_MICROFIT3_20PIN">
<attribute name="NAME"/>
</element>
<element name="K2" library="parts" package="IXYX_DIP_6" value="PLA150X_DC">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U10" library="parts" package="COOLCUBE" value="COOLCUBE"/>
<element name="U3" library="parts" package="MINCO_CT335" value="MINCO_CT335XX2">
<attribute name="NAME"/>
</element>
<element name="U1" library="parts" package="DIP_08" value="MCP6021XX/P">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U7" library="parts" package="CUI_PDQXX-D" value="PDQ30-SINGLE">
<attribute name="NAME"/>
</element>
<element name="R1" library="parts" package="RES_1/4_WATT" value="240">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="parts" package="BEADC2016X70" value="JP_OPEN"/>
<element name="JP2" library="parts" package="BEADC2016X70" value="JP_OPEN"/>
<element name="JP3" library="parts" package="BEADC2016X70" value="JP_OPEN"/>
<element name="U2" library="parts" package="RECOM_R-78C-1.0" value="R-78C-1.0">
<attribute name="NAME"/>
</element>
<element name="R5" library="parts" package="RES_1/4_WATT" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U4" library="parts" package="DIP_08" value="REF01">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="parts" package="BOURNS_3296" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="parts" package="BOURNS_3296" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="parts" package="BOURNS_3296" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J69" library="parts" package="TE_641964" value="TE_641964">
<attribute name="NAME"/>
</element>
<element name="C1" library="parts" package="EPCOS_B32529" value=".1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="parts" package="EPCOS_B32529" value=".1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="parts" package="EPCOS_B32529" value=".1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="parts" package="EPCOS_B32529" value=".1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="parts" package="EPCOS_B32529" value=".1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="parts" package="EPCOS_B32529" value=".1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="parts" package="EPCOS_B32529" value=".1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="parts" package="RES_1/4_WATT" value="2M">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JMP1" library="parts" package="6PINHEADER" value="6PIN_HEADER">
<attribute name="NAME"/>
</element>
<element name="U$1" library="mastar_components" package="MEATBALL_4IN_SILK" value=""/>
</elements>
<signals>
<signal name="LED+">
<contactref element="J70" pad="P$1"/>
<contactref element="J71" pad="P$5"/>
</signal>
<signal name="LED-">
<contactref element="J70" pad="P$2"/>
<contactref element="J71" pad="P$6"/>
</signal>
<signal name="TEC+">
<contactref element="J70" pad="P$3"/>
<contactref element="J72" pad="P$5"/>
</signal>
<signal name="TEC-">
<contactref element="J72" pad="P$6"/>
<contactref element="J70" pad="P$4"/>
</signal>
<signal name="COLD_SENSE+">
<contactref element="J72" pad="P$1"/>
<contactref element="J70" pad="P$5"/>
</signal>
<signal name="COLD_SENSE-">
<contactref element="J72" pad="P$2"/>
<contactref element="J70" pad="P$6"/>
</signal>
<signal name="ENABLE_OUT">
<contactref element="J72" pad="P$7"/>
<contactref element="J70" pad="P$10"/>
</signal>
<signal name="LED_I">
<contactref element="J71" pad="P$3"/>
<contactref element="J88" pad="P$4"/>
</signal>
<signal name="CELL_SENSE+">
<contactref element="J73" pad="P$1"/>
<contactref element="J74" pad="P$1"/>
</signal>
<signal name="CELL_SENSE-">
<contactref element="J73" pad="P$2"/>
<contactref element="J74" pad="P$2"/>
</signal>
<signal name="CELLHTR+">
<contactref element="J73" pad="P$5"/>
<contactref element="J74" pad="P$3"/>
</signal>
<signal name="CELL_T">
<contactref element="J73" pad="P$7"/>
<contactref element="J88" pad="P$5"/>
</signal>
<signal name="PMT_SENSE+">
<contactref element="J75" pad="P$1"/>
<contactref element="J76" pad="P$1"/>
</signal>
<signal name="PMT_SENSE-">
<contactref element="J75" pad="P$2"/>
<contactref element="J76" pad="P$2"/>
</signal>
<signal name="PMTHTR+">
<contactref element="J75" pad="P$5"/>
<contactref element="J76" pad="P$3"/>
</signal>
<signal name="PMT_T">
<contactref element="J75" pad="P$7"/>
<contactref element="J88" pad="P$9"/>
</signal>
<signal name="INLET_T1+">
<contactref element="J79" pad="P$5"/>
<contactref element="J88" pad="P$10"/>
</signal>
<signal name="INLET_T2+">
<contactref element="J80" pad="P$5"/>
<contactref element="J88" pad="P$11"/>
</signal>
<signal name="CC+LOAD">
<contactref element="U10" pad="P$1"/>
<contactref element="J81" pad="P$1"/>
</signal>
<signal name="CC-LOAD">
<contactref element="J81" pad="P$2"/>
<contactref element="U10" pad="P$2"/>
</signal>
<signal name="+24V">
<contactref element="J78" pad="P$1"/>
<contactref element="J77" pad="P$1"/>
<contactref element="J73" pad="P$3"/>
<contactref element="J74" pad="P$4"/>
<contactref element="J75" pad="P$3"/>
<contactref element="J76" pad="P$4"/>
<contactref element="J79" pad="P$3"/>
<contactref element="J80" pad="P$3"/>
<contactref element="J84" pad="P$1"/>
<contactref element="J85" pad="P$1"/>
<contactref element="U3" pad="P$1"/>
<contactref element="U2" pad="P$1"/>
<contactref element="U7" pad="P$1"/>
<contactref element="K2" pad="4"/>
<contactref element="K2" pad="6"/>
<contactref element="U4" pad="2"/>
<contactref element="J69" pad="P$1"/>
<contactref element="C5" pad="P$2"/>
<contactref element="C4" pad="P$2"/>
<contactref element="C1" pad="P$2"/>
</signal>
<signal name="+5V">
<contactref element="J86" pad="P$1"/>
<contactref element="J87" pad="P$4"/>
<contactref element="R1" pad="2"/>
<contactref element="J70" pad="P$11"/>
<contactref element="U7" pad="P$3"/>
<contactref element="J72" pad="P$3"/>
<contactref element="R5" pad="2"/>
<contactref element="C6" pad="P$2"/>
</signal>
<signal name="HUM_T+">
<contactref element="J87" pad="P$1"/>
<contactref element="J88" pad="P$18"/>
</signal>
<signal name="RHUMIDITY">
<contactref element="J87" pad="P$3"/>
<contactref element="J88" pad="P$3"/>
</signal>
<signal name="RTD1+">
<contactref element="J79" pad="P$1"/>
<contactref element="U3" pad="P$13"/>
</signal>
<signal name="RTD1-">
<contactref element="J79" pad="P$2"/>
<contactref element="U3" pad="P$12"/>
</signal>
<signal name="HTR1">
<contactref element="J79" pad="P$4"/>
<contactref element="U3" pad="P$4"/>
</signal>
<signal name="RTD2+">
<contactref element="J80" pad="P$1"/>
<contactref element="U3" pad="P$11"/>
</signal>
<signal name="RTD2-">
<contactref element="J80" pad="P$2"/>
<contactref element="U3" pad="P$10"/>
</signal>
<signal name="HTR2">
<contactref element="J80" pad="P$4"/>
<contactref element="U3" pad="P$5"/>
</signal>
<signal name="GND">
<contactref element="U3" pad="P$3"/>
<contactref element="U3" pad="P$2"/>
<contactref element="J77" pad="P$2"/>
<contactref element="J78" pad="P$2"/>
<contactref element="J75" pad="P$4"/>
<contactref element="J75" pad="P$6"/>
<contactref element="J73" pad="P$4"/>
<contactref element="J73" pad="P$6"/>
<contactref element="J79" pad="P$6"/>
<contactref element="J80" pad="P$6"/>
<contactref element="J85" pad="P$2"/>
<contactref element="J84" pad="P$3"/>
<contactref element="JP3" pad="2"/>
<contactref element="JP2" pad="2"/>
<contactref element="JP1" pad="2"/>
<contactref element="U7" pad="P$2"/>
<contactref element="J86" pad="P$2"/>
<contactref element="J83" pad="P$2"/>
<contactref element="J87" pad="P$2"/>
<contactref element="J87" pad="P$5"/>
<contactref element="U1" pad="4"/>
<contactref element="J70" pad="P$12"/>
<contactref element="U7" pad="P$5"/>
<contactref element="J72" pad="P$4"/>
<contactref element="U10" pad="P$3"/>
<contactref element="J72" pad="P$8"/>
<contactref element="J70" pad="P$8"/>
<contactref element="U4" pad="4"/>
<contactref element="J71" pad="P$2"/>
<contactref element="J71" pad="P$4"/>
<contactref element="U2" pad="P$2"/>
<contactref element="J69" pad="P$2"/>
<contactref element="C4" pad="P$1"/>
<contactref element="C1" pad="P$1"/>
<contactref element="C5" pad="P$1"/>
<contactref element="C6" pad="P$1"/>
<contactref element="C2" pad="P$1"/>
<contactref element="C3" pad="P$1"/>
<contactref element="J70" pad="P$13"/>
<contactref element="U1" pad="3"/>
<contactref element="JMP1" pad="1"/>
<contactref element="JMP1" pad="2"/>
<contactref element="JMP1" pad="3"/>
</signal>
<signal name="UV_PD-">
<contactref element="J70" pad="P$14"/>
<contactref element="U1" pad="2"/>
<contactref element="R4" pad="1"/>
<contactref element="C7" pad="P$1"/>
</signal>
<signal name="COLD_T">
<contactref element="J72" pad="P$9"/>
<contactref element="J88" pad="P$1"/>
</signal>
<signal name="+9V">
<contactref element="J71" pad="P$1"/>
<contactref element="U2" pad="P$3"/>
<contactref element="C3" pad="P$2"/>
</signal>
<signal name="GND_JUMPER2">
<contactref element="J88" pad="P$15"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="GND_JUMPER3">
<contactref element="J88" pad="P$16"/>
<contactref element="JP3" pad="1"/>
</signal>
<signal name="GND_JUMPER1">
<contactref element="J88" pad="P$14"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="UV_MON">
<contactref element="U1" pad="6"/>
<contactref element="J88" pad="P$19"/>
<contactref element="R4" pad="2"/>
<contactref element="C7" pad="P$2"/>
</signal>
<signal name="N$7">
<contactref element="K2" pad="5"/>
<contactref element="U10" pad="P$4"/>
</signal>
<signal name="VALVE">
<contactref element="K2" pad="1"/>
<contactref element="J88" pad="P$12"/>
</signal>
<signal name="HOT_T">
<contactref element="J70" pad="P$7"/>
<contactref element="J88" pad="P$2"/>
</signal>
<signal name="ENABLE_IN">
<contactref element="J70" pad="P$9"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="VALVE_RTN">
<contactref element="K2" pad="2"/>
<contactref element="J88" pad="P$13"/>
</signal>
<signal name="FAST">
<contactref element="J82" pad="P$2"/>
<contactref element="R3" pad="P$3"/>
</signal>
<signal name="MEDIUM">
<contactref element="J82" pad="P$3"/>
<contactref element="R2" pad="P$3"/>
</signal>
<signal name="SLOW">
<contactref element="J82" pad="P$4"/>
<contactref element="R6" pad="P$3"/>
</signal>
<signal name="MOTOR_SPEED_SETTING">
<contactref element="R6" pad="P$2"/>
<contactref element="J83" pad="P$1"/>
<contactref element="R2" pad="P$2"/>
<contactref element="R3" pad="P$2"/>
</signal>
<signal name="N$3">
<contactref element="J82" pad="P$1"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="+5V_QUIET">
<contactref element="U4" pad="6"/>
<contactref element="C2" pad="P$2"/>
<contactref element="U1" pad="7"/>
</signal>
<signal name="N$1">
<contactref element="R6" pad="P$1"/>
<contactref element="JMP1" pad="4"/>
</signal>
<signal name="N$2">
<contactref element="R2" pad="P$1"/>
<contactref element="JMP1" pad="5"/>
</signal>
<signal name="N$4">
<contactref element="R3" pad="P$1"/>
<contactref element="JMP1" pad="6"/>
</signal>
<signal name="N$14">
</signal>
<signal name="N$15">
</signal>
</signals>
</board>
</drawing>
</eagle>
