(kicad_pcb (version 20171130) (host pcbnew "(5.0.0-rc2-183-g147c1e6)")
  (general
    (thickness 1.6)
    (drawings 6)
    (tracks 139)
    (zones 0)
    (modules 10)
    (nets 17)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(D1-Pad2)")
  (net 2 "Net-(J3-Pad3)")
  (net 3 "Net-(J3-Pad4)")
  (net 4 "Net-(R3-Pad1)")
  (net 5 "Net-(R4-Pad1)")
  (net 6 "Net-(U1-Pad3)")
  (net 7 "Net-(U1-Pad4)")
  (net 8 "Net-(U1-Pad13)")
  (net 9 "Net-(U1-Pad14)")
  (net 10 "Net-(U1-Pad12)")
  (net 11 GND)
  (net 12 "Net-(J1-Pad2)")
  (net 13 "Net-(J1-Pad3)")
  (net 14 "Net-(J1-Pad4)")
  (net 15 "Net-(J2-Pad4)")
  (net 16 "Net-(J2-Pad3)")
  (net_class Default "Это класс цепей по умолчанию."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(J3-Pad3)")
    (add_net "Net-(J3-Pad4)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(R4-Pad1)")
    (add_net "Net-(U1-Pad12)")
    (add_net "Net-(U1-Pad13)")
    (add_net "Net-(U1-Pad14)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U1-Pad4)")
  )
  (module LEDs:LED_1206_HandSoldering (layer F.Cu) (tedit 595FC724)
    (at 168.91 90.5195 90)
    (descr "LED SMD 1206, hand soldering")
    (tags "LED 1206")
    (attr smd)
    (fp_text reference D1 (at 4.1595 0 180) (layer F.SilkS))
    (fp_text value LED (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 11 GND))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58307BE8)
    (at 134.62 96.52 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R1 (at 0 -2.54) (layer F.SilkS))
    (fp_text value 4.7k (at 0 2.3 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J3-Pad3)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(J1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58307BE8)
    (at 140.335 96.52)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R2 (at 0 2.54) (layer F.SilkS))
    (fp_text value 4.7k (at 0 2.3) (layer F.Fab))
    (pad 2 smd rect (at 1.45 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(J1-Pad2)"))
    (pad 1 smd rect (at -1.45 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J3-Pad4)"))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58307BE8)
    (at 146.05 96.52 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R3 (at 0.127 -2.54 180) (layer F.SilkS))
    (fp_text value 200 (at 0 2.3 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(R3-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(J1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58307BE8)
    (at 164.465 89.916)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R4 (at 0 -2.3) (layer F.SilkS))
    (fp_text value 200 (at 0 2.3) (layer F.Fab))
    (pad 2 smd rect (at 1.45 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -1.45 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(R4-Pad1)"))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module wsens:HOLYIOT_17095 (layer F.Cu) (tedit 5B2A2753)
    (at 155.575 91.44)
    (fp_text reference U1 (at 5.715 -5.08) (layer F.SilkS))
    (fp_text value HOLYIOT-17095 (at -0.1 -5.08) (layer F.Fab))
    (pad 1 smd rect (at -4.74 -1.35) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(J1-Pad4)"))
    (pad 2 smd rect (at -4.74 -0.08) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(J1-Pad3)"))
    (pad 3 smd rect (at -4.74 1.19) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(U1-Pad3)"))
    (pad 4 smd rect (at -4.74 2.46) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(U1-Pad4)"))
    (pad 5 smd rect (at -4.74 3.73) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(R4-Pad1)"))
    (pad 13 smd rect (at 4.67 1.19) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(U1-Pad13)"))
    (pad 15 smd rect (at 4.67 -1.35) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 11 GND))
    (pad 11 smd rect (at 4.67 3.73) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(J1-Pad2)"))
    (pad 14 smd rect (at 4.67 -0.08) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(U1-Pad14)"))
    (pad 12 smd rect (at 4.67 2.46) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(U1-Pad12)"))
    (pad 8 smd rect (at -0.03 4.6 90) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(J2-Pad4)"))
    (pad 6 smd rect (at -2.57 4.6 90) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(R3-Pad1)"))
    (pad 10 smd rect (at 2.51 4.6 90) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J3-Pad3)"))
    (pad 7 smd rect (at -1.3 4.6 90) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(J2-Pad3)"))
    (pad 9 smd rect (at 1.24 4.6 90) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J3-Pad4)"))
  )
  (module Connectors_JST:JST_PH_B4B-PH-K_04x2.00mm_Straight (layer F.Cu) (tedit 56B07786)
    (at 139.954 91.44)
    (descr http://www.jst-mfg.com/product/pdf/eng/ePH.pdf)
    (tags "connector jst ph")
    (fp_text reference J1 (at 0 -3) (layer F.SilkS))
    (fp_text value SWD (at 3 4) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.2 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 11 GND))
    (pad 2 thru_hole oval (at 2 0) (size 1.2 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad2)"))
    (pad 3 thru_hole oval (at 4 0) (size 1.2 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 13 "Net-(J1-Pad3)"))
    (pad 4 thru_hole oval (at 6 0) (size 1.2 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 14 "Net-(J1-Pad4)"))
  )
  (module Connectors_JST:JST_PH_B4B-PH-K_04x2.00mm_Straight (layer F.Cu) (tedit 56B07786)
    (at 127.762 91.44)
    (descr http://www.jst-mfg.com/product/pdf/eng/ePH.pdf)
    (tags "connector jst ph")
    (fp_text reference J2 (at 0 -3) (layer F.SilkS))
    (fp_text value UART (at 3 4) (layer F.Fab))
    (pad 4 thru_hole oval (at 6 0) (size 1.2 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 15 "Net-(J2-Pad4)"))
    (pad 3 thru_hole oval (at 4 0) (size 1.2 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 16 "Net-(J2-Pad3)"))
    (pad 2 thru_hole oval (at 2 0) (size 1.2 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.2 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 11 GND))
  )
  (module Connectors_JST:JST_PH_B4B-PH-K_04x2.00mm_Straight (layer F.Cu) (tedit 56B07786)
    (at 173.1645 95.631 90)
    (descr http://www.jst-mfg.com/product/pdf/eng/ePH.pdf)
    (tags "connector jst ph")
    (fp_text reference J3 (at 0 -3 90) (layer F.SilkS))
    (fp_text value I2C (at 3 4 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.2 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 11 GND))
    (pad 2 thru_hole oval (at 2 0 90) (size 1.2 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad2)"))
    (pad 3 thru_hole oval (at 4 0 90) (size 1.2 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 "Net-(J3-Pad3)"))
    (pad 4 thru_hole oval (at 6 0 90) (size 1.2 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 3 "Net-(J3-Pad4)"))
  )
  (module Connectors_JST:JST_PH_B2B-PH-K_02x2.00mm_Straight (layer F.Cu) (tedit 56B07786)
    (at 164.1475 96.3295 90)
    (descr http://www.jst-mfg.com/product/pdf/eng/ePH.pdf)
    (tags "connector jst ph")
    (fp_text reference J4 (at -2.7305 -1.5875 180) (layer F.SilkS))
    (fp_text value Batt (at 1 4 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.2 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad2)"))
    (pad 2 thru_hole oval (at 2 0 90) (size 1.2 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 11 GND))
  )
  (gr_text "prototype v20.06.2018-0.1" (at 141.351 98.298) (layer B.SilkS))
  (gr_line (start 124.46 100.33) (end 124.46 85.09) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 177.8 100.33) (end 124.46 100.33) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 177.8 85.09) (end 177.8 100.33) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 124.46 85.09) (end 177.8 85.09) (layer Edge.Cuts) (width 0.15))
  (gr_text "nRF52832 w.sensor" (at 137.16 87.63) (layer B.SilkS))
  (zone (net 11) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 177.038 85.852) (xy 177.038 99.568) (xy 125.222 99.568) (xy 125.222 85.852)
      )
    )
  )
  (zone (net 11) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 125.222 85.852) (xy 177.038 85.852) (xy 177.038 99.568) (xy 125.222 99.568)
      )
    )
  )
)
