(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (41 "Cmts.User" user "User.Comments")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (color "#412C53FF") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (color "#412C53FF") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (solder_mask_min_width 0.1016)
    (grid_origin 112.5 92.45)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "VCC")
  (net 2 "GND")
  (net 3 "+5V")
  (net 4 "/RX")
  (net 5 "Net-(D2-A)")
  (net 6 "/MISO{slash}PA5")
  (net 7 "/SCL{slash}SCK")
  (net 8 "/SDA{slash}MOSI")
  (net 9 "/RST")
  (net 10 "/TEMP")
  (net 11 "/PB2")
  (net 12 "/TX")
  (net 13 "/CUR_SENSE")
  (net 14 "/PWM")
  (net 15 "unconnected-(U1-NC-Pad6)")
  (net 16 "unconnected-(U1-NC-Pad7)")
  (net 17 "unconnected-(U1-NC-Pad10)")
  (net 18 "unconnected-(U1-NC-Pad17)")
  (net 19 "unconnected-(U1-NC-Pad18)")
  (net 20 "unconnected-(U1-NC-Pad19)")
  (net 21 "unconnected-(U2-NC-Pad4)")
  (net 22 "/LED")
  (net 23 "/Drain")
  (net 24 "/Gate")
  (net 25 "/PA7")
  (net 26 "/PB1")
  (net 27 "/Vin")
  (footprint "Package_DFN_QFN:QFN-20-1EP_4x4mm_P0.5mm_EP2.6x2.6mm" (layer "F.Cu")
    (at 140.7 80.8 -90)
    (descr "QFN, 20 Pin (http://ww1.microchip.com/downloads/en/DeviceDoc/doc2535.pdf#page=164), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "QFN NoLead")
    (property "Sheetfile" "enegate_kicad.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "16MHz, 8kB Flash, 512B SRAM, 512B EEPROM, ADC, ACI, debugWIRE, QFN-20")
    (property "ki_keywords" "AVR 8bit Microcontroller tinyAVR")
    (attr smd)
    (fp_text reference "U1" (at 0 -3.3 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "ATtiny841MUR" (at 0 3.3 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "" smd roundrect (at -0.65 -0.65 270) (size 1.05 1.05) (layers "F.Paste") (roundrect_rratio 0.238095))
    (pad "" smd roundrect (at -0.65 0.65 270) (size 1.05 1.05) (layers "F.Paste") (roundrect_rratio 0.238095))
    (pad "" smd roundrect (at 0.65 -0.65 270) (size 1.05 1.05) (layers "F.Paste") (roundrect_rratio 0.238095))
    (pad "" smd roundrect (at 0.65 0.65 270) (size 1.05 1.05) (layers "F.Paste") (roundrect_rratio 0.238095))
    (pad "1" smd roundrect (at -1.925 -1 270) (size 0.85 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "/SCL{slash}SCK") (pinfunction "PA4") (pintype "bidirectional"))
    (pad "2" smd roundrect (at -1.925 -0.5 270) (size 0.85 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "/PWM") (pinfunction "PA3") (pintype "bidirectional"))
    (pad "3" smd roundrect (at -1.925 0 270) (size 0.85 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(D2-A)") (pinfunction "PA2") (pintype "bidirectional"))
    (pad "4" smd roundrect (at -1.925 0.5 270) (size 0.85 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "/TX") (pinfunction "PA1") (pintype "bidirectional"))
    (pad "5" smd roundrect (at -1.925 1 270) (size 0.85 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "/CUR_SENSE") (pinfunction "AREF/PA0") (pintype "bidirectional"))
    (pad "6" smd roundrect (at -1 1.925 270) (size 0.25 0.85) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "unconnected-(U1-NC-Pad6)") (pinfunction "NC") (pintype "no_connect"))
    (pad "7" smd roundrect (at -0.5 1.925 270) (size 0.25 0.85) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "unconnected-(U1-NC-Pad7)") (pinfunction "NC") (pintype "no_connect"))
    (pad "8" smd roundrect (at 0 1.925 270) (size 0.25 0.85) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "9" smd roundrect (at 0.5 1.925 270) (size 0.25 0.85) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "VCC") (pinfunction "VCC") (pintype "power_in"))
    (pad "10" smd roundrect (at 1 1.925 270) (size 0.25 0.85) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "unconnected-(U1-NC-Pad10)") (pinfunction "NC") (pintype "no_connect"))
    (pad "11" smd roundrect (at 1.925 1 270) (size 0.85 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "/TEMP") (pinfunction "XTAL1/PB0") (pintype "bidirectional"))
    (pad "12" smd roundrect (at 1.925 0.5 270) (size 0.85 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "/PB1") (pinfunction "XTAL2/PB1") (pintype "bidirectional"))
    (pad "13" smd roundrect (at 1.925 0 270) (size 0.85 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "/RST") (pinfunction "~{RESET}/PB3") (pintype "bidirectional"))
    (pad "14" smd roundrect (at 1.925 -0.5 270) (size 0.85 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "/PB2") (pinfunction "PB2") (pintype "bidirectional"))
    (pad "15" smd roundrect (at 1.925 -1 270) (size 0.85 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "/PA7") (pinfunction "PA7") (pintype "bidirectional"))
    (pad "16" smd roundrect (at 1 -1.925 270) (size 0.25 0.85) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "/SDA{slash}MOSI") (pinfunction "PA6") (pintype "bidirectional"))
    (pad "17" smd roundrect (at 0.5 -1.925 270) (size 0.25 0.85) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 18 "unconnected-(U1-NC-Pad17)") (pinfunction "NC") (pintype "no_connect"))
    (pad "18" smd roundrect (at 0 -1.925 270) (size 0.25 0.85) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 19 "unconnected-(U1-NC-Pad18)") (pinfunction "NC") (pintype "no_connect"))
    (pad "19" smd roundrect (at -0.5 -1.925 270) (size 0.25 0.85) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "unconnected-(U1-NC-Pad19)") (pinfunction "NC") (pintype "no_connect"))
    (pad "20" smd roundrect (at -1 -1.925 270) (size 0.25 0.85) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "/MISO{slash}PA5") (pinfunction "PA5") (pintype "bidirectional"))
    (pad "21" smd rect (at 0 0 270) (size 2.6 2.6) (layers "F.Cu" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "passive"))
    (model "${KICAD7_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/QFN-20-1EP_4x4mm_P0.5mm_EP2.5x2.5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 134.15 81.7 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "enegate_kicad.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R2" (at 2.6 0 90 unlocked) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "/RST") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "VCC") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "enegate_foot_Library:JST_PH_S5B-PH-SM4-TB_1x05-1MP_P2.00mm_Horizontal" (layer "F.Cu")
    (at 153.05 73 90)
    (descr "JST PH series connector, S5B-PH-SM4-TB (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST PH top entry")
    (property "Sheetfile" "enegate_kicad.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x05, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J6" (at 0 -5.8 90 unlocked) (layer "F.Fab"))
    (fp_text value "Port 2" (at 0 5.8 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.5 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -4 -2.85 90) (size 1 3.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" smd roundrect (at -2 -2.85 90) (size 1 3.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "/SCL{slash}SCK") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" smd roundrect (at 0 -2.85 90) (size 1 3.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "/SDA{slash}MOSI") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" smd roundrect (at 2 -2.85 90) (size 1 3.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "+5V") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" smd roundrect (at 4 -2.85 90) (size 1 3.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "/Vin") (pinfunction "Pin_5") (pintype "passive"))
    (pad "MP" smd roundrect (at -6.35 2.9 90) (size 1.5 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.166667))
    (pad "MP" smd roundrect (at 6.35 2.9 90) (size 1.5 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.166667))
    (model "${KIPRJMOD}/downloaded_parts/S5B-PH-SM4-TB.STEP"
      (offset (xyz -13.9 12.5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:LFPAK56" (layer "F.Cu")
    (at 141.13 70.79 180)
    (descr "LFPAK56 https://assets.nexperia.com/documents/outline-drawing/SOT669.pdf")
    (tags "LFPAK56 SOT-669 Power-SO8")
    (property "Sheetfile" "enegate_kicad.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "N-channel 30 V 7.1 mΩ logic level MOSFET in LFPAK")
    (property "ki_keywords" "N-Channel MOSFET")
    (solder_mask_margin 0.075)
    (solder_paste_margin -0.05)
    (attr smd)
    (fp_text reference "Q1" (at -0.67 1.64 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "PSMN7R0-30YLC" (at -0.245 3.52) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.165 0 90) (layer "F.Fab"))
    (pad "" smd rect (at -0.5 -1.15 180) (size 0.6 0.9) (layers "F.Paste"))
    (pad "" smd rect (at -0.5 0 180) (size 0.6 0.9) (layers "F.Paste"))
    (pad "" smd rect (at -0.5 1.15 180) (size 0.6 0.9) (layers "F.Paste"))
    (pad "" smd rect (at 0.35 -1.15 180) (size 0.6 0.9) (layers "F.Paste"))
    (pad "" smd rect (at 0.35 0 180) (size 0.6 0.9) (layers "F.Paste"))
    (pad "" smd rect (at 0.35 1.15 180) (size 0.6 0.9) (layers "F.Paste"))
    (pad "" smd rect (at 1.2 -1.15 180) (size 0.6 0.9) (layers "F.Paste"))
    (pad "" smd rect (at 1.2 0 180) (size 0.6 0.9) (layers "F.Paste"))
    (pad "" smd rect (at 1.2 1.15 180) (size 0.6 0.9) (layers "F.Paste"))
    (pad "" smd rect (at 3.05 -1.88 90) (size 0.6 0.9) (layers "F.Paste"))
    (pad "" smd rect (at 3.05 -0.6 90) (size 0.6 0.9) (layers "F.Paste"))
    (pad "" smd rect (at 3.05 0.6 90) (size 0.6 0.9) (layers "F.Paste"))
    (pad "" smd rect (at 3.05 1.88 90) (size 0.6 0.9) (layers "F.Paste"))
    (pad "1" smd rect (at -2.67 -1.91 90) (size 0.7 1.15) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "/CUR_SENSE") (pinfunction "S") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (pad "2" smd rect (at -2.67 -0.64 90) (size 0.7 1.15) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "/CUR_SENSE") (pinfunction "S") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (pad "3" smd rect (at -2.67 0.64 90) (size 0.7 1.15) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "/CUR_SENSE") (pinfunction "S") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (pad "4" smd rect (at -2.67 1.91 90) (size 0.7 1.15) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 24 "/Gate") (pinfunction "G") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (pad "5" smd custom (at 0.6 0 180) (size 3.3 4.2) (layers "F.Cu" "F.Mask")
      (net 23 "/Drain") (pinfunction "D") (pintype "passive") (solder_mask_margin 0.07) (zone_connect 2) (thermal_bridge_angle 45)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly
          (pts
            (xy 2.975 2.35)
            (xy 1.425 2.35)
            (xy 1.425 -2.35)
            (xy 2.975 -2.35)
          )
          (width 0) (fill yes))
      ))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/LFPAK56.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_2512_6332Metric_Pad1.40x3.35mm_HandSolder" (layer "F.Cu")
    (at 140.71 75.73 180)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "enegate_kicad.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R7" (at 5.91 0.08 unlocked) (layer "F.SilkS"))
    (fp_text value "100m" (at 0 2.62) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -3.05 0 180) (size 1.4 3.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.178571)
      (net 13 "/CUR_SENSE") (pintype "passive"))
    (pad "2" smd roundrect (at 3.05 0 180) (size 1.4 3.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.178571)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (at 130.6875 79.95 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "enegate_kicad.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C3" (at 0 -1.43 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "1uF" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0 270) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "VCC") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 270) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "enegate_foot_Library:D_2-DFN1006" (layer "F.Cu")
    (at 126.8 84.75)
    (descr "DIODE SCHOTTKY 30V 100MA 2TDFN")
    (tags "diode")
    (property "Sheetfile" "enegate_kicad.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Schottky diode")
    (property "ki_keywords" "diode Schottky")
    (attr smd)
    (fp_text reference "D2" (at -1.5 0 unlocked) (layer "F.SilkS") hide)
    (fp_text value "D_Schottky" (at 0 1.05) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.68) (layer "F.Fab"))
    (pad "" smd roundrect (at -0.325 0) (size 0.2 0.4) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.325 0) (size 0.2 0.4) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "1" smd roundrect (at -0.325 0) (size 0.3 0.55) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "/RX") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 0.325 0) (size 0.3 0.55) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(D2-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_0201_0603Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (at 124.9875 79.9375 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "enegate_kicad.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C2" (at 0 1.405 90 unlocked) (layer "F.SilkS"))
    (fp_text value "1uF" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0 270) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 270) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 135.7 81.7 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "enegate_kicad.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R1" (at -2.6 0 90 unlocked) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "VCC") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "/TEMP") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 117.7 81.7 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "enegate_kicad.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C5" (at 2.9 -0.1 unlocked) (layer "F.SilkS"))
    (fp_text value "10uF" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 3 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 143 67 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "enegate_kicad.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R5" (at -2.3 -0.05 unlocked) (layer "F.SilkS"))
    (fp_text value "100R" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "/PWM") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "/Gate") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 132.6 81.7 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "enegate_kicad.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R4" (at -2.6 0 90 unlocked) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "VCC") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(D2-A)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "enegate_foot_Library:PHOENIX_1702473" (layer "F.Cu")
    (at 130.65 70.2 180)
    (property "Sheetfile" "enegate_kicad.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J7" (at -3.25 -6 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Load" (at 0 5.9) (layer "F.Fab"))
    (pad "1" smd rect (at 1.25 -5.8 180) (size 1.4 3.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 27 "/Vin") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" smd rect (at -1.25 -5.8 180) (size 1.4 3.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "/Drain") (pinfunction "Pin_2") (pintype "passive"))
    (pad "SH1" smd rect (at 3.85 0.8 180) (size 2.3 5.6) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "SH2" smd rect (at -3.85 0.8 180) (size 2.3 5.6) (layers "F.Cu" "F.Paste" "F.Mask"))
    (model "${KIPRJMOD}/downloaded_parts/1702473/1702473.step"
      (offset (xyz 0 -4.5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 -90))
    )
  )
  (footprint "enegate_foot_Library:JST_PH_S5B-PH-SM4-TB_1x05-1MP_P2.00mm_Horizontal" (layer "F.Cu")
    (at 117.5 73 -90)
    (descr "JST PH series connector, S5B-PH-SM4-TB (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST PH top entry")
    (property "Sheetfile" "enegate_kicad.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x05, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J5" (at 0 -5.8 -90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Port 1" (at 0 5.8 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.5 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -4 -2.85 270) (size 1 3.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" smd roundrect (at -2 -2.85 270) (size 1 3.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "/SCL{slash}SCK") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" smd roundrect (at 0 -2.85 270) (size 1 3.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "/SDA{slash}MOSI") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" smd roundrect (at 2 -2.85 270) (size 1 3.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "+5V") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" smd roundrect (at 4 -2.85 270) (size 1 3.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "/Vin") (pinfunction "Pin_5") (pintype "passive"))
    (pad "MP" smd roundrect (at -6.35 2.9 270) (size 1.5 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.166667))
    (pad "MP" smd roundrect (at 6.35 2.9 270) (size 1.5 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.166667))
    (model "${KIPRJMOD}/downloaded_parts/S5B-PH-SM4-TB.STEP"
      (offset (xyz -13.9 12.5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (at 137.25 81.7 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "enegate_kicad.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C1" (at -2.65 0 90 unlocked) (layer "F.SilkS"))
    (fp_text value "0.1uF" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0 270) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "VCC") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 270) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (at 138.375 87.15)
    (descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x02 2.54mm single row")
    (property "Sheetfile" "enegate_kicad.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J2" (at 3.425 0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "10K Thermistor" (at 0 5.31) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.27 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 10 "/TEMP") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x02_P2.54mm_Vertical.wrl" hide
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2" (layer "F.Cu")
    (at 115.1 89.85)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (property "Sheetfile" "enegate_kicad.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H1" (at 0 -3.2 unlocked) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 3.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 138.95 67 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "enegate_kicad.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R6" (at 2.3 -0.05 unlocked) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "/Gate") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "enegate_foot_Library:JST_S3B-ZR-SM4A-TF" (layer "F.Cu")
    (at 121.9 86.45)
    (property "Sheetfile" "enegate_kicad.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J4" (at -0.576705 -2.336415 unlocked) (layer "F.SilkS") hide)
    (fp_text value "UART" (at -0.05 7.05) (layer "F.Fab"))
    (pad "1" smd rect (at -1.5 0) (size 0.7 2.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "/TX") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" smd rect (at 0 0) (size 0.7 2.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "/RX") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" smd rect (at 1.5 0) (size 0.7 2.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "Pin_3") (pintype "passive"))
    (pad "SH1" smd rect (at -3.45 3.6) (size 1.1 1.9) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "SH2" smd rect (at 3.45 3.6) (size 1.1 1.9) (layers "F.Cu" "F.Paste" "F.Mask"))
    (model "${KIPRJMOD}/downloaded_parts/S3B-ZR-SM4A-TF.STEP"
      (offset (xyz 0 0.5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 117.7 83.8 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "enegate_kicad.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C4" (at 2.9 -0.1 unlocked) (layer "F.SilkS"))
    (fp_text value "10uF" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 27 "/Vin") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (at 127.85 79.95)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "Sheetfile" "enegate_kicad.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "300mA Low Dropout Voltage Regulator, Fixed Output 4.5V, SOT-23-5")
    (property "ki_keywords" "300mA LDO Regulator Fixed Positive")
    (attr smd)
    (fp_text reference "U2" (at 2.635 4 180 unlocked) (layer "F.SilkS") hide)
    (fp_text value "TLV70245_SOT23-5" (at 0 2.4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.1375 -0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "+5V") (pinfunction "IN") (pintype "power_in"))
    (pad "2" smd roundrect (at -1.1375 0) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "+5V") (pinfunction "EN") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "unconnected-(U2-NC-Pad4)") (pinfunction "NC") (pintype "no_connect"))
    (pad "5" smd roundrect (at 1.1375 -0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "VCC") (pinfunction "OUT") (pintype "power_out"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 125.8875 82.5)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "enegate_kicad.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R3" (at -0.0375 1.25 unlocked) (layer "F.SilkS"))
    (fp_text value "330R" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LED") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_2x03_P2.54mm_Vertical" (layer "F.Cu")
    (at 129.025 89.675 90)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (property "Sheetfile" "enegate_kicad.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, double row, 02x03, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J1" (at 1.27 -2.33 270 unlocked) (layer "F.SilkS") hide)
    (fp_text value "ISP Programmer" (at 1.27 7.41 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 2.54) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 6 "/MISO{slash}PA5") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "VCC") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "/SCL{slash}SCK") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 8 "/SDA{slash}MOSI") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 9 "/RST") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x03_P2.54mm_Vertical.wrl" hide
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "F.Cu")
    (at 129.7875 82.5)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (property "Sheetfile" "enegate_kicad.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode")
    (property "ki_keywords" "LED diode")
    (attr smd)
    (fp_text reference "D1" (at -0.0375 1.35 unlocked) (layer "F.SilkS"))
    (fp_text value "PWR" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.875 0) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LED") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 0.875 0) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "VCC") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2" (layer "F.Cu")
    (at 155.75 89.9)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (property "Sheetfile" "enegate_kicad.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H2" (at 0 -3.2 unlocked) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 3.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers "*.Cu" "*.Mask"))
  )
  (footprint "enegate_foot_Library:JST_S6B-ZR-SM4A-TF" (layer "F.Cu")
    (at 146.7 86.5)
    (property "Sheetfile" "enegate_kicad.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J3" (at -8.726705 -0.936415 unlocked) (layer "F.Fab"))
    (fp_text value "Remote" (at 0 6.55) (layer "F.Fab"))
    (pad "1" smd rect (at -3.75 0) (size 0.7 2.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "+5V") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" smd rect (at -2.25 0) (size 0.7 2.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "/MISO{slash}PA5") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" smd rect (at -0.75 0) (size 0.7 2.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 25 "/PA7") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" smd rect (at 0.75 0) (size 0.7 2.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "/PB1") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" smd rect (at 2.25 0) (size 0.7 2.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "/PB2") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" smd rect (at 3.75 0) (size 0.7 2.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "Pin_6") (pintype "passive"))
    (pad "SH1" smd rect (at -5.7 3.6) (size 1.1 1.9) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "SH2" smd rect (at 5.7 3.6) (size 1.1 1.9) (layers "F.Cu" "F.Paste" "F.Mask"))
    (model "${KIPRJMOD}/downloaded_parts/S6B-ZR-SM4A-TF.STEP"
      (offset (xyz 0 0.5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (gr_rect (start 112.5 65.3) (end 158.3 92.45)
    (fill none) (layer "Edge.Cuts"))
  (gr_text "EneGate Rev. 3.0\n05/23\nPaul Bupe Jr" (at 151.75 69.35) (layer "B.SilkS"))
  (gr_text "TX" (at 120.9 84.95 90) (layer "F.SilkS"))
  (gr_text "Vin: 0-15V" (at 156.15 87.6 90) (layer "F.SilkS"))
  (gr_text "SDA" (at 147.9 72.5 180) (layer "F.SilkS"))
  (gr_text "5V" (at 143.4 84.9 90) (layer "F.SilkS"))
  (gr_text "GND" (at 150.9 84.9 90) (layer "F.SilkS"))
  (gr_text "RX" (at 122.4 84.95 90) (layer "F.SilkS"))
  (gr_text "PA7" (at 146.4 84.9 90) (layer "F.SilkS"))
  (gr_text "5V" (at 122.7 75.5) (layer "F.SilkS"))
  (gr_text "SCL" (at 122.7 71.4) (layer "F.SilkS"))
  (gr_text "5V" (at 147.95 70.5 180) (layer "F.SilkS"))
  (gr_text "GND" (at 123.85 84.9 90) (layer "F.SilkS"))
  (gr_text "SCL" (at 147.9 74.55 180) (layer "F.SilkS"))
  (gr_text "GND" (at 147.9 76.55 180) (layer "F.SilkS"))
  (gr_text "ISP" (at 130.7 85.3) (layer "F.SilkS"))
  (gr_text "PB1" (at 147.9 84.9 90) (layer "F.SilkS"))
  (gr_text "Vin" (at 147.95 68.5 180) (layer "F.SilkS"))
  (gr_text "GND" (at 122.7 69.45) (layer "F.SilkS"))
  (gr_text "PA5" (at 144.9 84.9 90) (layer "F.SilkS"))
  (gr_text "NTC" (at 137.4 85.25) (layer "F.SilkS"))
  (gr_text "SDA" (at 122.7 73.45) (layer "F.SilkS"))
  (gr_text "PB2" (at 149.4 84.9 90) (layer "F.SilkS"))
  (gr_text "Vin" (at 122.7 77.5) (layer "F.SilkS"))
  (zone (net 27) (net_name "/Vin") (layer "F.Cu") (hatch edge 0.5)
    (priority 1)
    (connect_pads yes (clearance 0.3))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.2) (thermal_bridge_width 0.3) (smoothing chamfer) (radius 0.5))
    (polygon
      (pts
        (xy 151.2 68.1)
        (xy 154.5 68.1)
        (xy 154.5 69.8)
        (xy 151.2 69.8)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "F.Cu") (hatch edge 0.5)
    (priority 7)
    (connect_pads (clearance 0.3))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.2) (thermal_bridge_width 0.6) (smoothing chamfer) (radius 0.5))
    (polygon
      (pts
        (xy 135.65 73.45)
        (xy 139.2 73.45)
        (xy 139.2 77.55)
        (xy 135.65 77.55)
      )
    )
  )
  (zone (net 3) (net_name "+5V") (layer "F.Cu") (hatch edge 0.5)
    (priority 1)
    (connect_pads yes (clearance 0.3))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.2) (thermal_bridge_width 0.3) (smoothing chamfer) (radius 0.5))
    (polygon
      (pts
        (xy 151.2 70.1)
        (xy 154.5 70.1)
        (xy 154.5 71.8)
        (xy 151.2 71.8)
      )
    )
  )
  (zone (net 3) (net_name "+5V") (layer "F.Cu") (hatch edge 0.5)
    (priority 4)
    (connect_pads yes (clearance 0.3))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.2) (thermal_bridge_width 0.3) (smoothing chamfer) (radius 0.3))
    (polygon
      (pts
        (xy 121.1 74.3)
        (xy 125.4 74.3)
        (xy 125.4 75.7)
        (xy 121.1 75.7)
      )
    )
  )
  (zone (net 13) (net_name "/CUR_SENSE") (layer "F.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.3))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.2) (thermal_bridge_width 0.6) (smoothing chamfer) (radius 0.5))
    (polygon
      (pts
        (xy 142.55 69.7)
        (xy 145.6 69.7)
        (xy 145.65 77.4)
        (xy 142.6 77.4)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "F.Cu") (hatch edge 0.5)
    (priority 5)
    (connect_pads (clearance 0.3))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.2) (thermal_bridge_width 0.3) (smoothing chamfer) (radius 0.3))
    (polygon
      (pts
        (xy 114.9 80.5)
        (xy 117.7 80.5)
        (xy 117.7 85)
        (xy 114.9 85)
      )
    )
  )
  (zone (net 23) (net_name "/Drain") (layer "B.Cu") (hatch edge 0.5)
    (priority 6)
    (connect_pads (clearance 0.3))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.2) (thermal_bridge_width 0.3))
    (polygon
      (pts
        (xy 142.3 70.25)
        (xy 142.3 73.3)
        (xy 132.8 73.3)
        (xy 132.8 77.7)
        (xy 130.9 77.7)
        (xy 130.9 70.25)
      )
    )
  )
  (zone (net 27) (net_name "/Vin") (layer "B.Cu") (hatch edge 0.5)
    (priority 2)
    (connect_pads yes (clearance 0.3))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.2) (thermal_bridge_width 0.3) (smoothing chamfer) (radius 0.3))
    (polygon
      (pts
        (xy 118.5 66)
        (xy 154.5 66)
        (xy 154.5 69.8)
        (xy 151.5 69.8)
        (xy 151.5 68.5)
        (xy 122 68.5)
        (xy 122 76)
        (xy 125.4 76)
        (xy 125.4 78)
        (xy 118.5 78)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "B.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.3))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.2) (thermal_bridge_width 0.3) (smoothing chamfer) (radius 0.3))
    (polygon
      (pts
        (xy 112.9 65.8)
        (xy 157.7 65.8)
        (xy 157.7 92)
        (xy 112.9 92)
      )
    )
  )
  (zone (net 3) (net_name "+5V") (layer "B.Cu") (hatch edge 0.5)
    (priority 3)
    (connect_pads yes (clearance 0.3))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.2) (thermal_bridge_width 0.3) (smoothing chamfer) (radius 0.3))
    (polygon
      (pts
        (xy 151.2 68.8)
        (xy 151.2 70.1)
        (xy 154.5 70.1)
        (xy 154.5 71.8)
        (xy 149.8 71.8)
        (xy 149.85 69.9)
        (xy 123.9 69.9)
        (xy 123.9 74.5)
        (xy 125.4 74.5)
        (xy 125.4 75.5)
        (xy 122.3 75.5)
        (xy 122.3 68.8)
      )
    )
  )
)
