(kicad_pcb (version 20171130) (host pcbnew "(5.0.1)-3")
  (general
    (thickness 1.6)
    (drawings 6)
    (tracks 108)
    (zones 0)
    (modules 11)
    (nets 54)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (solder_mask_min_width 0.101)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 /5V)
  (net 3 /3.3V)
  (net 4 /CS)
  (net 5 /MOSI)
  (net 6 /SCK)
  (net 7 /INT)
  (net 8 /MISO)
  (net 9 "Net-(BK3254-Pad11)")
  (net 10 "Net-(BK3254-Pad10)")
  (net 11 "Net-(ESP8266-Pad6)")
  (net 12 "Net-(ESP8266-Pad5)")
  (net 13 "Net-(ESP8266-Pad4)")
  (net 14 "Net-(ESP8266-Pad3)")
  (net 15 "Net-(ESP8266-Pad13)")
  (net 16 "Net-(ESP8266-Pad11)")
  (net 17 "Net-(ESP8266-Pad10)")
  (net 18 "Net-(ESP8266-Pad9)")
  (net 19 "Net-(BK3254-Pad22)")
  (net 20 "Net-(BK3254-Pad21)")
  (net 21 "Net-(BK3254-Pad23)")
  (net 22 "Net-(BK3254-Pad24)")
  (net 23 "Net-(BK3254-Pad20)")
  (net 24 "Net-(BK3254-Pad19)")
  (net 25 "Net-(BK3254-Pad18)")
  (net 26 "Net-(BK3254-Pad17)")
  (net 27 "Net-(BK3254-Pad30)")
  (net 28 "Net-(BK3254-Pad40)")
  (net 29 "Net-(BK3254-Pad37)")
  (net 30 "Net-(BK3254-Pad35)")
  (net 31 "Net-(BK3254-Pad28)")
  (net 32 "Net-(BK3254-Pad27)")
  (net 33 "Net-(BK3254-Pad29)")
  (net 34 "Net-(BK3254-Pad33)")
  (net 35 "Net-(BK3254-Pad39)")
  (net 36 "Net-(BK3254-Pad34)")
  (net 37 "Net-(BK3254-Pad38)")
  (net 38 "Net-(BK3254-Pad31)")
  (net 39 "Net-(BK3254-Pad32)")
  (net 40 "Net-(BK3254-Pad26)")
  (net 41 "Net-(BK3254-Pad4)")
  (net 42 "Net-(BK3254-Pad1)")
  (net 43 "Net-(BK3254-Pad2)")
  (net 44 "Net-(BK3254-Pad7)")
  (net 45 "Net-(BK3254-Pad8)")
  (net 46 "Net-(BK3254-Pad6)")
  (net 47 "Net-(BK3254-Pad3)")
  (net 48 "Net-(BK3254-Pad5)")
  (net 49 "Net-(BK3254-Pad9)")
  (net 50 "Net-(BK3254-Pad12)")
  (net 51 "Net-(BK3254-Pad13)")
  (net 52 "Net-(BK3254-Pad14)")
  (net 53 "Net-(BK3254-Pad15)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /3.3V)
    (add_net /5V)
    (add_net /CS)
    (add_net /INT)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /SCK)
    (add_net GND)
    (add_net "Net-(BK3254-Pad1)")
    (add_net "Net-(BK3254-Pad10)")
    (add_net "Net-(BK3254-Pad11)")
    (add_net "Net-(BK3254-Pad12)")
    (add_net "Net-(BK3254-Pad13)")
    (add_net "Net-(BK3254-Pad14)")
    (add_net "Net-(BK3254-Pad15)")
    (add_net "Net-(BK3254-Pad17)")
    (add_net "Net-(BK3254-Pad18)")
    (add_net "Net-(BK3254-Pad19)")
    (add_net "Net-(BK3254-Pad2)")
    (add_net "Net-(BK3254-Pad20)")
    (add_net "Net-(BK3254-Pad21)")
    (add_net "Net-(BK3254-Pad22)")
    (add_net "Net-(BK3254-Pad23)")
    (add_net "Net-(BK3254-Pad24)")
    (add_net "Net-(BK3254-Pad26)")
    (add_net "Net-(BK3254-Pad27)")
    (add_net "Net-(BK3254-Pad28)")
    (add_net "Net-(BK3254-Pad29)")
    (add_net "Net-(BK3254-Pad3)")
    (add_net "Net-(BK3254-Pad30)")
    (add_net "Net-(BK3254-Pad31)")
    (add_net "Net-(BK3254-Pad32)")
    (add_net "Net-(BK3254-Pad33)")
    (add_net "Net-(BK3254-Pad34)")
    (add_net "Net-(BK3254-Pad35)")
    (add_net "Net-(BK3254-Pad37)")
    (add_net "Net-(BK3254-Pad38)")
    (add_net "Net-(BK3254-Pad39)")
    (add_net "Net-(BK3254-Pad4)")
    (add_net "Net-(BK3254-Pad40)")
    (add_net "Net-(BK3254-Pad5)")
    (add_net "Net-(BK3254-Pad6)")
    (add_net "Net-(BK3254-Pad7)")
    (add_net "Net-(BK3254-Pad8)")
    (add_net "Net-(BK3254-Pad9)")
    (add_net "Net-(ESP8266-Pad10)")
    (add_net "Net-(ESP8266-Pad11)")
    (add_net "Net-(ESP8266-Pad13)")
    (add_net "Net-(ESP8266-Pad3)")
    (add_net "Net-(ESP8266-Pad4)")
    (add_net "Net-(ESP8266-Pad5)")
    (add_net "Net-(ESP8266-Pad6)")
    (add_net "Net-(ESP8266-Pad9)")
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x08_P2.54mm_Vertical (layer F.Cu) (tedit 5A19A420)
    (at 86.36 88.9 180)
    (descr "Through hole straight socket strip, 1x08, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x08 2.54mm single row")
    (fp_text reference J4 (at 0 -2.77 180) (layer F.SilkS))
    (fp_text value Conn_01x08_Female (at 0 20.55 180) (layer F.Fab))
    (fp_text user %R (at 0 8.89 270) (layer F.Fab))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(ESP8266-Pad9)"))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(ESP8266-Pad10)"))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(ESP8266-Pad11)"))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /SCK))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(ESP8266-Pad13)"))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /MOSI))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /CS))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /3.3V))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x08_P2.54mm_Vertical (layer F.Cu) (tedit 5A19A420)
    (at 109.22 88.9 180)
    (descr "Through hole straight socket strip, 1x08, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x08 2.54mm single row")
    (fp_text reference J1 (at 0 -2.77 180) (layer F.SilkS))
    (fp_text value Conn_01x08_Female (at 0 20.55 180) (layer F.Fab))
    (fp_text user %R (at 0 8.89 270) (layer F.Fab))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(BK3254-Pad11)"))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(BK3254-Pad10)"))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(ESP8266-Pad6)"))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(ESP8266-Pad5)"))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(ESP8266-Pad4)"))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(ESP8266-Pad3)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /5V))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x07_P2.54mm_Vertical (layer B.Cu) (tedit 5A19A433)
    (at 88.9 99.695 270)
    (descr "Through hole straight socket strip, 1x07, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x07 2.54mm single row")
    (fp_text reference J3 (at 0 2.77 270) (layer B.SilkS))
    (fp_text value MCP2515_Connector_01x07_Female (at 0 -18.01 270) (layer B.Fab))
    (fp_text user %R (at 0 -7.62 180) (layer B.Fab))
    (pad 7 thru_hole oval (at 0 -15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /5V))
    (pad 6 thru_hole oval (at 0 -12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole oval (at 0 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /CS))
    (pad 4 thru_hole oval (at 0 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /MISO))
    (pad 3 thru_hole oval (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /MOSI))
    (pad 2 thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /SCK))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /INT))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x07_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module F-6888_BK3254:F-6888 (layer B.Cu) (tedit 5AE5EB9F)
    (at 90.805 69.215)
    (fp_text reference BK3254 (at 6.95 2.25) (layer B.SilkS) hide)
    (fp_text value F-6888 (at 6.985 17.78) (layer B.SilkS))
    (fp_text user GND (at 2.3 18.1) (layer B.SilkS))
    (fp_text user FMINN (at 2.8 17) (layer B.SilkS))
    (fp_text user FMINP (at 2.8 15.95) (layer B.SilkS))
    (fp_text user "PREV/VOL-(19)" (at 5.05 14.8) (layer B.SilkS))
    (fp_text user GND (at 11.3 18.05) (layer B.SilkS))
    (fp_text user ADC (at 11.25 17.05) (layer B.SilkS))
    (fp_text user V3OUT (at 10.7 15.9) (layer B.SilkS))
    (fp_text user VBAT (at 10.95 14.75) (layer B.SilkS))
    (fp_text user NEXT/VOL+ (at 4.05 13.7) (layer B.SilkS))
    (fp_text user "P.P./CALL(21)" (at 4.6 12.5) (layer B.SilkS))
    (fp_text user VCCIO (at 10.7 13.7) (layer B.SilkS))
    (fp_text user AUDIORN (at 10.15 12.5) (layer B.SilkS))
    (fp_text user AUDIORP (at 10.15 11.5) (layer B.SilkS))
    (fp_text user AUDIOLP (at 10.2 10.5) (layer B.SilkS))
    (fp_text user AUDIOLN (at 10.15 9.35) (layer B.SilkS))
    (fp_text user "FM/TF/BT(20)" (at 4.65 11.45) (layer B.SilkS))
    (fp_text user RST (at 2.25 10.4) (layer B.SilkS))
    (fp_text user GPIO6 (at 2.8 9.3) (layer B.SilkS))
    (fp_text user "TX(0)" (at 2.7 8.15) (layer B.SilkS))
    (fp_text user "RX(1)" (at 2.75 7.1) (layer B.SilkS))
    (fp_text user "MUTE(17)" (at 3.6 5.95) (layer B.SilkS))
    (fp_text user "L1(15)" (at 2.45 4.95) (layer B.SilkS))
    (fp_text user "L2(17)" (at 2.5 3.85) (layer B.SilkS))
    (fp_text user 16 (at 1.65 2.75) (layer B.SilkS))
    (fp_text user GND (at 1.7 1.2 -90) (layer B.SilkS))
    (fp_text user VMIC (at 10.95 8.1) (layer B.SilkS))
    (fp_text user MICP (at 10.95 7.05) (layer B.SilkS))
    (fp_text user MICL (at 11.35 5.95) (layer B.SilkS))
    (fp_text user AIL (at 11.6 4.9) (layer B.SilkS))
    (fp_text user AIR (at 11.55 3.8) (layer B.SilkS))
    (fp_text user 10 (at 2.95 1.9 -90) (layer B.SilkS))
    (fp_text user "SDCMD(13)" (at 4.05 3.3 -90) (layer B.SilkS))
    (fp_text user 5 (at 5.15 1.8 -90) (layer B.SilkS))
    (fp_text user "SD_DATA(14)" (at 6.2 4.15 -90) (layer B.SilkS))
    (fp_text user "SD_CLK(12)" (at 7.3 3.95 -90) (layer B.SilkS))
    (fp_text user "USB+(2)" (at 8.35 3.25 -90) (layer B.SilkS))
    (fp_text user "USB-(3)" (at 9.5 3.25 -90) (layer B.SilkS))
    (fp_text user 22 (at 10.45 1.85 -90) (layer B.SilkS))
    (fp_text user ADET (at 11.2 2.85) (layer B.SilkS))
    (fp_text user GND (at 11.8 1.35 -90) (layer B.SilkS))
    (pad 15 smd rect (at 0 2.7) (size 2 0.8) (layers B.Cu B.Paste B.Mask)
      (net 53 "Net-(BK3254-Pad15)"))
    (pad 14 smd rect (at 0 3.8) (size 2 0.8) (layers B.Cu B.Paste B.Mask)
      (net 52 "Net-(BK3254-Pad14)"))
    (pad 13 smd rect (at 0 4.9) (size 2 0.8) (layers B.Cu B.Paste B.Mask)
      (net 51 "Net-(BK3254-Pad13)"))
    (pad 12 smd rect (at 0 6) (size 2 0.8) (layers B.Cu B.Paste B.Mask)
      (net 50 "Net-(BK3254-Pad12)"))
    (pad 11 smd rect (at 0 7.1) (size 2 0.8) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(BK3254-Pad11)"))
    (pad 10 smd rect (at 0 8.2) (size 2 0.8) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(BK3254-Pad10)"))
    (pad 9 smd rect (at 0 9.3) (size 2 0.8) (layers B.Cu B.Paste B.Mask)
      (net 49 "Net-(BK3254-Pad9)"))
    (pad 5 smd rect (at 0 13.7) (size 2 0.8) (layers B.Cu B.Paste B.Mask)
      (net 48 "Net-(BK3254-Pad5)"))
    (pad 3 smd rect (at 0 15.9) (size 2 0.8) (layers B.Cu B.Paste B.Mask)
      (net 47 "Net-(BK3254-Pad3)"))
    (pad 6 smd rect (at 0 12.6) (size 2 0.8) (layers B.Cu B.Paste B.Mask)
      (net 46 "Net-(BK3254-Pad6)"))
    (pad 8 smd rect (at 0 10.4) (size 2 0.8) (layers B.Cu B.Paste B.Mask)
      (net 45 "Net-(BK3254-Pad8)"))
    (pad 7 smd rect (at 0 11.5) (size 2 0.8) (layers B.Cu B.Paste B.Mask)
      (net 44 "Net-(BK3254-Pad7)"))
    (pad 2 smd rect (at 0 17) (size 2 0.8) (layers B.Cu B.Paste B.Mask)
      (net 43 "Net-(BK3254-Pad2)"))
    (pad 16 smd rect (at 0 1.6) (size 2 0.8) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0 18.1) (size 2 0.8) (layers B.Cu B.Paste B.Mask)
      (net 42 "Net-(BK3254-Pad1)"))
    (pad 4 smd rect (at 0 14.8) (size 2 0.8) (layers B.Cu B.Paste B.Mask)
      (net 41 "Net-(BK3254-Pad4)"))
    (pad 36 smd rect (at 13.5 13.7) (size 2 0.8) (layers B.Cu B.Paste B.Mask)
      (net 3 /3.3V))
    (pad 26 smd rect (at 13.5 2.7) (size 2 0.8) (layers B.Cu B.Paste B.Mask)
      (net 40 "Net-(BK3254-Pad26)"))
    (pad 32 smd rect (at 13.5 9.3) (size 2 0.8) (layers B.Cu B.Paste B.Mask)
      (net 39 "Net-(BK3254-Pad32)"))
    (pad 31 smd rect (at 13.5 8.2) (size 2 0.8) (layers B.Cu B.Paste B.Mask)
      (net 38 "Net-(BK3254-Pad31)"))
    (pad 38 smd rect (at 13.5 15.9) (size 2 0.8) (layers B.Cu B.Paste B.Mask)
      (net 37 "Net-(BK3254-Pad38)"))
    (pad 34 smd rect (at 13.5 11.5) (size 2 0.8) (layers B.Cu B.Paste B.Mask)
      (net 36 "Net-(BK3254-Pad34)"))
    (pad 25 smd rect (at 13.5 1.6) (size 2 0.8) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 39 smd rect (at 13.5 17) (size 2 0.8) (layers B.Cu B.Paste B.Mask)
      (net 35 "Net-(BK3254-Pad39)"))
    (pad 33 smd rect (at 13.5 10.4) (size 2 0.8) (layers B.Cu B.Paste B.Mask)
      (net 34 "Net-(BK3254-Pad33)"))
    (pad 29 smd rect (at 13.5 6) (size 2 0.8) (layers B.Cu B.Paste B.Mask)
      (net 33 "Net-(BK3254-Pad29)"))
    (pad 27 smd rect (at 13.5 3.8) (size 2 0.8) (layers B.Cu B.Paste B.Mask)
      (net 32 "Net-(BK3254-Pad27)"))
    (pad 28 smd rect (at 13.5 4.9) (size 2 0.8) (layers B.Cu B.Paste B.Mask)
      (net 31 "Net-(BK3254-Pad28)"))
    (pad 35 smd rect (at 13.5 12.6) (size 2 0.8) (layers B.Cu B.Paste B.Mask)
      (net 30 "Net-(BK3254-Pad35)"))
    (pad 37 smd rect (at 13.5 14.8) (size 2 0.8) (layers B.Cu B.Paste B.Mask)
      (net 29 "Net-(BK3254-Pad37)"))
    (pad 40 smd rect (at 13.5 18.1) (size 2 0.8) (layers B.Cu B.Paste B.Mask)
      (net 28 "Net-(BK3254-Pad40)"))
    (pad 30 smd rect (at 13.5 7.1) (size 2 0.8) (layers B.Cu B.Paste B.Mask)
      (net 27 "Net-(BK3254-Pad30)"))
    (pad 17 smd rect (at 2.9 0) (size 0.8 2) (layers B.Cu B.Paste B.Mask)
      (net 26 "Net-(BK3254-Pad17)"))
    (pad 18 smd rect (at 4 0) (size 0.8 2) (layers B.Cu B.Paste B.Mask)
      (net 25 "Net-(BK3254-Pad18)"))
    (pad 19 smd rect (at 5.1 0) (size 0.8 2) (layers B.Cu B.Paste B.Mask)
      (net 24 "Net-(BK3254-Pad19)"))
    (pad 20 smd rect (at 6.2 0) (size 0.8 2) (layers B.Cu B.Paste B.Mask)
      (net 23 "Net-(BK3254-Pad20)"))
    (pad 24 smd rect (at 10.399996 0) (size 0.8 2) (layers B.Cu B.Paste B.Mask)
      (net 22 "Net-(BK3254-Pad24)"))
    (pad 23 smd rect (at 9.35 0) (size 0.8 2) (layers B.Cu B.Paste B.Mask)
      (net 21 "Net-(BK3254-Pad23)"))
    (pad 21 smd rect (at 7.25 0) (size 0.8 2) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(BK3254-Pad21)"))
    (pad 22 smd rect (at 8.3 0) (size 0.8 2) (layers B.Cu B.Paste B.Mask)
      (net 19 "Net-(BK3254-Pad22)"))
  )
  (module Connector_Audio:Jack_3.5mm_PJ320D_Horizontal (layer F.Cu) (tedit 5A1DBF1B)
    (at 102.235 66.04 180)
    (descr "Headphones with microphone connector, 3.5mm, 4 pins.")
    (tags "3.5mm jack mic microphone phones headphones 4pins audio plug")
    (attr smd)
    (fp_text reference Jack1 (at 0.05 -5.35 180) (layer F.SilkS))
    (fp_text value PJ-320B (at -0.025 6.35 180) (layer F.Fab))
    (fp_text user %R (at -1.195 0 180) (layer F.Fab))
    (pad "" np_thru_hole circle (at 2.225 0 180) (size 1.5 1.5) (drill 1.5) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -4.775 0 180) (size 1.5 1.5) (drill 1.5) (layers *.Cu *.Mask))
    (pad 3 smd rect (at -3.175 -3.25 180) (size 1.2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(BK3254-Pad35)"))
    (pad 2 smd rect (at -0.175 -3.25 180) (size 1.2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(BK3254-Pad34)"))
    (pad 1 smd rect (at 3.825 -3.25 180) (size 1.2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(BK3254-Pad33)"))
    (pad 4 smd rect (at 4.925 3.25 180) (size 1.2 2.5) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Connector_Audio.3dshapes/Jack_3.5mm_PJ320D_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock:TerminalBlock_bornier-2_P5.08mm (layer F.Cu) (tedit 59FF03AB)
    (at 92.71 65.405 180)
    (descr "simple 2-pin terminal block, pitch 5.08mm, revamped version of bornier2")
    (tags "terminal block bornier2")
    (fp_text reference J2 (at 2.54 -5.08 180) (layer F.SilkS))
    (fp_text value Screw_Terminal_01x02 (at 2.54 5.08 180) (layer F.Fab))
    (fp_text user %R (at 2.54 0 180) (layer F.Fab))
    (pad 2 thru_hole circle (at 5.08 0 180) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 180) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 2 /5V))
    (model ${KISYS3DMOD}/TerminalBlock.3dshapes/TerminalBlock_bornier-2_P5.08mm.wrl
      (offset (xyz 2.539999961853027 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module wemos_d1_mini:D1_mini_board (layer B.Cu) (tedit 5766F65E)
    (at 97.79 81.28 180)
    (fp_text reference ESP8266 (at 1.27 -18.81 180) (layer B.SilkS))
    (fp_text value WeMos_mini (at 1.27 19.05 180) (layer B.Fab))
    (fp_text user WeMos (at 0 15.24 180) (layer B.SilkS))
    (pad 9 thru_hole circle (at 11.43 10.16 180) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 18 "Net-(ESP8266-Pad9)"))
    (pad 10 thru_hole circle (at 11.43 7.62 180) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 17 "Net-(ESP8266-Pad10)"))
    (pad 11 thru_hole circle (at 11.43 5.08 180) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 16 "Net-(ESP8266-Pad11)"))
    (pad 12 thru_hole circle (at 11.43 2.54 180) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 6 /SCK))
    (pad 13 thru_hole circle (at 11.43 0 180) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 15 "Net-(ESP8266-Pad13)"))
    (pad 14 thru_hole circle (at 11.43 -2.54 180) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 5 /MOSI))
    (pad 15 thru_hole circle (at 11.43 -5.08 180) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 4 /CS))
    (pad 16 thru_hole circle (at 11.43 -7.62 180) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 3 /3.3V))
    (pad 1 thru_hole circle (at -11.43 -7.62 180) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 2 /5V))
    (pad 2 thru_hole circle (at -11.43 -5.08 180) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 1 GND))
    (pad 3 thru_hole circle (at -11.43 -2.54 180) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 14 "Net-(ESP8266-Pad3)"))
    (pad 4 thru_hole circle (at -11.43 0 180) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 13 "Net-(ESP8266-Pad4)"))
    (pad 5 thru_hole circle (at -11.43 2.54 180) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 12 "Net-(ESP8266-Pad5)"))
    (pad 6 thru_hole circle (at -11.43 5.08 180) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 11 "Net-(ESP8266-Pad6)"))
    (pad 7 thru_hole circle (at -11.43 7.62 180) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 10 "Net-(BK3254-Pad10)"))
    (pad 8 thru_hole circle (at -11.43 10.16 180) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 9 "Net-(BK3254-Pad11)"))
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 96.52 93.218 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R4 (at 5.334 2.032 180) (layer F.SilkS))
    (fp_text value 2.2k (at 4.826 -2.286 180) (layer F.Fab))
    (fp_text user %R (at 5.08 0 180) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(ESP8266-Pad13)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 /MISO))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 99.06 93.218)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R3 (at 5.08 -2.37) (layer F.SilkS))
    (fp_text value 2.2k (at 5.08 2.37) (layer F.Fab))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(ESP8266-Pad5)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 /INT))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 88.265 80.01 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at 5.08 -2.37 90) (layer F.SilkS))
    (fp_text value 3.3k (at 5.08 2.37 90) (layer F.Fab))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(ESP8266-Pad13)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 106.68 78.74 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 5.08 -2.37 270) (layer F.SilkS))
    (fp_text value 3.3k (at 5.08 2.37 270) (layer F.Fab))
    (fp_text user %R (at 5.08 0 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(ESP8266-Pad5)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 84.836 60.96) (end 110.998 60.96) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 84.582 61.468) (end 84.836 60.96) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 84.582 101.346) (end 84.582 61.468) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 110.998 101.346) (end 84.582 101.346) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 110.998 60.96) (end 110.998 101.346) (layer Edge.Cuts) (width 0.15))
  (gr_text 5V (at 92.456 62.738) (layer B.SilkS))
  (zone (net 0) (net_name "") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 110.744 86.868) (xy 110.744 101.346) (xy 84.582 101.346) (xy 84.582 86.868) (xy 88.9 86.868)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 84.582 61.214) (xy 110.744 61.214) (xy 110.744 101.346) (xy 84.582 101.346)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 110.744 61.214) (xy 110.744 101.346) (xy 84.582 101.346) (xy 84.582 61.214)
      )
    )
  )
)
