(kicad_pcb (version 4) (host pcbnew 4.0.4-1.fc25-product)
  (general
    (links 48)
    (no_connects 1)
    (area 93.218001 23.274019 178.510001 123.265001)
    (thickness 1.6)
    (drawings 22)
    (tracks 477)
    (zones 0)
    (modules 18)
    (nets 55)
  )
  (page USLetter)
  (title_block
    (title "Project Title")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.127)
    (user_trace_width 0.1524)
    (user_trace_width 0.254)
    (user_trace_width 0.3302)
    (user_trace_width 0.508)
    (user_trace_width 0.762)
    (user_trace_width 1.27)
    (trace_clearance 0.127)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.127)
    (segment_width 0.1524)
    (edge_width 0.1524)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (user_via 0.6858 0.3302)
    (user_via 0.762 0.4064)
    (user_via 0.8636 0.508)
    (uvia_size 0.3556)
    (uvia_drill 0.254)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.1524)
    (pcb_text_size 1.016 1.016)
    (mod_edge_width 0.1524)
    (mod_text_size 1.016 1.016)
    (mod_text_width 0.1524)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0762)
    (solder_mask_min_width 0.1016)
    (pad_to_paste_clearance -0.0762)
    (aux_axis_origin 196.5452 123.5456)
    (visible_elements FFFFFFFF)
    (pcbplotparams
      (layerselection 0x310fc_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerbers))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad2)")
  (net 2 "Net-(J1-Pad1)")
  (net 3 "Net-(J1-Pad3)")
  (net 4 "Net-(J1-Pad4)")
  (net 5 "Net-(J1-Pad5)")
  (net 6 "Net-(J1-Pad6)")
  (net 7 "Net-(J1-Pad7)")
  (net 8 "Net-(J1-Pad8)")
  (net 9 "Net-(J1-Pad9)")
  (net 10 "Net-(J1-Pad10)")
  (net 11 "Net-(J1-Pad12)")
  (net 12 "Net-(J1-Pad18)")
  (net 13 "Net-(J1-Pad19)")
  (net 14 "Net-(J1-Pad20)")
  (net 15 "Net-(J1-Pad21)")
  (net 16 "Net-(J1-Pad22)")
  (net 17 "Net-(J1-Pad23)")
  (net 18 BS1)
  (net 19 "Net-(C2-Pad1)")
  (net 20 "Net-(C2-Pad2)")
  (net 21 VGH)
  (net 22 PRVGL)
  (net 23 VGL)
  (net 24 VDD)
  (net 25 VSH)
  (net 26 VGH2)
  (net 27 VSL)
  (net 28 VCOM)
  (net 29 NC2)
  (net 30 NC1)
  (net 31 NC3)
  (net 32 NC4)
  (net 33 NC5)
  (net 34 NC6)
  (net 35 GDR)
  (net 36 RESE)
  (net 37 TSCL)
  (net 38 TSDA)
  (net 39 BUSY)
  (net 40 ^RES)
  (net 41 ^D/C)
  (net 42 ^CS)
  (net 43 SCK)
  (net 44 DOUT)
  (net 45 VPP)
  (net 46 NC7)
  (net 47 NC8)
  (net 48 VDDIO)
  (net 49 "Net-(J1-Pad0)")
  (net 50 "Net-(J1-PadPGM)")
  (net 51 "Net-(J1-PadDAC)")
  (net 52 "Net-(J1-Pad3V2)")
  (net 53 "Net-(J1-PadVIN)")
  (net 54 "Net-(J1-PadVBAT)")
  (net_class Default "This is the default net class."
    (clearance 0.127)
    (trace_width 0.127)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.3556)
    (uvia_drill 0.254)
    (add_net BS1)
    (add_net BUSY)
    (add_net DOUT)
    (add_net GDR)
    (add_net NC1)
    (add_net NC2)
    (add_net NC3)
    (add_net NC4)
    (add_net NC5)
    (add_net NC6)
    (add_net NC7)
    (add_net NC8)
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(J1-Pad0)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad10)")
    (add_net "Net-(J1-Pad12)")
    (add_net "Net-(J1-Pad18)")
    (add_net "Net-(J1-Pad19)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad20)")
    (add_net "Net-(J1-Pad21)")
    (add_net "Net-(J1-Pad22)")
    (add_net "Net-(J1-Pad23)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad3V2)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J1-Pad9)")
    (add_net "Net-(J1-PadDAC)")
    (add_net "Net-(J1-PadPGM)")
    (add_net "Net-(J1-PadVBAT)")
    (add_net "Net-(J1-PadVIN)")
    (add_net PRVGL)
    (add_net RESE)
    (add_net SCK)
    (add_net TSCL)
    (add_net TSDA)
    (add_net VCOM)
    (add_net VDD)
    (add_net VDDIO)
    (add_net VGH)
    (add_net VGH2)
    (add_net VGL)
    (add_net VPP)
    (add_net VSH)
    (add_net VSL)
    (add_net ^CS)
    (add_net ^D/C)
    (add_net ^RES)
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 541A9B8D)
    (at 98.89262 34.967299)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 0 -2.1) (layer F.SilkS))
    (fp_text value CAP-CER-1UF (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 18 BS1))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 48 VDDIO))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 541A9B8D)
    (at 110.29262 34.967299)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 0 -2.1) (layer F.SilkS))
    (fp_text value CAP-CER-1UF (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(C2-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 541A9B8D)
    (at 121.69262 34.967299)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at 0 -2.1) (layer F.SilkS))
    (fp_text value CAP-CER-1UF (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 18 BS1))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 21 VGH))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 541A9B8D)
    (at 98.89262 41.117299)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at 0 -2.1) (layer F.SilkS))
    (fp_text value CAP-CER-1UF (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 18 BS1))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 22 PRVGL))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 541A9B8D)
    (at 110.29262 41.117299)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C5 (at 0 -2.1) (layer F.SilkS))
    (fp_text value CAP-CER-1UF (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 18 BS1))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 23 VGL))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 541A9B8D)
    (at 121.69262 41.117299)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C6 (at 0 -2.1) (layer F.SilkS))
    (fp_text value CAP-CER-1UF (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 18 BS1))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 24 VDD))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 541A9B8D)
    (at 98.89262 47.267299)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C7 (at 0 -2.1) (layer F.SilkS))
    (fp_text value CAP-CER-1UF (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 18 BS1))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 25 VSH))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 541A9B8D)
    (at 110.29262 47.267299)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C8 (at 0 -2.1) (layer F.SilkS))
    (fp_text value CAP-CER-1UF (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 18 BS1))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 26 VGH2))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 541A9B8D)
    (at 121.69262 47.267299)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C9 (at 0 -2.1) (layer F.SilkS))
    (fp_text value CAP-CER-1UF (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 18 BS1))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 28 VCOM))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 541A9B8D)
    (at 98.89262 53.417299)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C10 (at 0 -2.1) (layer F.SilkS))
    (fp_text value CAP-CER-1UF (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 18 BS1))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 27 VSL))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:SOD-123 (layer F.Cu) (tedit 5530FCB9)
    (at 160.8201 30.0482)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D1 (at 0 -2) (layer F.SilkS))
    (fp_text value DIODE (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.635 0) (size 0.91 1.22) (layers F.Cu F.Paste F.Mask)
      (net 18 BS1))
    (pad 2 smd rect (at 1.635 0) (size 0.91 1.22) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(C2-Pad1)"))
  )
  (module Diodes_SMD:SOD-123 (layer F.Cu) (tedit 5530FCB9)
    (at 160.8201 36.1823)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D2 (at 0 -2) (layer F.SilkS))
    (fp_text value DIODE (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.635 0) (size 0.91 1.22) (layers F.Cu F.Paste F.Mask)
      (net 21 VGH))
    (pad 2 smd rect (at 1.635 0) (size 0.91 1.22) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(C2-Pad2)"))
  )
  (module Diodes_SMD:SOD-123 (layer F.Cu) (tedit 5530FCB9)
    (at 160.4645 42.0497 180)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D3 (at 0 -2 180) (layer F.SilkS))
    (fp_text value DIODE (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.635 0 180) (size 0.91 1.22) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 1.635 0 180) (size 0.91 1.22) (layers F.Cu F.Paste F.Mask)
      (net 22 PRVGL))
  )
  (module Wickerlib:TEENSY-3.2-SILK (layer F.Cu) (tedit 583B5CF0)
    (at 143.600002 37.5473)
    (fp_text reference J1 (at -2 0) (layer F.Fab))
    (fp_text value TEENSY3.2-72MHz (at -2.54 20.32) (layer F.Fab) hide)
    (fp_text user VIN (at 8.382095 -10.16) (layer F.SilkS))
    (fp_text user %R (at 5.08 -12.7) (layer F.SilkS))
    (fp_text user AGND (at 9.144 -7.62) (layer F.SilkS))
    (fp_text user 3.3V (at 8.810666 -5.08) (layer F.SilkS))
    (fp_text user 23 (at 8.144 -2.54) (layer F.SilkS))
    (fp_text user 22 (at 8.144 0) (layer F.SilkS))
    (fp_text user 21 (at 8.144 2.54) (layer F.SilkS))
    (fp_text user 20 (at 8.144 5.08) (layer F.SilkS))
    (fp_text user 19 (at 8.144 7.62) (layer F.SilkS))
    (fp_text user 18 (at 8.144 10.16) (layer F.SilkS))
    (fp_text user 17 (at 8.144 12.7) (layer F.SilkS))
    (fp_text user 16 (at 8.144 15.24) (layer F.SilkS))
    (fp_text user 15 (at 8.144 17.78) (layer F.SilkS))
    (fp_text user 14 (at 8.144 20.32) (layer F.SilkS))
    (fp_text user 13 (at 8.144 22.86) (layer F.SilkS))
    (fp_text user 0 (at -12.668381 -7.62) (layer F.SilkS))
    (fp_text user GND (at -13.716 -10.16) (layer F.SilkS))
    (fp_text user VBAT (at -7.62 26.416 90) (layer F.SilkS))
    (fp_text user 3.3V (at -5.08 26.416 90) (layer F.SilkS))
    (fp_text user GND (at -2.54 26.416 90) (layer F.SilkS))
    (fp_text user PGM (at 0 26.416 90) (layer F.SilkS))
    (fp_text user DAC (at 2.54 26.416 90) (layer F.SilkS))
    (fp_text user 1 (at -12.668381 -5.08) (layer F.SilkS))
    (fp_text user 2 (at -12.668381 -2.54) (layer F.SilkS))
    (fp_text user 3 (at -12.668381 0) (layer F.SilkS))
    (fp_text user 4 (at -12.668381 2.54) (layer F.SilkS))
    (fp_text user 5 (at -12.668381 5.08) (layer F.SilkS))
    (fp_text user 6 (at -12.668381 7.62) (layer F.SilkS))
    (fp_text user 7 (at -12.668381 10.16) (layer F.SilkS))
    (fp_text user 8 (at -12.668381 12.7) (layer F.SilkS))
    (fp_text user 9 (at -12.668381 15.24) (layer F.SilkS))
    (fp_text user 10 (at -13.144571 17.78) (layer F.SilkS))
    (fp_text user 11 (at -13.144571 20.32) (layer F.SilkS))
    (fp_text user 12 (at -13.144571 22.86) (layer F.SilkS))
    (pad G1 thru_hole circle (at -10.16 -10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 BS1))
    (pad 0 thru_hole circle (at -10.16 -7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 49 "Net-(J1-Pad0)"))
    (pad 1 thru_hole circle (at -10.16 -5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(J1-Pad1)"))
    (pad 2 thru_hole circle (at -10.16 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(J1-Pad2)"))
    (pad 3 thru_hole circle (at -10.16 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(J1-Pad3)"))
    (pad 4 thru_hole circle (at -10.16 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(J1-Pad4)"))
    (pad 5 thru_hole circle (at -10.16 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(J1-Pad5)"))
    (pad 6 thru_hole circle (at -10.16 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(J1-Pad6)"))
    (pad 7 thru_hole circle (at -10.16 10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(J1-Pad7)"))
    (pad 8 thru_hole circle (at -10.16 12.7) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(J1-Pad8)"))
    (pad 9 thru_hole circle (at -10.16 15.24) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(J1-Pad9)"))
    (pad 10 thru_hole circle (at -10.16 17.78) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(J1-Pad10)"))
    (pad 11 thru_hole circle (at -10.16 20.32) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 44 DOUT))
    (pad 12 thru_hole circle (at -10.16 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(J1-Pad12)"))
    (pad VBAT thru_hole circle (at -7.62 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 54 "Net-(J1-PadVBAT)"))
    (pad 3V1 thru_hole circle (at -5.08 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 48 VDDIO))
    (pad G2 thru_hole circle (at -2.54 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 BS1))
    (pad PGM thru_hole circle (at 0 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 50 "Net-(J1-PadPGM)"))
    (pad DAC thru_hole circle (at 2.54 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 "Net-(J1-PadDAC)"))
    (pad 13 thru_hole circle (at 5.08 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 43 SCK))
    (pad 16 thru_hole circle (at 5.08 15.24) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 41 ^D/C))
    (pad 3V2 thru_hole circle (at 5.08 -5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 52 "Net-(J1-Pad3V2)"))
    (pad 18 thru_hole circle (at 5.08 10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(J1-Pad18)"))
    (pad 17 thru_hole circle (at 5.08 12.7) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 42 ^CS))
    (pad AG thru_hole circle (at 5.08 -7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 BS1))
    (pad 22 thru_hole circle (at 5.08 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(J1-Pad22)"))
    (pad VIN thru_hole circle (at 5.08 -10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 53 "Net-(J1-PadVIN)"))
    (pad 21 thru_hole circle (at 5.08 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(J1-Pad21)"))
    (pad 20 thru_hole circle (at 5.08 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(J1-Pad20)"))
    (pad 19 thru_hole circle (at 5.08 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(J1-Pad19)"))
    (pad 23 thru_hole circle (at 5.08 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(J1-Pad23)"))
    (pad 14 thru_hole circle (at 5.08 20.32) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 40 ^RES))
    (pad 15 thru_hole circle (at 5.08 17.78) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 39 BUSY))
  )
  (module Wickerlib:CONN-HEADER-FH34SRJ-34S-0.5SH (layer F.Cu) (tedit 58425DB7)
    (at 112.559286 28.01762)
    (fp_text reference J2 (at -0.225 -0.325 180) (layer F.Fab))
    (fp_text value HEADER-FEMALE-34POS-FFC-SMT-1x34-P0.5MM (at 0 2.9 180) (layer F.Fab) hide)
    (fp_text user %R (at -10.425 -0.075 90) (layer F.SilkS))
    (pad 2 smd rect (at 9.175 -1.325 90) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 29 NC2))
    (pad 1 smd rect (at -8.225 1.175 90) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 30 NC1))
    (pad 2 smd rect (at -7.725 1.175 90) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 29 NC2))
    (pad 3 smd rect (at -7.225 1.175 90) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 31 NC3))
    (pad 4 smd rect (at -6.725 1.175 90) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 32 NC4))
    (pad 5 smd rect (at -6.225 1.175 90) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 33 NC5))
    (pad 6 smd rect (at -5.725 1.175 90) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 34 NC6))
    (pad 7 smd rect (at -5.225 1.175 90) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 35 GDR))
    (pad 8 smd rect (at -4.725 1.175 90) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 36 RESE))
    (pad 9 smd rect (at -4.225 1.175 90) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 23 VGL))
    (pad 10 smd rect (at -3.725 1.175 90) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 21 VGH))
    (pad 11 smd rect (at -3.225 1.175 90) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 37 TSCL))
    (pad 12 smd rect (at -2.725 1.175 90) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 38 TSDA))
    (pad 13 smd rect (at -2.225 1.175 90) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 18 BS1))
    (pad 14 smd rect (at -1.725 1.175 90) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 39 BUSY))
    (pad 15 smd rect (at -1.225 1.175 90) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 40 ^RES))
    (pad 16 smd rect (at -0.725 1.175 90) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 41 ^D/C))
    (pad 17 smd rect (at -0.225 1.175 90) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 42 ^CS))
    (pad 18 smd rect (at 0.275 1.175 90) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 43 SCK))
    (pad 19 smd rect (at 0.775 1.175 90) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 44 DOUT))
    (pad 20 smd rect (at 1.275 1.175 90) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 48 VDDIO))
    (pad 21 smd rect (at 1.775 1.175 90) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 48 VDDIO))
    (pad 22 smd rect (at 2.275 1.175 90) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 18 BS1))
    (pad 23 smd rect (at 2.775 1.175 90) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 24 VDD))
    (pad 24 smd rect (at 3.275 1.175 90) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 45 VPP))
    (pad 25 smd rect (at 3.775 1.175 90) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 25 VSH))
    (pad 26 smd rect (at 4.275 1.175 90) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 26 VGH2))
    (pad 27 smd rect (at 4.775 1.175 90) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 27 VSL))
    (pad 28 smd rect (at 5.275 1.175 90) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 22 PRVGL))
    (pad 29 smd rect (at 5.775 1.175 90) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 28 VCOM))
    (pad 30 smd rect (at 6.275 1.175 90) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 46 NC7))
    (pad 31 smd rect (at 6.775 1.175 90) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 47 NC8))
    (pad 32 smd rect (at 7.275 1.175 90) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 47 NC8))
    (pad 33 smd rect (at 7.775 1.175 90) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 47 NC8))
    (pad 34 smd rect (at 8.275 1.175 90) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 47 NC8))
    (pad 2 smd rect (at -9.125 -1.325 90) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 29 NC2))
  )
  (module Inductors:Inductor_1212 (layer F.Cu) (tedit 5652586A)
    (at 118.445477 54.067299)
    (attr smd)
    (fp_text reference L1 (at 0 2.75) (layer F.SilkS))
    (fp_text value INDUCTOR (at 0 -2.75) (layer F.Fab))
    (pad 1 smd rect (at -1.75 0) (size 2.5 2.5) (layers F.Cu F.Paste F.Mask)
      (net 48 VDDIO))
    (pad 2 smd rect (at 1.75 0) (size 2.5 2.5) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(C2-Pad2)"))
  )
  (module TO_SOT_Packages_SMD:SOT-23_Handsoldering (layer F.Cu) (tedit 54E9291B)
    (at 109.602144 55.127299)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at 0 -3.81) (layer F.SilkS))
    (fp_text value Q_NMOS_GDS (at 0 3.81) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.50114) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 35 GDR))
    (pad 2 smd rect (at 0.95 1.50114) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 36 RESE))
    (pad 3 smd rect (at 0 -1.50114) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(C2-Pad2)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 54189DEE)
    (at 125.554048 53.417299)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0 -2.1) (layer F.SilkS))
    (fp_text value "2.2R 1%" (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 36 RESE))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 18 BS1))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 164.36848 23.4315) (end 164.36848 23.40864) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 95.3643 23.4315) (end 164.36848 23.4315) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 95.4024 65.79616) (end 95.4024 23.40864) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 164.3761 65.79616) (end 95.4024 65.79616) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 164.3761 23.35022) (end 164.3761 65.79616) (angle 90) (layer Edge.Cuts) (width 0.1524))
)
