(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (title_block
    (title "300K SPLIT-STAGE HEMT AMPLIFIER BREAK OUT BOARD")
    (date "2023-07-18")
    (rev "V3.0")
    (company "SPLENDOR PROJECT")
    (comment 1 "IVAR RYDSTROM")
    (comment 2 "SLAC NATIONAL ACCELERATOR LABORATORY")
  )
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "Gerbers/")
    )
  )
  (net 0 "")
  (net 1 "Net-(J1-Pin_2)")
  (net 2 "Net-(C1-Pad2)")
  (net 3 "Net-(J1-Pin_3)")
  (net 4 "Net-(C3-Pad2)")
  (net 5 "Net-(J1-Pin_6)")
  (net 6 "Net-(C5-Pad2)")
  (net 7 "Net-(J1-Pin_7)")
  (net 8 "Net-(J3-P17)")
  (net 9 "Net-(J1-Pin_1)")
  (net 10 "Net-(J1-Pin_4)")
  (net 11 "Net-(J1-Pin_5)")
  (net 12 "Net-(J1-Pin_8)")
  (net 13 "GND")
  (net 14 "Net-(J2-Pad2)")
  (net 15 "Net-(J3-P14)")
  (net 16 "Net-(J2-Pad4)")
  (net 17 "Net-(J3-P19)")
  (net 18 "unconnected-(J3-Pad2)")
  (net 19 "unconnected-(J3-Pad7)")
  (net 20 "unconnected-(J3-Pad8)")
  (net 21 "unconnected-(J3-Pad9)")
  (net 22 "unconnected-(J3-Pad10)")
  (net 23 "unconnected-(J3-Pad11)")
  (net 24 "unconnected-(J3-Pad12)")
  (net 25 "unconnected-(J3-Pad13)")
  (net 26 "unconnected-(J3-P15-Pad15)")
  (net 27 "unconnected-(J3-P20-Pad20)")
  (net 28 "unconnected-(J3-P21-Pad21)")
  (net 29 "unconnected-(J3-P22-Pad22)")
  (net 30 "unconnected-(J3-P23-Pad23)")
  (net 31 "unconnected-(J3-P24-Pad24)")
  (net 32 "unconnected-(J3-P25-Pad25)")
  (footprint "lib:CONN_5747846-4_TYC" (layer "F.Cu")
    (at 235.6612 99.53 -90)
    (tags "5747846-4 ")
    (property "Sheetfile" "hemt_breakout_board_V3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "25-pin female receptacle socket D-SUB connector, Mounting Hole")
    (property "ki_keywords" "female receptacle D-SUB connector")
    (attr through_hole)
    (fp_text reference "J3" (at 0 0 -90 unlocked) (layer "F.SilkS"))
    (fp_text value "DB25_Female_Fridge" (at 0 0 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -16.6116 10.922 270) (size 1.651 1.651) (drill 1.143) (layers "*.Cu" "*.Mask")
      (net 14 "Net-(J2-Pad2)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at -13.843 10.922 270) (size 1.651 1.651) (drill 1.143) (layers "*.Cu" "*.Mask")
      (net 18 "unconnected-(J3-Pad2)") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at -11.0744 10.922 270) (size 1.651 1.651) (drill 1.143) (layers "*.Cu" "*.Mask")
      (net 2 "Net-(C1-Pad2)") (pinfunction "3") (pintype "passive"))
    (pad "4" thru_hole circle (at -8.3058 10.922 270) (size 1.651 1.651) (drill 1.143) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(C3-Pad2)") (pinfunction "4") (pintype "passive"))
    (pad "5" thru_hole circle (at -5.5372 10.922 270) (size 1.651 1.651) (drill 1.143) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(C5-Pad2)") (pinfunction "5") (pintype "passive"))
    (pad "6" thru_hole circle (at -2.7686 10.922 270) (size 1.651 1.651) (drill 1.143) (layers "*.Cu" "*.Mask")
      (net 16 "Net-(J2-Pad4)") (pinfunction "6") (pintype "passive"))
    (pad "7" thru_hole circle (at 0 10.922 270) (size 1.651 1.651) (drill 1.143) (layers "*.Cu" "*.Mask")
      (net 19 "unconnected-(J3-Pad7)") (pinfunction "7") (pintype "passive"))
    (pad "8" thru_hole circle (at 2.7686 10.922 270) (size 1.651 1.651) (drill 1.143) (layers "*.Cu" "*.Mask")
      (net 20 "unconnected-(J3-Pad8)") (pinfunction "8") (pintype "passive"))
    (pad "9" thru_hole circle (at 5.5372 10.922 270) (size 1.651 1.651) (drill 1.143) (layers "*.Cu" "*.Mask")
      (net 21 "unconnected-(J3-Pad9)") (pinfunction "9") (pintype "passive"))
    (pad "10" thru_hole circle (at 8.3058 10.922 270) (size 1.651 1.651) (drill 1.143) (layers "*.Cu" "*.Mask")
      (net 22 "unconnected-(J3-Pad10)") (pinfunction "10") (pintype "passive"))
    (pad "11" thru_hole circle (at 11.0744 10.922 270) (size 1.651 1.651) (drill 1.143) (layers "*.Cu" "*.Mask")
      (net 23 "unconnected-(J3-Pad11)") (pinfunction "11") (pintype "passive"))
    (pad "12" thru_hole circle (at 13.843 10.922 270) (size 1.651 1.651) (drill 1.143) (layers "*.Cu" "*.Mask")
      (net 24 "unconnected-(J3-Pad12)") (pinfunction "12") (pintype "passive"))
    (pad "13" thru_hole circle (at 16.6116 10.922 270) (size 1.651 1.651) (drill 1.143) (layers "*.Cu" "*.Mask")
      (net 25 "unconnected-(J3-Pad13)") (pinfunction "13") (pintype "passive"))
    (pad "14" thru_hole circle (at -15.2273 8.0772 270) (size 1.651 1.651) (drill 1.143) (layers "*.Cu" "*.Mask")
      (net 15 "Net-(J3-P14)") (pinfunction "P14") (pintype "passive"))
    (pad "15" thru_hole circle (at -12.4587 8.0772 270) (size 1.651 1.651) (drill 1.143) (layers "*.Cu" "*.Mask")
      (net 26 "unconnected-(J3-P15-Pad15)") (pinfunction "P15") (pintype "passive"))
    (pad "16" thru_hole circle (at -9.6901 8.0772 270) (size 1.651 1.651) (drill 1.143) (layers "*.Cu" "*.Mask")
      (net 1 "Net-(J1-Pin_2)") (pinfunction "P16") (pintype "passive"))
    (pad "17" thru_hole circle (at -6.9215 8.0772 270) (size 1.651 1.651) (drill 1.143) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(J3-P17)") (pinfunction "P17") (pintype "passive"))
    (pad "18" thru_hole circle (at -4.1529 8.0772 270) (size 1.651 1.651) (drill 1.143) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(J1-Pin_3)") (pinfunction "P18") (pintype "passive"))
    (pad "19" thru_hole circle (at -1.3843 8.0772 270) (size 1.651 1.651) (drill 1.143) (layers "*.Cu" "*.Mask")
      (net 17 "Net-(J3-P19)") (pinfunction "P19") (pintype "passive"))
    (pad "20" thru_hole circle (at 1.3843 8.0772 270) (size 1.651 1.651) (drill 1.143) (layers "*.Cu" "*.Mask")
      (net 27 "unconnected-(J3-P20-Pad20)") (pinfunction "P20") (pintype "passive"))
    (pad "21" thru_hole circle (at 4.1529 8.0772 270) (size 1.651 1.651) (drill 1.143) (layers "*.Cu" "*.Mask")
      (net 28 "unconnected-(J3-P21-Pad21)") (pinfunction "P21") (pintype "passive"))
    (pad "22" thru_hole circle (at 6.9215 8.0772 270) (size 1.651 1.651) (drill 1.143) (layers "*.Cu" "*.Mask")
      (net 29 "unconnected-(J3-P22-Pad22)") (pinfunction "P22") (pintype "passive"))
    (pad "23" thru_hole circle (at 9.6901 8.0772 270) (size 1.651 1.651) (drill 1.143) (layers "*.Cu" "*.Mask")
      (net 30 "unconnected-(J3-P23-Pad23)") (pinfunction "P23") (pintype "passive"))
    (pad "24" thru_hole circle (at 12.4587 8.0772 270) (size 1.651 1.651) (drill 1.143) (layers "*.Cu" "*.Mask")
      (net 31 "unconnected-(J3-P24-Pad24)") (pinfunction "P24") (pintype "passive"))
    (pad "25" thru_hole circle (at 15.2273 8.0772 270) (size 1.651 1.651) (drill 1.143) (layers "*.Cu" "*.Mask")
      (net 32 "unconnected-(J3-P25-Pad25)") (pinfunction "P25") (pintype "passive"))
    (pad "26" thru_hole circle (at -23.6474 9.4996 270) (size 3.302 3.302) (drill 3.302) (layers "*.Cu" "*.Mask"))
    (pad "27" thru_hole circle (at 23.6474 9.4996 270) (size 3.302 3.302) (drill 3.302) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 185.259 110.1435)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "hemt_breakout_board_V3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R3" (at 0.034 -1.5585) (layer "B.SilkS"))
    (fp_text value "100" (at 0.034 1.7435) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 11 "Net-(J1-Pin_5)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 6 "Net-(C5-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1812_4532Metric" (layer "B.Cu")
    (at 201.269 67.945 180)
    (descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "hemt_breakout_board_V3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C2" (at 0 2.65) (layer "B.SilkS"))
    (fp_text value "470uF" (at 0 -2.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -2.05 0 180) (size 1.4 3.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1785707143)
      (net 1 "Net-(J1-Pin_2)") (pintype "passive"))
    (pad "2" smd roundrect (at 2.05 0 180) (size 1.4 3.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1785707143)
      (net 2 "Net-(C1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "B.Cu")
    (at 192.769 67.945)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "hemt_breakout_board_V3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C1" (at 0 -1.8034) (layer "B.SilkS"))
    (fp_text value "10nF" (at 0.017 1.905) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.475 0) (size 1.15 1.8) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2173913043)
      (net 1 "Net-(J1-Pin_2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0) (size 1.15 1.8) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2173913043)
      (net 2 "Net-(C1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 185.259 88.9165)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "hemt_breakout_board_V3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R2" (at 0 -1.6675) (layer "B.SilkS"))
    (fp_text value "100" (at 0 1.7615) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 10 "Net-(J1-Pin_4)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 4 "Net-(C3-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 185.259 131.4975)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "hemt_breakout_board_V3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R4" (at 0 -1.6019) (layer "B.SilkS"))
    (fp_text value "100" (at 0.0086 1.7509) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 12 "Net-(J1-Pin_8)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 8 "Net-(J3-P17)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 185.269 67.945)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "hemt_breakout_board_V3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R1" (at -0.0014 -1.6002) (layer "B.SilkS"))
    (fp_text value "100" (at -0.0014 1.7018) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 9 "Net-(J1-Pin_1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 2 "Net-(C1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "B.Cu")
    (at 192.759 110.1435 180)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "hemt_breakout_board_V3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C5" (at 0 1.85) (layer "B.SilkS"))
    (fp_text value "10nF" (at 0 -1.85) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.475 0 180) (size 1.15 1.8) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2173913043)
      (net 5 "Net-(J1-Pin_6)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0 180) (size 1.15 1.8) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2173913043)
      (net 6 "Net-(C5-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "B.Cu")
    (at 192.759 88.9165 180)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "hemt_breakout_board_V3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C3" (at 0 1.85) (layer "B.SilkS"))
    (fp_text value "10nF" (at 0 -1.85) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.475 0 180) (size 1.15 1.8) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2173913043)
      (net 3 "Net-(J1-Pin_3)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0 180) (size 1.15 1.8) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2173913043)
      (net 4 "Net-(C3-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.00mm:PinSocket_2x04_P2.00mm_Vertical" (layer "B.Cu")
    (at 168.021 63.91475 180)
    (descr "Through hole straight socket strip, 2x04, 2.00mm pitch, double cols (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 2x04 2.00mm double row")
    (property "Sheetfile" "hemt_breakout_board_V3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, double row, 02x04, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins), script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J1" (at -1 2.5) (layer "B.SilkS"))
    (fp_text value "DA-15_Solder_Cups_Harvard_PS" (at -1.016 -10.517) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at -1 -3 90) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.35 1.35) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(J1-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at -2 0 180) (size 1.35 1.35) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "Net-(J1-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 -2 180) (size 1.35 1.35) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(J1-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at -2 -2 180) (size 1.35 1.35) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(J1-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 -4 180) (size 1.35 1.35) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(J1-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at -2 -4 180) (size 1.35 1.35) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(J1-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 -6 180) (size 1.35 1.35) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(J1-Pin_7)") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at -2 -6 180) (size 1.35 1.35) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 12 "Net-(J1-Pin_8)") (pinfunction "Pin_8") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.00mm.3dshapes/PinSocket_2x04_P2.00mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "B.Cu")
    (at 192.759 131.3705 180)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "hemt_breakout_board_V3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C7" (at 0 1.85) (layer "B.SilkS"))
    (fp_text value "10nF" (at 0 -1.85) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.475 0 180) (size 1.15 1.8) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2173913043)
      (net 7 "Net-(J1-Pin_7)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0 180) (size 1.15 1.8) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2173913043)
      (net 8 "Net-(J3-P17)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "lib:MILL-MAX_830-10-006-10-005000" (layer "B.Cu")
    (at 169.021 124.587 -90)
    (property "MANUFACTURER" "Mill-Max")
    (property "MAXIMUM_PACKAGE_HEIGHT" "6.40mm")
    (property "PARTREV" "10/21/21")
    (property "STANDARD" "IPC 7351B")
    (property "Sheetfile" "hemt_breakout_board_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at 7.493 0.127 90) (layer "B.SilkS"))
    (fp_text value "BNC_Solder_Cups" (at 0.254 -3.953 -90) (layer "B.Fab"))
    (pad "1" thru_hole rect (at -5 0 270) (size 1.218 1.218) (drill 0.71) (layers "*.Cu" "*.Mask")
      (net 13 "GND") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at -3 0 270) (size 1.218 1.218) (drill 0.71) (layers "*.Cu" "*.Mask")
      (net 14 "Net-(J2-Pad2)") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at -1 0 270) (size 1.218 1.218) (drill 0.71) (layers "*.Cu" "*.Mask")
      (net 15 "Net-(J3-P14)") (pinfunction "3") (pintype "passive"))
    (pad "4" thru_hole circle (at 1 0 270) (size 1.218 1.218) (drill 0.71) (layers "*.Cu" "*.Mask")
      (net 16 "Net-(J2-Pad4)") (pinfunction "4") (pintype "passive"))
    (pad "5" thru_hole circle (at 3 0 270) (size 1.218 1.218) (drill 0.71) (layers "*.Cu" "*.Mask")
      (net 17 "Net-(J3-P19)") (pinfunction "5") (pintype "passive"))
    (pad "6" thru_hole circle (at 5 0 270) (size 1.218 1.218) (drill 0.71) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(C3-Pad2)") (pinfunction "6") (pintype "passive"))
  )
  (footprint "Capacitor_SMD:C_1812_4532Metric" (layer "B.Cu")
    (at 201.259 88.9165)
    (descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "hemt_breakout_board_V3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C4" (at 0 -2.4295) (layer "B.SilkS"))
    (fp_text value "470uF" (at 0 2.6505) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -2.05 0) (size 1.4 3.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1785707143)
      (net 3 "Net-(J1-Pin_3)") (pintype "passive"))
    (pad "2" smd roundrect (at 2.05 0) (size 1.4 3.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1785707143)
      (net 4 "Net-(C3-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1812_4532Metric" (layer "B.Cu")
    (at 201.259 131.3705)
    (descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "hemt_breakout_board_V3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C8" (at 0 -2.5925) (layer "B.SilkS"))
    (fp_text value "470uF" (at 0 2.6907) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -2.05 0) (size 1.4 3.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1785707143)
      (net 7 "Net-(J1-Pin_7)") (pintype "passive"))
    (pad "2" smd roundrect (at 2.05 0) (size 1.4 3.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1785707143)
      (net 8 "Net-(J3-P17)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1812_4532Metric" (layer "B.Cu")
    (at 201.259 110.1435)
    (descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "hemt_breakout_board_V3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C6" (at 0 2.65) (layer "B.SilkS"))
    (fp_text value "470uF" (at 0 -2.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -2.05 0) (size 1.4 3.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1785707143)
      (net 5 "Net-(J1-Pin_6)") (pintype "passive"))
    (pad "2" smd roundrect (at 2.05 0) (size 1.4 3.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1785707143)
      (net 6 "Net-(C5-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 85 50) (end 85 80)
    (layer "Edge.Cuts"))
  (gr_line (start 85 80) (end 155.946 80)
    (layer "Edge.Cuts"))
  (gr_line (start 155.946 149.06) (end 231.892 149.06)
    (layer "Edge.Cuts"))
  (gr_line (start 155.946 80) (end 155.946 149.06)
    (layer "Edge.Cuts"))
  (gr_line (start 85 50) (end 231.892 50)
    (layer "Edge.Cuts"))
  (gr_line (start 231.892 149.06) (end 231.892 50)
    (layer "Edge.Cuts"))
  (gr_text "Vgg2" (at 206.629 129.5925 90) (layer "B.SilkS"))
  (gr_text "Vgg2(8)" (at 177.546 70.48675) (layer "B.SilkS"))
  (gr_text "DETBIAS-" (at 167.767 124.206) (layer "B.SilkS"))
  (gr_text "Vdd2(5)" (at 177.546 64.51775) (layer "B.SilkS"))
  (gr_text "Vgg1(4)\n" (at 166.243 70.48675) (layer "B.SilkS"))
  (gr_text "Vdd1" (at 206.502 66.167 90) (layer "B.SilkS"))
  (gr_text "INJ" (at 167.767 130.302) (layer "B.SilkS"))
  (gr_text "GND(9)" (at 166.37 66.42275) (layer "B.SilkS"))
  (gr_text "OUT-" (at 167.767 128.27) (layer "B.SilkS"))
  (gr_text "SPLENDOR PROJECT\n300K SPLIT-STAGE HEMT AMPLIFIER\nBREAK OUT BOARD\nSLAC NATIONAL ACCELERATOR LABORATORY\nIVAR RYDSTROM  |  7/18/2023" (at 164.338 80.01 90) (layer "B.SilkS"))
  (gr_text "DETBIAS+" (at 167.767 122.174) (layer "B.SilkS"))
  (gr_text "GND(22)\n" (at 166.37 68.45475) (layer "B.SilkS"))
  (gr_text "GND(15)" (at 177.927 68.45475) (layer "B.SilkS"))
  (gr_text "Vdd2" (at 206.629 108.458 90) (layer "B.SilkS"))
  (gr_text "Vgg1" (at 206.629 87.122 90) (layer "B.SilkS"))
  (gr_text "Vdd1(1)" (at 166.37 64.51775) (layer "B.SilkS"))
  (gr_text "GND(13)" (at 177.927 66.42275) (layer "B.SilkS"))
  (gr_text "OUT+" (at 167.767 126.238) (layer "B.SilkS"))
  (gr_text "GND" (at 167.767 120.142) (layer "B.SilkS"))
  (gr_text "BNC LINE-IN" (at 171.704 119.761 90) (layer "B.SilkS"))
  (gr_text "Harvard_PS_IN" (at 174.117 73.03475) (layer "B.SilkS"))
  (zone (net 13) (net_name "GND") (layers "F&B.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 84.328 49.056392)
        (xy 232.74 49.08)
        (xy 232.74 149.918)
        (xy 155.143 149.918)
        (xy 155.143 80.449)
        (xy 84.328 80.449)
      )
    )
  )
)
