<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.1.3">
<drawing>
<board>
<plain>
<wire x1="12.319" y1="8.5" x2="16.12" y2="8.5" width="0.1524" layer="20"/>
<wire x1="16.12" y1="8.5" x2="19.05" y2="11.43" width="0.1524" layer="20" curve="90"/>
<wire x1="19.05" y1="11.43" x2="19.05" y2="13.335" width="0.1524" layer="20"/>
<wire x1="19.05" y1="13.335" x2="20.32" y2="14.605" width="0.1524" layer="20" curve="-90"/>
<wire x1="20.32" y1="14.605" x2="24.13" y2="14.605" width="0.1524" layer="20"/>
<wire x1="24.13" y1="14.605" x2="25" y2="13.735" width="0.1524" layer="20" curve="-90"/>
<wire x1="25" y1="13.735" x2="25" y2="8.5" width="0.1524" layer="20"/>
<wire x1="25" y1="8.5" x2="25" y2="4.2" width="0.1524" layer="20"/>
<wire x1="12.319" y1="-8.5" x2="12.7" y2="-8.5" width="0.1524" layer="20"/>
<wire x1="12.7" y1="-8.5" x2="13.09" y2="-8.5" width="0.1524" layer="20"/>
<wire x1="13.09" y1="-8.5" x2="13.58" y2="-8.5" width="0.1524" layer="20"/>
<wire x1="13.58" y1="-8.5" x2="13.97" y2="-8.509" width="0.1524" layer="20"/>
<wire x1="13.97" y1="-8.509" x2="13.97" y2="-6.223" width="0.1524" layer="20"/>
<wire x1="13.97" y1="-6.223" x2="13.97" y2="-5.08" width="0.1524" layer="20"/>
<wire x1="13.97" y1="-5.08" x2="20.32" y2="1.27" width="0.1524" layer="20" curve="-90"/>
<wire x1="20.32" y1="1.27" x2="24.13" y2="1.27" width="0.1524" layer="20"/>
<wire x1="24.13" y1="1.27" x2="25" y2="2.14" width="0.1524" layer="20" curve="90"/>
<wire x1="25" y1="2.14" x2="25" y2="4.2" width="0.1524" layer="20"/>
<wire x1="-8" y1="-12.7" x2="-8.001" y2="-19.05" width="0.1524" layer="20"/>
<wire x1="-8.001" y1="-19.05" x2="8.001" y2="-19.05" width="0.1524" layer="20"/>
<wire x1="8.001" y1="-19.05" x2="8" y2="-12.7" width="0.1524" layer="20"/>
<circle x="0" y="0" radius="3.5" width="0.1524" layer="20"/>
<wire x1="-7.5" y1="12.954" x2="-7.5" y2="19.05" width="0.1524" layer="20"/>
<wire x1="-7.5" y1="19.05" x2="7.5" y2="19.05" width="0.1524" layer="20"/>
<wire x1="7.5" y1="19.05" x2="7.5" y2="12.954" width="0.1524" layer="20"/>
<wire x1="12.319" y1="-8.5" x2="8" y2="-12.7" width="0.1524" layer="20" curve="-23.088402"/>
<wire x1="-8" y1="-12.7" x2="-15" y2="0" width="0.1524" layer="20" curve="-57.789072"/>
<wire x1="7.5" y1="12.954" x2="12.319" y2="8.5" width="0.1524" layer="20" curve="-25.247512"/>
<wire x1="-15" y1="0" x2="-7.5" y2="12.954" width="0.1524" layer="20" curve="-59.832072"/>
<text>The Real Phoenix @2019</text>
<text>Hori Fighting Commander X Project

DPad replacement</text>
<text>GND

UP

LEFT

DOWN

RIGHT</text>
</plain>
<libraries>
<library name="pinhead-2">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de, Modified by Cougar@CasaDelGato.Com&lt;/author&gt;</description>
<packages>
<package name="1X05M">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt; - 2</description>
</package>
</packages>
</library>
<library name="TRP_Custom">
<packages>
<package name="D2FC-F-K">
</package>
<package name="LOGO">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP1" library="pinhead-2" package="1X05M" value="">
<attribute name="VALUE"/>
</element>
<element name="UP" library="TRP_Custom" package="D2FC-F-K" value="OMRON_D2FC-F-7N"/>
<element name="LEFT" library="TRP_Custom" package="D2FC-F-K" value="OMRON_D2FC-F-7N"/>
<element name="DOWN" library="TRP_Custom" package="D2FC-F-K" value="OMRON_D2FC-F-7N"/>
<element name="RIGHT" library="TRP_Custom" package="D2FC-F-K" value="OMRON_D2FC-F-7N"/>
<element name="U$1" library="TRP_Custom" package="LOGO" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="UP" pad="P$1"/>
<contactref element="RIGHT" pad="P$1"/>
<contactref element="LEFT" pad="P$1"/>
<contactref element="DOWN" pad="P$1"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="RIGHT">
<contactref element="JP1" pad="1"/>
<contactref element="RIGHT" pad="P$2"/>
</signal>
<signal name="DOWN">
<contactref element="JP1" pad="2"/>
<contactref element="DOWN" pad="P$2"/>
</signal>
<signal name="LEFT">
<contactref element="JP1" pad="3"/>
<contactref element="LEFT" pad="P$2"/>
</signal>
<signal name="UP">
<contactref element="JP1" pad="4"/>
<contactref element="UP" pad="P$2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
