(kicad_pcb (version 4) (host pcbnew 4.0.4-stable)
  (general
    (links 49)
    (no_connects 0)
    (area 109.424999 63.924999 141.575001 122.075001)
    (thickness 1.6)
    (drawings 29)
    (tracks 175)
    (zones 0)
    (modules 27)
    (nets 21)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user hide)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.2 2.2)
    (pad_drill 2.2)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFF7FF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C2-Pad2)")
  (net 2 VCC)
  (net 3 GND)
  (net 4 "Net-(IC2-Pad19)")
  (net 5 "Net-(IC2-Pad15)")
  (net 6 "Net-(IC2-Pad16)")
  (net 7 "Net-(P1-Pad1)")
  (net 8 RST)
  (net 9 "Net-(D1-Pad3)")
  (net 10 "Net-(D1-Pad4)")
  (net 11 "Net-(D1-Pad1)")
  (net 12 RXI)
  (net 13 TXO)
  (net 14 SCL)
  (net 15 SDA)
  (net 16 BTN1)
  (net 17 RGB3)
  (net 18 BTN2)
  (net 19 RGB2)
  (net 20 RGB1)
  (net_class Default "Ceci est la Netclass par défaut"
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net BTN1)
    (add_net BTN2)
    (add_net GND)
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad3)")
    (add_net "Net-(D1-Pad4)")
    (add_net "Net-(IC2-Pad15)")
    (add_net "Net-(IC2-Pad16)")
    (add_net "Net-(IC2-Pad19)")
    (add_net "Net-(P1-Pad1)")
    (add_net RGB1)
    (add_net RGB2)
    (add_net RGB3)
    (add_net RST)
    (add_net RXI)
    (add_net SCL)
    (add_net SDA)
    (add_net TXO)
    (add_net VCC)
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58418D33)
    (at 118.364 87.376 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C19 (at 3.81 0 180) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2.1 180) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 58418B89)
    (at 137.127 77.5)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2 (at 0 3.2) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 58418B87)
    (at 113.873 77.5)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2 (at 0 3.2) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 58433C05)
    (at 113.873 101.554)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2 (at 0 3.2) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 58418B51)
    (at 137.5 110.5)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 58418B8B)
    (at 137.5 70)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 58418B8E)
    (at 113.5 70)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 5845869B)
    (at 128.524 95.25 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 1.5875 1.778 270) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -2.1 180) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 8 RST))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(C2-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58418D17)
    (at 118.364 85.344 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C15 (at 3.81 0 180) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2.1 180) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SSOP:SSOP-28_5.3x10.2mm_Pitch0.65mm (layer B.Cu) (tedit 58458677)
    (at 120.396 93.726 90)
    (descr "28-Lead Plastic Shrink Small Outline (SS)-5.30 mm Body [SSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference IC2 (at -1.8415 -3.4925 180) (layer B.SilkS))
    (fp_text value FT232RL (at 0 -6.25 90) (layer B.Fab))
    (pad 1 smd rect (at -3.6 4.225 90) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 12 RXI))
    (pad 2 smd rect (at -3.6 3.575 90) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(C2-Pad2)"))
    (pad 3 smd rect (at -3.6 2.925 90) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask))
    (pad 4 smd rect (at -3.6 2.275 90) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
    (pad 5 smd rect (at -3.6 1.625 90) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 13 TXO))
    (pad 6 smd rect (at -3.6 0.975 90) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask))
    (pad 7 smd rect (at -3.6 0.325 90) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 8 smd rect (at -3.6 -0.325 90) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask))
    (pad 9 smd rect (at -3.6 -0.975 90) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask))
    (pad 10 smd rect (at -3.6 -1.625 90) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask))
    (pad 11 smd rect (at -3.6 -2.275 90) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask))
    (pad 12 smd rect (at -3.6 -2.925 90) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask))
    (pad 13 smd rect (at -3.6 -3.575 90) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask))
    (pad 14 smd rect (at -3.6 -4.225 90) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask))
    (pad 15 smd rect (at 3.6 -4.225 90) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(IC2-Pad15)"))
    (pad 16 smd rect (at 3.6 -3.575 90) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(IC2-Pad16)"))
    (pad 17 smd rect (at 3.6 -2.925 90) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask))
    (pad 18 smd rect (at 3.6 -2.275 90) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 19 smd rect (at 3.6 -1.625 90) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(IC2-Pad19)"))
    (pad 20 smd rect (at 3.6 -0.975 90) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
    (pad 21 smd rect (at 3.6 -0.325 90) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 22 smd rect (at 3.6 0.325 90) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask))
    (pad 23 smd rect (at 3.6 0.975 90) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask))
    (pad 24 smd rect (at 3.6 1.625 90) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask))
    (pad 25 smd rect (at 3.6 2.275 90) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 26 smd rect (at 3.6 2.925 90) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 27 smd rect (at 3.6 3.575 90) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask))
    (pad 28 smd rect (at 3.6 4.225 90) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask))
    (model Housings_SSOP.3dshapes/SSOP-28_5.3x10.2mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58458630)
    (at 128.524 117.856 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R15 (at 0.0635 1.651 450) (layer F.SilkS))
    (fp_text value 10K (at 3.302 0.254 360) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 16 BTN1))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58458646)
    (at 122.174 99.06 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R16 (at 0 -1.778 270) (layer F.SilkS) hide)
    (fp_text value 100 (at 0 2.1 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 20 RGB1))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(D1-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 584479C7)
    (at 124.206 85.344 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R20 (at 0.116 1.624 180) (layer B.SilkS))
    (fp_text value 4k7 (at 0 -2.1 180) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(P1-Pad1)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(IC2-Pad19)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 584586B4)
    (at 124.206 87.376)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R21 (at 2.032 2.413 90) (layer B.SilkS))
    (fp_text value 10k (at 0 -2.1) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(IC2-Pad19)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5845864C)
    (at 125.73 99.06 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R22 (at 0 -1.778 270) (layer F.SilkS) hide)
    (fp_text value 100 (at 0 2.1 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 19 RGB2))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D1-Pad4)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58458654)
    (at 129.286 99.06 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R23 (at 0 -1.778 270) (layer F.SilkS) hide)
    (fp_text value 100 (at 0 2.1 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 17 RGB3))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D1-Pad3)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5845861F)
    (at 122.174 117.856 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R27 (at 0.0635 -1.7145 450) (layer F.SilkS))
    (fp_text value 10K (at -3.302 0 360) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 18 BTN2))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:MolexUSB_Mini-B_67503-1020 (layer F.Cu) (tedit 58418D71)
    (at 125.476 68.072 270)
    (descr "USB Mini-B 5-pin SMD connector")
    (tags "USB USB_B USB_Mini connector")
    (attr smd)
    (fp_text reference P1 (at 6.604 0 360) (layer F.SilkS) hide)
    (fp_text value USB_MINI (at 0 -7.112 270) (layer F.Fab) hide)
    (pad 1 smd rect (at 4.225 -1.6 270) (size 2.25 0.5) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(P1-Pad1)"))
    (pad 2 smd rect (at 4.225 -0.8 270) (size 2.25 0.5) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(IC2-Pad16)"))
    (pad 3 smd rect (at 4.225 0 270) (size 2.25 0.5) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(IC2-Pad15)"))
    (pad 4 smd rect (at 4.225 0.8 270) (size 2.25 0.5) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 4.225 1.6 270) (size 2.25 0.5) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 6 smd rect (at 4.25 -4.925 270) (size 3.5 2.05) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 6 smd rect (at 0 -4.925 270) (size 4 2.05) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 6 smd rect (at 4.25 4.925 270) (size 3.5 2.05) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 6 smd rect (at 0 4.925 270) (size 4 2.05) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad "" np_thru_hole circle (at 1.9 -2.2 270) (size 0.9 0.9) (drill 0.89916) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 1.9 2.2 270) (size 0.9 0.9) (drill 0.89916) (layers *.Cu *.Mask))
    (model ${KIPRJMOD}/libs/MolexMiniUsb.wrl
      (at (xyz 0.044 0 -0.04))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz -90 0 90))
    )
  )
  (module footprints:LedRGB_MULTICOMP_703-1028 (layer F.Cu) (tedit 58458637)
    (at 124.968 106.426)
    (descr http://www.farnell.com/datasheets/1648438.pdf?_ga=1.175449188.710131191.1477566658)
    (fp_text reference D1 (at 0.802 1.664) (layer F.SilkS) hide)
    (fp_text value LED_RABG (at 0 -2.032) (layer F.Fab) hide)
    (pad 2 smd rect (at 0 3.2) (size 0.7 1.4) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 3 smd rect (at 1.524 3.2) (size 0.7 1.4) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D1-Pad3)"))
    (pad 4 smd rect (at 1.5 0) (size 0.7 1.4) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D1-Pad4)"))
    (pad 1 smd rect (at 0 0) (size 0.7 1.4) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(D1-Pad1)"))
  )
  (module Pin_Headers:Pin_Header_Straight_1x12 (layer B.Cu) (tedit 58418D44)
    (at 133.5 106.5)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P2 (at 0 5.1) (layer B.SilkS) hide)
    (fp_text value CONN_01X12 (at 0 3.1) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 VCC))
    (pad 2 thru_hole oval (at 0 -2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 13 TXO))
    (pad 3 thru_hole oval (at 0 -5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 4 thru_hole oval (at 0 -7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 RXI))
    (pad 5 thru_hole oval (at 0 -10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 14 SCL))
    (pad 6 thru_hole oval (at 0 -12.7) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 RST))
    (pad 7 thru_hole oval (at 0 -15.24) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 15 SDA))
    (pad 8 thru_hole oval (at 0 -17.78) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 16 BTN1))
    (pad 9 thru_hole oval (at 0 -20.32) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 17 RGB3))
    (pad 10 thru_hole oval (at 0 -22.86) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 18 BTN2))
    (pad 11 thru_hole oval (at 0 -25.4) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 RGB2))
    (pad 12 thru_hole oval (at 0 -27.94) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 RGB1))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x12.wrl
      (at (xyz 0 -0.55 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x04 (layer F.Cu) (tedit 58418D76)
    (at 121.666 77.119)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P4 (at 0 -5.1) (layer F.SilkS) hide)
    (fp_text value CONN_OLED_SCREEN (at -25.146 -1.778) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 VCC))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 14 SCL))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 15 SDA))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x04.wrl
      (at (xyz 0.15 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Buttons_Switches_ThroughHole:SW_PUSH_6mm (layer F.Cu) (tedit 58447B51)
    (at 131.572 115.824)
    (descr https://www.omron.com/ecb/products/pdf/en-b3f.pdf)
    (tags "tact sw push 6mm")
    (fp_text reference SW1 (at 3.188 2.246) (layer F.SilkS))
    (fp_text value SW_PUSH (at 3.75 6.7) (layer F.Fab) hide)
    (pad 2 thru_hole circle (at 0 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 16 BTN1))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 VCC))
    (pad 2 thru_hole circle (at 6.5 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 16 BTN1))
    (pad 1 thru_hole circle (at 6.5 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 VCC))
  )
  (module Buttons_Switches_ThroughHole:SW_PUSH_6mm (layer F.Cu) (tedit 58447B4C)
    (at 112.522 115.824)
    (descr https://www.omron.com/ecb/products/pdf/en-b3f.pdf)
    (tags "tact sw push 6mm")
    (fp_text reference SW2 (at 3.188 2.286) (layer F.SilkS))
    (fp_text value SW_PUSH (at 3.75 6.7) (layer F.Fab) hide)
    (pad 2 thru_hole circle (at 0 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 18 BTN2))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 VCC))
    (pad 2 thru_hole circle (at 6.5 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 18 BTN2))
    (pad 1 thru_hole circle (at 6.5 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 VCC))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 58418B4E)
    (at 113.5 110.5)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 58418B48)
    (at 137.127 101.554)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2 (at 0 3.2) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module libs:calaos_logo_small (layer F.Cu) (tedit 0)
    (at 125.23 91.97)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module libs:calaos_logo_single (layer F.Cu) (tedit 0)
    (at 125.51 110.73)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (gr_arc (start 127.762 122) (end 127.762 120.984) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 127.762 120.984) (end 123.19 120.984) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 123.19 122) (end 122.174 122) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 141.5 122) (end 128.778 122) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 128.778 64) (end 141.5 64) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 123.19 65.024) (end 127.762 65.024) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 123.19 64.008) (end 123.19 65.024) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 127.762 64.008) (end 128.778 64.008) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text GND (at 121.65 73.91 270) (layer B.SilkS))
  (gr_text VCC (at 124.19 73.9 270) (layer B.SilkS))
  (gr_text SCL (at 126.74 74.05 270) (layer B.SilkS))
  (gr_text SDA (at 129.28 74.02 270) (layer B.SilkS))
  (gr_text VCC (at 130.29 106.53) (layer B.SilkS))
  (gr_text TXO (at 130.34 103.98) (layer B.SilkS))
  (gr_text GND (at 130.3 101.41) (layer B.SilkS))
  (gr_text RXI (at 130.66 98.89) (layer B.SilkS))
  (gr_text SCL (at 130.44 96.34) (layer B.SilkS))
  (gr_text RST (at 130.52 93.81) (layer B.SilkS))
  (gr_text SDA (at 130.4 91.26) (layer B.SilkS))
  (gr_text BTN1 (at 129.97 88.73) (layer B.SilkS))
  (gr_text RGB3 (at 129.89 86.18) (layer B.SilkS))
  (gr_text BTN2 (at 129.97 83.62) (layer B.SilkS))
  (gr_text RGB2 (at 129.89 81.1) (layer B.SilkS))
  (gr_text RGB1 (at 129.92 78.56) (layer B.SilkS))
  (gr_text "Gateway v1.0" (at 120.84 112.74) (layer F.SilkS))
  (gr_line (start 109.5 122) (end 109.5 64) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 122.174 122) (end 109.5 122) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 141.5 64) (end 141.5 122) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 109.5 64) (end 122.174 64) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 3) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 141.224 120.7135) (xy 109.728 120.7135) (xy 109.728 65.278) (xy 141.224 65.278)
      )
    )
  )
  (zone (net 3) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 141.224 120.7135) (xy 109.728 120.7135) (xy 109.728 65.278) (xy 141.224 65.278)
      )
    )
  )
)
