(kicad_pcb (version 20171130) (host pcbnew "(5.1.8)-1")
  (general
    (thickness 1.6002)
    (drawings 239)
    (tracks 1314)
    (zones 0)
    (modules 34)
    (nets 135)
  )
  (page User 279.4 215.9)
  (title_block
    (title "ISA 8-Bit Ethernet Controller")
    (date 2021-04-22)
    (rev 1.0)
    (company "Designed by Sergey Kiselev")
    (comment 2 "Licensed under CERN-OHL-S: https://cern-ohl.web.cern.ch")
    (comment 3 "Documentation and design files: https://github.com/skiselev/isa8_eth")
    (comment 4 "ISA 8-Bit Ethernet Controller is an open source hardware project")
  )
  (layers
    (0 Front signal)
    (31 Back signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
  )
  (setup
    (last_trace_width 1.016)
    (user_trace_width 0.254)
    (user_trace_width 0.762)
    (user_trace_width 1.016)
    (user_trace_width 1.524)
    (trace_clearance 0.2)
    (zone_clearance 0.3556)
    (zone_45_only yes)
    (trace_min 0.2032)
    (via_size 0.889)
    (via_drill 0.635)
    (via_min_size 0.889)
    (via_min_drill 0.508)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (edge_width 0.381)
    (segment_width 0.254)
    (pcb_text_width 0.3048)
    (pcb_text_size 1.524 2.032)
    (mod_edge_width 0.254)
    (mod_text_size 1.524 1.524)
    (mod_text_width 0.3048)
    (pad_size 1.778 8.128)
    (pad_drill 0)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFF7FF)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions true)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerber"))
  )
  (net 0 "")
  (net 1 /A0)
  (net 2 /A1)
  (net 3 /A10)
  (net 4 /A11)
  (net 5 /A12)
  (net 6 /A13)
  (net 7 /A14)
  (net 8 /A15)
  (net 9 /A16)
  (net 10 /A17)
  (net 11 /A18)
  (net 12 /A19)
  (net 13 /A2)
  (net 14 /A3)
  (net 15 /A4)
  (net 16 /A5)
  (net 17 /A6)
  (net 18 /A7)
  (net 19 /A8)
  (net 20 /A9)
  (net 21 /AEN)
  (net 22 /D0)
  (net 23 /D1)
  (net 24 /D2)
  (net 25 /D3)
  (net 26 /D4)
  (net 27 /D5)
  (net 28 /D6)
  (net 29 /D7)
  (net 30 /~IOR)
  (net 31 /~IOW)
  (net 32 GND)
  (net 33 VCC)
  (net 34 /RSTDRV)
  (net 35 /IRQ9)
  (net 36 "Net-(BUS1-Pad5)")
  (net 37 "Net-(BUS1-Pad6)")
  (net 38 "Net-(BUS1-Pad7)")
  (net 39 "Net-(BUS1-Pad8)")
  (net 40 "Net-(BUS1-Pad9)")
  (net 41 /~SMEMW)
  (net 42 /~SMEMR)
  (net 43 "Net-(BUS1-Pad15)")
  (net 44 "Net-(BUS1-Pad16)")
  (net 45 "Net-(BUS1-Pad17)")
  (net 46 "Net-(BUS1-Pad18)")
  (net 47 "Net-(BUS1-Pad19)")
  (net 48 "Net-(BUS1-Pad20)")
  (net 49 "Net-(BUS1-Pad21)")
  (net 50 "Net-(BUS1-Pad22)")
  (net 51 /IRQ5)
  (net 52 /IRQ4)
  (net 53 /IRQ3)
  (net 54 "Net-(BUS1-Pad26)")
  (net 55 "Net-(BUS1-Pad27)")
  (net 56 "Net-(BUS1-Pad28)")
  (net 57 "Net-(BUS1-Pad30)")
  (net 58 "Net-(BUS1-Pad32)")
  (net 59 /IOCHRDY)
  (net 60 /~IOCS16)
  (net 61 "Net-(C1-Pad2)")
  (net 62 "Net-(C2-Pad2)")
  (net 63 "Net-(C3-Pad1)")
  (net 64 "Net-(C4-Pad1)")
  (net 65 /TP_RX-)
  (net 66 /TP_RX+)
  (net 67 /TP_TX-)
  (net 68 /TP_TX+)
  (net 69 /LED_LINK)
  (net 70 /JP)
  (net 71 /BA18)
  (net 72 /BA17)
  (net 73 /BA16)
  (net 74 /BD6)
  (net 75 /BD5)
  (net 76 /BD4)
  (net 77 /BD3)
  (net 78 /BD2)
  (net 79 /BD1)
  (net 80 /BD0)
  (net 81 "Net-(U1-Pad48)")
  (net 82 "Net-(U1-Pad49)")
  (net 83 "Net-(U1-Pad53)")
  (net 84 "Net-(U1-Pad54)")
  (net 85 "Net-(U1-Pad55)")
  (net 86 "Net-(U1-Pad56)")
  (net 87 "Net-(U1-Pad60)")
  (net 88 /BA15)
  (net 89 /BA14)
  (net 90 /~BCS)
  (net 91 /EECS)
  (net 92 /BD7)
  (net 93 "Net-(U3-Pad7)")
  (net 94 /BA19)
  (net 95 /BA20)
  (net 96 /BA21)
  (net 97 /LED_CRS)
  (net 98 "Net-(U1-Pad63)")
  (net 99 "Net-(U1-Pad87)")
  (net 100 "Net-(U1-Pad88)")
  (net 101 "Net-(U1-Pad90)")
  (net 102 "Net-(U1-Pad91)")
  (net 103 "Net-(U1-Pad92)")
  (net 104 "Net-(U1-Pad93)")
  (net 105 "Net-(U1-Pad94)")
  (net 106 "Net-(U1-Pad95)")
  (net 107 "Net-(U1-Pad97)")
  (net 108 "Net-(U1-Pad98)")
  (net 109 "Net-(U1-Pad99)")
  (net 110 "Net-(U1-Pad100)")
  (net 111 "Net-(RN1-Pad7)")
  (net 112 "Net-(RN1-Pad8)")
  (net 113 "Net-(RN1-Pad6)")
  (net 114 "Net-(RN1-Pad5)")
  (net 115 "Net-(RN2-Pad5)")
  (net 116 "Net-(RN2-Pad6)")
  (net 117 "Net-(RN2-Pad8)")
  (net 118 "Net-(RN2-Pad7)")
  (net 119 "Net-(RN3-Pad7)")
  (net 120 "Net-(RN3-Pad8)")
  (net 121 "Net-(RN3-Pad6)")
  (net 122 "Net-(RN3-Pad5)")
  (net 123 "Net-(J1-PadR7)")
  (net 124 "Net-(J1-PadL2)")
  (net 125 "Net-(J1-PadL3)")
  (net 126 "Net-(J2-Pad3)")
  (net 127 "Net-(J2-Pad5)")
  (net 128 "Net-(J2-Pad7)")
  (net 129 "Net-(RN4-Pad3)")
  (net 130 /AUI)
  (net 131 "Net-(RN4-Pad4)")
  (net 132 "Net-(RN4-Pad6)")
  (net 133 "Net-(RN4-Pad5)")
  (net 134 "Net-(RN4-Pad7)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.3683)
    (via_dia 0.889)
    (via_drill 0.635)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (diff_pair_width 0.254)
    (diff_pair_gap 0.254)
    (add_net /A0)
    (add_net /A1)
    (add_net /A10)
    (add_net /A11)
    (add_net /A12)
    (add_net /A13)
    (add_net /A14)
    (add_net /A15)
    (add_net /A16)
    (add_net /A17)
    (add_net /A18)
    (add_net /A19)
    (add_net /A2)
    (add_net /A3)
    (add_net /A4)
    (add_net /A5)
    (add_net /A6)
    (add_net /A7)
    (add_net /A8)
    (add_net /A9)
    (add_net /AEN)
    (add_net /AUI)
    (add_net /BA14)
    (add_net /BA15)
    (add_net /BA16)
    (add_net /BA17)
    (add_net /BA18)
    (add_net /BA19)
    (add_net /BA20)
    (add_net /BA21)
    (add_net /BD0)
    (add_net /BD1)
    (add_net /BD2)
    (add_net /BD3)
    (add_net /BD4)
    (add_net /BD5)
    (add_net /BD6)
    (add_net /BD7)
    (add_net /D0)
    (add_net /D1)
    (add_net /D2)
    (add_net /D3)
    (add_net /D4)
    (add_net /D5)
    (add_net /D6)
    (add_net /D7)
    (add_net /EECS)
    (add_net /IOCHRDY)
    (add_net /IRQ3)
    (add_net /IRQ4)
    (add_net /IRQ5)
    (add_net /IRQ9)
    (add_net /JP)
    (add_net /LED_CRS)
    (add_net /LED_LINK)
    (add_net /RSTDRV)
    (add_net /TP_RX+)
    (add_net /TP_RX-)
    (add_net /TP_TX+)
    (add_net /TP_TX-)
    (add_net /~BCS)
    (add_net /~IOCS16)
    (add_net /~IOR)
    (add_net /~IOW)
    (add_net /~SMEMR)
    (add_net /~SMEMW)
    (add_net GND)
    (add_net "Net-(BUS1-Pad15)")
    (add_net "Net-(BUS1-Pad16)")
    (add_net "Net-(BUS1-Pad17)")
    (add_net "Net-(BUS1-Pad18)")
    (add_net "Net-(BUS1-Pad19)")
    (add_net "Net-(BUS1-Pad20)")
    (add_net "Net-(BUS1-Pad21)")
    (add_net "Net-(BUS1-Pad22)")
    (add_net "Net-(BUS1-Pad26)")
    (add_net "Net-(BUS1-Pad27)")
    (add_net "Net-(BUS1-Pad28)")
    (add_net "Net-(BUS1-Pad30)")
    (add_net "Net-(BUS1-Pad32)")
    (add_net "Net-(BUS1-Pad5)")
    (add_net "Net-(BUS1-Pad6)")
    (add_net "Net-(BUS1-Pad7)")
    (add_net "Net-(BUS1-Pad8)")
    (add_net "Net-(BUS1-Pad9)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(J1-PadL2)")
    (add_net "Net-(J1-PadL3)")
    (add_net "Net-(J1-PadR7)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad5)")
    (add_net "Net-(J2-Pad7)")
    (add_net "Net-(RN1-Pad5)")
    (add_net "Net-(RN1-Pad6)")
    (add_net "Net-(RN1-Pad7)")
    (add_net "Net-(RN1-Pad8)")
    (add_net "Net-(RN2-Pad5)")
    (add_net "Net-(RN2-Pad6)")
    (add_net "Net-(RN2-Pad7)")
    (add_net "Net-(RN2-Pad8)")
    (add_net "Net-(RN3-Pad5)")
    (add_net "Net-(RN3-Pad6)")
    (add_net "Net-(RN3-Pad7)")
    (add_net "Net-(RN3-Pad8)")
    (add_net "Net-(RN4-Pad3)")
    (add_net "Net-(RN4-Pad4)")
    (add_net "Net-(RN4-Pad5)")
    (add_net "Net-(RN4-Pad6)")
    (add_net "Net-(RN4-Pad7)")
    (add_net "Net-(U1-Pad100)")
    (add_net "Net-(U1-Pad48)")
    (add_net "Net-(U1-Pad49)")
    (add_net "Net-(U1-Pad53)")
    (add_net "Net-(U1-Pad54)")
    (add_net "Net-(U1-Pad55)")
    (add_net "Net-(U1-Pad56)")
    (add_net "Net-(U1-Pad60)")
    (add_net "Net-(U1-Pad63)")
    (add_net "Net-(U1-Pad87)")
    (add_net "Net-(U1-Pad88)")
    (add_net "Net-(U1-Pad90)")
    (add_net "Net-(U1-Pad91)")
    (add_net "Net-(U1-Pad92)")
    (add_net "Net-(U1-Pad93)")
    (add_net "Net-(U1-Pad94)")
    (add_net "Net-(U1-Pad95)")
    (add_net "Net-(U1-Pad97)")
    (add_net "Net-(U1-Pad98)")
    (add_net "Net-(U1-Pad99)")
    (add_net "Net-(U3-Pad7)")
    (add_net VCC)
  )
  (net_class Power ""
    (clearance 0.254)
    (trace_width 0.63246)
    (via_dia 0.889)
    (via_drill 0.635)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (diff_pair_width 0.254)
    (diff_pair_gap 0.254)
  )
  (module My_Components:Conn_Pin_Header_20x2_2.54mm (layer Front) (tedit 60824E6D)
    (at 106.68 88.9 270)
    (descr "Pin Header, 20x2, 2.54mm pitch")
    (tags "CONN PIN HEADER 20x2")
    (fp_text reference J2 (at 4.445 -3.81 90) (layer F.SilkS))
    (fp_text value MEM_EXT (at -1.5875 -3.81 90) (layer F.SilkS))
    (pad 40 thru_hole circle (at 24.13 -1.27 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 32 GND))
    (pad 39 thru_hole circle (at 24.13 1.27 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 32 GND))
    (pad 38 thru_hole circle (at 21.59 -1.27 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 77 /BD3))
    (pad 37 thru_hole circle (at 21.59 1.27 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 78 /BD2))
    (pad 36 thru_hole circle (at 19.05 -1.27 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 76 /BD4))
    (pad 35 thru_hole circle (at 19.05 1.27 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 79 /BD1))
    (pad 34 thru_hole circle (at 16.51 -1.27 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 75 /BD5))
    (pad 33 thru_hole circle (at 16.51 1.27 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 80 /BD0))
    (pad 32 thru_hole circle (at 13.97 -1.27 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 74 /BD6))
    (pad 31 thru_hole circle (at 13.97 1.27 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 /A0))
    (pad 29 thru_hole circle (at 11.43 1.27 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 /A1))
    (pad 30 thru_hole circle (at 11.43 -1.27 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 92 /BD7))
    (pad 27 thru_hole circle (at 8.89 1.27 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 13 /A2))
    (pad 28 thru_hole circle (at 8.89 -1.27 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 90 /~BCS))
    (pad 26 thru_hole circle (at 6.35 -1.27 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 /A10))
    (pad 25 thru_hole circle (at 6.35 1.27 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 14 /A3))
    (pad 24 thru_hole circle (at 3.81 -1.27 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 42 /~SMEMR))
    (pad 23 thru_hole circle (at 3.81 1.27 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 15 /A4))
    (pad 22 thru_hole circle (at 1.27 -1.27 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 /A11))
    (pad 21 thru_hole circle (at 1.27 1.27 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 16 /A5))
    (pad 20 thru_hole circle (at -1.27 -1.27 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 /A9))
    (pad 19 thru_hole circle (at -1.27 1.27 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 17 /A6))
    (pad 18 thru_hole circle (at -3.81 -1.27 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 /A8))
    (pad 17 thru_hole circle (at -3.81 1.27 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 18 /A7))
    (pad 16 thru_hole circle (at -6.35 -1.27 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 /A13))
    (pad 15 thru_hole circle (at -6.35 1.27 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 /A12))
    (pad 14 thru_hole circle (at -8.89 -1.27 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 89 /BA14))
    (pad 13 thru_hole circle (at -8.89 1.27 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 88 /BA15))
    (pad 12 thru_hole circle (at -11.43 -1.27 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 72 /BA17))
    (pad 11 thru_hole circle (at -11.43 1.27 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 73 /BA16))
    (pad 10 thru_hole circle (at -13.97 -1.27 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 41 /~SMEMW))
    (pad 9 thru_hole circle (at -13.97 1.27 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 71 /BA18))
    (pad 8 thru_hole circle (at -16.51 -1.27 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 94 /BA19))
    (pad 7 thru_hole circle (at -16.51 1.27 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 128 "Net-(J2-Pad7)"))
    (pad 6 thru_hole circle (at -19.05 -1.27 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 95 /BA20))
    (pad 5 thru_hole circle (at -19.05 1.27 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 127 "Net-(J2-Pad5)"))
    (pad 4 thru_hole circle (at -21.59 -1.27 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 96 /BA21))
    (pad 3 thru_hole circle (at -21.59 1.27 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 126 "Net-(J2-Pad3)"))
    (pad 2 thru_hole circle (at -24.13 -1.27 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 33 VCC))
    (pad 1 thru_hole rect (at -24.13 1.27 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 33 VCC))
    (model pin_array/pins_array_13x2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Conn_Edge_PCB_ISA8 (layer Front) (tedit 608C86FB)
    (at 142.24 130.4925)
    (descr "Connector, PCB Edge, ISA8")
    (tags "CONN BUS ISA")
    (fp_text reference BUS1 (at -36.83 -6.35) (layer F.SilkS) hide)
    (fp_text value BUSPC_DEV (at -29.21 -6.35) (layer F.SilkS) hide)
    (pad 1 connect roundrect (at 38.1 0) (size 1.778 8.128) (layers Back B.Mask) (roundrect_rratio 0.25)
      (net 32 GND))
    (pad 2 connect roundrect (at 35.56 0) (size 1.778 8.128) (layers Back B.Mask) (roundrect_rratio 0.25)
      (net 34 /RSTDRV))
    (pad 3 connect roundrect (at 33.02 0) (size 1.778 8.128) (layers Back B.Mask) (roundrect_rratio 0.25)
      (net 33 VCC))
    (pad 4 connect roundrect (at 30.48 0) (size 1.778 8.128) (layers Back B.Mask) (roundrect_rratio 0.25)
      (net 35 /IRQ9))
    (pad 5 connect roundrect (at 27.94 0) (size 1.778 8.128) (layers Back B.Mask) (roundrect_rratio 0.25)
      (net 36 "Net-(BUS1-Pad5)"))
    (pad 6 connect roundrect (at 25.4 0) (size 1.778 8.128) (layers Back B.Mask) (roundrect_rratio 0.25)
      (net 37 "Net-(BUS1-Pad6)"))
    (pad 7 connect roundrect (at 22.86 0) (size 1.778 8.128) (layers Back B.Mask) (roundrect_rratio 0.25)
      (net 38 "Net-(BUS1-Pad7)"))
    (pad 8 connect roundrect (at 20.32 0) (size 1.778 8.128) (layers Back B.Mask) (roundrect_rratio 0.25)
      (net 39 "Net-(BUS1-Pad8)"))
    (pad 9 connect roundrect (at 17.78 0) (size 1.778 8.128) (layers Back B.Mask) (roundrect_rratio 0.25)
      (net 40 "Net-(BUS1-Pad9)"))
    (pad 10 connect roundrect (at 15.24 0) (size 1.778 8.128) (layers Back B.Mask) (roundrect_rratio 0.25)
      (net 32 GND))
    (pad 11 connect roundrect (at 12.7 0) (size 1.778 8.128) (layers Back B.Mask) (roundrect_rratio 0.25)
      (net 41 /~SMEMW))
    (pad 12 connect roundrect (at 10.16 0) (size 1.778 8.128) (layers Back B.Mask) (roundrect_rratio 0.25)
      (net 42 /~SMEMR))
    (pad 13 connect roundrect (at 7.62 0) (size 1.778 8.128) (layers Back B.Mask) (roundrect_rratio 0.25)
      (net 31 /~IOW))
    (pad 14 connect roundrect (at 5.08 0) (size 1.778 8.128) (layers Back B.Mask) (roundrect_rratio 0.25)
      (net 30 /~IOR))
    (pad 15 connect roundrect (at 2.54 0) (size 1.778 8.128) (layers Back B.Mask) (roundrect_rratio 0.25)
      (net 43 "Net-(BUS1-Pad15)"))
    (pad 16 connect roundrect (at 0 0) (size 1.778 8.128) (layers Back B.Mask) (roundrect_rratio 0.25)
      (net 44 "Net-(BUS1-Pad16)"))
    (pad 17 connect roundrect (at -2.54 0) (size 1.778 8.128) (layers Back B.Mask) (roundrect_rratio 0.25)
      (net 45 "Net-(BUS1-Pad17)"))
    (pad 18 connect roundrect (at -5.08 0) (size 1.778 8.128) (layers Back B.Mask) (roundrect_rratio 0.25)
      (net 46 "Net-(BUS1-Pad18)"))
    (pad 19 connect roundrect (at -7.62 0) (size 1.778 8.128) (layers Back B.Mask) (roundrect_rratio 0.25)
      (net 47 "Net-(BUS1-Pad19)"))
    (pad 20 connect roundrect (at -10.16 0) (size 1.778 8.128) (layers Back B.Mask) (roundrect_rratio 0.25)
      (net 48 "Net-(BUS1-Pad20)"))
    (pad 21 connect roundrect (at -12.7 0) (size 1.778 8.128) (layers Back B.Mask) (roundrect_rratio 0.25)
      (net 49 "Net-(BUS1-Pad21)"))
    (pad 22 connect roundrect (at -15.24 0) (size 1.778 8.128) (layers Back B.Mask) (roundrect_rratio 0.25)
      (net 50 "Net-(BUS1-Pad22)"))
    (pad 23 connect roundrect (at -17.78 0) (size 1.778 8.128) (layers Back B.Mask) (roundrect_rratio 0.25)
      (net 51 /IRQ5))
    (pad 24 connect roundrect (at -20.32 0) (size 1.778 8.128) (layers Back B.Mask) (roundrect_rratio 0.25)
      (net 52 /IRQ4))
    (pad 25 connect roundrect (at -22.86 0) (size 1.778 8.128) (layers Back B.Mask) (roundrect_rratio 0.25)
      (net 53 /IRQ3))
    (pad 26 connect roundrect (at -25.4 0) (size 1.778 8.128) (layers Back B.Mask) (roundrect_rratio 0.25)
      (net 54 "Net-(BUS1-Pad26)"))
    (pad 27 connect roundrect (at -27.94 0) (size 1.778 8.128) (layers Back B.Mask) (roundrect_rratio 0.25)
      (net 55 "Net-(BUS1-Pad27)"))
    (pad 28 connect roundrect (at -30.48 0) (size 1.778 8.128) (layers Back B.Mask) (roundrect_rratio 0.25)
      (net 56 "Net-(BUS1-Pad28)"))
    (pad 29 connect roundrect (at -33.02 0) (size 1.778 8.128) (layers Back B.Mask) (roundrect_rratio 0.25)
      (net 33 VCC))
    (pad 30 connect roundrect (at -35.56 0) (size 1.778 8.128) (layers Back B.Mask) (roundrect_rratio 0.25)
      (net 57 "Net-(BUS1-Pad30)"))
    (pad 31 connect roundrect (at -38.1 0) (size 1.778 8.128) (layers Back B.Mask) (roundrect_rratio 0.25)
      (net 32 GND))
    (pad 32 connect roundrect (at 38.1 0) (size 1.778 8.128) (layers Front F.Mask) (roundrect_rratio 0.25)
      (net 58 "Net-(BUS1-Pad32)"))
    (pad 33 connect roundrect (at 35.56 0) (size 1.778 8.128) (layers Front F.Mask) (roundrect_rratio 0.25)
      (net 29 /D7))
    (pad 34 connect roundrect (at 33.02 0) (size 1.778 8.128) (layers Front F.Mask) (roundrect_rratio 0.25)
      (net 28 /D6))
    (pad 35 connect roundrect (at 30.48 0) (size 1.778 8.128) (layers Front F.Mask) (roundrect_rratio 0.25)
      (net 27 /D5))
    (pad 36 connect roundrect (at 27.94 0) (size 1.778 8.128) (layers Front F.Mask) (roundrect_rratio 0.25)
      (net 26 /D4))
    (pad 37 connect roundrect (at 25.4 0) (size 1.778 8.128) (layers Front F.Mask) (roundrect_rratio 0.25)
      (net 25 /D3))
    (pad 38 connect roundrect (at 22.86 0) (size 1.778 8.128) (layers Front F.Mask) (roundrect_rratio 0.25)
      (net 24 /D2))
    (pad 39 connect roundrect (at 20.32 0) (size 1.778 8.128) (layers Front F.Mask) (roundrect_rratio 0.25)
      (net 23 /D1))
    (pad 40 connect roundrect (at 17.78 0) (size 1.778 8.128) (layers Front F.Mask) (roundrect_rratio 0.25)
      (net 22 /D0))
    (pad 41 connect roundrect (at 15.24 0) (size 1.778 8.128) (layers Front F.Mask) (roundrect_rratio 0.25)
      (net 59 /IOCHRDY))
    (pad 42 connect roundrect (at 12.7 0) (size 1.778 8.128) (layers Front F.Mask) (roundrect_rratio 0.25)
      (net 21 /AEN))
    (pad 43 connect roundrect (at 10.16 0) (size 1.778 8.128) (layers Front F.Mask) (roundrect_rratio 0.25)
      (net 12 /A19))
    (pad 44 connect roundrect (at 7.62 0) (size 1.778 8.128) (layers Front F.Mask) (roundrect_rratio 0.25)
      (net 11 /A18))
    (pad 45 connect roundrect (at 5.08 0) (size 1.778 8.128) (layers Front F.Mask) (roundrect_rratio 0.25)
      (net 10 /A17))
    (pad 46 connect roundrect (at 2.54 0) (size 1.778 8.128) (layers Front F.Mask) (roundrect_rratio 0.25)
      (net 9 /A16))
    (pad 47 connect roundrect (at 0 0) (size 1.778 8.128) (layers Front F.Mask) (roundrect_rratio 0.25)
      (net 8 /A15))
    (pad 48 connect roundrect (at -2.54 0) (size 1.778 8.128) (layers Front F.Mask) (roundrect_rratio 0.25)
      (net 7 /A14))
    (pad 49 connect roundrect (at -5.08 0) (size 1.778 8.128) (layers Front F.Mask) (roundrect_rratio 0.25)
      (net 6 /A13))
    (pad 50 connect roundrect (at -7.62 0) (size 1.778 8.128) (layers Front F.Mask) (roundrect_rratio 0.25)
      (net 5 /A12))
    (pad 51 connect roundrect (at -10.16 0) (size 1.778 8.128) (layers Front F.Mask) (roundrect_rratio 0.25)
      (net 4 /A11))
    (pad 52 connect roundrect (at -12.7 0) (size 1.778 8.128) (layers Front F.Mask) (roundrect_rratio 0.25)
      (net 3 /A10))
    (pad 53 connect roundrect (at -15.24 0) (size 1.778 8.128) (layers Front F.Mask) (roundrect_rratio 0.25)
      (net 20 /A9))
    (pad 54 connect roundrect (at -17.78 0) (size 1.778 8.128) (layers Front F.Mask) (roundrect_rratio 0.25)
      (net 19 /A8))
    (pad 55 connect roundrect (at -20.32 0) (size 1.778 8.128) (layers Front F.Mask) (roundrect_rratio 0.25)
      (net 18 /A7))
    (pad 56 connect roundrect (at -22.86 0) (size 1.778 8.128) (layers Front F.Mask) (roundrect_rratio 0.25)
      (net 17 /A6))
    (pad 57 connect roundrect (at -25.4 0) (size 1.778 8.128) (layers Front F.Mask) (roundrect_rratio 0.25)
      (net 16 /A5))
    (pad 58 connect roundrect (at -27.94 0) (size 1.778 8.128) (layers Front F.Mask) (roundrect_rratio 0.25)
      (net 15 /A4))
    (pad 59 connect roundrect (at -30.48 0) (size 1.778 8.128) (layers Front F.Mask) (roundrect_rratio 0.25)
      (net 14 /A3))
    (pad 60 connect roundrect (at -33.02 0) (size 1.778 8.128) (layers Front F.Mask) (roundrect_rratio 0.25)
      (net 13 /A2))
    (pad 61 connect roundrect (at -35.56 0) (size 1.778 8.128) (layers Front F.Mask) (roundrect_rratio 0.25)
      (net 2 /A1))
    (pad 62 connect roundrect (at -38.1 0) (size 1.778 8.128) (layers Front F.Mask) (roundrect_rratio 0.25)
      (net 1 /A0))
  )
  (module My_Components:Switch_DIP_5_Positions (layer Front) (tedit 608256AF)
    (at 176.53 66.04)
    (descr "DIP Switch, 5 Positions")
    (tags "SWITCH DIP 5POS")
    (fp_text reference SW4 (at -8.5725 3.4925 90) (layer F.SilkS))
    (fp_text value ROM_ADDR (at -8.5725 -2.2225 90) (layer F.SilkS))
    (pad 10 thru_hole circle (at -5.08 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 33 VCC))
    (pad 9 thru_hole circle (at -2.54 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 33 VCC))
    (pad 8 thru_hole circle (at 0 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 33 VCC))
    (pad 7 thru_hole circle (at 2.54 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 33 VCC))
    (pad 6 thru_hole circle (at 5.08 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 33 VCC))
    (pad 5 thru_hole circle (at 5.08 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 134 "Net-(RN4-Pad7)"))
    (pad 4 thru_hole circle (at 2.54 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 122 "Net-(RN3-Pad5)"))
    (pad 3 thru_hole circle (at 0 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 121 "Net-(RN3-Pad6)"))
    (pad 2 thru_hole circle (at -2.54 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 119 "Net-(RN3-Pad7)"))
    (pad 1 thru_hole rect (at -5.08 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 120 "Net-(RN3-Pad8)"))
    (model dil/dil_8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Switch_DIP_4_Positions (layer Front) (tedit 60825638)
    (at 160.02 66.04)
    (descr "DIP Switch, 4 Positions")
    (tags "SWITCH DIP 4POS")
    (fp_text reference SW3 (at -7.3025 3.4925 90) (layer F.SilkS))
    (fp_text value IO_ADDR (at -7.3025 -2.2225 90) (layer F.SilkS))
    (pad 8 thru_hole circle (at -3.81 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 33 VCC))
    (pad 7 thru_hole circle (at -1.27 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 33 VCC))
    (pad 6 thru_hole circle (at 1.27 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 33 VCC))
    (pad 5 thru_hole circle (at 3.81 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 33 VCC))
    (pad 4 thru_hole circle (at 3.81 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 115 "Net-(RN2-Pad5)"))
    (pad 3 thru_hole circle (at 1.27 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 116 "Net-(RN2-Pad6)"))
    (pad 2 thru_hole circle (at -1.27 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 118 "Net-(RN2-Pad7)"))
    (pad 1 thru_hole rect (at -3.81 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 117 "Net-(RN2-Pad8)"))
    (model dil/dil_8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Switch_DIP_2_Positions (layer Front) (tedit 6082553E)
    (at 147.32 66.04)
    (descr "DIP Switch, 2 Positions")
    (tags "SWITCH DIP 2POS")
    (fp_text reference SW2 (at -4.7625 3.4925 90) (layer F.SilkS))
    (fp_text value IRQ (at -4.7625 -2.2225 90) (layer F.SilkS))
    (pad 4 thru_hole circle (at -1.27 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 33 VCC))
    (pad 3 thru_hole circle (at 1.27 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 33 VCC))
    (pad 2 thru_hole circle (at 1.27 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 114 "Net-(RN1-Pad5)"))
    (pad 1 thru_hole rect (at -1.27 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 113 "Net-(RN1-Pad6)"))
    (model dil/dil_8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Switch_DIP_2_Positions (layer Front) (tedit 6082553E)
    (at 137.16 66.04)
    (descr "DIP Switch, 2 Positions")
    (tags "SWITCH DIP 2POS")
    (fp_text reference SW1 (at -4.7625 3.4925 90) (layer F.SilkS))
    (fp_text value CONFIG (at -4.7625 -2.2225 90) (layer F.SilkS))
    (pad 4 thru_hole circle (at -1.27 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 33 VCC))
    (pad 3 thru_hole circle (at 1.27 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 33 VCC))
    (pad 2 thru_hole circle (at 1.27 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 111 "Net-(RN1-Pad7)"))
    (pad 1 thru_hole rect (at -1.27 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 112 "Net-(RN1-Pad8)"))
    (model dil/dil_8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Crystal_HC-49U_Vert (layer Front) (tedit 60825482)
    (at 177.8 86.36 90)
    (descr "Quartz Crystal, HC-49U, Vertical")
    (tags "QUARTZ CRYSTAL HC49U VERT")
    (autoplace_cost180 10)
    (fp_text reference Y1 (at -2.54 3.4925 90) (layer F.SilkS))
    (fp_text value 20MHz (at 1.5875 3.4925 90) (layer F.SilkS))
    (pad 2 thru_hole circle (at 2.44094 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 62 "Net-(C2-Pad2)"))
    (pad 1 thru_hole circle (at -2.44094 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 61 "Net-(C1-Pad2)"))
    (model discret/crystal_hc18u_vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Socket_DIP32_600 (layer Front) (tedit 603D251C)
    (at 121.92 91.44 270)
    (descr "32 pins DIL package, round pads")
    (tags "DIP DIL DIP32 DIL32")
    (fp_text reference U2 (at -21.2725 7.9375 180) (layer F.SilkS))
    (fp_text value SST39SF040 (at 21.2725 3.81 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at -19.05 7.62 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 71 /BA18))
    (pad 2 thru_hole circle (at -16.51 7.62 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 73 /BA16))
    (pad 3 thru_hole circle (at -13.97 7.62 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 88 /BA15))
    (pad 4 thru_hole circle (at -11.43 7.62 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 5 /A12))
    (pad 5 thru_hole circle (at -8.89 7.62 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 18 /A7))
    (pad 6 thru_hole circle (at -6.35 7.62 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 17 /A6))
    (pad 7 thru_hole circle (at -3.81 7.62 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 16 /A5))
    (pad 8 thru_hole circle (at -1.27 7.62 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 15 /A4))
    (pad 9 thru_hole circle (at 1.27 7.62 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 14 /A3))
    (pad 10 thru_hole circle (at 3.81 7.62 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 13 /A2))
    (pad 11 thru_hole circle (at 6.35 7.62 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 2 /A1))
    (pad 12 thru_hole circle (at 8.89 7.62 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 /A0))
    (pad 13 thru_hole circle (at 11.43 7.62 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 80 /BD0))
    (pad 14 thru_hole circle (at 13.97 7.62 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 79 /BD1))
    (pad 15 thru_hole circle (at 16.51 7.62 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 78 /BD2))
    (pad 16 thru_hole circle (at 19.05 7.62 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 32 GND))
    (pad 17 thru_hole circle (at 19.05 -7.62 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 77 /BD3))
    (pad 18 thru_hole circle (at 16.51 -7.62 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 76 /BD4))
    (pad 19 thru_hole circle (at 13.97 -7.62 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 75 /BD5))
    (pad 20 thru_hole circle (at 11.43 -7.62 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 74 /BD6))
    (pad 21 thru_hole circle (at 8.89 -7.62 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 92 /BD7))
    (pad 22 thru_hole circle (at 6.35 -7.62 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 90 /~BCS))
    (pad 23 thru_hole circle (at 3.81 -7.62 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 3 /A10))
    (pad 24 thru_hole circle (at 1.27 -7.62 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 42 /~SMEMR))
    (pad 25 thru_hole circle (at -1.27 -7.62 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 4 /A11))
    (pad 26 thru_hole circle (at -3.81 -7.62 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 20 /A9))
    (pad 27 thru_hole circle (at -6.35 -7.62 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 19 /A8))
    (pad 28 thru_hole circle (at -8.89 -7.62 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 6 /A13))
    (pad 29 thru_hole circle (at -11.43 -7.62 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 89 /BA14))
    (pad 30 thru_hole circle (at -13.97 -7.62 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 72 /BA17))
    (pad 31 thru_hole circle (at -16.51 -7.62 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 41 /~SMEMW))
    (pad 32 thru_hole circle (at -19.05 -7.62 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 33 VCC))
    (model dil/dil_32-w600.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Symbol:OSHW-Logo_5.7x6mm_SilkScreen (layer Front) (tedit 0)
    (at 175.5775 110.49)
    (descr "Open Source Hardware Logo")
    (tags "Logo OSHW")
    (attr virtual)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value OSHW-Logo_5.7x6mm_SilkScreen (at 0.75 0) (layer F.Fab) hide)
  )
  (module Symbol:KiCad-Logo2_5mm_SilkScreen (layer Front) (tedit 0)
    (at 191.77 117.475)
    (descr "KiCad Logo")
    (tags "Logo KiCad")
    (attr virtual)
    (fp_text reference REF** (at 0 -5.08) (layer F.SilkS) hide)
    (fp_text value KiCad-Logo2_5mm_SilkScreen (at 0 5.08) (layer F.Fab) hide)
  )
  (module Resistor_SMD:R_Array_Convex_4x0603 (layer Front) (tedit 58E0A8B2)
    (at 149.86 74.93 90)
    (descr "Chip Resistor Network, ROHM MNR14 (see mnr_g.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RN2 (at 0 -2.54 90) (layer F.SilkS))
    (fp_text value 10k (at 0 2.54 90) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 5 smd rect (at 0.9 1.2 90) (size 0.8 0.5) (layers Front F.Paste F.Mask)
      (net 115 "Net-(RN2-Pad5)"))
    (pad 6 smd rect (at 0.9 0.4 90) (size 0.8 0.4) (layers Front F.Paste F.Mask)
      (net 116 "Net-(RN2-Pad6)"))
    (pad 8 smd rect (at 0.9 -1.2 90) (size 0.8 0.5) (layers Front F.Paste F.Mask)
      (net 117 "Net-(RN2-Pad8)"))
    (pad 7 smd rect (at 0.9 -0.4 90) (size 0.8 0.4) (layers Front F.Paste F.Mask)
      (net 118 "Net-(RN2-Pad7)"))
    (pad 4 smd rect (at -0.9 1.2 90) (size 0.8 0.5) (layers Front F.Paste F.Mask)
      (net 80 /BD0))
    (pad 2 smd rect (at -0.9 -0.4 90) (size 0.8 0.4) (layers Front F.Paste F.Mask)
      (net 78 /BD2))
    (pad 3 smd rect (at -0.9 0.4 90) (size 0.8 0.4) (layers Front F.Paste F.Mask)
      (net 79 /BD1))
    (pad 1 smd rect (at -0.9 -1.2 90) (size 0.8 0.5) (layers Front F.Paste F.Mask)
      (net 77 /BD3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Convex_4x0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_3.2mm_M3_Pad_Via (layer Front) (tedit 56DDBCCA)
    (at 201.041 66.04)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference HOLE1 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 32 GND))
    (pad 1 thru_hole circle (at 2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 32 GND))
    (pad 1 thru_hole circle (at 1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 32 GND))
    (pad 1 thru_hole circle (at 0 2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 32 GND))
    (pad 1 thru_hole circle (at -1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 32 GND))
    (pad 1 thru_hole circle (at -2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 32 GND))
    (pad 1 thru_hole circle (at -1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 32 GND))
    (pad 1 thru_hole circle (at 0 -2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 32 GND))
    (pad 1 thru_hole circle (at 1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 32 GND))
  )
  (module MountingHole:MountingHole_3.2mm_M3_Pad_Via (layer Front) (tedit 56DDBCCA)
    (at 201.041 122.555)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference HOLE2 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 32 GND))
    (pad 1 thru_hole circle (at 0 -2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 32 GND))
    (pad 1 thru_hole circle (at -1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 32 GND))
    (pad 1 thru_hole circle (at -2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 32 GND))
    (pad 1 thru_hole circle (at -1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 32 GND))
    (pad 1 thru_hole circle (at 0 2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 32 GND))
    (pad 1 thru_hole circle (at 1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 32 GND))
    (pad 1 thru_hole circle (at 2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 32 GND))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 32 GND))
  )
  (module Package_SO:SO-8_3.9x4.9mm_P1.27mm (layer Front) (tedit 5D9F72B1)
    (at 134.62 88.9 90)
    (descr "SO, 8 Pin (https://www.nxp.com/docs/en/data-sheet/PCF8523.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SO SO")
    (attr smd)
    (fp_text reference U3 (at -3.81 3.4925 90) (layer F.SilkS))
    (fp_text value 93LC46C (at 1.27 3.4925 90) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -2.575 -1.905 90) (size 1.75 0.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 91 /EECS))
    (pad 2 smd roundrect (at -2.575 -0.635 90) (size 1.75 0.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 75 /BD5))
    (pad 3 smd roundrect (at -2.575 0.635 90) (size 1.75 0.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 74 /BD6))
    (pad 4 smd roundrect (at -2.575 1.905 90) (size 1.75 0.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 92 /BD7))
    (pad 5 smd roundrect (at 2.575 1.905 90) (size 1.75 0.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 GND))
    (pad 6 smd roundrect (at 2.575 0.635 90) (size 1.75 0.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 VCC))
    (pad 7 smd roundrect (at 2.575 -0.635 90) (size 1.75 0.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 93 "Net-(U3-Pad7)"))
    (pad 8 smd roundrect (at 2.575 -1.905 90) (size 1.75 0.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 VCC))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SO-8_3.9x4.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder (layer Front) (tedit 5F68FEEF)
    (at 172.72 90.17 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C1 (at 2.8575 0) (layer F.SilkS))
    (fp_text value 10pF (at 1.27 -1.5875) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.8625 0 180) (size 1.075 0.95) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 61 "Net-(C1-Pad2)"))
    (pad 1 smd roundrect (at -0.8625 0 180) (size 1.075 0.95) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder (layer Front) (tedit 5F68FEEF)
    (at 172.72 82.55 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C2 (at 0.3175 1.27) (layer F.SilkS))
    (fp_text value 10pF (at 0 -1.5875) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.8625 0 180) (size 1.075 0.95) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 GND))
    (pad 2 smd roundrect (at 0.8625 0 180) (size 1.075 0.95) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 62 "Net-(C2-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder (layer Front) (tedit 5F68FEEF)
    (at 181.9275 92.71 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C3 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value 0.01uF (at 0 1.5875 90) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.8625 0 90) (size 1.075 0.95) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 63 "Net-(C3-Pad1)"))
    (pad 2 smd roundrect (at 0.8625 0 90) (size 1.075 0.95) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder (layer Front) (tedit 5F68FEEF)
    (at 190.8175 82.55)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C4 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 0.01uF (at 0 1.5875) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 GND))
    (pad 1 smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 64 "Net-(C4-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder (layer Front) (tedit 5F68FEEF)
    (at 167.64 82.55 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C5 (at 0 1.27) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.905 -1.5875) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.8625 0 180) (size 1.075 0.95) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 GND))
    (pad 1 smd roundrect (at -0.8625 0 180) (size 1.075 0.95) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder (layer Front) (tedit 5F68FEEF)
    (at 142.24 110.49 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C6 (at 0 1.27) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 -1.5875) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.8625 0 180) (size 1.075 0.95) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 VCC))
    (pad 2 smd roundrect (at 0.8625 0 180) (size 1.075 0.95) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder (layer Front) (tedit 5F68FEEF)
    (at 127 69.215 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C7 (at 0 1.27) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 -1.27) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.8625 0 180) (size 1.075 0.95) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 GND))
    (pad 1 smd roundrect (at -0.8625 0 180) (size 1.075 0.95) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder (layer Front) (tedit 5F68FEEF)
    (at 134.62 82.55)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C8 (at 0 -1.27) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.905) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 VCC))
    (pad 2 smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder (layer Front) (tedit 5F68FEEE)
    (at 185.7375 82.55 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 0 1.27) (layer F.SilkS))
    (fp_text value 200 (at 0 -1.5875) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 65 /TP_RX-))
    (pad 1 smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 66 /TP_RX+))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder (layer Front) (tedit 5F68FEEE)
    (at 195.8975 82.55 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R2 (at 0 1.27) (layer F.SilkS))
    (fp_text value 470 (at 0 -1.5875) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 125 "Net-(J1-PadL3)"))
    (pad 2 smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 69 /LED_LINK))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder (layer Front) (tedit 5F68FEEE)
    (at 200.9775 82.55 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R3 (at 0 1.27) (layer F.SilkS))
    (fp_text value 470 (at 0 -1.5875) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 97 /LED_CRS))
    (pad 1 smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 124 "Net-(J1-PadL2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder (layer Front) (tedit 5F68FEEE)
    (at 137.16 102.87)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R6 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 27k (at 0 1.5875) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 GND))
    (pad 2 smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 60 /~IOCS16))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder (layer Front) (tedit 5F68FEEE)
    (at 172.72 86.36 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R7 (at 2.8575 0) (layer F.SilkS))
    (fp_text value 1M (at 0 -1.5875) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 62 "Net-(C2-Pad2)"))
    (pad 1 smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 61 "Net-(C1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_Array_Convex_4x0603 (layer Front) (tedit 58E0A8B2)
    (at 142.24 74.93 90)
    (descr "Chip Resistor Network, ROHM MNR14 (see mnr_g.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RN1 (at 0 -2.54 270) (layer F.SilkS))
    (fp_text value 10k (at 0 2.54 90) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.9 -1.2 90) (size 0.8 0.5) (layers Front F.Paste F.Mask)
      (net 70 /JP))
    (pad 3 smd rect (at -0.9 0.4 90) (size 0.8 0.4) (layers Front F.Paste F.Mask)
      (net 74 /BD6))
    (pad 2 smd rect (at -0.9 -0.4 90) (size 0.8 0.4) (layers Front F.Paste F.Mask)
      (net 96 /BA21))
    (pad 4 smd rect (at -0.9 1.2 90) (size 0.8 0.5) (layers Front F.Paste F.Mask)
      (net 75 /BD5))
    (pad 7 smd rect (at 0.9 -0.4 90) (size 0.8 0.4) (layers Front F.Paste F.Mask)
      (net 111 "Net-(RN1-Pad7)"))
    (pad 8 smd rect (at 0.9 -1.2 90) (size 0.8 0.5) (layers Front F.Paste F.Mask)
      (net 112 "Net-(RN1-Pad8)"))
    (pad 6 smd rect (at 0.9 0.4 90) (size 0.8 0.4) (layers Front F.Paste F.Mask)
      (net 113 "Net-(RN1-Pad6)"))
    (pad 5 smd rect (at 0.9 1.2 90) (size 0.8 0.5) (layers Front F.Paste F.Mask)
      (net 114 "Net-(RN1-Pad5)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Convex_4x0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_Array_Convex_4x0603 (layer Front) (tedit 58E0A8B2)
    (at 165.1 74.93 90)
    (descr "Chip Resistor Network, ROHM MNR14 (see mnr_g.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RN3 (at 0 -2.54 90) (layer F.SilkS))
    (fp_text value 10k (at 0 2.54 90) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.9 -1.2 90) (size 0.8 0.5) (layers Front F.Paste F.Mask)
      (net 95 /BA20))
    (pad 3 smd rect (at -0.9 0.4 90) (size 0.8 0.4) (layers Front F.Paste F.Mask)
      (net 71 /BA18))
    (pad 2 smd rect (at -0.9 -0.4 90) (size 0.8 0.4) (layers Front F.Paste F.Mask)
      (net 94 /BA19))
    (pad 4 smd rect (at -0.9 1.2 90) (size 0.8 0.5) (layers Front F.Paste F.Mask)
      (net 72 /BA17))
    (pad 7 smd rect (at 0.9 -0.4 90) (size 0.8 0.4) (layers Front F.Paste F.Mask)
      (net 119 "Net-(RN3-Pad7)"))
    (pad 8 smd rect (at 0.9 -1.2 90) (size 0.8 0.5) (layers Front F.Paste F.Mask)
      (net 120 "Net-(RN3-Pad8)"))
    (pad 6 smd rect (at 0.9 0.4 90) (size 0.8 0.4) (layers Front F.Paste F.Mask)
      (net 121 "Net-(RN3-Pad6)"))
    (pad 5 smd rect (at 0.9 1.2 90) (size 0.8 0.5) (layers Front F.Paste F.Mask)
      (net 122 "Net-(RN3-Pad5)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Convex_4x0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:IC_PQFP-100_14x20mm_P0.65mm_Hand_Soldering (layer Front) (tedit 605193B2)
    (at 154.94 96.52 90)
    (descr "PQFP, 100 Pin (http://www.microsemi.com/index.php?option=com_docman&task=doc_download&gid=131095), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "PQFP QFP")
    (attr smd)
    (fp_text reference U1 (at -11.43 -7.3025 180) (layer F.SilkS))
    (fp_text value RTL8019AS (at -11.43 4.1275 180) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -9 -9.425 90) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 51 /IRQ5))
    (pad 2 smd roundrect (at -9 -8.775 90) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 52 /IRQ4))
    (pad 3 smd roundrect (at -9 -8.125 90) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 53 /IRQ3))
    (pad 4 smd roundrect (at -9 -7.475 90) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 35 /IRQ9))
    (pad 5 smd roundrect (at -9 -6.85 90) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 /A0))
    (pad 6 smd roundrect (at -9 -6.2 90) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 VCC))
    (pad 7 smd roundrect (at -9 -5.55 90) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 /A1))
    (pad 8 smd roundrect (at -9 -4.9 90) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 /A2))
    (pad 9 smd roundrect (at -9 -4.25 90) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 /A3))
    (pad 10 smd roundrect (at -9 -3.6 90) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 /A4))
    (pad 11 smd roundrect (at -9 -2.95 90) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 /A5))
    (pad 12 smd roundrect (at -9 -2.3 90) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 /A6))
    (pad 13 smd roundrect (at -9 -1.65 90) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 /A7))
    (pad 14 smd roundrect (at -9 -1 90) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 GND))
    (pad 15 smd roundrect (at -9 -0.35 90) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 /A8))
    (pad 16 smd roundrect (at -9 0.3 90) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 /A9))
    (pad 17 smd roundrect (at -9 0.95 90) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 VCC))
    (pad 18 smd roundrect (at -9 1.6 90) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 /A10))
    (pad 19 smd roundrect (at -9 2.25 90) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 /A11))
    (pad 20 smd roundrect (at -9 2.9 90) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /A12))
    (pad 21 smd roundrect (at -9 3.55 90) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 /A13))
    (pad 22 smd roundrect (at -9 4.2 90) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 /A14))
    (pad 23 smd roundrect (at -9 4.85 90) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 /A15))
    (pad 24 smd roundrect (at -9 5.5 90) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 /A16))
    (pad 25 smd roundrect (at -9 6.15 90) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 /A17))
    (pad 26 smd roundrect (at -9 6.8 90) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 /A18))
    (pad 27 smd roundrect (at -9 7.45 90) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 /A19))
    (pad 28 smd roundrect (at -9 8.1 90) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 GND))
    (pad 29 smd roundrect (at -9 8.75 90) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 /~IOR))
    (pad 30 smd roundrect (at -9 9.4 90) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 31 /~IOW))
    (pad 31 smd roundrect (at -6.175 12 180) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 42 /~SMEMR))
    (pad 32 smd roundrect (at -5.525 12 180) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 41 /~SMEMW))
    (pad 33 smd roundrect (at -4.875 12 180) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 34 /RSTDRV))
    (pad 34 smd roundrect (at -4.225 12 180) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 /AEN))
    (pad 35 smd roundrect (at -3.575 12 180) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 59 /IOCHRDY))
    (pad 36 smd roundrect (at -2.925 12 180) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 /D0))
    (pad 37 smd roundrect (at -2.275 12 180) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 /D1))
    (pad 38 smd roundrect (at -1.625 12 180) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 /D2))
    (pad 39 smd roundrect (at -0.975 12 180) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 /D3))
    (pad 40 smd roundrect (at -0.325 12 180) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 /D4))
    (pad 41 smd roundrect (at 0.325 12 180) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 /D5))
    (pad 42 smd roundrect (at 0.975 12 180) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 /D6))
    (pad 43 smd roundrect (at 1.625 12 180) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 /D7))
    (pad 44 smd roundrect (at 2.275 12 180) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 GND))
    (pad 45 smd roundrect (at 2.925 12 180) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 68 /TP_TX+))
    (pad 46 smd roundrect (at 3.575 12 180) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 67 /TP_TX-))
    (pad 47 smd roundrect (at 4.225 12 180) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 VCC))
    (pad 48 smd roundrect (at 4.875 12 180) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 81 "Net-(U1-Pad48)"))
    (pad 49 smd roundrect (at 5.525 12 180) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 82 "Net-(U1-Pad49)"))
    (pad 50 smd roundrect (at 6.175 12 180) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 61 "Net-(C1-Pad2)"))
    (pad 51 smd roundrect (at 9 9.425 90) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 62 "Net-(C2-Pad2)"))
    (pad 52 smd roundrect (at 9 8.775 90) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 GND))
    (pad 53 smd roundrect (at 9 8.125 90) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 83 "Net-(U1-Pad53)"))
    (pad 54 smd roundrect (at 9 7.475 90) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 84 "Net-(U1-Pad54)"))
    (pad 55 smd roundrect (at 9 6.825 90) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 85 "Net-(U1-Pad55)"))
    (pad 56 smd roundrect (at 9 6.175 90) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 86 "Net-(U1-Pad56)"))
    (pad 57 smd roundrect (at 9 5.525 90) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 VCC))
    (pad 58 smd roundrect (at 9 4.875 90) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 65 /TP_RX-))
    (pad 59 smd roundrect (at 9 4.225 90) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 66 /TP_RX+))
    (pad 60 smd roundrect (at 9 3.575 90) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 87 "Net-(U1-Pad60)"))
    (pad 61 smd roundrect (at 9 2.925 90) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 69 /LED_LINK))
    (pad 62 smd roundrect (at 9 2.275 90) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 97 /LED_CRS))
    (pad 63 smd roundrect (at 9 1.625 90) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 98 "Net-(U1-Pad63)"))
    (pad 64 smd roundrect (at 9 0.975 90) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 130 /AUI))
    (pad 65 smd roundrect (at 9 0.325 90) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 70 /JP))
    (pad 66 smd roundrect (at 9 -0.325 90) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 96 /BA21))
    (pad 67 smd roundrect (at 9 -0.975 90) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 95 /BA20))
    (pad 68 smd roundrect (at 9 -1.625 90) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 94 /BA19))
    (pad 69 smd roundrect (at 9 -2.275 90) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 71 /BA18))
    (pad 70 smd roundrect (at 9 -2.925 90) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 VCC))
    (pad 71 smd roundrect (at 9 -3.575 90) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 72 /BA17))
    (pad 72 smd roundrect (at 9 -4.225 90) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 73 /BA16))
    (pad 73 smd roundrect (at 9 -4.875 90) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 88 /BA15))
    (pad 74 smd roundrect (at 9 -5.525 90) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 89 /BA14))
    (pad 75 smd roundrect (at 9 -6.175 90) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 90 /~BCS))
    (pad 76 smd roundrect (at 9 -6.825 90) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 91 /EECS))
    (pad 77 smd roundrect (at 9 -7.475 90) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 92 /BD7))
    (pad 78 smd roundrect (at 9 -8.125 90) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 74 /BD6))
    (pad 79 smd roundrect (at 9 -8.775 90) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 75 /BD5))
    (pad 80 smd roundrect (at 9 -9.425 90) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 76 /BD4))
    (pad 81 smd roundrect (at 6.175 -12 180) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 77 /BD3))
    (pad 82 smd roundrect (at 5.525 -12 180) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 78 /BD2))
    (pad 83 smd roundrect (at 4.875 -12 180) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 GND))
    (pad 84 smd roundrect (at 4.225 -12 180) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 79 /BD1))
    (pad 85 smd roundrect (at 3.575 -12 180) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 80 /BD0))
    (pad 86 smd roundrect (at 2.925 -12 180) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 GND))
    (pad 87 smd roundrect (at 2.275 -12 180) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 99 "Net-(U1-Pad87)"))
    (pad 88 smd roundrect (at 1.625 -12 180) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 100 "Net-(U1-Pad88)"))
    (pad 89 smd roundrect (at 0.975 -12 180) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 VCC))
    (pad 90 smd roundrect (at 0.325 -12 180) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 101 "Net-(U1-Pad90)"))
    (pad 91 smd roundrect (at -0.325 -12 180) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 102 "Net-(U1-Pad91)"))
    (pad 92 smd roundrect (at -0.975 -12 180) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 103 "Net-(U1-Pad92)"))
    (pad 93 smd roundrect (at -1.625 -12 180) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 104 "Net-(U1-Pad93)"))
    (pad 94 smd roundrect (at -2.275 -12 180) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 105 "Net-(U1-Pad94)"))
    (pad 95 smd roundrect (at -2.925 -12 180) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 106 "Net-(U1-Pad95)"))
    (pad 96 smd roundrect (at -3.575 -12 180) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 60 /~IOCS16))
    (pad 97 smd roundrect (at -4.225 -12 180) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 107 "Net-(U1-Pad97)"))
    (pad 98 smd roundrect (at -4.875 -12 180) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 108 "Net-(U1-Pad98)"))
    (pad 99 smd roundrect (at -5.525 -12 180) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 109 "Net-(U1-Pad99)"))
    (pad 100 smd roundrect (at -6.175 -12 180) (size 2.5 0.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 110 "Net-(U1-Pad100)"))
    (model ${KISYS3DMOD}/Package_QFP.3dshapes/PQFP-100_14x20mm_P0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_RJ:RJ45_Amphenol_RJMG1BD3B8K1ANR (layer Front) (tedit 5ADFAE47)
    (at 189.23 99.06 90)
    (descr "1 Port RJ45 Magjack Connector Through Hole 10/100 Base-T, AutoMDIX, https://www.amphenolcanada.com/ProductSearch/Drawings/AC/RJMG1BD3B8K1ANR.PDF")
    (tags "RJ45 Magjack")
    (fp_text reference J1 (at -6.0325 -3.175 180) (layer F.SilkS))
    (fp_text value RJMG1BD3B8K1ANR (at -6.0325 7.62 180) (layer F.SilkS))
    (fp_text user %R (at 4.445 6.37 90) (layer F.Fab))
    (pad R1 thru_hole rect (at 0 0 90) (size 1.9 1.9) (drill 0.9) (layers *.Cu *.Mask)
      (net 68 /TP_TX+))
    (pad R2 thru_hole circle (at 1.27 -2.54 90) (size 1.9 1.9) (drill 0.9) (layers *.Cu *.Mask)
      (net 67 /TP_TX-))
    (pad R3 thru_hole circle (at 2.54 0 90) (size 1.9 1.9) (drill 0.9) (layers *.Cu *.Mask)
      (net 66 /TP_RX+))
    (pad R4 thru_hole circle (at 3.81 -2.54 90) (size 1.9 1.9) (drill 0.9) (layers *.Cu *.Mask)
      (net 63 "Net-(C3-Pad1)"))
    (pad R5 thru_hole circle (at 5.08 0 90) (size 1.9 1.9) (drill 0.9) (layers *.Cu *.Mask)
      (net 64 "Net-(C4-Pad1)"))
    (pad R6 thru_hole circle (at 6.35 -2.54 90) (size 1.9 1.9) (drill 0.9) (layers *.Cu *.Mask)
      (net 65 /TP_RX-))
    (pad R7 thru_hole circle (at 7.62 0 90) (size 1.9 1.9) (drill 0.9) (layers *.Cu *.Mask)
      (net 123 "Net-(J1-PadR7)"))
    (pad R8 thru_hole circle (at 8.89 -2.54 90) (size 1.9 1.9) (drill 0.9) (layers *.Cu *.Mask)
      (net 32 GND))
    (pad L1 thru_hole circle (at 10.77 9.72 90) (size 1.89 1.89) (drill 0.89) (layers *.Cu *.Mask)
      (net 33 VCC))
    (pad L2 thru_hole circle (at 8.23 11.24 90) (size 1.89 1.89) (drill 0.89) (layers *.Cu *.Mask)
      (net 124 "Net-(J1-PadL2)"))
    (pad L3 thru_hole circle (at 0.66 9.72 90) (size 1.89 1.89) (drill 0.89) (layers *.Cu *.Mask)
      (net 125 "Net-(J1-PadL3)"))
    (pad L4 thru_hole circle (at -1.88 11.24 90) (size 1.89 1.89) (drill 0.89) (layers *.Cu *.Mask)
      (net 33 VCC))
    (pad 13 thru_hole circle (at -3.33 3.29 90) (size 2.6 2.6) (drill 1.6) (layers *.Cu *.Mask)
      (net 32 GND))
    (pad 13 thru_hole circle (at 12.22 3.29 90) (size 2.6 2.6) (drill 1.6) (layers *.Cu *.Mask)
      (net 32 GND))
    (pad "" np_thru_hole circle (at -1.27 6.34 90) (size 3.25 3.25) (drill 3.25) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 10.16 6.34 90) (size 3.25 3.25) (drill 3.25) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_RJ.3dshapes/RJ45_Amphenol_RJMG1BD3B8K1ANR.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_Array_Convex_4x0603 (layer Front) (tedit 58E0A8B2)
    (at 157.48 74.93 90)
    (descr "Chip Resistor Network, ROHM MNR14 (see mnr_g.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RN4 (at 0 -2.54 90) (layer F.SilkS))
    (fp_text value 10k (at 0 2.54 90) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.9 -1.2 90) (size 0.8 0.5) (layers Front F.Paste F.Mask)
      (net 130 /AUI))
    (pad 3 smd rect (at -0.9 0.4 90) (size 0.8 0.4) (layers Front F.Paste F.Mask)
      (net 129 "Net-(RN4-Pad3)"))
    (pad 2 smd rect (at -0.9 -0.4 90) (size 0.8 0.4) (layers Front F.Paste F.Mask)
      (net 73 /BA16))
    (pad 4 smd rect (at -0.9 1.2 90) (size 0.8 0.5) (layers Front F.Paste F.Mask)
      (net 131 "Net-(RN4-Pad4)"))
    (pad 7 smd rect (at 0.9 -0.4 90) (size 0.8 0.4) (layers Front F.Paste F.Mask)
      (net 134 "Net-(RN4-Pad7)"))
    (pad 8 smd rect (at 0.9 -1.2 90) (size 0.8 0.5) (layers Front F.Paste F.Mask)
      (net 32 GND))
    (pad 6 smd rect (at 0.9 0.4 90) (size 0.8 0.4) (layers Front F.Paste F.Mask)
      (net 132 "Net-(RN4-Pad6)"))
    (pad 5 smd rect (at 0.9 1.2 90) (size 0.8 0.5) (layers Front F.Paste F.Mask)
      (net 133 "Net-(RN4-Pad5)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Convex_4x0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_Tantalum_SMD:CP_EIA-3528-15_AVX-H_Pad1.50x2.35mm_HandSolder (layer Front) (tedit 5EBA9318)
    (at 165.1 119.0625 180)
    (descr "Tantalum Capacitor SMD AVX-H (3528-15 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (attr smd)
    (fp_text reference C9 (at 0 -2.35) (layer F.SilkS))
    (fp_text value 22uF (at 0 2.35) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.625 0 180) (size 1.5 2.35) (layers Front F.Paste F.Mask) (roundrect_rratio 0.1666666666666667)
      (net 33 VCC))
    (pad 2 smd roundrect (at 1.625 0 180) (size 1.5 2.35) (layers Front F.Paste F.Mask) (roundrect_rratio 0.1666666666666667)
      (net 32 GND))
    (model ${KISYS3DMOD}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-3528-15_AVX-H.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_Tantalum_SMD:CP_EIA-3528-15_AVX-H_Pad1.50x2.35mm_HandSolder (layer Front) (tedit 5EBA9318)
    (at 106.68 119.0625 180)
    (descr "Tantalum Capacitor SMD AVX-H (3528-15 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (attr smd)
    (fp_text reference C10 (at 0 -2.35) (layer F.SilkS))
    (fp_text value 22uF (at 0 2.35) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.625 0 180) (size 1.5 2.35) (layers Front F.Paste F.Mask) (roundrect_rratio 0.1666666666666667)
      (net 32 GND))
    (pad 1 smd roundrect (at -1.625 0 180) (size 1.5 2.35) (layers Front F.Paste F.Mask) (roundrect_rratio 0.1666666666666667)
      (net 33 VCC))
    (model ${KISYS3DMOD}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-3528-15_AVX-H.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Licensed under CERN-OHL-S:\nhttps://cern-ohl.web.cern.ch" (at 179.705 112.395) (layer F.SilkS))
  (gr_text GND (at 108.9025 113.03) (layer B.SilkS))
  (gr_text D3 (at 108.9025 110.49) (layer B.SilkS))
  (gr_text D4 (at 108.9025 107.95) (layer B.SilkS))
  (gr_text D5 (at 108.9025 105.41) (layer B.SilkS))
  (gr_text D6 (at 108.9025 102.87) (layer B.SilkS))
  (gr_text D7 (at 108.9025 100.33) (layer B.SilkS))
  (gr_text GND (at 104.4575 113.03) (layer B.SilkS))
  (gr_text D2 (at 104.4575 110.49) (layer B.SilkS))
  (gr_text D1 (at 104.4575 107.95) (layer B.SilkS))
  (gr_text D0 (at 104.4575 105.41) (layer B.SilkS))
  (gr_text A0 (at 104.4575 102.87) (layer B.SilkS))
  (gr_text A1 (at 104.4575 100.33) (layer B.SilkS))
  (gr_text A2 (at 104.4575 97.79) (layer B.SilkS))
  (gr_text A3 (at 104.4575 95.25) (layer B.SilkS))
  (gr_text A4 (at 104.4575 92.71) (layer B.SilkS))
  (gr_text A5 (at 104.4575 90.17) (layer B.SilkS))
  (gr_text A6 (at 104.4575 87.63) (layer B.SilkS))
  (gr_text A7 (at 104.4575 85.09) (layer B.SilkS))
  (gr_text A12 (at 104.4575 82.55) (layer B.SilkS))
  (gr_text A15 (at 104.4575 80.01) (layer B.SilkS))
  (gr_text ~CS (at 108.9025 97.79) (layer B.SilkS))
  (gr_text A10 (at 108.9025 95.25) (layer B.SilkS))
  (gr_text ~MEMR (at 108.9025 92.71) (layer B.SilkS))
  (gr_text A11 (at 108.9025 90.17) (layer B.SilkS))
  (gr_text A9 (at 108.9025 87.63) (layer B.SilkS))
  (gr_text A8 (at 108.9025 85.09) (layer B.SilkS))
  (gr_text A13 (at 108.9025 82.55) (layer B.SilkS))
  (gr_text A14 (at 108.9025 80.01) (layer B.SilkS))
  (gr_text A17 (at 108.9025 77.47) (layer B.SilkS))
  (gr_text ~MEMW (at 108.9025 74.93) (layer B.SilkS))
  (gr_text A16 (at 104.4575 77.47) (layer B.SilkS))
  (gr_text NC (at 104.4575 67.31) (layer B.SilkS))
  (gr_text NC (at 104.4575 69.85) (layer B.SilkS))
  (gr_text NC (at 104.4575 72.39) (layer B.SilkS))
  (gr_text A19 (at 104.4575 74.93) (layer B.SilkS))
  (gr_text 5V (at 104.4575 64.77) (layer B.SilkS))
  (gr_text 5V (at 108.9025 64.77) (layer B.SilkS))
  (gr_text "Design files and documentation:\ngithub.com/skiselev/isa8_eth" (at 179.705 108.2675) (layer F.SilkS))
  (gr_text "Designed\nin\nOregon" (at 180.467 117.6655) (layer F.SilkS))
  (gr_text "I/O Address\n\n0x300\n0x320\n0x340\n0x360\n0x380\n0x3A0\n0x3C0\n0x3E0" (at 166.6875 79.0575) (layer B.SilkS))
  (gr_text "SW3.4\n\nOFF\nOFF\nOFF\nOFF\nON\nON\nON\nON" (at 141.2875 79.0575) (layer B.SilkS))
  (gr_text "SW3.3\n\nOFF\nOFF\nOFF\nOFF\nOFF\nOFF\nOFF\nOFF" (at 146.3675 79.0575) (layer B.SilkS))
  (gr_text "SW3.1\n\nOFF\nON\nOFF\nON\nOFF\nON\nOFF\nON" (at 156.5275 79.0575) (layer B.SilkS))
  (gr_text "SW3.2\n\nOFF\nOFF\nON\nON\nOFF\nOFF\nON\nON" (at 151.4475 79.0575) (layer B.SilkS))
  (gr_text A21 (at 108.9025 67.31) (layer B.SilkS))
  (gr_text A20 (at 108.9025 69.85) (layer B.SilkS))
  (gr_text A19 (at 108.9025 72.39) (layer B.SilkS))
  (gr_text JLCJLCJLCJLC (at 154.94 96.52) (layer F.SilkS))
  (gr_text "ROM Size\n\n\n16 KiB\n16 KiB\n16 KiB\n16 KiB\n16 KiB\n16 KiB\n16 KiB\n16 KiB\n32 KiB\n32 KiB\n32 KiB\n32 KiB\n64 KiB\n64 KiB" (at 167.64 105.7275) (layer B.SilkS))
  (gr_text "SW4.5\n\nOFF\nON\nON\nON\nON\nON\nON\nON\nON\nOFF\nOFF\nOFF\nOFF\nOFF\nOFF" (at 138.43 105.7275) (layer B.SilkS))
  (gr_text "SW4.4\n\nOFF\n\n\n\n\n\n\n\n\nON\nON\nON\nON\nON\nON" (at 143.51 105.7275) (layer B.SilkS))
  (gr_text "OFF: 16 KiB ROM\nON:  Page Mode" (at 142.24 96.52 90) (layer B.SilkS))
  (gr_text "SW3.1\n\nOFF\nON\nOFF\nON\nOFF\nON\nOFF\nON" (at 191.135 79.0575) (layer B.SilkS))
  (gr_text "SW3.2\n\nOFF\nOFF\nON\nON\nOFF\nOFF\nON\nON" (at 186.055 79.0575) (layer B.SilkS))
  (gr_text "SW3.3\n\nON\nON\nON\nON\nON\nON\nON\nON" (at 180.975 79.0575) (layer B.SilkS))
  (gr_text "SW3.4\n\nOFF\nOFF\nOFF\nOFF\nON\nON\nON\nON" (at 175.895 79.0575) (layer B.SilkS))
  (gr_text "I/O Address\n\n0x200\n0x220\n0x240\n0x260\n0x280\n0x2A0\n0x2C0\n0x2E0" (at 201.295 79.0575) (layer B.SilkS))
  (gr_text "ROM Address\n\nBoot ROM Disabled\n0xC0000\n0xC4000\n0xC8000\n0xCC000\n0xD0000\n0xD4000\n0xD8000\n0xDC000\n0xC0000\n0xC8000\n0xD0000\n0xD8000\n0xC0000\n0xD0000" (at 179.07 105.7275) (layer B.SilkS))
  (gr_text "SW4.3\n\n*\nOFF\nOFF\nOFF\nOFF\nON\nON\nON\nON\nOFF\nOFF\nOFF\nOFF\nON\nON" (at 148.59 105.7275) (layer B.SilkS))
  (gr_text "SW4.2\n\n*\nOFF\nOFF\nON\nON\nOFF\nOFF\nON\nON\nOFF\nOFF\nON\nON\nOFF\nOFF" (at 153.67 105.7275) (layer B.SilkS))
  (gr_text "SW2.1\n\nOFF\nON\nOFF\nON" (at 123.5075 72.7075) (layer B.SilkS))
  (gr_text "SW2.2\n\nOFF\nOFF\nON\nON" (at 118.4275 72.7075) (layer B.SilkS))
  (gr_text "IRQ\n\nIRQ2\nIRQ3\nIRQ4\nIRQ5" (at 128.5875 72.7075) (layer B.SilkS))
  (gr_text "SW4.1\n\n*\nOFF\nON\nOFF\nON\nOFF\nON\nOFF\nON\nOFF\nON\nOFF\nON\nOFF\nON" (at 158.75 105.7275) (layer B.SilkS))
  (gr_text PnP (at 138.43 71.12 90) (layer F.SilkS))
  (gr_text Switches (at 135.89 71.12 90) (layer F.SilkS))
  (gr_text "SW1.1: OFF - Jumperless; ON - Switches\nSW1.2: OFF - No PnP; ON - PnP Mode" (at 166.6875 66.04) (layer B.SilkS))
  (gr_text "ISA 8-bit Ethernet Controller\nVersion 1.0\nCopyright (C) 2021 Sergey Kiselev" (at 188.595 75.8825) (layer F.SilkS))
  (gr_line (start 203.2 59.69) (end 104.14 59.69) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 101.6 133.985) (end 101.6 62.23) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_text www.malinov.com (at 190.5 125.095) (layer F.SilkS))
  (gr_line (start 205.74 124.46) (end 205.74 62.23) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_arc (start 104.14 62.23) (end 101.6 62.23) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 203.2 127) (end 182.88 127) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_arc (start 203.2 124.46) (end 205.74 124.46) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_arc (start 203.2 62.23) (end 203.2 59.69) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 182.88 133.985) (end 182.88 127) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 102.235 134.62) (end 182.245 134.62) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_arc (start 182.245 133.985) (end 182.88 133.985) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_arc (start 102.235 133.985) (end 102.235 134.62) (angle 90) (layer Edge.Cuts) (width 0.381))
  (zone (net 32) (net_name GND) (layer Back) (hatch edge 0.508)
    (connect_pads (clearance 0.3556))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 205.74 85.725) (xy 193.675 85.725) (xy 191.135 88.265) (xy 191.135 100.965) (xy 193.675 103.505)
        (xy 205.74 103.505) (xy 205.74 127) (xy 182.88 127) (xy 182.88 122.8725) (xy 182.5625 122.555)
        (xy 182.245 122.555) (xy 180.975 123.825) (xy 179.705 123.825) (xy 178.435 122.555) (xy 178.435 114.6175)
        (xy 172.4025 108.585) (xy 172.4025 107.95) (xy 172.72 107.6325) (xy 179.3875 107.6325) (xy 179.705 107.315)
        (xy 179.705 106.045) (xy 179.3875 105.7275) (xy 167.9575 105.7275) (xy 166.6875 104.4575) (xy 166.6875 103.8225)
        (xy 167.3225 103.1875) (xy 169.545 101.2825) (xy 169.545 79.6925) (xy 169.8625 79.375) (xy 182.5625 79.375)
        (xy 182.88 79.0575) (xy 182.88 61.2775) (xy 182.5625 60.96) (xy 135.255 60.96) (xy 126.365 69.85)
        (xy 124.46 69.85) (xy 118.11 63.5) (xy 104.4575 63.5) (xy 104.14 63.8175) (xy 104.14 65.7225)
        (xy 104.4575 66.04) (xy 110.1725 66.04) (xy 110.49 66.3575) (xy 110.49 112.395) (xy 107.95 114.935)
        (xy 107.95 121.92) (xy 106.045 123.825) (xy 103.505 123.825) (xy 101.6 121.92) (xy 101.6 59.69)
        (xy 205.74 59.69)
      )
    )
  )
  (zone (net 32) (net_name GND) (layer Front) (hatch edge 0.508)
    (connect_pads (clearance 0.3556))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 184.15 81.915) (xy 184.15 100.0125) (xy 184.785 100.6475) (xy 191.4525 100.6475) (xy 194.31 103.505)
        (xy 194.31 104.775) (xy 193.9925 105.0925) (xy 165.735 105.0925) (xy 164.465 103.8225) (xy 145.415 103.8225)
        (xy 144.145 105.0925) (xy 137.795 105.0925) (xy 135.255 107.6325) (xy 135.255 102.87) (xy 135.89 102.235)
        (xy 136.8425 102.235) (xy 137.16 102.5525) (xy 137.16 103.505) (xy 137.4775 103.8225) (xy 139.7 103.8225)
        (xy 140.335 103.1875) (xy 144.4625 103.1875) (xy 144.78 102.87) (xy 144.78 93.345) (xy 148.59 93.345)
        (xy 148.59 91.44) (xy 145.415 91.44) (xy 145.415 90.805) (xy 147.0025 89.2175) (xy 164.7825 89.2175)
        (xy 165.1 88.9) (xy 165.1 86.0425) (xy 164.7825 85.725) (xy 163.195 85.725) (xy 162.56 85.09)
        (xy 167.005 80.645) (xy 182.88 80.645)
      )
    )
  )
  (zone (net 32) (net_name GND) (layer Back) (hatch edge 0.508)
    (connect_pads (clearance 0.3556))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 159.0675 73.025) (xy 159.0675 75.8825) (xy 158.75 76.2) (xy 142.24 76.2) (xy 141.605 76.835)
        (xy 141.605 87.63) (xy 143.51 89.535) (xy 144.4625 89.535) (xy 146.05 91.1225) (xy 146.05 92.3925)
        (xy 147.0025 93.345) (xy 147.0025 93.98) (xy 146.685 94.2975) (xy 142.24 94.2975) (xy 141.9225 94.615)
        (xy 141.9225 110.8075) (xy 143.1925 112.0775) (xy 145.0975 112.0775) (xy 147.6375 109.5375) (xy 156.845 109.5375)
        (xy 169.2275 121.92) (xy 169.2275 122.2375) (xy 168.91 122.555) (xy 158.4325 122.555) (xy 160.655 120.3325)
        (xy 160.655 119.6975) (xy 158.4325 117.475) (xy 145.0975 117.475) (xy 140.0175 112.395) (xy 140.0175 92.075)
        (xy 135.255 87.3125) (xy 135.255 81.28) (xy 143.8275 72.7075) (xy 158.75 72.7075)
      )
    )
  )
  (zone (net 33) (net_name VCC) (layer Back) (hatch edge 0.508)
    (connect_pads (clearance 0.3556))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 182.245 61.9125) (xy 182.245 78.4225) (xy 181.9275 78.74) (xy 169.2275 78.74) (xy 168.91 79.0575)
        (xy 168.91 100.6475) (xy 166.0525 103.505) (xy 166.0525 104.775) (xy 177.165 115.8875) (xy 177.165 122.555)
        (xy 175.895 123.825) (xy 174.625 123.825) (xy 172.72 121.92) (xy 171.1325 121.92) (xy 157.48 108.2675)
        (xy 149.86 108.2675) (xy 147.955 106.3625) (xy 147.0025 106.3625) (xy 147.0025 109.22) (xy 144.78 111.4425)
        (xy 143.51 111.4425) (xy 142.5575 110.49) (xy 142.5575 95.25) (xy 142.875 94.9325) (xy 147.0025 94.9325)
        (xy 149.225 92.71) (xy 149.225 86.0425) (xy 151.4475 83.82) (xy 157.7975 83.82) (xy 159.7025 81.915)
        (xy 159.7025 72.39) (xy 159.385 72.0725) (xy 143.1925 72.0725) (xy 134.62 80.645) (xy 134.62 84.455)
        (xy 134.3025 84.7725) (xy 133.0325 84.7725) (xy 132.715 84.455) (xy 132.715 75.8825) (xy 130.81 73.9775)
        (xy 118.4275 73.9775) (xy 115.8875 71.4375) (xy 112.7125 71.4375) (xy 112.395 71.755) (xy 111.125 71.755)
        (xy 111.125 64.135) (xy 117.7925 64.135) (xy 124.1425 70.485) (xy 126.6825 70.485) (xy 135.5725 61.595)
        (xy 181.9275 61.595)
      )
    )
  )
  (zone (net 32) (net_name GND) (layer Front) (hatch edge 0.508)
    (connect_pads (clearance 0.3556))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 127.9525 110.8075) (xy 128.5875 110.8075) (xy 129.2225 111.4425) (xy 129.8575 111.4425) (xy 130.4925 110.8075)
        (xy 132.3975 110.8075) (xy 130.4925 112.7125) (xy 127 112.7125) (xy 126.365 112.0775) (xy 123.825 112.0775)
        (xy 120.9675 114.935) (xy 115.2525 114.935) (xy 114.3 115.8875) (xy 106.9975 115.8875) (xy 105.41 117.475)
        (xy 105.41 121.285) (xy 105.0925 121.6025) (xy 102.5525 121.6025) (xy 101.6 120.65) (xy 101.6 112.7125)
        (xy 102.5525 111.76) (xy 110.49 111.76) (xy 112.395 109.855) (xy 127 109.855)
      )
    )
  )
)
