<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.3.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="25.375" y2="0.004" width="0" layer="20"/>
<wire x1="25.375" y1="0.004" x2="25.302" y2="0" width="0" layer="20"/>
<wire x1="25.302" y1="0" x2="25.4" y2="0" width="0" layer="20"/>
<wire x1="25.4" y1="0" x2="25.4" y2="38.1" width="0" layer="20"/>
<wire x1="25.4" y1="38.1" x2="0" y2="38.1" width="0" layer="20"/>
<wire x1="0" y1="38.1" x2="0" y2="0" width="0" layer="20"/>
<text>ATM16M1 Breakout Board v1</text>
<text>GND</text>
<text>GND</text>
<text>5V</text>
<text>5V</text>
<text>PC5</text>
<text>PC4</text>
<text>PB2</text>
<text>PD7</text>
<text>PD6</text>
<text>PD5</text>
<text>PB1</text>
<text>PB0</text>
<text>AREF</text>
<text>PC6</text>
<text>PB3</text>
<text>PB4</text>
<text>PC7</text>
<text>PB5</text>
<text>PB6</text>
<text>PB7</text>
<text>PD0</text>
<text>PC0</text>
<text>nRST</text>
<text>PD1</text>
<text>PC1</text>
<text>GND</text>
</plain>
<libraries>
<library name="Tova">
<packages>
<package name="SO08">
<description>&lt;b&gt;Small Outline Package 8&lt;/b&gt;&lt;br&gt;
NS Package M08A</description>
</package>
<package name="TQFP32-08">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm</description>
</package>
<package name="ABM3">
</package>
</packages>
</library>
<library name="rcl_custom">
<packages>
<package name="0603-B-NOSILK">
<description>&lt;b&gt;0603 (metric 1608) normal 'IPC-B' without silkscreen&lt;/b&gt;
&lt;br&gt;In house package for nominal spacing based on IPC-7351A. Cross-checked against other packages.
This package is identical to 0603-B, but has its tPlace silkscreen layer removed.</description>
</package>
<package name="0805-B-NOSILK">
<description>&lt;b&gt;0805 (metric 2012) normal 'IPC-B' without silkscreen&lt;/b&gt;
&lt;br&gt;In house package for nominal spacing based on IPC-7351A. Cross-checked against other packages.
This package is identical to 0805-B, but has its tPlace silkscreen layer removed.</description>
</package>
</packages>
</library>
<library name="pinhead">
<packages>
<package name="2X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X04">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X02">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X14">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U501" library="Tova" package="SO08" value="MCP2551">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C502" library="rcl_custom" package="0603-B-NOSILK" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R502" library="rcl_custom" package="0603-B-NOSILK" value="10">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C505" library="rcl_custom" package="0603-B-NOSILK" value="20p">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C506" library="rcl_custom" package="0603-B-NOSILK" value="20p">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R501" library="rcl_custom" package="0603-B-NOSILK" value="120">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C500" library="rcl_custom" package="0603-B-NOSILK" value="1n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C501" library="rcl_custom" package="0805-B-NOSILK" value="10u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U503" library="Tova" package="TQFP32-08" value="ATMEL16/32/64M1-AI">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATMEGA8-16AU"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="9171371"/>
<attribute name="OC_NEWARK" value="73M8863"/>
<attribute name="VALUE"/>
</element>
<element name="C503" library="rcl_custom" package="0603-B-NOSILK" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R500" library="rcl_custom" package="0603-B-NOSILK" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP500" library="pinhead" package="2X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C507" library="rcl_custom" package="0603-B-NOSILK" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X500" library="Tova" package="ABM3" value="16 MHz">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C508" library="rcl_custom" package="0603-B-NOSILK" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP3" library="pinhead" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP6" library="pinhead" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP8" library="pinhead" package="1X14" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP9" library="pinhead" package="1X14" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="C505" pad="2"/>
<contactref element="C506" pad="2"/>
<contactref element="U503" pad="5"/>
<contactref element="R502" pad="1"/>
<contactref element="U501" pad="2"/>
<contactref element="C502" pad="2"/>
<contactref element="C503" pad="1"/>
<contactref element="JP500" pad="6"/>
<contactref element="C501" pad="2"/>
<contactref element="C500" pad="2"/>
<contactref element="C507" pad="2"/>
<contactref element="U503" pad="20"/>
<contactref element="C508" pad="2"/>
<contactref element="JP3" pad="4"/>
<contactref element="JP9" pad="14"/>
<contactref element="JP8" pad="14"/>
</signal>
<signal name="5V">
<contactref element="U501" pad="3"/>
<contactref element="C502" pad="1"/>
<contactref element="C500" pad="1"/>
<contactref element="C501" pad="1"/>
<contactref element="R500" pad="2"/>
<contactref element="JP500" pad="2"/>
<contactref element="U503" pad="4"/>
<contactref element="C503" pad="2"/>
<contactref element="U503" pad="19"/>
<contactref element="C507" pad="1"/>
<contactref element="JP3" pad="1"/>
<contactref element="JP8" pad="1"/>
<contactref element="JP9" pad="1"/>
</signal>
<signal name="CAN_H">
<contactref element="JP3" pad="2"/>
<contactref element="JP6" pad="1"/>
<contactref element="U501" pad="7"/>
</signal>
<signal name="N$10">
<contactref element="U501" pad="8"/>
<contactref element="R502" pad="2"/>
</signal>
<signal name="CAN_L">
<contactref element="U501" pad="6"/>
<contactref element="R501" pad="1"/>
<contactref element="JP3" pad="3"/>
</signal>
<signal name="PE3">
<contactref element="C505" pad="1"/>
<contactref element="U503" pad="10"/>
<contactref element="X500" pad="P2"/>
</signal>
<signal name="TXCAN">
<contactref element="U501" pad="1"/>
<contactref element="U503" pad="6"/>
</signal>
<signal name="RXCAN">
<contactref element="U501" pad="4"/>
<contactref element="U503" pad="7"/>
</signal>
<signal name="PE2">
<contactref element="C506" pad="1"/>
<contactref element="U503" pad="11"/>
<contactref element="X500" pad="P1"/>
</signal>
<signal name="!RESET">
<contactref element="U503" pad="31"/>
<contactref element="JP500" pad="5"/>
<contactref element="R500" pad="1"/>
<contactref element="JP9" pad="11"/>
</signal>
<signal name="MISO">
<contactref element="U503" pad="1"/>
<contactref element="JP500" pad="1"/>
</signal>
<signal name="MOSI">
<contactref element="U503" pad="2"/>
<contactref element="JP500" pad="4"/>
</signal>
<signal name="SCK">
<contactref element="U503" pad="12"/>
<contactref element="JP500" pad="3"/>
</signal>
<signal name="AREF">
<contactref element="U503" pad="21"/>
<contactref element="C508" pad="1"/>
<contactref element="JP8" pad="10"/>
</signal>
<signal name="GNDA">
</signal>
<signal name="N$3">
<contactref element="R501" pad="2"/>
<contactref element="JP6" pad="2"/>
</signal>
<signal name="PD6">
<contactref element="U503" pad="14"/>
<contactref element="JP8" pad="6"/>
</signal>
<signal name="PD5">
<contactref element="U503" pad="13"/>
<contactref element="JP8" pad="7"/>
</signal>
<signal name="PD7">
<contactref element="U503" pad="15"/>
<contactref element="JP8" pad="5"/>
</signal>
<signal name="PC5">
<contactref element="U503" pad="18"/>
<contactref element="JP8" pad="2"/>
</signal>
<signal name="PC4">
<contactref element="U503" pad="17"/>
<contactref element="JP8" pad="3"/>
</signal>
<signal name="PB2">
<contactref element="U503" pad="16"/>
<contactref element="JP8" pad="4"/>
</signal>
<signal name="PB1">
<contactref element="U503" pad="9"/>
<contactref element="JP8" pad="8"/>
</signal>
<signal name="PB0">
<contactref element="U503" pad="8"/>
<contactref element="JP8" pad="9"/>
</signal>
<signal name="PC1">
<contactref element="U503" pad="3"/>
<contactref element="JP9" pad="13"/>
</signal>
<signal name="PC6">
<contactref element="U503" pad="22"/>
<contactref element="JP9" pad="2"/>
</signal>
<signal name="PB3">
<contactref element="U503" pad="23"/>
<contactref element="JP9" pad="3"/>
</signal>
<signal name="PB4">
<contactref element="U503" pad="24"/>
<contactref element="JP9" pad="4"/>
</signal>
<signal name="PC7">
<contactref element="U503" pad="25"/>
<contactref element="JP9" pad="5"/>
</signal>
<signal name="PB5">
<contactref element="U503" pad="26"/>
<contactref element="JP9" pad="6"/>
</signal>
<signal name="PB6">
<contactref element="U503" pad="27"/>
<contactref element="JP9" pad="7"/>
</signal>
<signal name="PB7">
<contactref element="U503" pad="28"/>
<contactref element="JP9" pad="8"/>
</signal>
<signal name="PD0">
<contactref element="U503" pad="29"/>
<contactref element="JP9" pad="9"/>
</signal>
<signal name="PC0">
<contactref element="U503" pad="30"/>
<contactref element="JP9" pad="10"/>
</signal>
<signal name="PD1">
<contactref element="U503" pad="32"/>
<contactref element="JP9" pad="12"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
