(kicad_pcb (version 20170123) (host pcbnew "(2017-07-25 revision 161045f)-master")
  (general
    (thickness 1.6)
    (drawings 99)
    (tracks 9690)
    (zones 0)
    (modules 522)
    (nets 427)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (1 In1.Cu signal hide)
    (2 In2.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.15)
    (user_trace_width 0.2)
    (user_trace_width 0.3)
    (user_trace_width 0.34)
    (user_trace_width 0.5)
    (user_trace_width 2.3)
    (trace_clearance 0.13)
    (zone_clearance 0.3)
    (zone_45_only yes)
    (trace_min 0.15)
    (segment_width 0.8)
    (edge_width 0.15)
    (via_size 0.46)
    (via_drill 0.254)
    (via_min_size 0.46)
    (via_min_drill 0.254)
    (user_via 0.7 0.4)
    (uvia_size 0.69)
    (uvia_drill 0.34)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0.3)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.76 2.4)
    (pad_drill 0)
    (pad_to_mask_clearance 0.08)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF3F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerbers))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 /transmitter/RF_OUT_P)
  (net 3 "Net-(C6-Pad1)")
  (net 4 /transmitter/RF_OUT_N)
  (net 5 "Net-(C16-Pad1)")
  (net 6 "Net-(C21-Pad1)")
  (net 7 "Net-(C28-Pad2)")
  (net 8 "Net-(C30-Pad1)")
  (net 9 "Net-(C30-Pad2)")
  (net 10 "Net-(C32-Pad1)")
  (net 11 "Net-(C44-Pad2)")
  (net 12 "Net-(C45-Pad1)")
  (net 13 "Net-(C46-Pad2)")
  (net 14 /receiver/DETO)
  (net 15 "Net-(C58-Pad1)")
  (net 16 "Net-(C63-Pad1)")
  (net 17 "Net-(C72-Pad1)")
  (net 18 "Net-(C72-Pad2)")
  (net 19 "Net-(C74-Pad1)")
  (net 20 "Net-(R15-Pad2)")
  (net 21 "Net-(R33-Pad2)")
  (net 22 /filter_bank/RF_IN)
  (net 23 /filter_bank/RF_OUT)
  (net 24 "Net-(C12-Pad2)")
  (net 25 "Net-(C15-Pad1)")
  (net 26 "Net-(C17-Pad1)")
  (net 27 "Net-(C18-Pad1)")
  (net 28 "Net-(C19-Pad1)")
  (net 29 "Net-(C37-Pad2)")
  (net 30 "Net-(C38-Pad1)")
  (net 31 "Net-(C52-Pad2)")
  (net 32 "Net-(C57-Pad1)")
  (net 33 "Net-(C59-Pad1)")
  (net 34 "Net-(C60-Pad1)")
  (net 35 "Net-(C61-Pad1)")
  (net 36 "Net-(C92-Pad2)")
  (net 37 "Net-(C93-Pad2)")
  (net 38 "Net-(C94-Pad2)")
  (net 39 "Net-(C95-Pad2)")
  (net 40 "Net-(C96-Pad1)")
  (net 41 "Net-(C97-Pad1)")
  (net 42 "Net-(C98-Pad1)")
  (net 43 "Net-(C99-Pad1)")
  (net 44 "Net-(R4-Pad2)")
  (net 45 "Net-(R11-Pad1)")
  (net 46 /receiver/RF_IN)
  (net 47 "Net-(R29-Pad1)")
  (net 48 "Net-(C92-Pad1)")
  (net 49 "Net-(C93-Pad1)")
  (net 50 "Net-(C94-Pad1)")
  (net 51 "Net-(C95-Pad1)")
  (net 52 "Net-(C96-Pad2)")
  (net 53 "Net-(C97-Pad2)")
  (net 54 "Net-(C98-Pad2)")
  (net 55 "Net-(C99-Pad2)")
  (net 56 /power/12V)
  (net 57 "Net-(C101-Pad1)")
  (net 58 "Net-(C101-Pad2)")
  (net 59 "Net-(C11-Pad1)")
  (net 60 "Net-(C104-Pad1)")
  (net 61 "Net-(C104-Pad2)")
  (net 62 "Net-(C105-Pad1)")
  (net 63 "Net-(C106-Pad1)")
  (net 64 "Net-(C108-Pad1)")
  (net 65 "Net-(C109-Pad1)")
  (net 66 "Net-(C110-Pad1)")
  (net 67 "Net-(C111-Pad1)")
  (net 68 "Net-(D2-Pad1)")
  (net 69 "Net-(D3-Pad1)")
  (net 70 "Net-(R12-Pad2)")
  (net 71 "Net-(R13-Pad2)")
  (net 72 "Net-(R30-Pad2)")
  (net 73 "Net-(R31-Pad2)")
  (net 74 "Net-(R32-Pad1)")
  (net 75 "Net-(R34-Pad1)")
  (net 76 /power/SYNC_3V3)
  (net 77 /receiver/IF-)
  (net 78 /receiver/IF+)
  (net 79 "Net-(C115-Pad1)")
  (net 80 /receiver/DITHER)
  (net 81 "Net-(C125-Pad2)")
  (net 82 "Net-(C129-Pad1)")
  (net 83 "Net-(C130-Pad1)")
  (net 84 "Net-(C132-Pad2)")
  (net 85 "Net-(C133-Pad1)")
  (net 86 "Net-(R50-Pad2)")
  (net 87 "Net-(R51-Pad2)")
  (net 88 "Net-(C135-Pad2)")
  (net 89 "Net-(R2-Pad2)")
  (net 90 "Net-(R82-Pad2)")
  (net 91 "Net-(C138-Pad1)")
  (net 92 "Net-(C139-Pad1)")
  (net 93 /transmitter/3V3_RF)
  (net 94 /receiver/lo_synth/3V3_RF)
  (net 95 /receiver/5VF)
  (net 96 /power/12V_IN)
  (net 97 "Net-(C135-Pad1)")
  (net 98 /tx_amp/RF_IN)
  (net 99 "Net-(C142-Pad1)")
  (net 100 "Net-(C145-Pad1)")
  (net 101 "Net-(C146-Pad1)")
  (net 102 "Net-(C146-Pad2)")
  (net 103 "Net-(C150-Pad1)")
  (net 104 "Net-(R91-Pad2)")
  (net 105 "Net-(C152-Pad1)")
  (net 106 "Net-(C152-Pad2)")
  (net 107 "Net-(C151-Pad2)")
  (net 108 "Net-(R97-Pad1)")
  (net 109 "Net-(C113-Pad1)")
  (net 110 "Net-(C144-Pad2)")
  (net 111 /SPI_CLK)
  (net 112 "Net-(C7-Pad2)")
  (net 113 "Net-(C52-Pad1)")
  (net 114 "Net-(U7-Pad22)")
  (net 115 "Net-(C144-Pad1)")
  (net 116 /ADC_VCM)
  (net 117 /tx_amp/OUTP)
  (net 118 "Net-(C166-Pad1)")
  (net 119 "Net-(C157-Pad2)")
  (net 120 "Net-(U24-Pad4)")
  (net 121 "Net-(U24-Pad1)")
  (net 122 /fpga/usb/USB_5V)
  (net 123 /fpga/usb/USBDP)
  (net 124 /fpga/usb/USBDM)
  (net 125 "Net-(U31-Pad4)")
  (net 126 "Net-(U31-PadSH)")
  (net 127 /LO_SPI_DATA)
  (net 128 /LO_LE)
  (net 129 /LO_CE)
  (net 130 /receiver/LOP)
  (net 131 /receiver/LON)
  (net 132 /LO_LD)
  (net 133 /LO_RF_ENABLE)
  (net 134 /LO_MUXOUT)
  (net 135 /SOURCE_SPI_DATA)
  (net 136 /SOURCE_LE)
  (net 137 /SOURCE_CE)
  (net 138 /SOURCE_LD)
  (net 139 /SOURCE_RF_ENABLE)
  (net 140 /SOURCE_MUXOUT)
  (net 141 "Net-(R8-Pad2)")
  (net 142 "Net-(R9-Pad2)")
  (net 143 "Net-(C85-Pad1)")
  (net 144 "Net-(C82-Pad1)")
  (net 145 "Net-(C8-Pad2)")
  (net 146 "Net-(C9-Pad2)")
  (net 147 "Net-(R1-Pad2)")
  (net 148 "Net-(R3-Pad2)")
  (net 149 "Net-(C81-Pad1)")
  (net 150 "Net-(C168-Pad1)")
  (net 151 "/port switch/RFC")
  (net 152 "Net-(C180-Pad2)")
  (net 153 "Net-(R67-Pad1)")
  (net 154 "Net-(R56-Pad2)")
  (net 155 "Net-(R54-Pad2)")
  (net 156 "Net-(C171-Pad1)")
  (net 157 "Net-(C172-Pad1)")
  (net 158 "Net-(R55-Pad2)")
  (net 159 "Net-(R66-Pad2)")
  (net 160 "Net-(C179-Pad2)")
  (net 161 "Net-(R68-Pad1)")
  (net 162 /receiver/RF_BALUN)
  (net 163 "Net-(C7-Pad1)")
  (net 164 /fpga/usb/EECS)
  (net 165 /fpga/usb/EESK)
  (net 166 /fpga/usb/EEDATA)
  (net 167 /fpga/usb/DO)
  (net 168 /3V6)
  (net 169 "Net-(U25-Pad4)")
  (net 170 /ADC+)
  (net 171 /3V3A)
  (net 172 /ADC-)
  (net 173 /PORT_SW1)
  (net 174 /PORT_SW0)
  (net 175 "Net-(R14-Pad1)")
  (net 176 "Net-(C123-Pad2)")
  (net 177 "Net-(C126-Pad2)")
  (net 178 /DITHER)
  (net 179 "Net-(C122-Pad2)")
  (net 180 "Net-(R80-Pad1)")
  (net 181 "Net-(R81-Pad1)")
  (net 182 "Net-(R84-Pad2)")
  (net 183 /fpga/TCK)
  (net 184 /CLK_SOURCE)
  (net 185 /CLK_LO)
  (net 186 "Net-(R88-Pad2)")
  (net 187 /fpga/TDI)
  (net 188 "Net-(R93-Pad1)")
  (net 189 /PWDN)
  (net 190 "Net-(R69-Pad2)")
  (net 191 "Net-(R85-Pad2)")
  (net 192 /fpga/TMS)
  (net 193 "Net-(R71-Pad2)")
  (net 194 /FILTER_V1)
  (net 195 /FILTER_V2)
  (net 196 /FILTER_V4)
  (net 197 /FILTER_V3)
  (net 198 "Net-(C3-Pad2)")
  (net 199 /1V8)
  (net 200 "Net-(U30-PadB1)")
  (net 201 "Net-(U30-PadC1)")
  (net 202 /RX_SW5)
  (net 203 /RX_SW4)
  (net 204 /RX_SW1)
  (net 205 /RX_SW0)
  (net 206 "Net-(U30-PadM1)")
  (net 207 "Net-(U30-PadN1)")
  (net 208 /fpga/RXF#)
  (net 209 "Net-(U30-PadB2)")
  (net 210 "Net-(U30-PadC2)")
  (net 211 "Net-(U30-PadE2)")
  (net 212 "Net-(U30-PadF2)")
  (net 213 /RX_SW3)
  (net 214 /RX_SW2)
  (net 215 /MIXER_ENABLE)
  (net 216 "Net-(U30-PadL2)")
  (net 217 "Net-(U30-PadM2)")
  (net 218 "Net-(U30-PadN2)")
  (net 219 "Net-(U30-PadR2)")
  (net 220 /fpga/TXE#)
  (net 221 "Net-(U30-PadC3)")
  (net 222 "Net-(U30-PadD3)")
  (net 223 "Net-(U30-PadE3)")
  (net 224 "Net-(U30-PadF3)")
  (net 225 "Net-(U30-PadH3)")
  (net 226 "Net-(U30-PadJ3)")
  (net 227 "Net-(U30-PadK3)")
  (net 228 "Net-(U30-PadN3)")
  (net 229 "Net-(U30-PadP3)")
  (net 230 /fpga/WR)
  (net 231 /fpga/RD#)
  (net 232 "Net-(U30-PadC4)")
  (net 233 "Net-(U30-PadD4)")
  (net 234 "Net-(U30-PadF4)")
  (net 235 "Net-(U30-PadG4)")
  (net 236 "Net-(U30-PadH4)")
  (net 237 "Net-(U30-PadJ4)")
  (net 238 "Net-(U30-PadL4)")
  (net 239 "Net-(U30-PadM4)")
  (net 240 "Net-(U30-PadN4)")
  (net 241 "Net-(U30-PadP4)")
  (net 242 /fpga/SI/WUB)
  (net 243 "Net-(U30-PadB5)")
  (net 244 "Net-(U30-PadD5)")
  (net 245 "Net-(U30-PadE5)")
  (net 246 "Net-(U30-PadF5)")
  (net 247 "Net-(U30-PadG5)")
  (net 248 "Net-(U30-PadH5)")
  (net 249 "Net-(U30-PadJ5)")
  (net 250 "Net-(U30-PadK5)")
  (net 251 "Net-(U30-PadL5)")
  (net 252 "Net-(U30-PadM5)")
  (net 253 "Net-(U30-PadP5)")
  (net 254 /fpga/D4)
  (net 255 /fpga/D3)
  (net 256 "Net-(U30-PadB6)")
  (net 257 "Net-(U30-PadC6)")
  (net 258 "Net-(U30-PadD6)")
  (net 259 "Net-(U30-PadE6)")
  (net 260 /fpga/D12)
  (net 261 /fpga/D11)
  (net 262 /fpga/D0)
  (net 263 /fpga/D2)
  (net 264 "Net-(U30-PadA7)")
  (net 265 "Net-(U30-PadB7)")
  (net 266 "Net-(U30-PadC7)")
  (net 267 "Net-(C205-Pad2)")
  (net 268 /fpga/D1)
  (net 269 /fpga/D8)
  (net 270 /fpga/FT_D7)
  (net 271 "Net-(U30-PadC8)")
  (net 272 "Net-(U30-PadD8)")
  (net 273 "Net-(C205-Pad1)")
  (net 274 /fpga/TDO)
  (net 275 /fpga/D10)
  (net 276 /fpga/D9)
  (net 277 /fpga/D7)
  (net 278 /fpga/FT_D6)
  (net 279 /fpga/FT_D4)
  (net 280 "Net-(U30-PadC9)")
  (net 281 "Net-(U30-PadD9)")
  (net 282 "Net-(U30-PadN9)")
  (net 283 /fpga/D13)
  (net 284 /fpga/D6)
  (net 285 /fpga/FT_D5)
  (net 286 /fpga/FT_D3)
  (net 287 "Net-(U30-PadD10)")
  (net 288 "Net-(U30-PadP10)")
  (net 289 "Net-(U30-PadR10)")
  (net 290 /fpga/D5)
  (net 291 /fpga/FT_D2)
  (net 292 "Net-(U30-PadC11)")
  (net 293 "Net-(U30-PadD11)")
  (net 294 "Net-(U30-PadE11)")
  (net 295 "Net-(U30-PadG11)")
  (net 296 "Net-(U30-PadH11)")
  (net 297 /CLK_FPGA)
  (net 298 "Net-(U30-PadP11)")
  (net 299 "Net-(U30-PadR11)")
  (net 300 /fpga/FT_D0)
  (net 301 /fpga/FT_D1)
  (net 302 "Net-(U30-PadC12)")
  (net 303 "Net-(U30-PadE12)")
  (net 304 "Net-(U30-PadG12)")
  (net 305 "Net-(U30-PadH12)")
  (net 306 "Net-(U30-PadK12)")
  (net 307 "Net-(U30-PadM12)")
  (net 308 "Net-(U30-PadN12)")
  (net 309 "Net-(U30-PadR12)")
  (net 310 "Net-(U30-PadC13)")
  (net 311 "Net-(U30-PadD13)")
  (net 312 "Net-(U30-PadE13)")
  (net 313 "Net-(U30-PadH13)")
  (net 314 "Net-(U30-PadK13)")
  (net 315 "Net-(U30-PadL13)")
  (net 316 "Net-(U30-PadN13)")
  (net 317 "Net-(U30-PadP13)")
  (net 318 "Net-(U30-PadR13)")
  (net 319 "Net-(U30-PadB14)")
  (net 320 /ATTEN_SPI_DATA)
  (net 321 "Net-(U30-PadD14)")
  (net 322 "Net-(U30-PadH14)")
  (net 323 "Net-(U30-PadL14)")
  (net 324 "Net-(U30-PadP14)")
  (net 325 "Net-(U30-PadD15)")
  (net 326 "Net-(U30-PadE15)")
  (net 327 "Net-(U30-PadF15)")
  (net 328 /ATTEN_LE)
  (net 329 "Net-(U30-PadJ15)")
  (net 330 "Net-(U30-PadM15)")
  (net 331 "Net-(U30-PadP15)")
  (net 332 "Net-(U30-PadR15)")
  (net 333 "Net-(U30-PadG16)")
  (net 334 "Net-(U30-PadM16)")
  (net 335 "Net-(U30-PadN16)")
  (net 336 "Net-(C90-Pad1)")
  (net 337 "Net-(C121-Pad2)")
  (net 338 "Net-(C3-Pad1)")
  (net 339 /CLK_ADC)
  (net 340 /3V3D)
  (net 341 /5V)
  (net 342 "Net-(C208-Pad1)")
  (net 343 "Net-(C210-Pad1)")
  (net 344 "Net-(C209-Pad1)")
  (net 345 /RX2)
  (net 346 /A)
  (net 347 /RX1)
  (net 348 /B)
  (net 349 /PORT2)
  (net 350 /PORT1)
  (net 351 "Net-(U33-Pad41)")
  (net 352 "Net-(U33-Pad20)")
  (net 353 "Net-(U33-Pad19)")
  (net 354 "Net-(U33-Pad17)")
  (net 355 "Net-(U33-Pad16)")
  (net 356 "Net-(U33-Pad15)")
  (net 357 "Net-(U33-Pad13)")
  (net 358 "Net-(U33-Pad12)")
  (net 359 "Net-(U33-Pad11)")
  (net 360 /fpga/OF)
  (net 361 /fpga/ADC_OE)
  (net 362 /fpga/ADC_SHDN)
  (net 363 "Net-(R94-Pad1)")
  (net 364 /tx_amp/DET_IN)
  (net 365 /PDET)
  (net 366 "Net-(C226-Pad1)")
  (net 367 "Net-(D1-Pad1)")
  (net 368 /1V0)
  (net 369 "Net-(D4-Pad1)")
  (net 370 /fpga/adc/3V0)
  (net 371 "Net-(C235-Pad2)")
  (net 372 "Net-(C236-Pad1)")
  (net 373 "Net-(C234-Pad1)")
  (net 374 "Net-(C235-Pad1)")
  (net 375 "Net-(C237-Pad1)")
  (net 376 "Net-(C234-Pad2)")
  (net 377 "Net-(R96-Pad1)")
  (net 378 "Net-(R98-Pad1)")
  (net 379 "Net-(C238-Pad1)")
  (net 380 "Net-(C239-Pad1)")
  (net 381 /power/fpga_power/SYNC_1V8)
  (net 382 "Net-(C213-Pad1)")
  (net 383 /fpga/adc/REFH)
  (net 384 /fpga/adc/REFL)
  (net 385 "Net-(R46-Pad2)")
  (net 386 "Net-(R45-Pad2)")
  (net 387 /power/fpga_power/SYNC_1V0)
  (net 388 "Net-(C132-Pad1)")
  (net 389 /1V8_OSC)
  (net 390 /fpga/LED)
  (net 391 "Net-(D6-Pad2)")
  (net 392 "Net-(D5-Pad2)")
  (net 393 /fpga/CCLK)
  (net 394 "Net-(P9-Pad1)")
  (net 395 /fpga/SPI_DIN)
  (net 396 /fpga/SPI_MOSI)
  (net 397 /fpga/M0)
  (net 398 /fpga/INIT_B)
  (net 399 /fpga/M2)
  (net 400 /fpga/SPI_CS)
  (net 401 /fpga/M1)
  (net 402 /fpga/PROGRAM_B)
  (net 403 "/receiver/RX switch/3V3")
  (net 404 "Net-(F2-Pad1)")
  (net 405 "Net-(F1-Pad1)")
  (net 406 /fpga/usb/5V)
  (net 407 "Net-(U30-PadP6)")
  (net 408 "Net-(U30-PadN6)")
  (net 409 "Net-(U30-PadM6)")
  (net 410 "Net-(F15-Pad1)")
  (net 411 "Net-(F16-Pad1)")
  (net 412 "Net-(C255-Pad1)")
  (net 413 "Net-(R119-Pad2)")
  (net 414 "Net-(R120-Pad2)")
  (net 415 3V3A_RX)
  (net 416 "Net-(U30-PadG15)")
  (net 417 "Net-(U30-PadC14)")
  (net 418 "Net-(R130-Pad1)")
  (net 419 "Net-(R132-Pad2)")
  (net 420 "Net-(R131-Pad2)")
  (net 421 "Net-(R133-Pad1)")
  (net 422 "Net-(C261-Pad1)")
  (net 423 "Net-(P27-Pad1)")
  (net 424 "Net-(P26-Pad1)")
  (net 425 "Net-(P28-Pad1)")
  (net 426 "Net-(R122-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.13)
    (trace_width 0.15)
    (via_dia 0.46)
    (via_drill 0.254)
    (uvia_dia 0.69)
    (uvia_drill 0.34)
    (add_net /1V0)
    (add_net /1V8)
    (add_net /1V8_OSC)
    (add_net /3V3A)
    (add_net /3V3D)
    (add_net /3V6)
    (add_net /5V)
    (add_net /A)
    (add_net /ADC+)
    (add_net /ADC-)
    (add_net /ADC_VCM)
    (add_net /ATTEN_LE)
    (add_net /ATTEN_SPI_DATA)
    (add_net /B)
    (add_net /CLK_ADC)
    (add_net /CLK_FPGA)
    (add_net /CLK_LO)
    (add_net /CLK_SOURCE)
    (add_net /DITHER)
    (add_net /FILTER_V1)
    (add_net /FILTER_V2)
    (add_net /FILTER_V3)
    (add_net /FILTER_V4)
    (add_net /LO_CE)
    (add_net /LO_LD)
    (add_net /LO_LE)
    (add_net /LO_MUXOUT)
    (add_net /LO_RF_ENABLE)
    (add_net /LO_SPI_DATA)
    (add_net /MIXER_ENABLE)
    (add_net /PDET)
    (add_net /PORT1)
    (add_net /PORT2)
    (add_net /PORT_SW0)
    (add_net /PORT_SW1)
    (add_net /PWDN)
    (add_net /RX1)
    (add_net /RX2)
    (add_net /RX_SW0)
    (add_net /RX_SW1)
    (add_net /RX_SW2)
    (add_net /RX_SW3)
    (add_net /RX_SW4)
    (add_net /RX_SW5)
    (add_net /SOURCE_CE)
    (add_net /SOURCE_LD)
    (add_net /SOURCE_LE)
    (add_net /SOURCE_MUXOUT)
    (add_net /SOURCE_RF_ENABLE)
    (add_net /SOURCE_SPI_DATA)
    (add_net /SPI_CLK)
    (add_net /filter_bank/RF_IN)
    (add_net /filter_bank/RF_OUT)
    (add_net /fpga/ADC_OE)
    (add_net /fpga/ADC_SHDN)
    (add_net /fpga/CCLK)
    (add_net /fpga/D0)
    (add_net /fpga/D1)
    (add_net /fpga/D10)
    (add_net /fpga/D11)
    (add_net /fpga/D12)
    (add_net /fpga/D13)
    (add_net /fpga/D2)
    (add_net /fpga/D3)
    (add_net /fpga/D4)
    (add_net /fpga/D5)
    (add_net /fpga/D6)
    (add_net /fpga/D7)
    (add_net /fpga/D8)
    (add_net /fpga/D9)
    (add_net /fpga/FT_D0)
    (add_net /fpga/FT_D1)
    (add_net /fpga/FT_D2)
    (add_net /fpga/FT_D3)
    (add_net /fpga/FT_D4)
    (add_net /fpga/FT_D5)
    (add_net /fpga/FT_D6)
    (add_net /fpga/FT_D7)
    (add_net /fpga/INIT_B)
    (add_net /fpga/LED)
    (add_net /fpga/M0)
    (add_net /fpga/M1)
    (add_net /fpga/M2)
    (add_net /fpga/OF)
    (add_net /fpga/PROGRAM_B)
    (add_net /fpga/RD#)
    (add_net /fpga/RXF#)
    (add_net /fpga/SI/WUB)
    (add_net /fpga/SPI_CS)
    (add_net /fpga/SPI_DIN)
    (add_net /fpga/SPI_MOSI)
    (add_net /fpga/TCK)
    (add_net /fpga/TDI)
    (add_net /fpga/TDO)
    (add_net /fpga/TMS)
    (add_net /fpga/TXE#)
    (add_net /fpga/WR)
    (add_net /fpga/adc/3V0)
    (add_net /fpga/adc/REFH)
    (add_net /fpga/adc/REFL)
    (add_net /fpga/usb/5V)
    (add_net /fpga/usb/DO)
    (add_net /fpga/usb/EECS)
    (add_net /fpga/usb/EEDATA)
    (add_net /fpga/usb/EESK)
    (add_net /fpga/usb/USBDM)
    (add_net /fpga/usb/USBDP)
    (add_net /fpga/usb/USB_5V)
    (add_net "/port switch/RFC")
    (add_net /power/12V)
    (add_net /power/12V_IN)
    (add_net /power/SYNC_3V3)
    (add_net /power/fpga_power/SYNC_1V0)
    (add_net /power/fpga_power/SYNC_1V8)
    (add_net /receiver/5VF)
    (add_net /receiver/DETO)
    (add_net /receiver/DITHER)
    (add_net /receiver/IF+)
    (add_net /receiver/IF-)
    (add_net /receiver/LON)
    (add_net /receiver/LOP)
    (add_net /receiver/RF_BALUN)
    (add_net /receiver/RF_IN)
    (add_net "/receiver/RX switch/3V3")
    (add_net /receiver/lo_synth/3V3_RF)
    (add_net /transmitter/3V3_RF)
    (add_net /transmitter/RF_OUT_N)
    (add_net /transmitter/RF_OUT_P)
    (add_net /tx_amp/DET_IN)
    (add_net /tx_amp/OUTP)
    (add_net /tx_amp/RF_IN)
    (add_net 3V3A_RX)
    (add_net GND)
    (add_net "Net-(C101-Pad1)")
    (add_net "Net-(C101-Pad2)")
    (add_net "Net-(C104-Pad1)")
    (add_net "Net-(C104-Pad2)")
    (add_net "Net-(C105-Pad1)")
    (add_net "Net-(C106-Pad1)")
    (add_net "Net-(C108-Pad1)")
    (add_net "Net-(C109-Pad1)")
    (add_net "Net-(C11-Pad1)")
    (add_net "Net-(C110-Pad1)")
    (add_net "Net-(C111-Pad1)")
    (add_net "Net-(C113-Pad1)")
    (add_net "Net-(C115-Pad1)")
    (add_net "Net-(C12-Pad2)")
    (add_net "Net-(C121-Pad2)")
    (add_net "Net-(C122-Pad2)")
    (add_net "Net-(C123-Pad2)")
    (add_net "Net-(C125-Pad2)")
    (add_net "Net-(C126-Pad2)")
    (add_net "Net-(C129-Pad1)")
    (add_net "Net-(C130-Pad1)")
    (add_net "Net-(C132-Pad1)")
    (add_net "Net-(C132-Pad2)")
    (add_net "Net-(C133-Pad1)")
    (add_net "Net-(C135-Pad1)")
    (add_net "Net-(C135-Pad2)")
    (add_net "Net-(C138-Pad1)")
    (add_net "Net-(C139-Pad1)")
    (add_net "Net-(C142-Pad1)")
    (add_net "Net-(C144-Pad1)")
    (add_net "Net-(C144-Pad2)")
    (add_net "Net-(C145-Pad1)")
    (add_net "Net-(C146-Pad1)")
    (add_net "Net-(C146-Pad2)")
    (add_net "Net-(C15-Pad1)")
    (add_net "Net-(C150-Pad1)")
    (add_net "Net-(C151-Pad2)")
    (add_net "Net-(C152-Pad1)")
    (add_net "Net-(C152-Pad2)")
    (add_net "Net-(C157-Pad2)")
    (add_net "Net-(C16-Pad1)")
    (add_net "Net-(C166-Pad1)")
    (add_net "Net-(C168-Pad1)")
    (add_net "Net-(C17-Pad1)")
    (add_net "Net-(C171-Pad1)")
    (add_net "Net-(C172-Pad1)")
    (add_net "Net-(C179-Pad2)")
    (add_net "Net-(C18-Pad1)")
    (add_net "Net-(C180-Pad2)")
    (add_net "Net-(C19-Pad1)")
    (add_net "Net-(C205-Pad1)")
    (add_net "Net-(C205-Pad2)")
    (add_net "Net-(C208-Pad1)")
    (add_net "Net-(C209-Pad1)")
    (add_net "Net-(C21-Pad1)")
    (add_net "Net-(C210-Pad1)")
    (add_net "Net-(C213-Pad1)")
    (add_net "Net-(C226-Pad1)")
    (add_net "Net-(C234-Pad1)")
    (add_net "Net-(C234-Pad2)")
    (add_net "Net-(C235-Pad1)")
    (add_net "Net-(C235-Pad2)")
    (add_net "Net-(C236-Pad1)")
    (add_net "Net-(C237-Pad1)")
    (add_net "Net-(C238-Pad1)")
    (add_net "Net-(C239-Pad1)")
    (add_net "Net-(C255-Pad1)")
    (add_net "Net-(C261-Pad1)")
    (add_net "Net-(C28-Pad2)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(C30-Pad1)")
    (add_net "Net-(C30-Pad2)")
    (add_net "Net-(C32-Pad1)")
    (add_net "Net-(C37-Pad2)")
    (add_net "Net-(C38-Pad1)")
    (add_net "Net-(C44-Pad2)")
    (add_net "Net-(C45-Pad1)")
    (add_net "Net-(C46-Pad2)")
    (add_net "Net-(C52-Pad1)")
    (add_net "Net-(C52-Pad2)")
    (add_net "Net-(C57-Pad1)")
    (add_net "Net-(C58-Pad1)")
    (add_net "Net-(C59-Pad1)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C60-Pad1)")
    (add_net "Net-(C61-Pad1)")
    (add_net "Net-(C63-Pad1)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(C7-Pad2)")
    (add_net "Net-(C72-Pad1)")
    (add_net "Net-(C72-Pad2)")
    (add_net "Net-(C74-Pad1)")
    (add_net "Net-(C8-Pad2)")
    (add_net "Net-(C81-Pad1)")
    (add_net "Net-(C82-Pad1)")
    (add_net "Net-(C85-Pad1)")
    (add_net "Net-(C9-Pad2)")
    (add_net "Net-(C90-Pad1)")
    (add_net "Net-(C92-Pad1)")
    (add_net "Net-(C92-Pad2)")
    (add_net "Net-(C93-Pad1)")
    (add_net "Net-(C93-Pad2)")
    (add_net "Net-(C94-Pad1)")
    (add_net "Net-(C94-Pad2)")
    (add_net "Net-(C95-Pad1)")
    (add_net "Net-(C95-Pad2)")
    (add_net "Net-(C96-Pad1)")
    (add_net "Net-(C96-Pad2)")
    (add_net "Net-(C97-Pad1)")
    (add_net "Net-(C97-Pad2)")
    (add_net "Net-(C98-Pad1)")
    (add_net "Net-(C98-Pad2)")
    (add_net "Net-(C99-Pad1)")
    (add_net "Net-(C99-Pad2)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(D5-Pad2)")
    (add_net "Net-(D6-Pad2)")
    (add_net "Net-(F1-Pad1)")
    (add_net "Net-(F15-Pad1)")
    (add_net "Net-(F16-Pad1)")
    (add_net "Net-(F2-Pad1)")
    (add_net "Net-(P26-Pad1)")
    (add_net "Net-(P27-Pad1)")
    (add_net "Net-(P28-Pad1)")
    (add_net "Net-(P9-Pad1)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R11-Pad1)")
    (add_net "Net-(R119-Pad2)")
    (add_net "Net-(R12-Pad2)")
    (add_net "Net-(R120-Pad2)")
    (add_net "Net-(R122-Pad2)")
    (add_net "Net-(R13-Pad2)")
    (add_net "Net-(R130-Pad1)")
    (add_net "Net-(R131-Pad2)")
    (add_net "Net-(R132-Pad2)")
    (add_net "Net-(R133-Pad1)")
    (add_net "Net-(R14-Pad1)")
    (add_net "Net-(R15-Pad2)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(R29-Pad1)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(R30-Pad2)")
    (add_net "Net-(R31-Pad2)")
    (add_net "Net-(R32-Pad1)")
    (add_net "Net-(R33-Pad2)")
    (add_net "Net-(R34-Pad1)")
    (add_net "Net-(R4-Pad2)")
    (add_net "Net-(R45-Pad2)")
    (add_net "Net-(R46-Pad2)")
    (add_net "Net-(R50-Pad2)")
    (add_net "Net-(R51-Pad2)")
    (add_net "Net-(R54-Pad2)")
    (add_net "Net-(R55-Pad2)")
    (add_net "Net-(R56-Pad2)")
    (add_net "Net-(R66-Pad2)")
    (add_net "Net-(R67-Pad1)")
    (add_net "Net-(R68-Pad1)")
    (add_net "Net-(R69-Pad2)")
    (add_net "Net-(R71-Pad2)")
    (add_net "Net-(R8-Pad2)")
    (add_net "Net-(R80-Pad1)")
    (add_net "Net-(R81-Pad1)")
    (add_net "Net-(R82-Pad2)")
    (add_net "Net-(R84-Pad2)")
    (add_net "Net-(R85-Pad2)")
    (add_net "Net-(R88-Pad2)")
    (add_net "Net-(R9-Pad2)")
    (add_net "Net-(R91-Pad2)")
    (add_net "Net-(R93-Pad1)")
    (add_net "Net-(R94-Pad1)")
    (add_net "Net-(R96-Pad1)")
    (add_net "Net-(R97-Pad1)")
    (add_net "Net-(R98-Pad1)")
    (add_net "Net-(U24-Pad1)")
    (add_net "Net-(U24-Pad4)")
    (add_net "Net-(U25-Pad4)")
    (add_net "Net-(U30-PadA7)")
    (add_net "Net-(U30-PadB1)")
    (add_net "Net-(U30-PadB14)")
    (add_net "Net-(U30-PadB2)")
    (add_net "Net-(U30-PadB5)")
    (add_net "Net-(U30-PadB6)")
    (add_net "Net-(U30-PadB7)")
    (add_net "Net-(U30-PadC1)")
    (add_net "Net-(U30-PadC11)")
    (add_net "Net-(U30-PadC12)")
    (add_net "Net-(U30-PadC13)")
    (add_net "Net-(U30-PadC14)")
    (add_net "Net-(U30-PadC2)")
    (add_net "Net-(U30-PadC3)")
    (add_net "Net-(U30-PadC4)")
    (add_net "Net-(U30-PadC6)")
    (add_net "Net-(U30-PadC7)")
    (add_net "Net-(U30-PadC8)")
    (add_net "Net-(U30-PadC9)")
    (add_net "Net-(U30-PadD10)")
    (add_net "Net-(U30-PadD11)")
    (add_net "Net-(U30-PadD13)")
    (add_net "Net-(U30-PadD14)")
    (add_net "Net-(U30-PadD15)")
    (add_net "Net-(U30-PadD3)")
    (add_net "Net-(U30-PadD4)")
    (add_net "Net-(U30-PadD5)")
    (add_net "Net-(U30-PadD6)")
    (add_net "Net-(U30-PadD8)")
    (add_net "Net-(U30-PadD9)")
    (add_net "Net-(U30-PadE11)")
    (add_net "Net-(U30-PadE12)")
    (add_net "Net-(U30-PadE13)")
    (add_net "Net-(U30-PadE15)")
    (add_net "Net-(U30-PadE2)")
    (add_net "Net-(U30-PadE3)")
    (add_net "Net-(U30-PadE5)")
    (add_net "Net-(U30-PadE6)")
    (add_net "Net-(U30-PadF15)")
    (add_net "Net-(U30-PadF2)")
    (add_net "Net-(U30-PadF3)")
    (add_net "Net-(U30-PadF4)")
    (add_net "Net-(U30-PadF5)")
    (add_net "Net-(U30-PadG11)")
    (add_net "Net-(U30-PadG12)")
    (add_net "Net-(U30-PadG15)")
    (add_net "Net-(U30-PadG16)")
    (add_net "Net-(U30-PadG4)")
    (add_net "Net-(U30-PadG5)")
    (add_net "Net-(U30-PadH11)")
    (add_net "Net-(U30-PadH12)")
    (add_net "Net-(U30-PadH13)")
    (add_net "Net-(U30-PadH14)")
    (add_net "Net-(U30-PadH3)")
    (add_net "Net-(U30-PadH4)")
    (add_net "Net-(U30-PadH5)")
    (add_net "Net-(U30-PadJ15)")
    (add_net "Net-(U30-PadJ3)")
    (add_net "Net-(U30-PadJ4)")
    (add_net "Net-(U30-PadJ5)")
    (add_net "Net-(U30-PadK12)")
    (add_net "Net-(U30-PadK13)")
    (add_net "Net-(U30-PadK3)")
    (add_net "Net-(U30-PadK5)")
    (add_net "Net-(U30-PadL13)")
    (add_net "Net-(U30-PadL14)")
    (add_net "Net-(U30-PadL2)")
    (add_net "Net-(U30-PadL4)")
    (add_net "Net-(U30-PadL5)")
    (add_net "Net-(U30-PadM1)")
    (add_net "Net-(U30-PadM12)")
    (add_net "Net-(U30-PadM15)")
    (add_net "Net-(U30-PadM16)")
    (add_net "Net-(U30-PadM2)")
    (add_net "Net-(U30-PadM4)")
    (add_net "Net-(U30-PadM5)")
    (add_net "Net-(U30-PadM6)")
    (add_net "Net-(U30-PadN1)")
    (add_net "Net-(U30-PadN12)")
    (add_net "Net-(U30-PadN13)")
    (add_net "Net-(U30-PadN16)")
    (add_net "Net-(U30-PadN2)")
    (add_net "Net-(U30-PadN3)")
    (add_net "Net-(U30-PadN4)")
    (add_net "Net-(U30-PadN6)")
    (add_net "Net-(U30-PadN9)")
    (add_net "Net-(U30-PadP10)")
    (add_net "Net-(U30-PadP11)")
    (add_net "Net-(U30-PadP13)")
    (add_net "Net-(U30-PadP14)")
    (add_net "Net-(U30-PadP15)")
    (add_net "Net-(U30-PadP3)")
    (add_net "Net-(U30-PadP4)")
    (add_net "Net-(U30-PadP5)")
    (add_net "Net-(U30-PadP6)")
    (add_net "Net-(U30-PadR10)")
    (add_net "Net-(U30-PadR11)")
    (add_net "Net-(U30-PadR12)")
    (add_net "Net-(U30-PadR13)")
    (add_net "Net-(U30-PadR15)")
    (add_net "Net-(U30-PadR2)")
    (add_net "Net-(U31-Pad4)")
    (add_net "Net-(U31-PadSH)")
    (add_net "Net-(U33-Pad11)")
    (add_net "Net-(U33-Pad12)")
    (add_net "Net-(U33-Pad13)")
    (add_net "Net-(U33-Pad15)")
    (add_net "Net-(U33-Pad16)")
    (add_net "Net-(U33-Pad17)")
    (add_net "Net-(U33-Pad19)")
    (add_net "Net-(U33-Pad20)")
    (add_net "Net-(U33-Pad41)")
    (add_net "Net-(U7-Pad22)")
  )
  (module VNA:C_0805b (layer F.Cu) (tedit 55A401FA)
    (at 153.97 117.65 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C272 (at 0 -1.675 270) (layer F.SilkS))
    (fp_text value DNP (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 403 "/receiver/RX switch/3V3"))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0805b (layer F.Cu) (tedit 55A401FA)
    (at 142.73 117.8 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C271 (at 0 -1.675 270) (layer F.SilkS))
    (fp_text value DNP (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 403 "/receiver/RX switch/3V3"))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 55A40188)
    (at 148.64 68.09 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C270 (at 0 -1.7 270) (layer F.SilkS))
    (fp_text value 1n (at 0 1.7 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 365 /PDET))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer F.Cu) (tedit 55A401B2)
    (at 153.49 61.29 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R122 (at 0 -1.4 90) (layer F.SilkS))
    (fp_text value 100 (at 0 1.8 90) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 365 /PDET))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 426 "Net-(R122-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:FTG256 (layer F.Cu) (tedit 5870D8C7)
    (at 136.675 68.25)
    (zone_connect 0)
    (fp_text reference U30 (at -7.175 9.47) (layer F.SilkS))
    (fp_text value XC7A15T-1FTG256C (at 0 -9) (layer F.Fab))
    (pad T16 smd circle (at 7.5 7.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (zone_connect 0))
    (pad R16 smd circle (at 7.5 6.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 138 /SOURCE_LD) (solder_mask_margin 0.05) (zone_connect 0))
    (pad P16 smd circle (at 7.5 5.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 132 /LO_LD) (solder_mask_margin 0.05) (zone_connect 0))
    (pad N16 smd circle (at 7.5 4.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 335 "Net-(U30-PadN16)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad M16 smd circle (at 7.5 3.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 334 "Net-(U30-PadM16)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad L16 smd circle (at 7.5 2.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 340 /3V3D) (solder_mask_margin 0.05) (zone_connect 0))
    (pad K16 smd circle (at 7.5 1.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 178 /DITHER) (solder_mask_margin 0.05) (zone_connect 0))
    (pad J16 smd circle (at 7.5 0.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 134 /LO_MUXOUT) (solder_mask_margin 0.05) (zone_connect 0))
    (pad H16 smd circle (at 7.5 -0.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 140 /SOURCE_MUXOUT) (solder_mask_margin 0.05) (zone_connect 0))
    (pad G16 smd circle (at 7.5 -1.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 333 "Net-(U30-PadG16)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad F16 smd circle (at 7.5 -2.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (zone_connect 0))
    (pad E16 smd circle (at 7.5 -3.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 174 /PORT_SW0) (solder_mask_margin 0.05) (zone_connect 0))
    (pad D16 smd circle (at 7.5 -4.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 173 /PORT_SW1) (solder_mask_margin 0.05) (zone_connect 0))
    (pad C16 smd circle (at 7.5 -5.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 328 /ATTEN_LE) (solder_mask_margin 0.05) (zone_connect 0))
    (pad B16 smd circle (at 7.5 -6.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 195 /FILTER_V2) (solder_mask_margin 0.05) (zone_connect 0))
    (pad A16 smd circle (at 7.5 -7.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 340 /3V3D) (solder_mask_margin 0.05) (zone_connect 0))
    (pad T15 smd circle (at 6.5 7.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 139 /SOURCE_RF_ENABLE) (solder_mask_margin 0.05) (zone_connect 0))
    (pad R15 smd circle (at 6.5 6.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 332 "Net-(U30-PadR15)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad P15 smd circle (at 6.5 5.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 331 "Net-(U30-PadP15)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad N15 smd circle (at 6.5 4.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (zone_connect 0))
    (pad M15 smd circle (at 6.5 3.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 330 "Net-(U30-PadM15)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad L15 smd circle (at 6.5 2.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 190 "Net-(R69-Pad2)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad K15 smd circle (at 6.5 1.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 135 /SOURCE_SPI_DATA) (solder_mask_margin 0.05) (zone_connect 0))
    (pad J15 smd circle (at 6.5 0.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 329 "Net-(U30-PadJ15)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad H15 smd circle (at 6.5 -0.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 340 /3V3D) (solder_mask_margin 0.05) (zone_connect 0))
    (pad G15 smd circle (at 6.5 -1.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 416 "Net-(U30-PadG15)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad F15 smd circle (at 6.5 -2.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 327 "Net-(U30-PadF15)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad E15 smd circle (at 6.5 -3.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 326 "Net-(U30-PadE15)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad D15 smd circle (at 6.5 -4.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 325 "Net-(U30-PadD15)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad C15 smd circle (at 6.5 -5.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (zone_connect 0))
    (pad B15 smd circle (at 6.5 -6.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 320 /ATTEN_SPI_DATA) (solder_mask_margin 0.05) (zone_connect 0))
    (pad A15 smd circle (at 6.5 -7.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 194 /FILTER_V1) (solder_mask_margin 0.05) (zone_connect 0))
    (pad T14 smd circle (at 5.5 7.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 133 /LO_RF_ENABLE) (solder_mask_margin 0.05) (zone_connect 0))
    (pad R14 smd circle (at 5.5 6.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 340 /3V3D) (solder_mask_margin 0.05) (zone_connect 0))
    (pad P14 smd circle (at 5.5 5.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 324 "Net-(U30-PadP14)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad N14 smd circle (at 5.5 4.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 418 "Net-(R130-Pad1)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad M14 smd circle (at 5.5 3.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 127 /LO_SPI_DATA) (solder_mask_margin 0.05) (zone_connect 0))
    (pad L14 smd circle (at 5.5 2.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 323 "Net-(U30-PadL14)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad K14 smd circle (at 5.5 1.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (zone_connect 0))
    (pad J14 smd circle (at 5.5 0.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 395 /fpga/SPI_DIN) (solder_mask_margin 0.05) (zone_connect 0))
    (pad H14 smd circle (at 5.5 -0.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 322 "Net-(U30-PadH14)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad G14 smd circle (at 5.5 -1.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 128 /LO_LE) (solder_mask_margin 0.05) (zone_connect 0))
    (pad F14 smd circle (at 5.5 -2.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 129 /LO_CE) (solder_mask_margin 0.05) (zone_connect 0))
    (pad E14 smd circle (at 5.5 -3.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 340 /3V3D) (solder_mask_margin 0.05) (zone_connect 0))
    (pad D14 smd circle (at 5.5 -4.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 321 "Net-(U30-PadD14)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad C14 smd circle (at 5.5 -5.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 417 "Net-(U30-PadC14)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad B14 smd circle (at 5.5 -6.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 319 "Net-(U30-PadB14)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad A14 smd circle (at 5.5 -7.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 197 /FILTER_V3) (solder_mask_margin 0.05) (zone_connect 0))
    (pad T13 smd circle (at 4.5 7.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 362 /fpga/ADC_SHDN) (solder_mask_margin 0.05) (zone_connect 0))
    (pad R13 smd circle (at 4.5 6.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 318 "Net-(U30-PadR13)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad P13 smd circle (at 4.5 5.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 317 "Net-(U30-PadP13)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad N13 smd circle (at 4.5 4.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 316 "Net-(U30-PadN13)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad M13 smd circle (at 4.5 3.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 340 /3V3D) (solder_mask_margin 0.05) (zone_connect 0))
    (pad L13 smd circle (at 4.5 2.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 315 "Net-(U30-PadL13)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad K13 smd circle (at 4.5 1.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 314 "Net-(U30-PadK13)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad J13 smd circle (at 4.5 0.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 396 /fpga/SPI_MOSI) (solder_mask_margin 0.05) (zone_connect 0))
    (pad H13 smd circle (at 4.5 -0.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 313 "Net-(U30-PadH13)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad G13 smd circle (at 4.5 -1.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (zone_connect 0))
    (pad F13 smd circle (at 4.5 -2.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 137 /SOURCE_CE) (solder_mask_margin 0.05) (zone_connect 0))
    (pad E13 smd circle (at 4.5 -3.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 312 "Net-(U30-PadE13)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad D13 smd circle (at 4.5 -4.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 311 "Net-(U30-PadD13)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad C13 smd circle (at 4.5 -5.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 310 "Net-(U30-PadC13)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad B13 smd circle (at 4.5 -6.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 340 /3V3D) (solder_mask_margin 0.05) (zone_connect 0))
    (pad A13 smd circle (at 4.5 -7.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 196 /FILTER_V4) (solder_mask_margin 0.05) (zone_connect 0))
    (pad T12 smd circle (at 3.5 7.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 361 /fpga/ADC_OE) (solder_mask_margin 0.05) (zone_connect 0))
    (pad R12 smd circle (at 3.5 6.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 309 "Net-(U30-PadR12)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad P12 smd circle (at 3.5 5.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (zone_connect 0))
    (pad N12 smd circle (at 3.5 4.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 308 "Net-(U30-PadN12)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad M12 smd circle (at 3.5 3.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 307 "Net-(U30-PadM12)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad L12 smd circle (at 3.5 2.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 400 /fpga/SPI_CS) (solder_mask_margin 0.05) (zone_connect 0))
    (pad K12 smd circle (at 3.5 1.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 306 "Net-(U30-PadK12)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad J12 smd circle (at 3.5 0.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 340 /3V3D) (solder_mask_margin 0.05) (zone_connect 0))
    (pad H12 smd circle (at 3.5 -0.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 305 "Net-(U30-PadH12)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad G12 smd circle (at 3.5 -1.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 304 "Net-(U30-PadG12)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad F12 smd circle (at 3.5 -2.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 136 /SOURCE_LE) (solder_mask_margin 0.05) (zone_connect 0))
    (pad E12 smd circle (at 3.5 -3.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 303 "Net-(U30-PadE12)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad D12 smd circle (at 3.5 -4.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (zone_connect 0))
    (pad C12 smd circle (at 3.5 -5.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 302 "Net-(U30-PadC12)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad B12 smd circle (at 3.5 -6.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 301 /fpga/FT_D1) (solder_mask_margin 0.05) (zone_connect 0))
    (pad A12 smd circle (at 3.5 -7.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 300 /fpga/FT_D0) (solder_mask_margin 0.05) (zone_connect 0))
    (pad T11 smd circle (at 2.5 7.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 340 /3V3D) (solder_mask_margin 0.05) (zone_connect 0))
    (pad R11 smd circle (at 2.5 6.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 299 "Net-(U30-PadR11)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad P11 smd circle (at 2.5 5.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 298 "Net-(U30-PadP11)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad N11 smd circle (at 2.5 4.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 297 /CLK_FPGA) (solder_mask_margin 0.05) (zone_connect 0))
    (pad M11 smd circle (at 2.5 3.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 399 /fpga/M2) (solder_mask_margin 0.05) (zone_connect 0))
    (pad L11 smd circle (at 2.5 2.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (zone_connect 0))
    (pad K11 smd circle (at 2.5 1.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 199 /1V8) (solder_mask_margin 0.05) (zone_connect 0))
    (pad J11 smd circle (at 2.5 0.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (zone_connect 0))
    (pad H11 smd circle (at 2.5 -0.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 296 "Net-(U30-PadH11)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad G11 smd circle (at 2.5 -1.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 295 "Net-(U30-PadG11)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad F11 smd circle (at 2.5 -2.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 368 /1V0) (solder_mask_margin 0.05) (zone_connect 0))
    (pad E11 smd circle (at 2.5 -3.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 294 "Net-(U30-PadE11)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad D11 smd circle (at 2.5 -4.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 293 "Net-(U30-PadD11)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad C11 smd circle (at 2.5 -5.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 292 "Net-(U30-PadC11)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad B11 smd circle (at 2.5 -6.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 291 /fpga/FT_D2) (solder_mask_margin 0.05) (zone_connect 0))
    (pad A11 smd circle (at 2.5 -7.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (zone_connect 0))
    (pad T10 smd circle (at 1.5 7.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 262 /fpga/D0) (solder_mask_margin 0.05) (zone_connect 0))
    (pad R10 smd circle (at 1.5 6.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 289 "Net-(U30-PadR10)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad P10 smd circle (at 1.5 5.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 288 "Net-(U30-PadP10)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad N10 smd circle (at 1.5 4.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 340 /3V3D) (solder_mask_margin 0.05) (zone_connect 0))
    (pad M10 smd circle (at 1.5 3.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 401 /fpga/M1) (solder_mask_margin 0.05) (zone_connect 0))
    (pad L10 smd circle (at 1.5 2.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 199 /1V8) (solder_mask_margin 0.05) (zone_connect 0))
    (pad K10 smd circle (at 1.5 1.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 398 /fpga/INIT_B) (solder_mask_margin 0.05) (zone_connect 0))
    (pad J10 smd circle (at 1.5 0.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 199 /1V8) (solder_mask_margin 0.05) (zone_connect 0))
    (pad H10 smd circle (at 1.5 -0.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 394 "Net-(P9-Pad1)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad G10 smd circle (at 1.5 -1.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 199 /1V8) (solder_mask_margin 0.05) (zone_connect 0))
    (pad F10 smd circle (at 1.5 -2.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (zone_connect 0))
    (pad E10 smd circle (at 1.5 -3.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 368 /1V0) (solder_mask_margin 0.05) (zone_connect 0))
    (pad D10 smd circle (at 1.5 -4.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 287 "Net-(U30-PadD10)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad C10 smd circle (at 1.5 -5.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 340 /3V3D) (solder_mask_margin 0.05) (zone_connect 0))
    (pad B10 smd circle (at 1.5 -6.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 286 /fpga/FT_D3) (solder_mask_margin 0.05) (zone_connect 0))
    (pad A10 smd circle (at 1.5 -7.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 285 /fpga/FT_D5) (solder_mask_margin 0.05) (zone_connect 0))
    (pad T9 smd circle (at 0.5 7.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 268 /fpga/D1) (solder_mask_margin 0.05) (zone_connect 0))
    (pad R9 smd circle (at 0.5 6.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (zone_connect 0))
    (pad P9 smd circle (at 0.5 5.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 263 /fpga/D2) (solder_mask_margin 0.05) (zone_connect 0))
    (pad N9 smd circle (at 0.5 4.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 282 "Net-(U30-PadN9)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad M9 smd circle (at 0.5 3.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 397 /fpga/M0) (solder_mask_margin 0.05) (zone_connect 0))
    (pad L9 smd circle (at 0.5 2.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 402 /fpga/PROGRAM_B) (solder_mask_margin 0.05) (zone_connect 0))
    (pad K9 smd circle (at 0.5 1.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 368 /1V0) (solder_mask_margin 0.05) (zone_connect 0))
    (pad J9 smd circle (at 0.5 0.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (zone_connect 0))
    (pad H9 smd circle (at 0.5 -0.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 368 /1V0) (solder_mask_margin 0.05) (zone_connect 0))
    (pad G9 smd circle (at 0.5 -1.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (zone_connect 0))
    (pad F9 smd circle (at 0.5 -2.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 368 /1V0) (solder_mask_margin 0.05) (zone_connect 0))
    (pad E9 smd circle (at 0.5 -3.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (zone_connect 0))
    (pad D9 smd circle (at 0.5 -4.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 281 "Net-(U30-PadD9)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad C9 smd circle (at 0.5 -5.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 280 "Net-(U30-PadC9)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad B9 smd circle (at 0.5 -6.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 279 /fpga/FT_D4) (solder_mask_margin 0.05) (zone_connect 0))
    (pad A9 smd circle (at 0.5 -7.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 278 /fpga/FT_D6) (solder_mask_margin 0.05) (zone_connect 0))
    (pad T8 smd circle (at -0.5 7.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 290 /fpga/D5) (solder_mask_margin 0.05) (zone_connect 0))
    (pad R8 smd circle (at -0.5 6.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 254 /fpga/D4) (solder_mask_margin 0.05) (zone_connect 0))
    (pad P8 smd circle (at -0.5 5.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 255 /fpga/D3) (solder_mask_margin 0.05) (zone_connect 0))
    (pad N8 smd circle (at -0.5 4.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 274 /fpga/TDO) (solder_mask_margin 0.05) (zone_connect 0))
    (pad M8 smd circle (at -0.5 3.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (zone_connect 0))
    (pad L8 smd circle (at -0.5 2.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 368 /1V0) (solder_mask_margin 0.05) (zone_connect 0))
    (pad K8 smd circle (at -0.5 1.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (zone_connect 0))
    (pad J8 smd circle (at -0.5 0.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (zone_connect 0))
    (pad H8 smd circle (at -0.5 -0.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 365 /PDET) (solder_mask_margin 0.05) (zone_connect 0))
    (pad G8 smd circle (at -0.5 -1.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 273 "Net-(C205-Pad1)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad F8 smd circle (at -0.5 -2.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (zone_connect 0))
    (pad E8 smd circle (at -0.5 -3.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 393 /fpga/CCLK) (solder_mask_margin 0.05) (zone_connect 0))
    (pad D8 smd circle (at -0.5 -4.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 272 "Net-(U30-PadD8)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad C8 smd circle (at -0.5 -5.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 271 "Net-(U30-PadC8)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad B8 smd circle (at -0.5 -6.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (zone_connect 0))
    (pad A8 smd circle (at -0.5 -7.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 270 /fpga/FT_D7) (solder_mask_margin 0.05) (zone_connect 0))
    (pad T7 smd circle (at -1.5 7.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 277 /fpga/D7) (solder_mask_margin 0.05) (zone_connect 0))
    (pad R7 smd circle (at -1.5 6.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 284 /fpga/D6) (solder_mask_margin 0.05) (zone_connect 0))
    (pad P7 smd circle (at -1.5 5.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 340 /3V3D) (solder_mask_margin 0.05) (zone_connect 0))
    (pad N7 smd circle (at -1.5 4.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 187 /fpga/TDI) (solder_mask_margin 0.05) (zone_connect 0))
    (pad M7 smd circle (at -1.5 3.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 192 /fpga/TMS) (solder_mask_margin 0.05) (zone_connect 0))
    (pad L7 smd circle (at -1.5 2.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 183 /fpga/TCK) (solder_mask_margin 0.05) (zone_connect 0))
    (pad K7 smd circle (at -1.5 1.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (zone_connect 0))
    (pad J7 smd circle (at -1.5 0.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (zone_connect 0))
    (pad H7 smd circle (at -1.5 -0.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (zone_connect 0))
    (pad G7 smd circle (at -1.5 -1.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 267 "Net-(C205-Pad2)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad F7 smd circle (at -1.5 -2.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 368 /1V0) (solder_mask_margin 0.05) (zone_connect 0))
    (pad E7 smd circle (at -1.5 -3.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 340 /3V3D) (solder_mask_margin 0.05) (zone_connect 0))
    (pad D7 smd circle (at -1.5 -4.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 340 /3V3D) (solder_mask_margin 0.05) (zone_connect 0))
    (pad C7 smd circle (at -1.5 -5.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 266 "Net-(U30-PadC7)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad B7 smd circle (at -1.5 -6.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 265 "Net-(U30-PadB7)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad A7 smd circle (at -1.5 -7.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 264 "Net-(U30-PadA7)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad T6 smd circle (at -2.5 7.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (zone_connect 0))
    (pad R6 smd circle (at -2.5 6.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 269 /fpga/D8) (solder_mask_margin 0.05) (zone_connect 0))
    (pad P6 smd circle (at -2.5 5.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 407 "Net-(U30-PadP6)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad N6 smd circle (at -2.5 4.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 408 "Net-(U30-PadN6)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad M6 smd circle (at -2.5 3.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 409 "Net-(U30-PadM6)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad L6 smd circle (at -2.5 2.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 340 /3V3D) (solder_mask_margin 0.05) (zone_connect 0))
    (pad K6 smd circle (at -2.5 1.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (zone_connect 0))
    (pad J6 smd circle (at -2.5 0.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 368 /1V0) (solder_mask_margin 0.05) (zone_connect 0))
    (pad H6 smd circle (at -2.5 -0.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (zone_connect 0))
    (pad G6 smd circle (at -2.5 -1.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 368 /1V0) (solder_mask_margin 0.05) (zone_connect 0))
    (pad F6 smd circle (at -2.5 -2.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (zone_connect 0))
    (pad E6 smd circle (at -2.5 -3.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 259 "Net-(U30-PadE6)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad D6 smd circle (at -2.5 -4.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 258 "Net-(U30-PadD6)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad C6 smd circle (at -2.5 -5.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 257 "Net-(U30-PadC6)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad B6 smd circle (at -2.5 -6.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 256 "Net-(U30-PadB6)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad A6 smd circle (at -2.5 -7.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 340 /3V3D) (solder_mask_margin 0.05) (zone_connect 0))
    (pad T5 smd circle (at -3.5 7.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 276 /fpga/D9) (solder_mask_margin 0.05) (zone_connect 0))
    (pad R5 smd circle (at -3.5 6.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 275 /fpga/D10) (solder_mask_margin 0.05) (zone_connect 0))
    (pad P5 smd circle (at -3.5 5.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 253 "Net-(U30-PadP5)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad N5 smd circle (at -3.5 4.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (zone_connect 0))
    (pad M5 smd circle (at -3.5 3.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 252 "Net-(U30-PadM5)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad L5 smd circle (at -3.5 2.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 251 "Net-(U30-PadL5)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad K5 smd circle (at -3.5 1.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 250 "Net-(U30-PadK5)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad J5 smd circle (at -3.5 0.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 249 "Net-(U30-PadJ5)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad H5 smd circle (at -3.5 -0.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 248 "Net-(U30-PadH5)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad G5 smd circle (at -3.5 -1.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 247 "Net-(U30-PadG5)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad F5 smd circle (at -3.5 -2.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 246 "Net-(U30-PadF5)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad E5 smd circle (at -3.5 -3.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 245 "Net-(U30-PadE5)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad D5 smd circle (at -3.5 -4.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 244 "Net-(U30-PadD5)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad C5 smd circle (at -3.5 -5.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (zone_connect 0))
    (pad B5 smd circle (at -3.5 -6.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 243 "Net-(U30-PadB5)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad A5 smd circle (at -3.5 -7.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 242 /fpga/SI/WUB) (solder_mask_margin 0.05) (zone_connect 0))
    (pad T4 smd circle (at -4.5 7.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 261 /fpga/D11) (solder_mask_margin 0.05) (zone_connect 0))
    (pad R4 smd circle (at -4.5 6.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 340 /3V3D) (solder_mask_margin 0.05) (zone_connect 0))
    (pad P4 smd circle (at -4.5 5.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 241 "Net-(U30-PadP4)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad N4 smd circle (at -4.5 4.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 240 "Net-(U30-PadN4)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad M4 smd circle (at -4.5 3.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 239 "Net-(U30-PadM4)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad L4 smd circle (at -4.5 2.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 238 "Net-(U30-PadL4)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad K4 smd circle (at -4.5 1.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (zone_connect 0))
    (pad J4 smd circle (at -4.5 0.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 237 "Net-(U30-PadJ4)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad H4 smd circle (at -4.5 -0.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 236 "Net-(U30-PadH4)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad G4 smd circle (at -4.5 -1.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 235 "Net-(U30-PadG4)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad F4 smd circle (at -4.5 -2.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 234 "Net-(U30-PadF4)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad E4 smd circle (at -4.5 -3.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 340 /3V3D) (solder_mask_margin 0.05) (zone_connect 0))
    (pad D4 smd circle (at -4.5 -4.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 233 "Net-(U30-PadD4)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad C4 smd circle (at -4.5 -5.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 232 "Net-(U30-PadC4)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad B4 smd circle (at -4.5 -6.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 231 /fpga/RD#) (solder_mask_margin 0.05) (zone_connect 0))
    (pad A4 smd circle (at -4.5 -7.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 230 /fpga/WR) (solder_mask_margin 0.05) (zone_connect 0))
    (pad T3 smd circle (at -5.5 7.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 260 /fpga/D12) (solder_mask_margin 0.05) (zone_connect 0))
    (pad R3 smd circle (at -5.5 6.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 283 /fpga/D13) (solder_mask_margin 0.05) (zone_connect 0))
    (pad P3 smd circle (at -5.5 5.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 229 "Net-(U30-PadP3)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad N3 smd circle (at -5.5 4.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 228 "Net-(U30-PadN3)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad M3 smd circle (at -5.5 3.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 340 /3V3D) (solder_mask_margin 0.05) (zone_connect 0))
    (pad L3 smd circle (at -5.5 2.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 189 /PWDN) (solder_mask_margin 0.05) (zone_connect 0))
    (pad K3 smd circle (at -5.5 1.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 227 "Net-(U30-PadK3)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad J3 smd circle (at -5.5 0.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 226 "Net-(U30-PadJ3)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad H3 smd circle (at -5.5 -0.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 225 "Net-(U30-PadH3)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad G3 smd circle (at -5.5 -1.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (zone_connect 0))
    (pad F3 smd circle (at -5.5 -2.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 224 "Net-(U30-PadF3)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad E3 smd circle (at -5.5 -3.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 223 "Net-(U30-PadE3)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad D3 smd circle (at -5.5 -4.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 222 "Net-(U30-PadD3)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad C3 smd circle (at -5.5 -5.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 221 "Net-(U30-PadC3)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad B3 smd circle (at -5.5 -6.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 340 /3V3D) (solder_mask_margin 0.05) (zone_connect 0))
    (pad A3 smd circle (at -5.5 -7.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 220 /fpga/TXE#) (solder_mask_margin 0.05) (zone_connect 0))
    (pad T2 smd circle (at -6.5 7.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 360 /fpga/OF) (solder_mask_margin 0.05) (zone_connect 0))
    (pad R2 smd circle (at -6.5 6.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 219 "Net-(U30-PadR2)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad P2 smd circle (at -6.5 5.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (zone_connect 0))
    (pad N2 smd circle (at -6.5 4.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 218 "Net-(U30-PadN2)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad M2 smd circle (at -6.5 3.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 217 "Net-(U30-PadM2)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad L2 smd circle (at -6.5 2.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 216 "Net-(U30-PadL2)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad K2 smd circle (at -6.5 1.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 215 /MIXER_ENABLE) (solder_mask_margin 0.05) (zone_connect 0))
    (pad J2 smd circle (at -6.5 0.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 340 /3V3D) (solder_mask_margin 0.05) (zone_connect 0))
    (pad H2 smd circle (at -6.5 -0.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 214 /RX_SW2) (solder_mask_margin 0.05) (zone_connect 0))
    (pad G2 smd circle (at -6.5 -1.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 213 /RX_SW3) (solder_mask_margin 0.05) (zone_connect 0))
    (pad F2 smd circle (at -6.5 -2.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 212 "Net-(U30-PadF2)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad E2 smd circle (at -6.5 -3.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 211 "Net-(U30-PadE2)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad D2 smd circle (at -6.5 -4.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (zone_connect 0))
    (pad C2 smd circle (at -6.5 -5.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 210 "Net-(U30-PadC2)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad B2 smd circle (at -6.5 -6.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 209 "Net-(U30-PadB2)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad A2 smd circle (at -6.5 -7.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 208 /fpga/RXF#) (solder_mask_margin 0.05) (zone_connect 0))
    (pad T1 smd circle (at -7.5 7.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 340 /3V3D) (solder_mask_margin 0.05) (zone_connect 0))
    (pad R1 smd circle (at -7.5 6.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 423 "Net-(P27-Pad1)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad P1 smd circle (at -7.5 5.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 424 "Net-(P26-Pad1)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad N1 smd circle (at -7.5 4.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 207 "Net-(U30-PadN1)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad M1 smd circle (at -7.5 3.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 206 "Net-(U30-PadM1)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad L1 smd circle (at -7.5 2.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (zone_connect 0))
    (pad K1 smd circle (at -7.5 1.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 205 /RX_SW0) (solder_mask_margin 0.05) (zone_connect 0))
    (pad J1 smd circle (at -7.5 0.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 204 /RX_SW1) (solder_mask_margin 0.05) (zone_connect 0))
    (pad H1 smd circle (at -7.5 -0.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 203 /RX_SW4) (solder_mask_margin 0.05) (zone_connect 0))
    (pad G1 smd circle (at -7.5 -1.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 202 /RX_SW5) (solder_mask_margin 0.05) (zone_connect 0))
    (pad F1 smd circle (at -7.5 -2.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 340 /3V3D) (solder_mask_margin 0.05) (zone_connect 0))
    (pad E1 smd circle (at -7.5 -3.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 425 "Net-(P28-Pad1)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad D1 smd circle (at -7.5 -4.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 390 /fpga/LED) (solder_mask_margin 0.05) (zone_connect 0))
    (pad C1 smd circle (at -7.5 -5.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 201 "Net-(U30-PadC1)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad B1 smd circle (at -7.5 -6.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 200 "Net-(U30-PadB1)") (solder_mask_margin 0.05) (zone_connect 0))
    (pad A1 smd circle (at -7.5 -7.5) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (zone_connect 0))
  )
  (module VNA:C_0805b (layer F.Cu) (tedit 55A401FA)
    (at 118.3 100.88 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C269 (at 0 -1.675 90) (layer F.SilkS))
    (fp_text value DNP (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 56 /power/12V))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0805b (layer F.Cu) (tedit 55A401FA)
    (at 119.53 100.87 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C268 (at 0 -1.675 90) (layer F.SilkS))
    (fp_text value DNP (at 0 2.1 90) (layer F.Fab))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 56 /power/12V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0805b (layer F.Cu) (tedit 55A401FA)
    (at 119.54 104.07 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C267 (at 0 -1.675 270) (layer F.SilkS))
    (fp_text value DNP (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 56 /power/12V))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:TP_1.00 (layer F.Cu) (tedit 55A404EB)
    (at 126.76 65.51)
    (fp_text reference P28 (at 0.125 0.05) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 -0.5) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 425 "Net-(P28-Pad1)"))
  )
  (module Housings_DFN_QFN:DFN-S-8-1EP_6x5mm_Pitch1.27mm (layer F.Cu) (tedit 5870D99E)
    (at 152.8 43.915)
    (descr "8-Lead Plastic Dual Flat, No Lead Package (MF) - 6x5 mm Body [DFN-S] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "DFN 1.27")
    (attr smd)
    (fp_text reference U40 (at 0.84 -4.085) (layer F.SilkS))
    (fp_text value W25Q32JV (at 0 3.575) (layer F.Fab))
    (pad 9 smd rect (at -0.6 -1.5375) (size 1.2 1.025) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (pad 9 smd rect (at -0.6 -0.5125) (size 1.2 1.025) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (pad 9 smd rect (at -0.6 0.512499) (size 1.2 1.025) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (pad 9 smd rect (at -0.6 1.5375) (size 1.2 1.025) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (pad 9 smd rect (at 0.6 -1.5375) (size 1.2 1.025) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (pad 9 smd rect (at 0.6 -0.5125) (size 1.2 1.025) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (pad 9 smd rect (at 0.6 0.512499) (size 1.2 1.025) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (pad 9 smd rect (at 0.6 1.5375) (size 1.2 1.025) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (pad 8 smd oval (at 2.8 -1.905) (size 1.1 0.45) (layers F.Cu F.Paste F.Mask)
      (net 340 /3V3D))
    (pad 7 smd oval (at 2.8 -0.635) (size 1.1 0.45) (layers F.Cu F.Paste F.Mask)
      (net 340 /3V3D))
    (pad 6 smd oval (at 2.8 0.635) (size 1.1 0.45) (layers F.Cu F.Paste F.Mask)
      (net 393 /fpga/CCLK))
    (pad 5 smd oval (at 2.8 1.905) (size 1.1 0.45) (layers F.Cu F.Paste F.Mask)
      (net 396 /fpga/SPI_MOSI))
    (pad 4 smd oval (at -2.8 1.905) (size 1.1 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd oval (at -2.8 0.635) (size 1.1 0.45) (layers F.Cu F.Paste F.Mask)
      (net 340 /3V3D))
    (pad 2 smd oval (at -2.8 -0.635) (size 1.1 0.45) (layers F.Cu F.Paste F.Mask)
      (net 395 /fpga/SPI_DIN))
    (pad 1 smd oval (at -2.8 -1.905) (size 1.1 0.45) (layers F.Cu F.Paste F.Mask)
      (net 400 /fpga/SPI_CS))
    (model Housings_DFN_QFN.3dshapes/DFN-S-8-1EP_6x5mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:RF_via (layer F.Cu) (tedit 5883112F)
    (at 170.955 71.225)
    (fp_text reference F19 (at 0.1 1) (layer F.SilkS) hide)
    (fp_text value Via (at 0 -1.5) (layer F.Fab))
    (pad 2 thru_hole circle (at -0.75 0) (size 0.55 0.55) (drill 0.26) (layers *.Cu F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 0.75 0) (size 0.55 0.55) (drill 0.26) (layers *.Cu F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 0 0) (size 0.55 0.55) (drill 0.26) (layers *.Cu F.Mask)
      (net 185 /CLK_LO))
  )
  (module VNA:RF_via (layer F.Cu) (tedit 5883112F)
    (at 172.56 67.75)
    (fp_text reference F20 (at 0.1 1) (layer F.SilkS) hide)
    (fp_text value Via (at 0 -1.5) (layer F.Fab))
    (pad 2 thru_hole circle (at -0.75 0) (size 0.55 0.55) (drill 0.26) (layers *.Cu F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 0.75 0) (size 0.55 0.55) (drill 0.26) (layers *.Cu F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 0 0) (size 0.55 0.55) (drill 0.26) (layers *.Cu F.Mask)
      (net 185 /CLK_LO))
  )
  (module VNA:RF_via (layer F.Cu) (tedit 5883112F)
    (at 135.8 117.25)
    (fp_text reference F12 (at 0.1 1) (layer F.SilkS) hide)
    (fp_text value Via (at 0 -1.5) (layer F.Fab))
    (pad 2 thru_hole circle (at -0.75 0) (size 0.55 0.55) (drill 0.26) (layers *.Cu F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 0.75 0) (size 0.55 0.55) (drill 0.26) (layers *.Cu F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 0 0) (size 0.55 0.55) (drill 0.26) (layers *.Cu F.Mask)
      (net 348 /B))
  )
  (module VNA:RF_via (layer F.Cu) (tedit 5883112F)
    (at 145.375 114.4 45)
    (fp_text reference F7 (at 0.1 1 45) (layer F.SilkS) hide)
    (fp_text value Via (at 0 -1.5 45) (layer F.Fab))
    (pad 2 thru_hole circle (at -0.75 0 45) (size 0.55 0.55) (drill 0.26) (layers *.Cu F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 0.75 0 45) (size 0.55 0.55) (drill 0.26) (layers *.Cu F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 0 0 45) (size 0.55 0.55) (drill 0.26) (layers *.Cu F.Mask)
      (net 345 /RX2))
  )
  (module VNA:RF_via (layer F.Cu) (tedit 5883112F)
    (at 137.325 114.425 135)
    (fp_text reference F8 (at 0.1 1 135) (layer F.SilkS) hide)
    (fp_text value Via (at 0 -1.5 135) (layer F.Fab))
    (pad 2 thru_hole circle (at -0.75 0 135) (size 0.55 0.55) (drill 0.26) (layers *.Cu F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 0.75 0 135) (size 0.55 0.55) (drill 0.26) (layers *.Cu F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 0 0 135) (size 0.55 0.55) (drill 0.26) (layers *.Cu F.Mask)
      (net 348 /B))
  )
  (module VNA:RF_via (layer F.Cu) (tedit 5883112F)
    (at 169.03 117.22)
    (fp_text reference F9 (at 0.1 1) (layer F.SilkS) hide)
    (fp_text value Via (at 0 -1.5) (layer F.Fab))
    (pad 2 thru_hole circle (at -0.75 0) (size 0.55 0.55) (drill 0.26) (layers *.Cu F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 0.75 0) (size 0.55 0.55) (drill 0.26) (layers *.Cu F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 0 0) (size 0.55 0.55) (drill 0.26) (layers *.Cu F.Mask)
      (net 347 /RX1))
  )
  (module VNA:RF_via (layer F.Cu) (tedit 5883112F)
    (at 147 117.275)
    (fp_text reference F11 (at 0.1 1) (layer F.SilkS) hide)
    (fp_text value Via (at 0 -1.5) (layer F.Fab))
    (pad 2 thru_hole circle (at -0.75 0) (size 0.55 0.55) (drill 0.26) (layers *.Cu F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 0.75 0) (size 0.55 0.55) (drill 0.26) (layers *.Cu F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 0 0) (size 0.55 0.55) (drill 0.26) (layers *.Cu F.Mask)
      (net 345 /RX2))
  )
  (module VNA:RF_via (layer F.Cu) (tedit 5883112F)
    (at 141.375 110.425)
    (fp_text reference F16 (at 0.1 1) (layer F.SilkS) hide)
    (fp_text value Via (at 0 -1.5) (layer F.Fab))
    (pad 2 thru_hole circle (at -0.75 0) (size 0.55 0.55) (drill 0.26) (layers *.Cu F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 0.75 0) (size 0.55 0.55) (drill 0.26) (layers *.Cu F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 0 0) (size 0.55 0.55) (drill 0.26) (layers *.Cu F.Mask)
      (net 411 "Net-(F16-Pad1)"))
  )
  (module VNA:RF_via (layer F.Cu) (tedit 5883112F)
    (at 167.975 114.225 45)
    (fp_text reference F13 (at 0.1 1 45) (layer F.SilkS) hide)
    (fp_text value Via (at 0 -1.5 45) (layer F.Fab))
    (pad 2 thru_hole circle (at -0.75 0 45) (size 0.55 0.55) (drill 0.26) (layers *.Cu F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 0.75 0 45) (size 0.55 0.55) (drill 0.26) (layers *.Cu F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 0 0 45) (size 0.55 0.55) (drill 0.26) (layers *.Cu F.Mask)
      (net 347 /RX1))
  )
  (module VNA:RF_via (layer F.Cu) (tedit 5883112F)
    (at 158.3 117.2)
    (fp_text reference F14 (at 0.1 1) (layer F.SilkS) hide)
    (fp_text value Via (at 0 -1.5) (layer F.Fab))
    (pad 2 thru_hole circle (at -0.75 0) (size 0.55 0.55) (drill 0.26) (layers *.Cu F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 0.75 0) (size 0.55 0.55) (drill 0.26) (layers *.Cu F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 0 0) (size 0.55 0.55) (drill 0.26) (layers *.Cu F.Mask)
      (net 346 /A))
  )
  (module VNA:RF_via (layer F.Cu) (tedit 5883112F)
    (at 150.025 112.575 270)
    (fp_text reference F18 (at 0.1 1 270) (layer F.SilkS) hide)
    (fp_text value Via (at 0 -1.5 270) (layer F.Fab))
    (pad 2 thru_hole circle (at -0.75 0 270) (size 0.55 0.55) (drill 0.26) (layers *.Cu F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 0.75 0 270) (size 0.55 0.55) (drill 0.26) (layers *.Cu F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 0 0 270) (size 0.55 0.55) (drill 0.26) (layers *.Cu F.Mask)
      (net 411 "Net-(F16-Pad1)"))
  )
  (module VNA:RF_via (layer F.Cu) (tedit 5883112F)
    (at 155.275 112.6 90)
    (fp_text reference F15 (at 0.1 1 90) (layer F.SilkS) hide)
    (fp_text value Via (at 0 -1.5 90) (layer F.Fab))
    (pad 2 thru_hole circle (at -0.75 0 90) (size 0.55 0.55) (drill 0.26) (layers *.Cu F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 0.75 0 90) (size 0.55 0.55) (drill 0.26) (layers *.Cu F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 0 0 90) (size 0.55 0.55) (drill 0.26) (layers *.Cu F.Mask)
      (net 410 "Net-(F15-Pad1)"))
  )
  (module VNA:RF_via (layer F.Cu) (tedit 5883112F)
    (at 164.15 110.275)
    (fp_text reference F17 (at 0.1 1) (layer F.SilkS) hide)
    (fp_text value Via (at 0 -1.5) (layer F.Fab))
    (pad 2 thru_hole circle (at -0.75 0) (size 0.55 0.55) (drill 0.26) (layers *.Cu F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 0.75 0) (size 0.55 0.55) (drill 0.26) (layers *.Cu F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 0 0) (size 0.55 0.55) (drill 0.26) (layers *.Cu F.Mask)
      (net 410 "Net-(F15-Pad1)"))
  )
  (module VNA:RF_via (layer F.Cu) (tedit 5883112F)
    (at 160.25 114.225 135)
    (fp_text reference F10 (at 0.1 1 135) (layer F.SilkS) hide)
    (fp_text value Via (at 0 -1.5 135) (layer F.Fab))
    (pad 2 thru_hole circle (at -0.75 0 135) (size 0.55 0.55) (drill 0.26) (layers *.Cu F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 0.75 0 135) (size 0.55 0.55) (drill 0.26) (layers *.Cu F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 0 0 135) (size 0.55 0.55) (drill 0.26) (layers *.Cu F.Mask)
      (net 346 /A))
  )
  (module VNA:RF_via (layer F.Cu) (tedit 5883112F)
    (at 152.75 109.95)
    (fp_text reference F5 (at 0.1 1) (layer F.SilkS) hide)
    (fp_text value Via (at 0 -1.5) (layer F.Fab))
    (pad 2 thru_hole circle (at -0.75 0) (size 0.55 0.55) (drill 0.26) (layers *.Cu F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 0.75 0) (size 0.55 0.55) (drill 0.26) (layers *.Cu F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 0 0) (size 0.55 0.55) (drill 0.26) (layers *.Cu F.Mask)
      (net 46 /receiver/RF_IN))
  )
  (module VNA:RF_via (layer F.Cu) (tedit 5883112F)
    (at 158.9 104.85 90)
    (fp_text reference F6 (at 0.1 1 90) (layer F.SilkS) hide)
    (fp_text value Via (at 0 -1.5 90) (layer F.Fab))
    (pad 2 thru_hole circle (at -0.75 0 90) (size 0.55 0.55) (drill 0.26) (layers *.Cu F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 0.75 0 90) (size 0.55 0.55) (drill 0.26) (layers *.Cu F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 0 0 90) (size 0.55 0.55) (drill 0.26) (layers *.Cu F.Mask)
      (net 46 /receiver/RF_IN))
  )
  (module VNA:RF_via (layer F.Cu) (tedit 5883112F)
    (at 178.06 107.82)
    (fp_text reference F3 (at 0.1 1) (layer F.SilkS) hide)
    (fp_text value Via (at 0 -1.5) (layer F.Fab))
    (pad 2 thru_hole circle (at -0.75 0) (size 0.55 0.55) (drill 0.26) (layers *.Cu F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 0.75 0) (size 0.55 0.55) (drill 0.26) (layers *.Cu F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 0 0) (size 0.55 0.55) (drill 0.26) (layers *.Cu F.Mask)
      (net 405 "Net-(F1-Pad1)"))
  )
  (module VNA:RF_via (layer F.Cu) (tedit 5883112F)
    (at 127.82 110.73)
    (fp_text reference F4 (at 0.1 1) (layer F.SilkS) hide)
    (fp_text value Via (at 0 -1.5) (layer F.Fab))
    (pad 2 thru_hole circle (at -0.75 0) (size 0.55 0.55) (drill 0.26) (layers *.Cu F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 0.75 0) (size 0.55 0.55) (drill 0.26) (layers *.Cu F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 0 0) (size 0.55 0.55) (drill 0.26) (layers *.Cu F.Mask)
      (net 404 "Net-(F2-Pad1)"))
  )
  (module VNA:RF_via (layer F.Cu) (tedit 5883112F)
    (at 165.49 64.11 90)
    (fp_text reference F1 (at 0.1 1 90) (layer F.SilkS) hide)
    (fp_text value Via (at 0 -1.5 90) (layer F.Fab))
    (pad 2 thru_hole circle (at -0.75 0 90) (size 0.55 0.55) (drill 0.26) (layers *.Cu F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 0.75 0 90) (size 0.55 0.55) (drill 0.26) (layers *.Cu F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 0 0 90) (size 0.55 0.55) (drill 0.26) (layers *.Cu F.Mask)
      (net 405 "Net-(F1-Pad1)"))
  )
  (module VNA:RF_via (layer F.Cu) (tedit 5883112F)
    (at 158.73 64.1 90)
    (fp_text reference F2 (at 0.1 1 90) (layer F.SilkS) hide)
    (fp_text value Via (at 0 -1.5 90) (layer F.Fab))
    (pad 2 thru_hole circle (at -0.75 0 90) (size 0.55 0.55) (drill 0.26) (layers *.Cu F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 0.75 0 90) (size 0.55 0.55) (drill 0.26) (layers *.Cu F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 0 0 90) (size 0.55 0.55) (drill 0.26) (layers *.Cu F.Mask)
      (net 404 "Net-(F2-Pad1)"))
  )
  (module VNA:TQFN-32 (layer F.Cu) (tedit 5884C4CE)
    (at 165.445 77.18)
    (fp_text reference U9 (at 0.115 3.55) (layer F.SilkS))
    (fp_text value MAX2871 (at -0.085 -3.55) (layer F.Fab))
    (pad EP thru_hole circle (at 0 1) (size 0.5 0.5) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
    (pad EP thru_hole circle (at -1 0) (size 0.5 0.5) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
    (pad EP thru_hole circle (at 0 -1) (size 0.5 0.5) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
    (pad EP thru_hole circle (at 1 0) (size 0.5 0.5) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
    (pad EP thru_hole circle (at 1 1) (size 0.5 0.5) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
    (pad EP thru_hole circle (at -1 1) (size 0.5 0.5) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
    (pad EP thru_hole circle (at 1 -1) (size 0.5 0.5) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
    (pad EP thru_hole circle (at -1 -1) (size 0.5 0.5) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
    (pad EP thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
    (pad 32 smd rect (at -1.75 -2.415 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 340 /3V3D))
    (pad 31 smd rect (at -1.25 -2.415 90) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 30 smd rect (at -0.75 -2.415 90) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 134 /LO_MUXOUT))
    (pad 29 smd rect (at -0.25 -2.415 90) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(C60-Pad1)"))
    (pad 28 smd rect (at 0.25 -2.415 90) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 340 /3V3D))
    (pad 27 smd rect (at 0.75 -2.415 90) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 26 smd rect (at 1.25 -2.415 90) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 133 /LO_RF_ENABLE))
    (pad 25 smd rect (at 1.75 -2.415 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 132 /LO_LD))
    (pad 16 smd rect (at 1.75 2.415 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C63-Pad1)"))
    (pad 15 smd rect (at 1.25 2.415 90) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(R31-Pad2)"))
    (pad 14 smd rect (at 0.75 2.415 90) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(R30-Pad2)"))
    (pad 13 smd rect (at 0.25 2.415 90) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 131 /receiver/LON))
    (pad 12 smd rect (at -0.25 2.415 90) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 130 /receiver/LOP))
    (pad 11 smd rect (at -0.75 2.415 90) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 10 smd rect (at -1.25 2.415 90) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C58-Pad1)"))
    (pad EP smd rect (at 0 0) (size 3.15 3.15) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.15))
    (pad 9 smd rect (at -1.75 2.415 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 24 smd rect (at 2.415 -1.75) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(C61-Pad1)"))
    (pad 23 smd rect (at 2.415 -1.25) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(C57-Pad1)"))
    (pad 22 smd rect (at 2.415 -0.75) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(R29-Pad1)"))
    (pad 21 smd rect (at 2.415 -0.25) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 20 smd rect (at 2.415 0.25) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(C74-Pad1)"))
    (pad 19 smd rect (at 2.415 0.75) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(C59-Pad1)"))
    (pad 18 smd rect (at 2.415 1.25) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 17 smd rect (at 2.415 1.75) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C63-Pad1)"))
    (pad 8 smd rect (at -2.415 1.75) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 7 smd rect (at -2.415 1.25) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(C72-Pad2)"))
    (pad 6 smd rect (at -2.415 0.75) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C58-Pad1)"))
    (pad 5 smd rect (at -2.415 0.25) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(R33-Pad2)"))
    (pad 4 smd rect (at -2.415 -0.25) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 129 /LO_CE))
    (pad 3 smd rect (at -2.415 -0.75) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 128 /LO_LE))
    (pad 2 smd rect (at -2.415 -1.25) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 127 /LO_SPI_DATA))
    (pad 1 smd rect (at -2.415 -1.75) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 111 /SPI_CLK))
  )
  (module VNA:TQFN-32 (layer F.Cu) (tedit 5884C4D7)
    (at 177.712 52.106 180)
    (fp_text reference U5 (at 0.115 3.55 180) (layer F.SilkS))
    (fp_text value MAX2871 (at -0.085 -3.55 180) (layer F.Fab))
    (pad EP thru_hole circle (at 0 1 180) (size 0.5 0.5) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
    (pad EP thru_hole circle (at -1 0 180) (size 0.5 0.5) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
    (pad EP thru_hole circle (at 0 -1 180) (size 0.5 0.5) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
    (pad EP thru_hole circle (at 1 0 180) (size 0.5 0.5) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
    (pad EP thru_hole circle (at 1 1 180) (size 0.5 0.5) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
    (pad EP thru_hole circle (at -1 1 180) (size 0.5 0.5) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
    (pad EP thru_hole circle (at 1 -1 180) (size 0.5 0.5) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
    (pad EP thru_hole circle (at -1 -1 180) (size 0.5 0.5) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
    (pad EP thru_hole circle (at 0 0 180) (size 0.5 0.5) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
    (pad 32 smd rect (at -1.75 -2.415 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 340 /3V3D))
    (pad 31 smd rect (at -1.25 -2.415 270) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 30 smd rect (at -0.75 -2.415 270) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 140 /SOURCE_MUXOUT))
    (pad 29 smd rect (at -0.25 -2.415 270) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(C18-Pad1)"))
    (pad 28 smd rect (at 0.25 -2.415 270) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 340 /3V3D))
    (pad 27 smd rect (at 0.75 -2.415 270) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 26 smd rect (at 1.25 -2.415 270) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 139 /SOURCE_RF_ENABLE))
    (pad 25 smd rect (at 1.75 -2.415 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 138 /SOURCE_LD))
    (pad 16 smd rect (at 1.75 2.415 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C21-Pad1)"))
    (pad 15 smd rect (at 1.25 2.415 270) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(R13-Pad2)"))
    (pad 14 smd rect (at 0.75 2.415 270) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(R12-Pad2)"))
    (pad 13 smd rect (at 0.25 2.415 270) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 4 /transmitter/RF_OUT_N))
    (pad 12 smd rect (at -0.25 2.415 270) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 /transmitter/RF_OUT_P))
    (pad 11 smd rect (at -0.75 2.415 270) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 10 smd rect (at -1.25 2.415 270) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C16-Pad1)"))
    (pad EP smd rect (at 0 0 180) (size 3.15 3.15) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.15))
    (pad 9 smd rect (at -1.75 2.415 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 24 smd rect (at 2.415 -1.75 180) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(C19-Pad1)"))
    (pad 23 smd rect (at 2.415 -1.25 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(C15-Pad1)"))
    (pad 22 smd rect (at 2.415 -0.75 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(R11-Pad1)"))
    (pad 21 smd rect (at 2.415 -0.25 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 20 smd rect (at 2.415 0.25 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C32-Pad1)"))
    (pad 19 smd rect (at 2.415 0.75 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(C17-Pad1)"))
    (pad 18 smd rect (at 2.415 1.25 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 17 smd rect (at 2.415 1.75 180) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C21-Pad1)"))
    (pad 8 smd rect (at -2.415 1.75 180) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 7 smd rect (at -2.415 1.25 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C30-Pad2)"))
    (pad 6 smd rect (at -2.415 0.75 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C16-Pad1)"))
    (pad 5 smd rect (at -2.415 0.25 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(R15-Pad2)"))
    (pad 4 smd rect (at -2.415 -0.25 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 137 /SOURCE_CE))
    (pad 3 smd rect (at -2.415 -0.75 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 136 /SOURCE_LE))
    (pad 2 smd rect (at -2.415 -1.25 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 135 /SOURCE_SPI_DATA))
    (pad 1 smd rect (at -2.415 -1.75 180) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 111 /SPI_CLK))
  )
  (module VNA:CONSMA003.062 (layer F.Cu) (tedit 587D0CE3)
    (at 135.825 119.875 270)
    (fp_text reference P7 (at 4.765 -0.365) (layer F.SilkS))
    (fp_text value SMA (at 0 -7.62 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0 0 270) (size 4.06 1.52) (layers F.Cu F.Mask)
      (net 348 /B) (solder_mask_margin 0.5))
    (pad 2 smd rect (at 0 -2.54 270) (size 4.06 1.52) (layers F.Cu F.Mask)
      (net 1 GND) (zone_connect 2) (thermal_width 4) (thermal_gap 0.3))
    (pad 2 smd rect (at 0 2.54 270) (size 4.06 1.52) (layers F.Cu F.Mask)
      (net 1 GND) (zone_connect 2) (thermal_width 4) (thermal_gap 0.3))
    (pad 2 smd rect (at 0 -2.54 270) (size 4.06 1.52) (layers B.Cu B.Mask)
      (net 1 GND) (zone_connect 2) (thermal_width 4) (thermal_gap 0.3))
    (pad 2 smd rect (at 0 2.54 270) (size 4.06 1.52) (layers B.Cu B.Mask)
      (net 1 GND) (zone_connect 2) (thermal_width 4) (thermal_gap 0.3))
    (pad 2 thru_hole circle (at 1.75 -2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 1.25 -2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 0.75 -2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 0.25 -2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at -0.25 -2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at -0.75 -2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at -1.25 -2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at -1.75 -2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 1.75 2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 1.25 2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 0.75 2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 0.25 2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at -0.25 2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at -0.75 2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at -1.25 2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at -1.75 2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
  )
  (module VNA:CONSMA003.062 (layer F.Cu) (tedit 587D0CE3)
    (at 147.025 119.875 270)
    (fp_text reference P8 (at 4.415 0.155) (layer F.SilkS))
    (fp_text value SMA (at 0 -7.62 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0 0 270) (size 4.06 1.52) (layers F.Cu F.Mask)
      (net 345 /RX2) (solder_mask_margin 0.5))
    (pad 2 smd rect (at 0 -2.54 270) (size 4.06 1.52) (layers F.Cu F.Mask)
      (net 1 GND) (zone_connect 2) (thermal_width 4) (thermal_gap 0.3))
    (pad 2 smd rect (at 0 2.54 270) (size 4.06 1.52) (layers F.Cu F.Mask)
      (net 1 GND) (zone_connect 2) (thermal_width 4) (thermal_gap 0.3))
    (pad 2 smd rect (at 0 -2.54 270) (size 4.06 1.52) (layers B.Cu B.Mask)
      (net 1 GND) (zone_connect 2) (thermal_width 4) (thermal_gap 0.3))
    (pad 2 smd rect (at 0 2.54 270) (size 4.06 1.52) (layers B.Cu B.Mask)
      (net 1 GND) (zone_connect 2) (thermal_width 4) (thermal_gap 0.3))
    (pad 2 thru_hole circle (at 1.75 -2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 1.25 -2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 0.75 -2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 0.25 -2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at -0.25 -2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at -0.75 -2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at -1.25 -2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at -1.75 -2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 1.75 2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 1.25 2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 0.75 2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 0.25 2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at -0.25 2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at -0.75 2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at -1.25 2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at -1.75 2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
  )
  (module VNA:CONSMA003.062 (layer F.Cu) (tedit 587D0CE3)
    (at 169.03 119.86 270)
    (fp_text reference P6 (at 4.52 0) (layer F.SilkS))
    (fp_text value SMA (at 0 -7.62 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0 0 270) (size 4.06 1.52) (layers F.Cu F.Mask)
      (net 347 /RX1) (solder_mask_margin 0.5))
    (pad 2 smd rect (at 0 -2.54 270) (size 4.06 1.52) (layers F.Cu F.Mask)
      (net 1 GND) (zone_connect 2) (thermal_width 4) (thermal_gap 0.3))
    (pad 2 smd rect (at 0 2.54 270) (size 4.06 1.52) (layers F.Cu F.Mask)
      (net 1 GND) (zone_connect 2) (thermal_width 4) (thermal_gap 0.3))
    (pad 2 smd rect (at 0 -2.54 270) (size 4.06 1.52) (layers B.Cu B.Mask)
      (net 1 GND) (zone_connect 2) (thermal_width 4) (thermal_gap 0.3))
    (pad 2 smd rect (at 0 2.54 270) (size 4.06 1.52) (layers B.Cu B.Mask)
      (net 1 GND) (zone_connect 2) (thermal_width 4) (thermal_gap 0.3))
    (pad 2 thru_hole circle (at 1.75 -2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 1.25 -2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 0.75 -2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 0.25 -2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at -0.25 -2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at -0.75 -2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at -1.25 -2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at -1.75 -2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 1.75 2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 1.25 2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 0.75 2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 0.25 2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at -0.25 2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at -0.75 2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at -1.25 2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at -1.75 2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
  )
  (module VNA:CONSMA003.062 (layer F.Cu) (tedit 587D0CE3)
    (at 158.325 119.875 270)
    (fp_text reference P4 (at 4.705 -0.375) (layer F.SilkS))
    (fp_text value SMA (at 0 -7.62 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0 0 270) (size 4.06 1.52) (layers F.Cu F.Mask)
      (net 346 /A) (solder_mask_margin 0.5))
    (pad 2 smd rect (at 0 -2.54 270) (size 4.06 1.52) (layers F.Cu F.Mask)
      (net 1 GND) (zone_connect 2) (thermal_width 4) (thermal_gap 0.3))
    (pad 2 smd rect (at 0 2.54 270) (size 4.06 1.52) (layers F.Cu F.Mask)
      (net 1 GND) (zone_connect 2) (thermal_width 4) (thermal_gap 0.3))
    (pad 2 smd rect (at 0 -2.54 270) (size 4.06 1.52) (layers B.Cu B.Mask)
      (net 1 GND) (zone_connect 2) (thermal_width 4) (thermal_gap 0.3))
    (pad 2 smd rect (at 0 2.54 270) (size 4.06 1.52) (layers B.Cu B.Mask)
      (net 1 GND) (zone_connect 2) (thermal_width 4) (thermal_gap 0.3))
    (pad 2 thru_hole circle (at 1.75 -2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 1.25 -2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 0.75 -2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 0.25 -2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at -0.25 -2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at -0.75 -2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at -1.25 -2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at -1.75 -2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 1.75 2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 1.25 2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 0.75 2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 0.25 2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at -0.25 2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at -0.75 2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at -1.25 2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at -1.75 2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
  )
  (module VNA:CONSMA003.062 (layer F.Cu) (tedit 587D0CE3)
    (at 123.625 119.875 270)
    (fp_text reference P2 (at 4.385 0.105) (layer F.SilkS))
    (fp_text value SMA (at 0 -7.62 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0 0 270) (size 4.06 1.52) (layers F.Cu F.Mask)
      (net 349 /PORT2) (solder_mask_margin 0.5))
    (pad 2 smd rect (at 0 -2.54 270) (size 4.06 1.52) (layers F.Cu F.Mask)
      (net 1 GND) (zone_connect 2) (thermal_width 4) (thermal_gap 0.3))
    (pad 2 smd rect (at 0 2.54 270) (size 4.06 1.52) (layers F.Cu F.Mask)
      (net 1 GND) (zone_connect 2) (thermal_width 4) (thermal_gap 0.3))
    (pad 2 smd rect (at 0 -2.54 270) (size 4.06 1.52) (layers B.Cu B.Mask)
      (net 1 GND) (zone_connect 2) (thermal_width 4) (thermal_gap 0.3))
    (pad 2 smd rect (at 0 2.54 270) (size 4.06 1.52) (layers B.Cu B.Mask)
      (net 1 GND) (zone_connect 2) (thermal_width 4) (thermal_gap 0.3))
    (pad 2 thru_hole circle (at 1.75 -2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 1.25 -2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 0.75 -2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 0.25 -2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at -0.25 -2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at -0.75 -2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at -1.25 -2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at -1.75 -2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 1.75 2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 1.25 2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 0.75 2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 0.25 2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at -0.25 2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at -0.75 2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at -1.25 2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at -1.75 2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
  )
  (module VNA:CONSMA003.062 (layer F.Cu) (tedit 587D0CE3)
    (at 179.28 119.86 270)
    (fp_text reference P1 (at 4.72 -0.28) (layer F.SilkS))
    (fp_text value SMA (at 0 -7.62 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0 0 270) (size 4.06 1.52) (layers F.Cu F.Mask)
      (net 350 /PORT1) (solder_mask_margin 0.5))
    (pad 2 smd rect (at 0 -2.54 270) (size 4.06 1.52) (layers F.Cu F.Mask)
      (net 1 GND) (zone_connect 2) (thermal_width 4) (thermal_gap 0.3))
    (pad 2 smd rect (at 0 2.54 270) (size 4.06 1.52) (layers F.Cu F.Mask)
      (net 1 GND) (zone_connect 2) (thermal_width 4) (thermal_gap 0.3))
    (pad 2 smd rect (at 0 -2.54 270) (size 4.06 1.52) (layers B.Cu B.Mask)
      (net 1 GND) (zone_connect 2) (thermal_width 4) (thermal_gap 0.3))
    (pad 2 smd rect (at 0 2.54 270) (size 4.06 1.52) (layers B.Cu B.Mask)
      (net 1 GND) (zone_connect 2) (thermal_width 4) (thermal_gap 0.3))
    (pad 2 thru_hole circle (at 1.75 -2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 1.25 -2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 0.75 -2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 0.25 -2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at -0.25 -2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at -0.75 -2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at -1.25 -2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at -1.75 -2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 1.75 2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 1.25 2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 0.75 2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 0.25 2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at -0.25 2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at -0.75 2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at -1.25 2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at -1.75 2.1 270) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
  )
  (module VNA:TFLGA-20 (layer F.Cu) (tedit 587D08AF)
    (at 127.825 113.35 180)
    (solder_mask_margin 0.1)
    (zone_connect 2)
    (fp_text reference U29 (at 0 3.125 180) (layer F.SilkS))
    (fp_text value PE42420 (at 0 -3.75 180) (layer F.Fab))
    (pad EP thru_hole circle (at 0.7 0.7 270) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad EP thru_hole circle (at 0 0.7 270) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad EP thru_hole circle (at -0.7 0.7 270) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad EP thru_hole circle (at 0.7 0 270) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad EP thru_hole circle (at 0 0 270) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad EP thru_hole circle (at -0.7 0 270) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad EP thru_hole circle (at 0.7 -0.7 270) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad EP thru_hole circle (at 0 -0.7 270) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad EP thru_hole circle (at -0.7 -0.7 270) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad EP smd rect (at 0 0 270) (size 2.05 2.05) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.1) (solder_paste_margin_ratio -0.2) (zone_connect 2))
    (pad 20 smd rect (at -1 -1.8 270) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 157 "Net-(C172-Pad1)") (zone_connect 2))
    (pad 19 smd rect (at -0.5 -1.8 270) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 18 smd rect (at 0 -1.8 270) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 17 smd rect (at 0.5 -1.8 270) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 158 "Net-(R55-Pad2)") (zone_connect 2))
    (pad 16 smd rect (at 1 -1.8 270) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 159 "Net-(R66-Pad2)") (zone_connect 2))
    (pad 15 smd rect (at 1.8 -1 180) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 14 smd rect (at 1.8 -0.5 180) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 13 smd rect (at 1.8 0 180) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 160 "Net-(C179-Pad2)") (zone_connect 2))
    (pad 12 smd rect (at 1.8 0.5 180) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 11 smd rect (at 1.8 1 180) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 10 smd rect (at 1 1.8 270) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 9 smd rect (at 0.5 1.8 270) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 8 smd rect (at 0 1.8 270) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 404 "Net-(F2-Pad1)") (zone_connect 2))
    (pad 7 smd rect (at -0.5 1.8 270) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 6 smd rect (at -1 1.8 270) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 5 smd rect (at -1.8 1 180) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 4 smd rect (at -1.8 0.5 180) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 3 smd rect (at -1.8 0 180) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 161 "Net-(R68-Pad1)") (zone_connect 2))
    (pad 2 smd rect (at -1.8 -0.5 180) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 1 smd rect (at -1.8 -1 180) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
  )
  (module VNA:TFLGA-20 (layer F.Cu) (tedit 587D08AF)
    (at 178.06 110.98 180)
    (solder_mask_margin 0.1)
    (zone_connect 2)
    (fp_text reference U28 (at 0 3.125 180) (layer F.SilkS))
    (fp_text value PE42420 (at 0 -3.75 180) (layer F.Fab))
    (pad EP thru_hole circle (at 0.7 0.7 270) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad EP thru_hole circle (at 0 0.7 270) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad EP thru_hole circle (at -0.7 0.7 270) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad EP thru_hole circle (at 0.7 0 270) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad EP thru_hole circle (at 0 0 270) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad EP thru_hole circle (at -0.7 0 270) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad EP thru_hole circle (at 0.7 -0.7 270) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad EP thru_hole circle (at 0 -0.7 270) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad EP thru_hole circle (at -0.7 -0.7 270) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad EP smd rect (at 0 0 270) (size 2.05 2.05) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.1) (solder_paste_margin_ratio -0.2) (zone_connect 2))
    (pad 20 smd rect (at -1 -1.8 270) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 156 "Net-(C171-Pad1)") (zone_connect 2))
    (pad 19 smd rect (at -0.5 -1.8 270) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 18 smd rect (at 0 -1.8 270) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 17 smd rect (at 0.5 -1.8 270) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 155 "Net-(R54-Pad2)") (zone_connect 2))
    (pad 16 smd rect (at 1 -1.8 270) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 154 "Net-(R56-Pad2)") (zone_connect 2))
    (pad 15 smd rect (at 1.8 -1 180) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 14 smd rect (at 1.8 -0.5 180) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 13 smd rect (at 1.8 0 180) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 153 "Net-(R67-Pad1)") (zone_connect 2))
    (pad 12 smd rect (at 1.8 0.5 180) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 11 smd rect (at 1.8 1 180) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 10 smd rect (at 1 1.8 270) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 9 smd rect (at 0.5 1.8 270) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 8 smd rect (at 0 1.8 270) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 405 "Net-(F1-Pad1)") (zone_connect 2))
    (pad 7 smd rect (at -0.5 1.8 270) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 6 smd rect (at -1 1.8 270) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 5 smd rect (at -1.8 1 180) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 4 smd rect (at -1.8 0.5 180) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 3 smd rect (at -1.8 0 180) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 152 "Net-(C180-Pad2)") (zone_connect 2))
    (pad 2 smd rect (at -1.8 -0.5 180) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 1 smd rect (at -1.8 -1 180) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
  )
  (module VNA:TFLGA-20 (layer F.Cu) (tedit 587D08AF)
    (at 162.1 64.1 180)
    (solder_mask_margin 0.1)
    (zone_connect 2)
    (fp_text reference U27 (at 0 3.125 180) (layer F.SilkS))
    (fp_text value PE42420 (at 0 -3.75 180) (layer F.Fab))
    (pad EP thru_hole circle (at 0.7 0.7 270) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad EP thru_hole circle (at 0 0.7 270) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad EP thru_hole circle (at -0.7 0.7 270) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad EP thru_hole circle (at 0.7 0 270) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad EP thru_hole circle (at 0 0 270) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad EP thru_hole circle (at -0.7 0 270) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad EP thru_hole circle (at 0.7 -0.7 270) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad EP thru_hole circle (at 0 -0.7 270) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad EP thru_hole circle (at -0.7 -0.7 270) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad EP smd rect (at 0 0 270) (size 2.05 2.05) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.1) (solder_paste_margin_ratio -0.2) (zone_connect 2))
    (pad 20 smd rect (at -1 -1.8 270) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 150 "Net-(C168-Pad1)") (zone_connect 2))
    (pad 19 smd rect (at -0.5 -1.8 270) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 18 smd rect (at 0 -1.8 270) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 17 smd rect (at 0.5 -1.8 270) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 86 "Net-(R50-Pad2)") (zone_connect 2))
    (pad 16 smd rect (at 1 -1.8 270) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 87 "Net-(R51-Pad2)") (zone_connect 2))
    (pad 15 smd rect (at 1.8 -1 180) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 14 smd rect (at 1.8 -0.5 180) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 13 smd rect (at 1.8 0 180) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 404 "Net-(F2-Pad1)") (zone_connect 2))
    (pad 12 smd rect (at 1.8 0.5 180) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 11 smd rect (at 1.8 1 180) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 10 smd rect (at 1 1.8 270) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 9 smd rect (at 0.5 1.8 270) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 8 smd rect (at 0 1.8 270) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 151 "/port switch/RFC") (zone_connect 2))
    (pad 7 smd rect (at -0.5 1.8 270) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 6 smd rect (at -1 1.8 270) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 5 smd rect (at -1.8 1 180) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 4 smd rect (at -1.8 0.5 180) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 3 smd rect (at -1.8 0 180) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 405 "Net-(F1-Pad1)") (zone_connect 2))
    (pad 2 smd rect (at -1.8 -0.5 180) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 1 smd rect (at -1.8 -1 180) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
  )
  (module VNA:TFLGA-20 (layer F.Cu) (tedit 587D08AF)
    (at 164.149959 112.726639 180)
    (solder_mask_margin 0.1)
    (zone_connect 2)
    (fp_text reference U6 (at 0 3.125 180) (layer F.SilkS))
    (fp_text value PE42420 (at 0 -3.75 180) (layer F.Fab))
    (pad EP thru_hole circle (at 0.7 0.7 270) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad EP thru_hole circle (at 0 0.7 270) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad EP thru_hole circle (at -0.7 0.7 270) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad EP thru_hole circle (at 0.7 0 270) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad EP thru_hole circle (at 0 0 270) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad EP thru_hole circle (at -0.7 0 270) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad EP thru_hole circle (at 0.7 -0.7 270) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad EP thru_hole circle (at 0 -0.7 270) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad EP thru_hole circle (at -0.7 -0.7 270) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad EP smd rect (at 0 0 270) (size 2.05 2.05) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.1) (solder_paste_margin_ratio -0.2) (zone_connect 2))
    (pad 20 smd rect (at -1 -1.8 270) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 149 "Net-(C81-Pad1)") (zone_connect 2))
    (pad 19 smd rect (at -0.5 -1.8 270) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 18 smd rect (at 0 -1.8 270) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 17 smd rect (at 0.5 -1.8 270) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 148 "Net-(R3-Pad2)") (zone_connect 2))
    (pad 16 smd rect (at 1 -1.8 270) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 147 "Net-(R1-Pad2)") (zone_connect 2))
    (pad 15 smd rect (at 1.8 -1 180) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 14 smd rect (at 1.8 -0.5 180) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 13 smd rect (at 1.8 0 180) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 146 "Net-(C9-Pad2)") (zone_connect 2))
    (pad 12 smd rect (at 1.8 0.5 180) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 11 smd rect (at 1.8 1 180) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 10 smd rect (at 1 1.8 270) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 9 smd rect (at 0.5 1.8 270) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 8 smd rect (at 0 1.8 270) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 410 "Net-(F15-Pad1)") (zone_connect 2))
    (pad 7 smd rect (at -0.5 1.8 270) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 6 smd rect (at -1 1.8 270) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 5 smd rect (at -1.8 1 180) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 4 smd rect (at -1.8 0.5 180) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 3 smd rect (at -1.8 0 180) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 145 "Net-(C8-Pad2)") (zone_connect 2))
    (pad 2 smd rect (at -1.8 -0.5 180) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 1 smd rect (at -1.8 -1 180) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
  )
  (module VNA:TFLGA-20 (layer F.Cu) (tedit 587D08AF)
    (at 141.393058 112.872588 180)
    (solder_mask_margin 0.1)
    (zone_connect 2)
    (fp_text reference U10 (at 0 3.125 180) (layer F.SilkS))
    (fp_text value PE42420 (at 0 -3.75 180) (layer F.Fab))
    (pad EP thru_hole circle (at 0.7 0.7 270) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad EP thru_hole circle (at 0 0.7 270) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad EP thru_hole circle (at -0.7 0.7 270) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad EP thru_hole circle (at 0.7 0 270) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad EP thru_hole circle (at 0 0 270) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad EP thru_hole circle (at -0.7 0 270) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad EP thru_hole circle (at 0.7 -0.7 270) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad EP thru_hole circle (at 0 -0.7 270) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad EP thru_hole circle (at -0.7 -0.7 270) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad EP smd rect (at 0 0 270) (size 2.05 2.05) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.1) (solder_paste_margin_ratio -0.2) (zone_connect 2))
    (pad 20 smd rect (at -1 -1.8 270) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 144 "Net-(C82-Pad1)") (zone_connect 2))
    (pad 19 smd rect (at -0.5 -1.8 270) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 18 smd rect (at 0 -1.8 270) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 17 smd rect (at 0.5 -1.8 270) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(R4-Pad2)") (zone_connect 2))
    (pad 16 smd rect (at 1 -1.8 270) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 89 "Net-(R2-Pad2)") (zone_connect 2))
    (pad 15 smd rect (at 1.8 -1 180) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 14 smd rect (at 1.8 -0.5 180) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 13 smd rect (at 1.8 0 180) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C28-Pad2)") (zone_connect 2))
    (pad 12 smd rect (at 1.8 0.5 180) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 11 smd rect (at 1.8 1 180) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 10 smd rect (at 1 1.8 270) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 9 smd rect (at 0.5 1.8 270) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 8 smd rect (at 0 1.8 270) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 411 "Net-(F16-Pad1)") (zone_connect 2))
    (pad 7 smd rect (at -0.5 1.8 270) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 6 smd rect (at -1 1.8 270) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 5 smd rect (at -1.8 1 180) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 4 smd rect (at -1.8 0.5 180) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 3 smd rect (at -1.8 0 180) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(C12-Pad2)") (zone_connect 2))
    (pad 2 smd rect (at -1.8 -0.5 180) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 1 smd rect (at -1.8 -1 180) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
  )
  (module VNA:TFLGA-20 (layer F.Cu) (tedit 587D08AF)
    (at 152.775 112.6 180)
    (solder_mask_margin 0.1)
    (zone_connect 2)
    (fp_text reference U11 (at 0 3.125 180) (layer F.SilkS))
    (fp_text value PE42420 (at 0 -3.75 180) (layer F.Fab))
    (pad EP thru_hole circle (at 0.7 0.7 270) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad EP thru_hole circle (at 0 0.7 270) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad EP thru_hole circle (at -0.7 0.7 270) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad EP thru_hole circle (at 0.7 0 270) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad EP thru_hole circle (at 0 0 270) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad EP thru_hole circle (at -0.7 0 270) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad EP thru_hole circle (at 0.7 -0.7 270) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad EP thru_hole circle (at 0 -0.7 270) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad EP thru_hole circle (at -0.7 -0.7 270) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad EP smd rect (at 0 0 270) (size 2.05 2.05) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.1) (solder_paste_margin_ratio -0.2) (zone_connect 2))
    (pad 20 smd rect (at -1 -1.8 270) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 143 "Net-(C85-Pad1)") (zone_connect 2))
    (pad 19 smd rect (at -0.5 -1.8 270) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 18 smd rect (at 0 -1.8 270) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 17 smd rect (at 0.5 -1.8 270) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 142 "Net-(R9-Pad2)") (zone_connect 2))
    (pad 16 smd rect (at 1 -1.8 270) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 141 "Net-(R8-Pad2)") (zone_connect 2))
    (pad 15 smd rect (at 1.8 -1 180) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 14 smd rect (at 1.8 -0.5 180) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 13 smd rect (at 1.8 0 180) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 411 "Net-(F16-Pad1)") (zone_connect 2))
    (pad 12 smd rect (at 1.8 0.5 180) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 11 smd rect (at 1.8 1 180) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 10 smd rect (at 1 1.8 270) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 9 smd rect (at 0.5 1.8 270) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 8 smd rect (at 0 1.8 270) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 46 /receiver/RF_IN) (zone_connect 2))
    (pad 7 smd rect (at -0.5 1.8 270) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 6 smd rect (at -1 1.8 270) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 5 smd rect (at -1.8 1 180) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 4 smd rect (at -1.8 0.5 180) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 3 smd rect (at -1.8 0 180) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 410 "Net-(F15-Pad1)") (zone_connect 2))
    (pad 2 smd rect (at -1.8 -0.5 180) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 1 smd rect (at -1.8 -1 180) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
  )
  (module VNA:C_0805b (layer F.Cu) (tedit 55A401FA)
    (at 149.67 102.5 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C266 (at 0 -1.675 270) (layer F.SilkS))
    (fp_text value DNP (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 341 /5V))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0805b (layer F.Cu) (tedit 55A401FA)
    (at 169.35 91.3 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C265 (at 0 -1.675 270) (layer F.SilkS))
    (fp_text value DNP (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 95 /receiver/5VF))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0805b (layer F.Cu) (tedit 55A401FA)
    (at 110.81 55.76 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C264 (at 0 -1.675 270) (layer F.SilkS))
    (fp_text value DNP (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 56 /power/12V))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0805b (layer F.Cu) (tedit 55A401FA)
    (at 135.03 42.26 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C263 (at 0 -1.675 180) (layer F.SilkS))
    (fp_text value DNP (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 406 /fpga/usb/5V))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:TP_1.00 (layer F.Cu) (tedit 55A404EB)
    (at 126.62 73.6)
    (fp_text reference P26 (at 0.125 0.05) (layer F.SilkS) hide)
    (fp_text value TP (at 0 -0.5) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 424 "Net-(P26-Pad1)"))
  )
  (module VNA:TP_1.00 (layer F.Cu) (tedit 55A404EB)
    (at 126.63 75.15)
    (fp_text reference P27 (at 0.125 0.05) (layer F.SilkS) hide)
    (fp_text value TP (at 0 -0.5) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 423 "Net-(P27-Pad1)"))
  )
  (module VNA:C_0805b (layer F.Cu) (tedit 55A401FA)
    (at 137.45 96.41 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C262 (at 0 -1.675 90) (layer F.SilkS))
    (fp_text value DNP (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 415 3V3A_RX))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-353 (layer F.Cu) (tedit 583F3CBD)
    (at 178.23 59.5 90)
    (descr SOT353)
    (attr smd)
    (fp_text reference U42 (at 1.5 2.81 180) (layer F.SilkS))
    (fp_text value NC7S04P5X (at 0 2.25 270) (layer F.Fab))
    (pad 4 smd rect (at 0.95 0.65 90) (size 0.6 0.42) (layers F.Cu F.Paste F.Mask)
      (net 421 "Net-(R133-Pad1)"))
    (pad 2 smd rect (at -0.95 0 90) (size 0.6 0.42) (layers F.Cu F.Paste F.Mask)
      (net 338 "Net-(C3-Pad1)"))
    (pad 5 smd rect (at 0.95 -0.65 90) (size 0.6 0.42) (layers F.Cu F.Paste F.Mask)
      (net 422 "Net-(C261-Pad1)"))
    (pad 3 smd rect (at -0.95 0.65 90) (size 0.6 0.42) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.95 -0.65 90) (size 0.6 0.42) (layers F.Cu F.Paste F.Mask))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-353.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.07000000000000001 0.09 0.08))
      (rotate (xyz 0 0 90))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 55A40188)
    (at 178.13 57.73)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C261 (at -1.91 0.34 90) (layer F.SilkS))
    (fp_text value 100n (at 0 1.7) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 422 "Net-(C261-Pad1)"))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer B.Cu) (tedit 55A401B2)
    (at 178.86 59.47 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R133 (at 0 1.4 270) (layer B.SilkS))
    (fp_text value 1M (at 0 -1.8 270) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 421 "Net-(R133-Pad1)"))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 338 "Net-(C3-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer F.Cu) (tedit 55A401B2)
    (at 173.62 56.75 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R131 (at 0 -1.4 180) (layer F.SilkS))
    (fp_text value 33 (at 0 1.8 180) (layer F.Fab))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 420 "Net-(R131-Pad2)"))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 184 /CLK_SOURCE))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer F.Cu) (tedit 55A401B2)
    (at 172.28 61.54 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R132 (at -0.59 -1.4 270) (layer F.SilkS))
    (fp_text value 33 (at 0 1.8 90) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 185 /CLK_LO))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 419 "Net-(R132-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 55A40188)
    (at 161 46.83 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C10 (at 0 -1.7 90) (layer F.SilkS))
    (fp_text value 1n (at 0 1.7 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 98 /tx_amp/RF_IN))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 23 /filter_bank/RF_OUT))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:S2711-46R (layer F.Cu) (tedit 586FF10A)
    (at 173.87 99.16 90)
    (fp_text reference P22 (at 0 2 90) (layer F.SilkS))
    (fp_text value CLIP (at 0.1 0 90) (layer F.Fab))
    (pad 1 smd rect (at 0 0 90) (size 9.4 2.3) (layers F.Cu F.Mask)
      (net 1 GND))
  )
  (module VNA:S2711-46R (layer F.Cu) (tedit 586FF10A)
    (at 173.87 77.7 90)
    (fp_text reference P21 (at 0 2 90) (layer F.SilkS))
    (fp_text value CLIP (at 0.1 0 90) (layer F.Fab))
    (pad 1 smd rect (at 0 0 90) (size 9.4 2.3) (layers F.Cu F.Mask)
      (net 1 GND))
  )
  (module VNA:S2711-46R (layer F.Cu) (tedit 586FF10A)
    (at 155.87 99.16 90)
    (fp_text reference P23 (at 0 2 90) (layer F.SilkS))
    (fp_text value CLIP (at 0.1 0 90) (layer F.Fab))
    (pad 1 smd rect (at 0 0 90) (size 9.4 2.3) (layers F.Cu F.Mask)
      (net 1 GND))
  )
  (module VNA:S2711-46R (layer F.Cu) (tedit 5870D7A6)
    (at 155.87 77.26 90)
    (fp_text reference P24 (at 0.27 -0.13 90) (layer F.SilkS))
    (fp_text value CLIP (at 0.1 0 90) (layer F.Fab))
    (pad 1 smd rect (at 0 0 90) (size 9.4 2.3) (layers F.Cu F.Mask)
      (net 1 GND))
  )
  (module VNA:S2711-46R (layer F.Cu) (tedit 586FF10A)
    (at 164.59 107.59)
    (fp_text reference P25 (at 0 2) (layer F.SilkS))
    (fp_text value CLIP (at 0.1 0) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 9.4 2.3) (layers F.Cu F.Mask)
      (net 1 GND))
  )
  (module VNA:S2711-46R (layer F.Cu) (tedit 5870D78B)
    (at 164.59 69.4)
    (fp_text reference P20 (at 0.06 0.07) (layer F.SilkS))
    (fp_text value CLIP (at 0.1 0) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 9.4 2.3) (layers F.Cu F.Mask)
      (net 1 GND))
  )
  (module VNA:C_0402b (layer B.Cu) (tedit 5870DAFD)
    (at 130.74 118.77 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C177 (at 0.07 1.21 90) (layer B.SilkS))
    (fp_text value 18p (at 0 -1.7 90) (layer B.Fab))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 174 /PORT_SW0))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer F.Cu) (tedit 55A401B2)
    (at 147.7 72.775)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R130 (at 0 -1.4) (layer F.SilkS))
    (fp_text value 16 (at 0 1.8) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 418 "Net-(R130-Pad1)"))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 111 /SPI_CLK))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:MountingHole_3.2mm_M3_Pad_Via_mod (layer F.Cu) (tedit 5870D80A)
    (at 113.907944 118.322944)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (fp_text reference P18 (at -0.077944 0.057056) (layer F.SilkS))
    (fp_text value MNT (at 0 4.2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 2.4 0) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 1.697056 1.697056) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 0 2.4) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at -1.697056 1.697056) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at -2.4 0) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at -1.697056 -1.697056) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 0 -2.4) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 1.697056 -1.697056) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
  )
  (module VNA:MountingHole_3.2mm_M3_Pad_Via_mod (layer F.Cu) (tedit 586E9C4D)
    (at 112.67 40.14)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (fp_text reference P17 (at 0 -4.2) (layer F.SilkS))
    (fp_text value MNT (at 0 4.2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 2.4 0) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 1.697056 1.697056) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 0 2.4) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at -1.697056 1.697056) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at -2.4 0) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at -1.697056 -1.697056) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 0 -2.4) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 1.697056 -1.697056) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
  )
  (module VNA:MountingHole_3.2mm_M3_Pad_Via_mod (layer F.Cu) (tedit 586E9C4D)
    (at 178.5 40.375)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (fp_text reference P19 (at 0 -4.2) (layer F.SilkS))
    (fp_text value MNT (at 0 4.2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 2.4 0) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 1.697056 1.697056) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 0 2.4) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at -1.697056 1.697056) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at -2.4 0) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at -1.697056 -1.697056) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 0 -2.4) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 1.697056 -1.697056) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 5870DA0C)
    (at 165.45 58.45)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C147 (at 0.39 -5.33 90) (layer F.SilkS))
    (fp_text value 10n (at 0 1.7) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 100 "Net-(C145-Pad1)"))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 5870D719)
    (at 163.51 98.94)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (zone_connect 2)
    (attr smd)
    (fp_text reference C259 (at -1.29 -1.07) (layer F.SilkS))
    (fp_text value DNP (at 0 1.7) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 337 "Net-(C121-Pad2)") (zone_connect 2))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 55A40188)
    (at 162.69 59.59 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (zone_connect 2)
    (attr smd)
    (fp_text reference C260 (at 0 -1.7 180) (layer F.SilkS))
    (fp_text value DNP (at 0 1.7 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 107 "Net-(C151-Pad2)") (zone_connect 2))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer F.Cu) (tedit 5870D7B7)
    (at 181.65 107.41 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R121 (at -1.52 -0.05) (layer F.SilkS))
    (fp_text value DNP (at 0 1.8 270) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 171 /3V3A))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 415 3V3A_RX))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0603b (layer F.Cu) (tedit 5870D884)
    (at 140.62 94.02 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C257 (at 1.43 1.32 180) (layer F.SilkS))
    (fp_text value 1u (at 0 1.9 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 168 /3V6))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0603b (layer F.Cu) (tedit 5870D880)
    (at 142.66 97.06 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C258 (at 0.04 1.24 270) (layer F.SilkS))
    (fp_text value 1u (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 415 3V3A_RX))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:SOT-23-5 (layer F.Cu) (tedit 5870D886)
    (at 141.3 95.25 180)
    (fp_text reference U41 (at 0.85 -1.32 180) (layer F.SilkS))
    (fp_text value LP5907 (at 0 -4.05 180) (layer F.SilkS))
    (pad 1 smd rect (at 0 0 180) (size 0.6 1.05) (layers F.Cu F.Paste F.Mask)
      (net 168 /3V6))
    (pad 2 smd rect (at 0.95 0 180) (size 0.6 1.05) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.9 0 180) (size 0.6 1.05) (layers F.Cu F.Paste F.Mask)
      (net 168 /3V6))
    (pad 4 smd rect (at 1.9 -2.6 180) (size 0.6 1.25) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 0 -2.6 180) (size 0.6 1.25) (layers F.Cu F.Paste F.Mask)
      (net 415 3V3A_RX))
  )
  (module VNA:C_0805b (layer F.Cu) (tedit 55A401FA)
    (at 174.51 61.76 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C256 (at 0 -1.675 180) (layer F.SilkS))
    (fp_text value 10u (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 340 /3V3D))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:SOT-23-5 (layer F.Cu) (tedit 55AA3491)
    (at 125.29 45.88 270)
    (fp_text reference U25 (at 0.875 -1.34 270) (layer F.SilkS))
    (fp_text value MCP1824T-3302E (at 0 -4.05 270) (layer F.SilkS))
    (pad 1 smd rect (at 0 0 270) (size 0.6 1.05) (layers F.Cu F.Paste F.Mask)
      (net 168 /3V6))
    (pad 2 smd rect (at 0.95 0 270) (size 0.6 1.05) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.9 0 270) (size 0.6 1.05) (layers F.Cu F.Paste F.Mask)
      (net 168 /3V6))
    (pad 4 smd rect (at 1.9 -2.6 270) (size 0.6 1.25) (layers F.Cu F.Paste F.Mask)
      (net 169 "Net-(U25-Pad4)"))
    (pad 5 smd rect (at 0 -2.6 270) (size 0.6 1.25) (layers F.Cu F.Paste F.Mask)
      (net 340 /3V3D))
  )
  (module VNA:SOT-23-5 (layer F.Cu) (tedit 5870D9A4)
    (at 161.08 40.435 180)
    (fp_text reference U36 (at 0.97 -1.415 180) (layer F.SilkS))
    (fp_text value LP5907-3V3 (at 0 -4.05 180) (layer F.SilkS))
    (pad 1 smd rect (at 0 0 180) (size 0.6 1.05) (layers F.Cu F.Paste F.Mask)
      (net 168 /3V6))
    (pad 2 smd rect (at 0.95 0 180) (size 0.6 1.05) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.9 0 180) (size 0.6 1.05) (layers F.Cu F.Paste F.Mask)
      (net 168 /3V6))
    (pad 4 smd rect (at 1.9 -2.6 180) (size 0.6 1.25) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 0 -2.6 180) (size 0.6 1.25) (layers F.Cu F.Paste F.Mask)
      (net 171 /3V3A))
  )
  (module VNA:R_0402b (layer F.Cu) (tedit 5870D9E3)
    (at 169.86 59.13 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R120 (at -2.32 -1.26 180) (layer F.SilkS))
    (fp_text value 33 (at 0 1.8 90) (layer F.Fab))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 414 "Net-(R120-Pad2)"))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 339 /CLK_ADC))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer F.Cu) (tedit 5870D9E1)
    (at 168.79 59.15 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R119 (at -1.57 -1.33 180) (layer F.SilkS))
    (fp_text value 33 (at 0 1.8 90) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 297 /CLK_FPGA))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 413 "Net-(R119-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 5870DA18)
    (at 160.075 58.875)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C255 (at -0.235 -1.065) (layer F.SilkS))
    (fp_text value 1n (at 0 1.7) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 412 "Net-(C255-Pad1)"))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 364 /tx_amp/DET_IN))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer B.Cu) (tedit 5870DC47)
    (at 135.625 67.75 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C205 (at 2.145 1.95 180) (layer B.SilkS))
    (fp_text value 470n (at 0 -1.7 180) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 273 "Net-(C205-Pad1)"))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 267 "Net-(C205-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0603b (layer B.Cu) (tedit 55A401E5)
    (at 142 45.85 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference FB12 (at 0 1.425 90) (layer B.SilkS))
    (fp_text value BLM18PG181SN1D (at 0 -1.9 90) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 341 /5V))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 406 /fpga/usb/5V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0805b (layer F.Cu) (tedit 5870D807)
    (at 119.66 113.61 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C111 (at 3.2 1.49) (layer F.SilkS))
    (fp_text value 10u (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(C111-Pad1)"))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0805b (layer F.Cu) (tedit 5870D805)
    (at 118.41 113.61 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C114 (at 2.41 0.32) (layer F.SilkS))
    (fp_text value 10u (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(C111-Pad1)"))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0603b (layer F.Cu) (tedit 5870D730)
    (at 159.13 92.43 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C55 (at -0.27 -1.25) (layer F.SilkS))
    (fp_text value 1u (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 168 /3V6))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 5870D7EB)
    (at 148.2 107 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C253 (at -0.14 1.24 180) (layer F.SilkS))
    (fp_text value 100n (at 0 1.7 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 415 3V3A_RX))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 5870D7E8)
    (at 148.25 108.5 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C254 (at 0.05 -1.27 180) (layer F.SilkS))
    (fp_text value 100n (at 0 1.7 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 403 "/receiver/RX switch/3V3"))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0603b (layer F.Cu) (tedit 5870D7ED)
    (at 149.925 107.75 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference FB11 (at -1.59 -0.985 270) (layer F.SilkS))
    (fp_text value BLM18PG181SN1D (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 415 3V3A_RX))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 403 "/receiver/RX switch/3V3"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:EVP-AWBA2A (layer F.Cu) (tedit 5870D8D0)
    (at 145.35 84.95 180)
    (fp_text reference SW1 (at -1.4 0.34 270) (layer F.SilkS))
    (fp_text value DNP (at 1 -1.9 180) (layer F.Fab))
    (pad 1 smd rect (at 0 0.5 180) (size 0.55 0.5) (layers F.Cu F.Paste F.Mask)
      (net 340 /3V3D))
    (pad 1 smd rect (at 0 -0.5 180) (size 0.55 0.5) (layers F.Cu F.Paste F.Mask)
      (net 340 /3V3D))
    (pad 2 smd rect (at 3.25 0.5 180) (size 0.55 0.5) (layers F.Cu F.Paste F.Mask)
      (net 397 /fpga/M0))
    (pad 2 smd rect (at 3.25 -0.4 180) (size 0.55 0.5) (layers F.Cu F.Paste F.Mask)
      (net 397 /fpga/M0))
    (pad 2 smd rect (at 3.25 0 180) (size 0.55 1.5) (layers F.Cu F.Mask)
      (net 397 /fpga/M0))
    (pad 1 smd rect (at 0 0 180) (size 0.55 1.5) (layers F.Cu F.Mask)
      (net 340 /3V3D))
  )
  (module VNA:EVP-AWBA2A (layer F.Cu) (tedit 5582E39A)
    (at 124.736958 82.415268 90)
    (fp_text reference SW2 (at 1.5 2.1 90) (layer F.SilkS))
    (fp_text value SW_PUSH (at 1 -1.9 90) (layer F.Fab))
    (pad 1 smd rect (at 0 0 90) (size 0.55 1.5) (layers F.Cu F.Mask)
      (net 402 /fpga/PROGRAM_B))
    (pad 2 smd rect (at 3.25 0 90) (size 0.55 1.5) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 3.25 -0.4 90) (size 0.55 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 3.25 0.5 90) (size 0.55 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0 -0.5 90) (size 0.55 0.5) (layers F.Cu F.Paste F.Mask)
      (net 402 /fpga/PROGRAM_B))
    (pad 1 smd rect (at 0 0.5 90) (size 0.55 0.5) (layers F.Cu F.Paste F.Mask)
      (net 402 /fpga/PROGRAM_B))
  )
  (module VNA:TP_1.00 (layer F.Cu) (tedit 55A404EB)
    (at 148.375 55.25 270)
    (fp_text reference P15 (at 0.125 0.05 270) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 -0.5 270) (layer F.Fab))
    (pad 1 smd circle (at 0 0 270) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 183 /fpga/TCK))
  )
  (module VNA:TP_1.00 (layer F.Cu) (tedit 55A404EB)
    (at 144.175 56.55 270)
    (fp_text reference P16 (at 0.125 0.05 270) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 -0.5 270) (layer F.Fab))
    (pad 1 smd circle (at 0 0 270) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 274 /fpga/TDO))
  )
  (module VNA:TP_1.00 (layer F.Cu) (tedit 55A404EB)
    (at 146.375 56.65 270)
    (fp_text reference P13 (at 0.125 0.05 270) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 -0.5 270) (layer F.Fab))
    (pad 1 smd circle (at 0 0 270) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 187 /fpga/TDI))
  )
  (module VNA:TP_1.00 (layer F.Cu) (tedit 55A404EB)
    (at 142.55 55.55 270)
    (fp_text reference P14 (at 0.125 0.05 270) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 -0.5 270) (layer F.Fab))
    (pad 1 smd circle (at 0 0 270) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 192 /fpga/TMS))
  )
  (module VNA:C_0402b (layer B.Cu) (tedit 55A40188)
    (at 155.1 42.625 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C252 (at 0 1.7 270) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.7 270) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 340 /3V3D))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer B.Cu) (tedit 55A401B2)
    (at 142.265 81.176786 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R113 (at 0 1.4 180) (layer B.SilkS))
    (fp_text value DNP (at 0 -1.8 180) (layer B.Fab))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 401 /fpga/M1))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 340 /3V3D))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer B.Cu) (tedit 55A401B2)
    (at 124.636958 81.365268 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R112 (at 0 1.4 270) (layer B.SilkS))
    (fp_text value 4.7k (at 0 -1.8 270) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 340 /3V3D))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 402 /fpga/PROGRAM_B))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer B.Cu) (tedit 5870DBF2)
    (at 150.63 61.93 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R111 (at -0.65 -1.125 90) (layer B.SilkS))
    (fp_text value 1k (at 0 -1.8 90) (layer B.Fab))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 394 "Net-(P9-Pad1)"))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 340 /3V3D))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer B.Cu) (tedit 55A401B2)
    (at 142.265 82.576786)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R114 (at 0 1.4) (layer B.SilkS))
    (fp_text value 0 (at 0 -1.8) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 401 /fpga/M1))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer B.Cu) (tedit 55A401B2)
    (at 144.62 81.036786 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R115 (at 0 1.4 180) (layer B.SilkS))
    (fp_text value DNP (at 0 -1.8 180) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 340 /3V3D))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 399 /fpga/M2))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer F.Cu) (tedit 5870D9A0)
    (at 151.025 40.225 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R118 (at -0.065 0.995 180) (layer F.SilkS))
    (fp_text value 4.7k (at 0 1.8 180) (layer F.Fab))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 400 /fpga/SPI_CS))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 340 /3V3D))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer B.Cu) (tedit 55A401B2)
    (at 144.67 82.536786)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R116 (at 0 1.4) (layer B.SilkS))
    (fp_text value 0 (at 0 -1.8) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 399 /fpga/M2))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer B.Cu) (tedit 5870DBEF)
    (at 146.49 68.03 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R117 (at -0.63 1.22 270) (layer B.SilkS))
    (fp_text value 4.7k (at 0 -1.8 270) (layer B.Fab))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 398 /fpga/INIT_B))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 340 /3V3D))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer B.Cu) (tedit 55A401B2)
    (at 142.85 84.95 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R110 (at 0 1.4 90) (layer B.SilkS))
    (fp_text value DNP (at 0 -1.8 90) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 397 /fpga/M0))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:TP_1.00 (layer F.Cu) (tedit 55A404EB)
    (at 157.64 46.58)
    (fp_text reference P11 (at 0.125 0.05) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 -0.5) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 396 /fpga/SPI_MOSI))
  )
  (module VNA:TP_1.00 (layer F.Cu) (tedit 55A404EB)
    (at 148.21 42.53)
    (fp_text reference P12 (at 0.125 0.05) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 -0.5) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 395 /fpga/SPI_DIN))
  )
  (module VNA:TP_1.00 (layer F.Cu) (tedit 55A404EB)
    (at 150.85 61.11)
    (fp_text reference P9 (at 0.125 0.05) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 -0.5) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 394 "Net-(P9-Pad1)"))
  )
  (module VNA:TP_1.00 (layer F.Cu) (tedit 55A404EB)
    (at 157.68 44.94)
    (fp_text reference P10 (at 0.125 0.05) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 -0.5) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 393 /fpga/CCLK))
  )
  (module VNA:C_0402b (layer B.Cu) (tedit 55A40188)
    (at 137.63 67.76)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C191 (at 0 1.7) (layer B.SilkS))
    (fp_text value 470n (at 0 -1.7) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 368 /1V0))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:LED_0603 (layer F.Cu) (tedit 57404998)
    (at 125.95 63.025 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference D6 (at -2.21 0.05 270) (layer F.SilkS))
    (fp_text value LED (at 0 1.9 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 391 "Net-(D6-Pad2)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:LED_0603 (layer F.Cu) (tedit 5870D973)
    (at 122.37 43.95 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference D5 (at 0.06 -1.52 180) (layer F.SilkS))
    (fp_text value LED (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 392 "Net-(D5-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer F.Cu) (tedit 5870D975)
    (at 123.96 43.59 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R108 (at 0.08 1.05 90) (layer F.SilkS))
    (fp_text value 240 (at 0 1.8 90) (layer F.Fab))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 392 "Net-(D5-Pad2)"))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 168 /3V6))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer B.Cu) (tedit 5870DC2D)
    (at 126.925 63.75 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R109 (at -1.015 1.08 180) (layer B.SilkS))
    (fp_text value 240 (at 0 -1.8 180) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 390 /fpga/LED))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 391 "Net-(D6-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer B.Cu) (tedit 5870DC1D)
    (at 128.525 75.75 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C251 (at 0.015 1.02 180) (layer B.SilkS))
    (fp_text value 470n (at 0 -1.7 180) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 340 /3V3D))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer B.Cu) (tedit 5870DC00)
    (at 140.725 66.75)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C250 (at -0.015 -1.56 90) (layer B.SilkS))
    (fp_text value 470n (at 0 -1.7) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 368 /1V0))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 5870D88B)
    (at 145.12 93.17)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C150 (at 0.13 -0.98) (layer F.SilkS))
    (fp_text value 10n (at 0 1.7) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 103 "Net-(C150-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 5870D88A)
    (at 145.23 95.08)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C153 (at 0.07 -0.95) (layer F.SilkS))
    (fp_text value 10n (at 0 1.7) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 80 /receiver/DITHER))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer F.Cu) (tedit 5870D88C)
    (at 143.48 92.68 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R59 (at 0.05 -1.02 90) (layer F.SilkS))
    (fp_text value 100 (at 0 1.8 90) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 103 "Net-(C150-Pad1)"))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 388 "Net-(C132-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer F.Cu) (tedit 5870D888)
    (at 143.49 94.66 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R107 (at 0.17 -1.1 90) (layer F.SilkS))
    (fp_text value 100 (at 0 1.8 90) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 80 /receiver/DITHER))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 103 "Net-(C150-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 55A40188)
    (at 162.125 60.7 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C151 (at 0 -1.7 90) (layer F.SilkS))
    (fp_text value 1n (at 0 1.7 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 151 "/port switch/RFC"))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 107 "Net-(C151-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1210 (layer F.Cu) (tedit 5870D94A)
    (at 126.85 51.66 90)
    (descr "Capacitor SMD 1210, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C181 (at 0 -2.67 90) (layer F.SilkS))
    (fp_text value 100u (at 0 2.7 90) (layer F.Fab))
    (pad 2 smd rect (at 1.5 0 90) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.5 0 90) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 368 /1V0))
    (model Capacitors_SMD.3dshapes/C_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer F.Cu) (tedit 5870D912)
    (at 111.19 71.54)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R87 (at -1.46 -0.03 90) (layer F.SilkS))
    (fp_text value 0 (at 0 1.8) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 381 /power/fpga_power/SYNC_1V8))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 387 /power/fpga_power/SYNC_1V0))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DFN_QFN:DFN-8-1EP_3x3mm_Pitch0.5mm (layer F.Cu) (tedit 5870D902)
    (at 114.69 82.05)
    (descr "DD Package; 8-Lead Plastic DFN (3mm x 3mm) (see Linear Technology DFN_8_05-08-1698.pdf)")
    (tags "DFN 0.5")
    (attr smd)
    (fp_text reference U38 (at 3.23 -3.33 90) (layer F.SilkS))
    (fp_text value L7980 (at 0 2.55) (layer F.Fab))
    (pad 1 smd rect (at -1.4 -0.75) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 369 "Net-(D4-Pad1)"))
    (pad 2 smd rect (at -1.4 -0.25) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 381 /power/fpga_power/SYNC_1V8))
    (pad 3 smd rect (at -1.4 0.25) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 341 /5V))
    (pad 4 smd rect (at -1.4 0.75) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 375 "Net-(C237-Pad1)"))
    (pad 5 smd rect (at 1.4 0.75) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 371 "Net-(C235-Pad2)"))
    (pad 6 smd rect (at 1.4 0.25) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 378 "Net-(R98-Pad1)"))
    (pad 7 smd rect (at 1.4 -0.25) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 8 smd rect (at 1.4 -0.75) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 56 /power/12V))
    (pad 9 smd rect (at 0.415 0.595) (size 0.83 1.19) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (pad 9 smd rect (at 0.415 -0.595) (size 0.83 1.19) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (pad 9 smd rect (at -0.415 0.595) (size 0.83 1.19) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (pad 9 smd rect (at -0.415 -0.595) (size 0.83 1.19) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (model Housings_DFN_QFN.3dshapes/DFN-8-1EP_3x3mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DFN_QFN:DFN-8-1EP_3x3mm_Pitch0.5mm (layer F.Cu) (tedit 5870D937)
    (at 115.25 68.33)
    (descr "DD Package; 8-Lead Plastic DFN (3mm x 3mm) (see Linear Technology DFN_8_05-08-1698.pdf)")
    (tags "DFN 0.5")
    (attr smd)
    (fp_text reference U37 (at 4.08 -3.26) (layer F.SilkS))
    (fp_text value L7980 (at 0 2.55) (layer F.Fab))
    (pad 9 smd rect (at -0.415 -0.595) (size 0.83 1.19) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (pad 9 smd rect (at -0.415 0.595) (size 0.83 1.19) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (pad 9 smd rect (at 0.415 -0.595) (size 0.83 1.19) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (pad 9 smd rect (at 0.415 0.595) (size 0.83 1.19) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (pad 8 smd rect (at 1.4 -0.75) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 56 /power/12V))
    (pad 7 smd rect (at 1.4 -0.25) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 1.4 0.25) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 377 "Net-(R96-Pad1)"))
    (pad 5 smd rect (at 1.4 0.75) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 376 "Net-(C234-Pad2)"))
    (pad 4 smd rect (at -1.4 0.75) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 372 "Net-(C236-Pad1)"))
    (pad 3 smd rect (at -1.4 0.25) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 341 /5V))
    (pad 2 smd rect (at -1.4 -0.25) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 387 /power/fpga_power/SYNC_1V0))
    (pad 1 smd rect (at -1.4 -0.75) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 367 "Net-(D1-Pad1)"))
    (model Housings_DFN_QFN.3dshapes/DFN-8-1EP_3x3mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 5870D8E4)
    (at 112.98 86.295)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C239 (at -2.39 0.075) (layer F.SilkS))
    (fp_text value 18n (at 0 1.7) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 380 "Net-(C239-Pad1)"))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 371 "Net-(C235-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 5870D926)
    (at 117.88 71.245)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C238 (at 0.02 0.985) (layer F.SilkS))
    (fp_text value 16n (at 0 1.7) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 376 "Net-(C234-Pad2)"))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 379 "Net-(C238-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 5870D8F1)
    (at 117.53 84.695)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C237 (at -0.09 -0.855) (layer F.SilkS))
    (fp_text value 33p (at 0 1.7) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 375 "Net-(C237-Pad1)"))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 371 "Net-(C235-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 5870D919)
    (at 113.75 71.3 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C236 (at 1.26 -0.73) (layer F.SilkS))
    (fp_text value 36p (at 0 1.7 270) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 376 "Net-(C234-Pad2)"))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 372 "Net-(C236-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 5870D8EF)
    (at 117.48 85.945)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C235 (at 2 0.165) (layer F.SilkS))
    (fp_text value 10n (at 0 1.7) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 371 "Net-(C235-Pad2)"))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 374 "Net-(C235-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer B.Cu) (tedit 5870DB38)
    (at 114.61 71.17 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C234 (at -2.13 0.09 180) (layer B.SilkS))
    (fp_text value 10n (at 0 -1.7 180) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 373 "Net-(C234-Pad1)"))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 376 "Net-(C234-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0603b (layer F.Cu) (tedit 55A401E5)
    (at 159.77 45.1 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C229 (at 0 -1.425 270) (layer F.SilkS))
    (fp_text value 1u (at 0 1.9 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 171 /3V3A))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0603b (layer F.Cu) (tedit 5870D9A6)
    (at 160.255 38.685 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C228 (at 0.055 1.115 180) (layer F.SilkS))
    (fp_text value 1u (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 168 /3V6))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0603b (layer F.Cu) (tedit 5870D82D)
    (at 124.425 91.875 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C249 (at -0.125 1.335 270) (layer F.SilkS))
    (fp_text value 1u (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 370 /fpga/adc/3V0))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0805b (layer F.Cu) (tedit 5870D932)
    (at 119.29 67.05)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C230 (at 2.79 -0.5) (layer F.SilkS))
    (fp_text value 10u (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 56 /power/12V))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0805b (layer F.Cu) (tedit 5870D947)
    (at 120.27 55.075)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C231 (at 2.42 -0.025 90) (layer F.SilkS))
    (fp_text value 10u (at 0 2.1) (layer F.Fab))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 56 /power/12V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0805b (layer F.Cu) (tedit 5870D934)
    (at 119.29 68.22)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C232 (at 2.87 -0.83) (layer F.SilkS))
    (fp_text value 10u (at 0 2.1) (layer F.Fab))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 56 /power/12V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0805b (layer F.Cu) (tedit 5870D93D)
    (at 120.98 58.795 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C240 (at 2.515 1.01) (layer F.SilkS))
    (fp_text value 10u (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 368 /1V0))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0805b (layer F.Cu) (tedit 5870D82E)
    (at 127.13 95.65)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C248 (at -0.05 1.63) (layer F.SilkS))
    (fp_text value 10u (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 168 /3V6))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0805b (layer F.Cu) (tedit 5870D8FD)
    (at 119.93 78.295 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C247 (at -0.815 -3.26) (layer F.SilkS))
    (fp_text value 10u (at 0 2.1 270) (layer F.Fab))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 199 /1V8))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0805b (layer F.Cu) (tedit 5870D93B)
    (at 115.075 57.475 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C246 (at 3.155 0.005 180) (layer F.SilkS))
    (fp_text value 10u (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 368 /1V0))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0805b (layer F.Cu) (tedit 5870D908)
    (at 121.03 74.295 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C245 (at 0.035 2.11 180) (layer F.SilkS))
    (fp_text value 10u (at 0 2.1 90) (layer F.Fab))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 199 /1V8))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0805b (layer F.Cu) (tedit 5870D93F)
    (at 119.78 58.795 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C244 (at 3.365 -0.24) (layer F.SilkS))
    (fp_text value 10u (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 368 /1V0))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0805b (layer F.Cu) (tedit 5870D942)
    (at 118.53 58.795 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C243 (at 4.275 -1.43) (layer F.SilkS))
    (fp_text value 10u (at 0 2.1 270) (layer F.Fab))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 368 /1V0))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0805b (layer F.Cu) (tedit 5870D905)
    (at 119.78 74.295 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C242 (at 0.895 3.36 180) (layer F.SilkS))
    (fp_text value 10u (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 199 /1V8))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0805b (layer F.Cu) (tedit 5870D8FE)
    (at 121.13 78.295 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C241 (at 0.025 -2.04) (layer F.SilkS))
    (fp_text value 10u (at 0 2.1 270) (layer F.Fab))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 199 /1V8))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0805b (layer F.Cu) (tedit 5870D8F6)
    (at 119.01 81.23)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C233 (at 2.81 0.11) (layer F.SilkS))
    (fp_text value 10u (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 56 /power/12V))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer F.Cu) (tedit 5870D8E3)
    (at 112.23 84.995 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R106 (at 1.98 -0.485 180) (layer F.SilkS))
    (fp_text value 33 (at 0 1.8 180) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 199 /1V8))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 380 "Net-(C239-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer F.Cu) (tedit 5870D92C)
    (at 115.97 70.89)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R105 (at -0.05 -0.59) (layer F.SilkS))
    (fp_text value 33 (at 0 1.8) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 368 /1V0))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 379 "Net-(C238-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer F.Cu) (tedit 5870D8F4)
    (at 118.11 82.87)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R98 (at 1.95 -0.15) (layer F.SilkS))
    (fp_text value 68k (at 0 1.8) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 378 "Net-(R98-Pad1)"))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer F.Cu) (tedit 5870D92F)
    (at 118.56 69.49)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R96 (at 2 0.05) (layer F.SilkS))
    (fp_text value 68k (at 0 1.8) (layer F.Fab))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 377 "Net-(R96-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer F.Cu) (tedit 5870D8E8)
    (at 113.98 84.995)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R103 (at 0.01 -0.955) (layer F.SilkS))
    (fp_text value 4.99k (at 0 1.8) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 199 /1V8))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 371 "Net-(C235-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer F.Cu) (tedit 5870D922)
    (at 119.3 70.76 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R102 (at 0.17 1.9 180) (layer F.SilkS))
    (fp_text value 7.5k (at 0 1.8 90) (layer F.Fab))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 376 "Net-(C234-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer F.Cu) (tedit 5870D928)
    (at 115.13 71.81 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R101 (at -1.33 -0.92 180) (layer F.SilkS))
    (fp_text value 4.99k (at 0 1.8 180) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 368 /1V0))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 376 "Net-(C234-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer F.Cu) (tedit 5870D8EC)
    (at 115.68 85.345 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R100 (at 1.115 0.5) (layer F.SilkS))
    (fp_text value 16k (at 0 1.8 270) (layer F.Fab))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 374 "Net-(C235-Pad1)"))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 375 "Net-(C237-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer B.Cu) (tedit 5870DB35)
    (at 113.97 69.88 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R99 (at 0.02 1.38 270) (layer B.SilkS))
    (fp_text value 15k (at 0 -1.8 180) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 372 "Net-(C236-Pad1)"))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 373 "Net-(C234-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer F.Cu) (tedit 5870D8F0)
    (at 119.43 84.695)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R104 (at 0.15 -1.115) (layer F.SilkS))
    (fp_text value 2.5k (at 0 1.8) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 371 "Net-(C235-Pad2)"))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:SOD-123F (layer F.Cu) (tedit 5870D8E2)
    (at 110.38 82.51 270)
    (fp_text reference D4 (at 1.09 -1.71 90) (layer F.SilkS))
    (fp_text value SS13FL (at -0.3 -2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1.5 -0.1 270) (size 1.34 1.8) (layers F.Cu F.Paste F.Mask)
      (net 369 "Net-(D4-Pad1)"))
    (pad 2 smd rect (at 1.36 -0.1 270) (size 1.34 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module VNA:SOD-123F (layer F.Cu) (tedit 5870D90F)
    (at 111.33 68.745 270)
    (fp_text reference D1 (at -0.155 1.57 270) (layer F.SilkS))
    (fp_text value SS13FL (at -0.3 -2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1.5 -0.1 270) (size 1.34 1.8) (layers F.Cu F.Paste F.Mask)
      (net 367 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 1.36 -0.1 270) (size 1.34 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module VNA:SOT-23-5 (layer F.Cu) (tedit 5870D82A)
    (at 125.866323 93.501517)
    (fp_text reference U39 (at 1.053677 -1.321517) (layer F.SilkS))
    (fp_text value LP5907-3V0 (at 0 -4.05) (layer F.SilkS))
    (pad 5 smd rect (at 0 -2.6) (size 0.6 1.25) (layers F.Cu F.Paste F.Mask)
      (net 370 /fpga/adc/3V0))
    (pad 4 smd rect (at 1.9 -2.6) (size 0.6 1.25) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 1.9 0) (size 0.6 1.05) (layers F.Cu F.Paste F.Mask)
      (net 168 /3V6))
    (pad 2 smd rect (at 0.95 0) (size 0.6 1.05) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0 0) (size 0.6 1.05) (layers F.Cu F.Paste F.Mask)
      (net 168 /3V6))
  )
  (module VNA:SRR6040A (layer F.Cu) (tedit 5870D900)
    (at 113.28 76.165 90)
    (fp_text reference L10 (at 0.205 0.21 90) (layer F.SilkS))
    (fp_text value "33u (SRR6040A-330M)" (at -0.25 -4.9 90) (layer F.Fab))
    (pad 2 smd rect (at 3.075 1.7 90) (size 0.65 1) (layers F.Cu F.Paste F.Mask)
      (net 199 /1V8))
    (pad 2 smd rect (at -3.575 1.7 90) (size 0.65 1) (layers F.Cu F.Paste F.Mask)
      (net 199 /1V8))
    (pad 1 smd rect (at 3.075 -1.7 90) (size 0.65 1) (layers F.Cu F.Paste F.Mask)
      (net 369 "Net-(D4-Pad1)"))
    (pad 1 smd rect (at -3.575 -1.7 90) (size 0.65 1) (layers F.Cu F.Paste F.Mask)
      (net 369 "Net-(D4-Pad1)"))
    (pad 2 smd rect (at -0.25 2.9 90) (size 7.3 1.4) (layers F.Cu F.Paste F.Mask)
      (net 199 /1V8))
    (pad 1 smd rect (at -0.25 -2.9 90) (size 7.3 1.4) (layers F.Cu F.Paste F.Mask)
      (net 369 "Net-(D4-Pad1)"))
  )
  (module VNA:SRR6040A (layer F.Cu) (tedit 5870D938)
    (at 113.88 62.17 90)
    (fp_text reference L9 (at -0.07 0.3 180) (layer F.SilkS))
    (fp_text value "33u (SRR6040A-330M)" (at -0.25 -4.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.25 -2.9 90) (size 7.3 1.4) (layers F.Cu F.Paste F.Mask)
      (net 367 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at -0.25 2.9 90) (size 7.3 1.4) (layers F.Cu F.Paste F.Mask)
      (net 368 /1V0))
    (pad 1 smd rect (at -3.575 -1.7 90) (size 0.65 1) (layers F.Cu F.Paste F.Mask)
      (net 367 "Net-(D1-Pad1)"))
    (pad 1 smd rect (at 3.075 -1.7 90) (size 0.65 1) (layers F.Cu F.Paste F.Mask)
      (net 367 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at -3.575 1.7 90) (size 0.65 1) (layers F.Cu F.Paste F.Mask)
      (net 368 /1V0))
    (pad 2 smd rect (at 3.075 1.7 90) (size 0.65 1) (layers F.Cu F.Paste F.Mask)
      (net 368 /1V0))
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 5870D9C4)
    (at 154.16 50.11 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C227 (at -0.05 1.14 270) (layer F.SilkS))
    (fp_text value 100n (at 0 1.7 270) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 171 /3V3A))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 5870D9C9)
    (at 156.91 53.69)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C226 (at 1.08 -1.05) (layer F.SilkS))
    (fp_text value 100p (at 0 1.7) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 366 "Net-(C226-Pad1)"))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer F.Cu) (tedit 5870D9BF)
    (at 155.35 54.1 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R94 (at 0 -1.21 90) (layer F.SilkS))
    (fp_text value 22k (at 0 1.8 90) (layer F.Fab))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 366 "Net-(C226-Pad1)"))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 363 "Net-(R94-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer F.Cu) (tedit 55A401B2)
    (at 155.79 52.88)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R95 (at 0 -1.4) (layer F.SilkS))
    (fp_text value 10k (at 0 1.8) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 366 "Net-(C226-Pad1)"))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:SOT-23-5 (layer F.Cu) (tedit 5870D9C2)
    (at 155.37 51.55)
    (fp_text reference U35 (at 1.01 -1.35) (layer F.SilkS))
    (fp_text value TSV911 (at 0 -4.05) (layer F.SilkS))
    (pad 1 smd rect (at 0 0) (size 0.6 1.05) (layers F.Cu F.Paste F.Mask)
      (net 426 "Net-(R122-Pad2)"))
    (pad 2 smd rect (at 0.95 0) (size 0.6 1.05) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.9 0) (size 0.6 1.05) (layers F.Cu F.Paste F.Mask)
      (net 366 "Net-(C226-Pad1)"))
    (pad 4 smd rect (at 1.9 -2.6) (size 0.6 1.25) (layers F.Cu F.Paste F.Mask)
      (net 426 "Net-(R122-Pad2)"))
    (pad 5 smd rect (at 0 -2.6) (size 0.6 1.25) (layers F.Cu F.Paste F.Mask)
      (net 171 /3V3A))
  )
  (module VNA:R_0402b (layer B.Cu) (tedit 5870DBEB)
    (at 146.45 71.17 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R74 (at 1.665 0.1 90) (layer B.SilkS))
    (fp_text value 220k (at 0 -1.8 270) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 178 /DITHER))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 82 "Net-(C129-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer B.Cu) (tedit 5870DBEC)
    (at 147.3 71.17 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R75 (at -1.73 0.085 270) (layer B.SilkS))
    (fp_text value 4.7k (at 0 -1.8 90) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 82 "Net-(C129-Pad1)"))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0603b (layer F.Cu) (tedit 5870D713)
    (at 168.325 101.1 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R21 (at -2.03 0.055 180) (layer F.SilkS))
    (fp_text value 1.8 (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 109 "Net-(C113-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 79 "Net-(C115-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0603b (layer F.Cu) (tedit 5870DA08)
    (at 164.7 56.95 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R89 (at 0.63 -1.91) (layer F.SilkS))
    (fp_text value 1.8 (at 0 1.9 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 100 "Net-(C145-Pad1)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 99 "Net-(C142-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 5870D953)
    (at 134.26 53.26 90)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C182 (at -0.14 2.35 90) (layer F.SilkS))
    (fp_text value 47u (at 0 2.3 90) (layer F.Fab))
    (pad 2 smd rect (at 1.5 0 90) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.5 0 90) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 199 /1V8))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 5870D94F)
    (at 129.65 51.58 90)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C184 (at -2.9 -1.05 180) (layer F.SilkS))
    (fp_text value 47u (at 0 2.3 90) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 90) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 368 /1V0))
    (pad 2 smd rect (at 1.5 0 90) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 5870D8CD)
    (at 143.15 78.7)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C196 (at -3.41 0.26 90) (layer F.SilkS))
    (fp_text value 47u (at 0 2.3) (layer F.Fab))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 340 /3V3D))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DFN_QFN:QFN-32-1EP_5x5mm_Pitch0.5mm (layer F.Cu) (tedit 5870D8B3)
    (at 133.9 85.575 90)
    (descr "UH Package; 32-Lead Plastic QFN (5mm x 5mm); (see Linear Technology QFN_32_05-08-1693.pdf)")
    (tags "QFN 0.5")
    (attr smd)
    (fp_text reference U34 (at 0.105 0.04 180) (layer F.SilkS))
    (fp_text value LTC2247 (at 0 3.75 90) (layer F.Fab))
    (pad 33 smd rect (at -0.8625 -0.8625 90) (size 1.725 1.725) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (pad 33 smd rect (at -0.8625 0.8625 90) (size 1.725 1.725) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (pad 33 smd rect (at 0.8625 -0.8625 90) (size 1.725 1.725) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (pad 33 smd rect (at 0.8625 0.8625 90) (size 1.725 1.725) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (pad 32 smd rect (at -1.75 -2.4 180) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 370 /fpga/adc/3V0))
    (pad 31 smd rect (at -1.25 -2.4 180) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 116 /ADC_VCM))
    (pad 30 smd rect (at -0.75 -2.4 180) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 188 "Net-(R93-Pad1)"))
    (pad 29 smd rect (at -0.25 -2.4 180) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 104 "Net-(R91-Pad2)"))
    (pad 28 smd rect (at 0.25 -2.4 180) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 360 /fpga/OF))
    (pad 27 smd rect (at 0.75 -2.4 180) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 283 /fpga/D13))
    (pad 26 smd rect (at 1.25 -2.4 180) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 260 /fpga/D12))
    (pad 25 smd rect (at 1.75 -2.4 180) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 261 /fpga/D11))
    (pad 24 smd rect (at 2.4 -1.75 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 275 /fpga/D10))
    (pad 23 smd rect (at 2.4 -1.25 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 276 /fpga/D9))
    (pad 22 smd rect (at 2.4 -0.75 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 269 /fpga/D8))
    (pad 21 smd rect (at 2.4 -0.25 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 340 /3V3D))
    (pad 20 smd rect (at 2.4 0.25 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 19 smd rect (at 2.4 0.75 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 277 /fpga/D7))
    (pad 18 smd rect (at 2.4 1.25 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 284 /fpga/D6))
    (pad 17 smd rect (at 2.4 1.75 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 290 /fpga/D5))
    (pad 16 smd rect (at 1.75 2.4 180) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 254 /fpga/D4))
    (pad 15 smd rect (at 1.25 2.4 180) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 255 /fpga/D3))
    (pad 14 smd rect (at 0.75 2.4 180) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 263 /fpga/D2))
    (pad 13 smd rect (at 0.25 2.4 180) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 268 /fpga/D1))
    (pad 12 smd rect (at -0.25 2.4 180) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 262 /fpga/D0))
    (pad 11 smd rect (at -0.75 2.4 180) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 361 /fpga/ADC_OE))
    (pad 10 smd rect (at -1.25 2.4 180) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 362 /fpga/ADC_SHDN))
    (pad 9 smd rect (at -1.75 2.4 180) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 339 /CLK_ADC))
    (pad 8 smd rect (at -2.4 1.75 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 7 smd rect (at -2.4 1.25 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 370 /fpga/adc/3V0))
    (pad 6 smd rect (at -2.4 0.75 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 384 /fpga/adc/REFL))
    (pad 5 smd rect (at -2.4 0.25 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 384 /fpga/adc/REFL))
    (pad 4 smd rect (at -2.4 -0.25 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 383 /fpga/adc/REFH))
    (pad 3 smd rect (at -2.4 -0.75 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 383 /fpga/adc/REFH))
    (pad 2 smd rect (at -2.4 -1.25 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 172 /ADC-))
    (pad 1 smd rect (at -2.4 -1.75 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 170 /ADC+))
    (model Housings_DFN_QFN.3dshapes/QFN-32-1EP_5x5mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_QFP:LQFP-48_7x7mm_Pitch0.5mm (layer F.Cu) (tedit 5870D999)
    (at 143.225 47.3)
    (descr "48 LEAD LQFP 7x7mm (see MICREL LQFP7x7-48LD-PL-1.pdf)")
    (tags "QFP 0.5")
    (attr smd)
    (fp_text reference U33 (at -0.015 -0.01) (layer F.SilkS))
    (fp_text value FT2232D (at 0 6) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 48 smd rect (at -2.75 -4.35 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 164 /fpga/usb/EECS))
    (pad 47 smd rect (at -2.25 -4.35 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 46 smd rect (at -1.75 -4.35 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 382 "Net-(C213-Pad1)"))
    (pad 45 smd rect (at -1.25 -4.35 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 44 smd rect (at -0.75 -4.35 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 344 "Net-(C209-Pad1)"))
    (pad 43 smd rect (at -0.25 -4.35 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 342 "Net-(C208-Pad1)"))
    (pad 42 smd rect (at 0.25 -4.35 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 406 /fpga/usb/5V))
    (pad 41 smd rect (at 0.75 -4.35 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 351 "Net-(U33-Pad41)"))
    (pad 40 smd rect (at 1.25 -4.35 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 300 /fpga/FT_D0))
    (pad 39 smd rect (at 1.75 -4.35 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 301 /fpga/FT_D1))
    (pad 38 smd rect (at 2.25 -4.35 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 291 /fpga/FT_D2))
    (pad 37 smd rect (at 2.75 -4.35 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 286 /fpga/FT_D3))
    (pad 36 smd rect (at 4.35 -2.75) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 279 /fpga/FT_D4))
    (pad 35 smd rect (at 4.35 -2.25) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 285 /fpga/FT_D5))
    (pad 34 smd rect (at 4.35 -1.75) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 33 smd rect (at 4.35 -1.25) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 278 /fpga/FT_D6))
    (pad 32 smd rect (at 4.35 -0.75) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 270 /fpga/FT_D7))
    (pad 31 smd rect (at 4.35 -0.25) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 340 /3V3D))
    (pad 30 smd rect (at 4.35 0.25) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 208 /fpga/RXF#))
    (pad 29 smd rect (at 4.35 0.75) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 220 /fpga/TXE#))
    (pad 28 smd rect (at 4.35 1.25) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 231 /fpga/RD#))
    (pad 27 smd rect (at 4.35 1.75) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 230 /fpga/WR))
    (pad 26 smd rect (at 4.35 2.25) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 242 /fpga/SI/WUB))
    (pad 25 smd rect (at 4.35 2.75) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 24 smd rect (at 2.75 4.35 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 182 "Net-(R84-Pad2)"))
    (pad 23 smd rect (at 2.25 4.35 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 186 "Net-(R88-Pad2)"))
    (pad 22 smd rect (at 1.75 4.35 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 274 /fpga/TDO))
    (pad 21 smd rect (at 1.25 4.35 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 191 "Net-(R85-Pad2)"))
    (pad 20 smd rect (at 0.75 4.35 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 352 "Net-(U33-Pad20)"))
    (pad 19 smd rect (at 0.25 4.35 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 353 "Net-(U33-Pad19)"))
    (pad 18 smd rect (at -0.25 4.35 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 17 smd rect (at -0.75 4.35 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 354 "Net-(U33-Pad17)"))
    (pad 16 smd rect (at -1.25 4.35 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 355 "Net-(U33-Pad16)"))
    (pad 15 smd rect (at -1.75 4.35 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 356 "Net-(U33-Pad15)"))
    (pad 14 smd rect (at -2.25 4.35 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 340 /3V3D))
    (pad 13 smd rect (at -2.75 4.35 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 357 "Net-(U33-Pad13)"))
    (pad 12 smd rect (at -4.35 2.75) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 358 "Net-(U33-Pad12)"))
    (pad 11 smd rect (at -4.35 2.25) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 359 "Net-(U33-Pad11)"))
    (pad 10 smd rect (at -4.35 1.75) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 340 /3V3D))
    (pad 9 smd rect (at -4.35 1.25) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 8 smd rect (at -4.35 0.75) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 180 "Net-(R80-Pad1)"))
    (pad 7 smd rect (at -4.35 0.25) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 181 "Net-(R81-Pad1)"))
    (pad 6 smd rect (at -4.35 -0.25) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 343 "Net-(C210-Pad1)"))
    (pad 5 smd rect (at -4.35 -0.75) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 90 "Net-(R82-Pad2)"))
    (pad 4 smd rect (at -4.35 -1.25) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 193 "Net-(R71-Pad2)"))
    (pad 3 smd rect (at -4.35 -1.75) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 406 /fpga/usb/5V))
    (pad 2 smd rect (at -4.35 -2.25) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 166 /fpga/usb/EEDATA))
    (pad 1 smd rect (at -4.35 -2.75) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 165 /fpga/usb/EESK))
    (model Housings_QFP.3dshapes/LQFP-48_7x7mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:ABMM (layer F.Cu) (tedit 584D6D1A)
    (at 146.41 38 180)
    (fp_text reference Y1 (at 3.3 -1.3 270) (layer F.SilkS))
    (fp_text value ABMM-6.000MHZ (at 3.075 -4.625 180) (layer F.Fab))
    (pad 1 smd rect (at 0 0 180) (size 2.2 1.4) (layers F.Cu F.Paste F.Mask)
      (net 342 "Net-(C208-Pad1)"))
    (pad 2 smd rect (at 6.3 0 180) (size 2.2 1.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 6.3 -2.54 180) (size 2.2 1.4) (layers F.Cu F.Paste F.Mask)
      (net 344 "Net-(C209-Pad1)"))
    (pad 4 smd rect (at 0 -2.54 180) (size 2.2 1.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 5870D717)
    (at 164.075 97.85 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C121 (at 0.05 -1.105 270) (layer F.SilkS))
    (fp_text value 1n (at 0 1.7 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 162 /receiver/RF_BALUN))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 337 "Net-(C121-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 5870D868)
    (at 131.875 101.25)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C140 (at 0.885 0.85) (layer F.SilkS))
    (fp_text value 36p (at 0 1.7) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 97 "Net-(C135-Pad1)"))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 88 "Net-(C135-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 5870D873)
    (at 130.875 98.8)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C144 (at -1.885 -0.84) (layer F.SilkS))
    (fp_text value 18p (at 0 1.7) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 110 "Net-(C144-Pad2)"))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 115 "Net-(C144-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 5870D862)
    (at 132.975 98.825 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C146 (at -2.395 0.575 180) (layer F.SilkS))
    (fp_text value 18p (at 0 1.7 180) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 102 "Net-(C146-Pad2)"))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 101 "Net-(C146-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 5870D879)
    (at 134.72 95.01 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C148 (at 2.35 0.01 90) (layer F.SilkS))
    (fp_text value 100n (at 0 1.7 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 415 3V3A_RX))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 5870D87A)
    (at 134.28 93.39)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C149 (at 2.38 -0.05) (layer F.SilkS))
    (fp_text value 100n (at 0 1.7) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 116 /ADC_VCM))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 55A40188)
    (at 134.05 91.6 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C154 (at 0 -1.7 180) (layer F.SilkS))
    (fp_text value 100p (at 0 1.7 180) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 172 /ADC-))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 5870D8B9)
    (at 132.05 91.634774 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C155 (at 1.43 1.134774 180) (layer F.SilkS))
    (fp_text value 220p (at 0 1.7 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 172 /ADC-))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 170 /ADC+))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer B.Cu) (tedit 5870DBA2)
    (at 168.659966 96.65524 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C124 (at -0.11524 -1.150034 270) (layer B.SilkS))
    (fp_text value DNP (at 0 -1.7 270) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 176 "Net-(C123-Pad2)"))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer B.Cu) (tedit 5870DB8F)
    (at 166.759966 91.95524 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C125 (at -1.70524 0.739966) (layer B.SilkS))
    (fp_text value DNP (at 0 -1.7 270) (layer B.Fab))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 81 "Net-(C125-Pad2)"))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer B.Cu) (tedit 5870DB95)
    (at 168.559966 94.15524 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C123 (at -2.91524 -1.440034 270) (layer B.SilkS))
    (fp_text value DNP (at 0 -1.7 270) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 179 "Net-(C122-Pad2)"))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 176 "Net-(C123-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer B.Cu) (tedit 5870DB84)
    (at 165.106873 94.048369 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C126 (at -2.138369 0.546873 90) (layer B.SilkS))
    (fp_text value DNP (at 0 -1.7 270) (layer B.Fab))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 177 "Net-(C126-Pad2)"))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 81 "Net-(C125-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 5870D84F)
    (at 135.825 99.875)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C139 (at 2.245 -0.055) (layer F.SilkS))
    (fp_text value 100n (at 0 1.7) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 80 /receiver/DITHER))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 92 "Net-(C139-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer B.Cu) (tedit 5870DAE7)
    (at 139.45 115.375)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C54 (at -0.74 1.075) (layer B.SilkS))
    (fp_text value 18p (at 0 -1.7) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 213 /RX_SW3))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer B.Cu) (tedit 5870DB7C)
    (at 166.759966 96.33 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C127 (at 1.82 0.299966) (layer B.SilkS))
    (fp_text value DNP (at 0 -1.7 270) (layer B.Fab))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 177 "Net-(C126-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer B.Cu) (tedit 5870DB81)
    (at 164.006873 94.048369 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C128 (at 2.161631 -0.013127 90) (layer B.SilkS))
    (fp_text value 18p (at 0 -1.7 270) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 81 "Net-(C125-Pad2)"))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 177 "Net-(C126-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 5870D84C)
    (at 128.125 99.925 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C138 (at 1.815 -0.135 270) (layer F.SilkS))
    (fp_text value DNP (at 0 1.7 180) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 91 "Net-(C138-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer B.Cu) (tedit 55A40188)
    (at 168.559966 91.95524 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C122 (at 0 1.7 270) (layer B.SilkS))
    (fp_text value DNP (at 0 -1.7 270) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 179 "Net-(C122-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer B.Cu) (tedit 55A40188)
    (at 159.98 94.15 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C135 (at 0 1.7 270) (layer B.SilkS))
    (fp_text value 100p (at 0 -1.7 270) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 97 "Net-(C135-Pad1)"))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 88 "Net-(C135-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 5870D710)
    (at 166.4 100.325 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (zone_connect 2)
    (attr smd)
    (fp_text reference C115 (at 2.405 -0.08) (layer F.SilkS))
    (fp_text value 10p (at 0 1.7 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 79 "Net-(C115-Pad1)") (zone_connect 2))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 5870D7BD)
    (at 180.98 113.8 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C180 (at 0.13 -2.94 180) (layer F.SilkS))
    (fp_text value 1n (at 0 1.7 90) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 152 "Net-(C180-Pad2)"))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 350 /PORT1))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer B.Cu) (tedit 5870DC22)
    (at 134.725 68.75)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (zone_connect 2)
    (attr smd)
    (fp_text reference C187 (at -1.515 0.95) (layer B.SilkS))
    (fp_text value 470n (at 0 -1.7) (layer B.Fab))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 368 /1V0) (zone_connect 2))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer B.Cu) (tedit 5870DC25)
    (at 133.175 67.25 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (zone_connect 2)
    (attr smd)
    (fp_text reference C189 (at 0.73 1.445) (layer B.SilkS))
    (fp_text value 470n (at 0 -1.7 270) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 368 /1V0) (zone_connect 2))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND) (zone_connect 2))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer B.Cu) (tedit 5870DC13)
    (at 138.675 70.75)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C190 (at 0.005 1.12) (layer B.SilkS))
    (fp_text value 470n (at 0 -1.7) (layer B.Fab))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 199 /1V8))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer B.Cu) (tedit 5870DC11)
    (at 139.725 69.75)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C192 (at 0.515 -0.93) (layer B.SilkS))
    (fp_text value 470n (at 0 -1.7) (layer B.Fab))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 199 /1V8))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer B.Cu) (tedit 5870DBFC)
    (at 142.575 67.75 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C198 (at -0.575 1.63 270) (layer B.SilkS))
    (fp_text value 470n (at 0 -1.7 180) (layer B.Fab))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 340 /3V3D))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer B.Cu) (tedit 5870DC36)
    (at 135.625 63.65)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C199 (at -1.485 -0.84) (layer B.SilkS))
    (fp_text value 470n (at 0 -1.7) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 340 /3V3D))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer B.Cu) (tedit 55A40188)
    (at 143.025 74.85)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C200 (at 0 1.7) (layer B.SilkS))
    (fp_text value 470n (at 0 -1.7) (layer B.Fab))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 340 /3V3D))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer B.Cu) (tedit 5870DC2A)
    (at 132.725 64.7)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C201 (at -2.255 -0.11) (layer B.SilkS))
    (fp_text value 470n (at 0 -1.7) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 340 /3V3D))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer B.Cu) (tedit 5870DC18)
    (at 134.48 73.92 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C202 (at 0.035 -1.16 180) (layer B.SilkS))
    (fp_text value 470n (at 0 -1.7 180) (layer B.Fab))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 340 /3V3D))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer B.Cu) (tedit 5870DC1B)
    (at 131.925 71.95)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (zone_connect 2)
    (attr smd)
    (fp_text reference C203 (at -2.085 0.04) (layer B.SilkS))
    (fp_text value 470n (at 0 -1.7) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 340 /3V3D) (zone_connect 2))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND) (zone_connect 2))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer B.Cu) (tedit 5870DC0D)
    (at 141.275 71.3 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C204 (at -2.1 -0.005 90) (layer B.SilkS))
    (fp_text value 470n (at 0 -1.7 90) (layer B.Fab))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 340 /3V3D))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 5870D993)
    (at 136.175 37.825 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C207 (at 2.345 -0.005 270) (layer F.SilkS))
    (fp_text value 100n (at 0 1.7 270) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 406 /fpga/usb/5V))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 5870D716)
    (at 168.675 98.65 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C120 (at 0.12 -1.095 90) (layer F.SilkS))
    (fp_text value 10n (at 0 1.7 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 79 "Net-(C115-Pad1)"))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 5870DA58)
    (at 165.29 66.19)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C167 (at 0.02 1.21 180) (layer F.SilkS))
    (fp_text value 100n (at 0 1.7) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 171 /3V3A))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 5870D9BE)
    (at 155.28 56.29 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C166 (at -0.05 -0.96 90) (layer F.SilkS))
    (fp_text value C (at 0 1.7 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 118 "Net-(C166-Pad1)"))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 5870DA1D)
    (at 158.25 61.35)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C165 (at 1.4 -0.28 90) (layer F.SilkS))
    (fp_text value 100n (at 0 1.7) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 171 /3V3A))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 5870D9CE)
    (at 156.925 54.675)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C160 (at 1.365 0.005 90) (layer F.SilkS))
    (fp_text value C (at 0 1.7) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 119 "Net-(C157-Pad2)"))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 5870DA21)
    (at 155.425 61.5 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C157 (at 1.605 0.16 270) (layer F.SilkS))
    (fp_text value 1p (at 0 1.7 180) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 119 "Net-(C157-Pad2)"))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 117 /tx_amp/OUTP))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 5870D831)
    (at 130.09 91.64 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C156 (at 0.18 -0.99 180) (layer F.SilkS))
    (fp_text value 100p (at 0 1.7 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 170 /ADC+))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer B.Cu) (tedit 5870DBCC)
    (at 164.5 65.8)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C168 (at 0.14 -1.79) (layer B.SilkS))
    (fp_text value 18p (at 0 -1.7) (layer B.Fab))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 150 "Net-(C168-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer B.Cu) (tedit 5870DBF9)
    (at 141.725 61.75)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C197 (at 0.025 -1.1) (layer B.SilkS))
    (fp_text value 470n (at 0 -1.7) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 340 /3V3D))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer B.Cu) (tedit 5870DC3E)
    (at 137.675 66.75 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C193 (at -1.555 -0.46 270) (layer B.SilkS))
    (fp_text value 470n (at 0 -1.7 180) (layer B.Fab))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 199 /1V8))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 5870DA35)
    (at 157.4 66.56)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C170 (at 0.03 0.92) (layer F.SilkS))
    (fp_text value 18p (at 0 1.7) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 173 /PORT_SW1))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 55A40188)
    (at 178.23 114.14 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C171 (at 1.26 -0.8 180) (layer F.SilkS))
    (fp_text value 18p (at 0 1.7 180) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 156 "Net-(C171-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 5870DA8A)
    (at 129.475 115.925)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C172 (at 0.605 0.845) (layer F.SilkS))
    (fp_text value 18p (at 0 1.7) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 157 "Net-(C172-Pad1)"))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer B.Cu) (tedit 5870DAA3)
    (at 176.96 114.85 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C173 (at 0.36 -1.25 180) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.7 180) (layer B.Fab))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 171 /3V3A))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer B.Cu) (tedit 5870DB05)
    (at 130.92 115.01)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C174 (at 2.18 -0.18 90) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.7) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 415 3V3A_RX))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer B.Cu) (tedit 5870DAAD)
    (at 176.41 111.73 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C175 (at -0.74 1.86) (layer B.SilkS))
    (fp_text value 18p (at 0 -1.7 270) (layer B.Fab))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 174 /PORT_SW0))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer B.Cu) (tedit 5870DAA9)
    (at 174.41 114.33 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C176 (at -0.04 -0.98 90) (layer B.SilkS))
    (fp_text value 18p (at 0 -1.7 90) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 173 /PORT_SW1))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer B.Cu) (tedit 5870DB00)
    (at 128.62 118.77 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C178 (at -0.46 1 90) (layer B.SilkS))
    (fp_text value 18p (at 0 -1.7 90) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 173 /PORT_SW1))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 5870D803)
    (at 123.62 115.44 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C179 (at 0.37 2.6 90) (layer F.SilkS))
    (fp_text value 1n (at 0 1.7 90) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 160 "Net-(C179-Pad2)"))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 349 /PORT2))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer B.Cu) (tedit 5870DACA)
    (at 163.21 114.44 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (zone_connect 2)
    (attr smd)
    (fp_text reference C35 (at 0.67 1.28 270) (layer B.SilkS))
    (fp_text value 18p (at 0 -1.7 180) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 204 /RX_SW1) (zone_connect 2))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer B.Cu) (tedit 5870DAC2)
    (at 163.58 116.97 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C36 (at -1.02 -1.17 180) (layer B.SilkS))
    (fp_text value 18p (at 0 -1.7 180) (layer B.Fab))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 205 /RX_SW0))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer B.Cu) (tedit 5870DC33)
    (at 135.375 65.95 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C206 (at -0.225 1.3 180) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.7 180) (layer B.Fab))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 267 "Net-(C205-Pad2)"))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 273 "Net-(C205-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer B.Cu) (tedit 5870DBD4)
    (at 159.9 66.1 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C169 (at -2.09 -0.49 90) (layer B.SilkS))
    (fp_text value 18p (at 0 -1.7 270) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 174 /PORT_SW0))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 5870D7F3)
    (at 138.225 113.425 45)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C28 (at 0.028284 -0.997021 45) (layer F.SilkS))
    (fp_text value 1n (at 0 1.7 45) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0 45) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C28-Pad2)"))
    (pad 1 smd rect (at -0.55 0 45) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 348 /B))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 5870D9FA)
    (at 181.02 59.43 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C3 (at -1.42 0.17 270) (layer F.SilkS))
    (fp_text value 10n (at 0 1.7 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 338 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 198 "Net-(C3-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 5871F374)
    (at 172.225 60.15 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C4 (at 1.525 -0.06 180) (layer F.SilkS))
    (fp_text value 100n (at 0 1.7 180) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 422 "Net-(C261-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 5870D738)
    (at 164.925 90.35 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C7 (at -0.45 -0.855 90) (layer F.SilkS))
    (fp_text value 1n (at 0 1.7 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 163 "Net-(C7-Pad1)"))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 112 "Net-(C7-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 5870D7CE)
    (at 167.086091 113.311091 135)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C8 (at 0.089931 1.198546 135) (layer F.SilkS))
    (fp_text value 1n (at 0 1.7 135) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0 135) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 145 "Net-(C8-Pad2)"))
    (pad 1 smd rect (at -0.55 0 135) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 347 /RX1))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 55A40188)
    (at 161.2 113.325 45)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C9 (at 0 -1.7 45) (layer F.SilkS))
    (fp_text value 1n (at 0 1.7 45) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 45) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 346 /A))
    (pad 2 smd rect (at 0.55 0 45) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 146 "Net-(C9-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 5870D7FF)
    (at 144.425 113.4 135)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C12 (at 0.060104 1.127835 135) (layer F.SilkS))
    (fp_text value 1n (at 0 1.7 135) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0 135) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(C12-Pad2)"))
    (pad 1 smd rect (at -0.55 0 135) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 345 /RX2))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer B.Cu) (tedit 5870DAD5)
    (at 150.875 115.15)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C83 (at -2.045 0.02) (layer B.SilkS))
    (fp_text value 18p (at 0 -1.7) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 202 /RX_SW5))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 5870D7DA)
    (at 165.725 115.325)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C81 (at -2.125 1.485) (layer F.SilkS))
    (fp_text value 18p (at 0 1.7) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 149 "Net-(C81-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer B.Cu) (tedit 5870DAE0)
    (at 150.525 116.05 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C84 (at 0.045 -1.19 180) (layer B.SilkS))
    (fp_text value 18p (at 0 -1.7 180) (layer B.Fab))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 203 /RX_SW4))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 5870D7E5)
    (at 154.575 115.15)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C85 (at 0.355 1.06) (layer F.SilkS))
    (fp_text value 18p (at 0 1.7) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 143 "Net-(C85-Pad1)"))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer B.Cu) (tedit 5870DAB7)
    (at 166.18 116.61 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C87 (at 0.86 -0.97 270) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.7 270) (layer B.Fab))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 403 "/receiver/RX switch/3V3"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 5870D703)
    (at 170.61 103.23 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C89 (at 0 -1.13 180) (layer F.SilkS))
    (fp_text value 100n (at 0 1.7 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 341 /5V))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 5870D701)
    (at 163.18 104.22 225)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C90 (at -2.095 -0.41 225) (layer F.SilkS))
    (fp_text value 1n (at 0 1.7 225) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0 225) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 46 /receiver/RF_IN))
    (pad 1 smd rect (at -0.55 0 225) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 336 "Net-(C90-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 5870D71F)
    (at 162.46 101.95 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (zone_connect 2)
    (attr smd)
    (fp_text reference C91 (at -1.64 -0.04 180) (layer F.SilkS))
    (fp_text value 100n (at 0 1.7 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 109 "Net-(C113-Pad1)") (zone_connect 2))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 5870D7FA)
    (at 143.125 115.425)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C82 (at 0.095 1.575) (layer F.SilkS))
    (fp_text value 18p (at 0 1.7) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 144 "Net-(C82-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 5870D8A1)
    (at 134 89.025)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C221 (at 0.67 -1.925) (layer F.SilkS))
    (fp_text value 100n (at 0 1.7) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 384 /fpga/adc/REFL))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 383 /fpga/adc/REFH))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 5870D7DC)
    (at 165.53 116.41 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C80 (at 1.88 -1.56 180) (layer F.SilkS))
    (fp_text value 100n (at 0 1.7 180) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 403 "/receiver/RX switch/3V3"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer B.Cu) (tedit 5870DAE8)
    (at 140.925 117.85 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C77 (at 0.355 -1.04 180) (layer B.SilkS))
    (fp_text value 18p (at 0 -1.7 180) (layer B.Fab))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 214 /RX_SW2))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer B.Cu) (tedit 5870DAF8)
    (at 143.975 114.025 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C78 (at -0.905 -0.975 270) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.7 270) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 403 "/receiver/RX switch/3V3"))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 5870D8C2)
    (at 133.925 81.85)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C225 (at 0.005 -1.77) (layer F.SilkS))
    (fp_text value 100n (at 0 1.7) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 340 /3V3D))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 5870D89C)
    (at 136.2 89.025)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C224 (at 1.36 -1.745 90) (layer F.SilkS))
    (fp_text value 100n (at 0 1.7) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 370 /fpga/adc/3V0))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 5870D8A4)
    (at 130.5 88.075 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C223 (at 1.455 -0.18) (layer F.SilkS))
    (fp_text value 100n (at 0 1.7 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 370 /fpga/adc/3V0))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 5870D992)
    (at 137.9 38.925 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C209 (at -1.975 -0.04 180) (layer F.SilkS))
    (fp_text value 33p (at 0 1.7 90) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 344 "Net-(C209-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 5870D968)
    (at 136.075 46.95 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C210 (at 0.055 -0.89 180) (layer F.SilkS))
    (fp_text value 100n (at 0 1.7 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 343 "Net-(C210-Pad1)"))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 5870D966)
    (at 136.375 49.15 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C211 (at 0.845 -1.17 180) (layer F.SilkS))
    (fp_text value 100n (at 0 1.7 180) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 340 /3V3D))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 5870D963)
    (at 141.225 53.65)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C212 (at -0.515 1.08) (layer F.SilkS))
    (fp_text value 100n (at 0 1.7) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 340 /3V3D))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer B.Cu) (tedit 55A40188)
    (at 140.725 43.05 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C213 (at 0 1.7 180) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.7 180) (layer B.Fab))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 382 "Net-(C213-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer B.Cu) (tedit 5870DB4A)
    (at 139.775 44.9 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C214 (at -0.09 1.135 270) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.7 270) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 406 /fpga/usb/5V))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 5870D988)
    (at 136.675 44.6 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C215 (at 1.62 0.145 180) (layer F.SilkS))
    (fp_text value 100n (at 0 1.7 90) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 406 /fpga/usb/5V))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 5870D99D)
    (at 148.8 39.075 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C208 (at -0.595 -1.79) (layer F.SilkS))
    (fp_text value 33p (at 0 1.7 270) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 342 "Net-(C208-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 5870D8B8)
    (at 129.4 87.475 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C219 (at 1.915 0.2 270) (layer F.SilkS))
    (fp_text value 100n (at 0 1.7 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 116 /ADC_VCM))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0603b (layer B.Cu) (tedit 5870DC3A)
    (at 137.56 65.46 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (zone_connect 2)
    (attr smd)
    (fp_text reference FB9 (at -1.815 0.45 270) (layer B.SilkS))
    (fp_text value BLM18PG181SN1D (at 0 -1.9 180) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 199 /1V8) (zone_connect 2))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 273 "Net-(C205-Pad1)") (zone_connect 2))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0603b (layer B.Cu) (tedit 5870DC44)
    (at 135.575 66.91)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference FB10 (at -0.055 0) (layer B.SilkS))
    (fp_text value BLM18PG181SN1D (at 0 -1.9) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 267 "Net-(C205-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0603b (layer F.Cu) (tedit 55A401E5)
    (at 164.83 99.56 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference L1 (at 0 -1.425 180) (layer F.SilkS))
    (fp_text value AISC-0603HP-R10J (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 79 "Net-(C115-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 337 "Net-(C121-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0603b (layer B.Cu) (tedit 5870DB61)
    (at 161.906873 93.398369 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference L3 (at -0.123127 1.248369 180) (layer B.SilkS))
    (fp_text value 1u (at 0 -1.9 180) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 97 "Net-(C135-Pad1)"))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 81 "Net-(C125-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0603b (layer B.Cu) (tedit 5870DB63)
    (at 161.906873 94.798369 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference L8 (at -0.083127 -1.431631 180) (layer B.SilkS))
    (fp_text value 1u (at 0 -1.9 180) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 88 "Net-(C135-Pad2)"))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 177 "Net-(C126-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0603b (layer F.Cu) (tedit 5870D707)
    (at 170.625 102.2 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference FB8 (at -1.645 0.02 270) (layer F.SilkS))
    (fp_text value BLM18PG181SN1D (at 0 1.9 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 109 "Net-(C113-Pad1)"))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 341 /5V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0603b (layer F.Cu) (tedit 55A401E5)
    (at 174.75 60.15 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference FB5 (at 0 -1.425 180) (layer F.SilkS))
    (fp_text value BLM18PG181SN1D (at 0 1.9 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 422 "Net-(C261-Pad1)"))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 340 /3V3D))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0603b (layer F.Cu) (tedit 5870D8A7)
    (at 128.1 87.725 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C216 (at -0.115 1.41 270) (layer F.SilkS))
    (fp_text value 2.2u (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 116 /ADC_VCM))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0603b (layer B.Cu) (tedit 55A401E5)
    (at 134.6 89.375 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C218 (at 0 1.425 90) (layer B.SilkS))
    (fp_text value 1u (at 0 -1.9 90) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 384 /fpga/adc/REFL))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0603b (layer B.Cu) (tedit 55A401E5)
    (at 133.675 89.35 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C217 (at 1.1 1.525 90) (layer B.SilkS))
    (fp_text value 1u (at 0 -1.9 90) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 383 /fpga/adc/REFH))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0603b (layer F.Cu) (tedit 55A401E5)
    (at 134 90.125)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C220 (at 0 -1.425) (layer F.SilkS))
    (fp_text value 2.2u (at 0 1.9) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 384 /fpga/adc/REFL))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 383 /fpga/adc/REFH))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0603b (layer F.Cu) (tedit 5870D89A)
    (at 137.2 90.425)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C222 (at -0.26 1.205) (layer F.SilkS))
    (fp_text value 1u (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 370 /fpga/adc/3V0))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0805b (layer F.Cu) (tedit 55A401FA)
    (at 148.42 61.69 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C195 (at 0 -1.675 270) (layer F.SilkS))
    (fp_text value 4.7u (at 0 2.1 270) (layer F.Fab))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 340 /3V3D))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0805b (layer F.Cu) (tedit 5870D956)
    (at 131.39 57.9)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C194 (at 0.01 -1.48) (layer F.SilkS))
    (fp_text value 4.7u (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 340 /3V3D))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0805b (layer F.Cu) (tedit 5870D70A)
    (at 170.925 99.5 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C88 (at 2.07 0.035 180) (layer F.SilkS))
    (fp_text value DNP (at 0 2.1 90) (layer F.Fab))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 341 /5V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0805b (layer F.Cu) (tedit 5870D71C)
    (at 160.79 101.07 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C113 (at -0.04 -1.6 90) (layer F.SilkS))
    (fp_text value 10u (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 109 "Net-(C113-Pad1)"))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0805b (layer B.Cu) (tedit 55A401FA)
    (at 111.4 51.545 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (zone_connect 2)
    (attr smd)
    (fp_text reference L2 (at 0 1.675 270) (layer B.SilkS))
    (fp_text value CIC21P101NE (at 0 -2.1 270) (layer B.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 96 /power/12V_IN) (zone_connect 2))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 56 /power/12V) (zone_connect 2))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0805b (layer F.Cu) (tedit 5870D96B)
    (at 131.62 51.94 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C183 (at 2.33 0.54 180) (layer F.SilkS))
    (fp_text value 4.7u (at 0 2.1 90) (layer F.Fab))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 368 /1V0))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0805b (layer F.Cu) (tedit 5870D827)
    (at 120.44 94.2 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference L6 (at -0.09 -1.54) (layer F.SilkS))
    (fp_text value 0 (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(C110-Pad1)"))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 168 /3V6))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0805b (layer F.Cu) (tedit 55A401FA)
    (at 119.18 111.03)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference L7 (at 0 -1.675) (layer F.SilkS))
    (fp_text value 0 (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(C111-Pad1)"))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 341 /5V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0805b (layer F.Cu) (tedit 55A401FA)
    (at 140.66 57.82)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C185 (at 0 -1.675) (layer F.SilkS))
    (fp_text value 4.7u (at 0 2.1) (layer F.Fab))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 199 /1V8))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0805b (layer B.Cu) (tedit 55A401FA)
    (at 135.6 60.15 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (zone_connect 2)
    (attr smd)
    (fp_text reference C186 (at 0 1.675 180) (layer B.SilkS))
    (fp_text value 4.7u (at 0 -2.1 180) (layer B.Fab))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 368 /1V0) (zone_connect 2))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0805b (layer B.Cu) (tedit 55A401FA)
    (at 125.35 72.675 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C188 (at 0 1.675 90) (layer B.SilkS))
    (fp_text value 4.7u (at 0 -2.1 90) (layer B.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 199 /1V8))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:DFN-8 (layer F.Cu) (tedit 584D633D)
    (at 171.675 58.35 270)
    (descr "DFN8 2x2, 0.5P; CASE 506CN (see ON Semiconductor 506CN.PDF)")
    (tags "DFN 0.5")
    (attr smd)
    (fp_text reference U2 (at -0.05 -2.075 270) (layer F.SilkS))
    (fp_text value NB3N551 (at -0.05 2.075 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 -0.75 270) (size 0.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 421 "Net-(R133-Pad1)"))
    (pad 2 smd rect (at -0.95 -0.25 270) (size 0.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 420 "Net-(R131-Pad2)"))
    (pad 3 smd rect (at -0.95 0.25 270) (size 0.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 413 "Net-(R119-Pad2)"))
    (pad 4 smd rect (at -0.95 0.75 270) (size 0.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 414 "Net-(R120-Pad2)"))
    (pad 5 smd rect (at 0.95 0.75 270) (size 0.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 419 "Net-(R132-Pad2)"))
    (pad 6 smd rect (at 0.95 0.25 270) (size 0.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 7 smd rect (at 0.95 -0.25 270) (size 0.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 422 "Net-(C261-Pad1)"))
    (pad 8 smd rect (at 0.95 -0.75 270) (size 0.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 422 "Net-(C261-Pad1)"))
    (pad EP smd rect (at 0 0.325 270) (size 0.9 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (pad EP smd rect (at 0 -0.325 270) (size 0.9 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (model Housings_DFN_QFN.3dshapes/DFN-8-1EP_2x2mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:DFN-8-1EP_2x2mm_Pitch0.5mm (layer F.Cu) (tedit 5870D722)
    (at 164.325 101.7 90)
    (descr "DFN8 2x2, 0.5P; CASE 506CN (see ON Semiconductor 506CN.PDF)")
    (tags "DFN 0.5")
    (zone_connect 2)
    (attr smd)
    (fp_text reference U12 (at -2.85 2.565 180) (layer F.SilkS))
    (fp_text value TRF37A75 (at -0.05 2.075 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 -0.75 90) (size 0.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 109 "Net-(C113-Pad1)") (zone_connect 2))
    (pad 2 smd rect (at -0.95 -0.25 90) (size 0.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 336 "Net-(C90-Pad1)") (zone_connect 2))
    (pad 3 smd rect (at -0.95 0.25 90) (size 0.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 4 smd rect (at -0.95 0.75 90) (size 0.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 5 smd rect (at 0.95 0.75 90) (size 0.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 175 "Net-(R14-Pad1)") (zone_connect 2))
    (pad 6 smd rect (at 0.95 0.25 90) (size 0.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 7 smd rect (at 0.95 -0.25 90) (size 0.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 337 "Net-(C121-Pad2)") (zone_connect 2))
    (pad 8 smd rect (at 0.95 -0.75 90) (size 0.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 9 smd rect (at 0 0.44 90) (size 1.06 0.88) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2) (zone_connect 2))
    (pad 9 smd rect (at 0 -0.44 90) (size 1.06 0.88) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2) (zone_connect 2))
    (model Housings_DFN_QFN.3dshapes/DFN-8-1EP_2x2mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:KT2520K (layer F.Cu) (tedit 5870D9EE)
    (at 181.06 61.505 90)
    (fp_text reference U1 (at 0.075 0.04 90) (layer F.SilkS))
    (fp_text value KT2520K-40MHz (at 0 -2.475 90) (layer F.Fab))
    (pad 1 smd rect (at -1.175 0.7 90) (size 0.5 0.825) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -0.025 0.9 90) (size 0.7 0.43) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 1.125 0.7 90) (size 0.5 0.825) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 1.125 -0.775 90) (size 0.5 0.825) (layers F.Cu F.Paste F.Mask)
      (net 198 "Net-(C3-Pad2)"))
    (pad 5 smd rect (at -0.025 -0.975 90) (size 0.7 0.43) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at -1.175 -0.775 90) (size 0.5 0.825) (layers F.Cu F.Paste F.Mask)
      (net 389 /1V8_OSC))
  )
  (module VNA:R_0402b (layer F.Cu) (tedit 5870D984)
    (at 133.575 44.15 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R71 (at -0.12 1.265 270) (layer F.SilkS))
    (fp_text value 4.7k (at 0 1.8 270) (layer F.Fab))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 193 "Net-(R71-Pad2)"))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 122 /fpga/usb/USB_5V))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer F.Cu) (tedit 5870D985)
    (at 134.475 44.15 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R72 (at 1.66 0.045 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.8 90) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 193 "Net-(R71-Pad2)"))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer B.Cu) (tedit 5870DC06)
    (at 142.51 70.22 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R70 (at 0.4 1.33 270) (layer B.SilkS))
    (fp_text value 0 (at 0 -1.8 90) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 190 "Net-(R69-Pad2)"))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer F.Cu) (tedit 5870D7C2)
    (at 174.86 111.48 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R67 (at -0.1 1.19 270) (layer F.SilkS))
    (fp_text value 49.9 (at 0 1.8 270) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 153 "Net-(R67-Pad1)"))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer B.Cu) (tedit 5870DB0A)
    (at 128.22 117.37 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R66 (at -0.28 0.81 180) (layer B.SilkS))
    (fp_text value 100 (at 0 -1.8 180) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 173 /PORT_SW1))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 159 "Net-(R66-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer F.Cu) (tedit 5870D961)
    (at 144.375 53.85 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R85 (at -0.02 -1.025 270) (layer F.SilkS))
    (fp_text value 33 (at 0 1.8 90) (layer F.Fab))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 191 "Net-(R85-Pad2)"))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 192 /fpga/TMS))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer B.Cu) (tedit 5870DC09)
    (at 142.22 71.85 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R69 (at 0.05 1.81 180) (layer B.SilkS))
    (fp_text value DNP (at 0 -1.8 90) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 340 /3V3D))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 190 "Net-(R69-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer F.Cu) (tedit 5870D8AB)
    (at 128.8 85.425 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R93 (at 1.72 -0.055 180) (layer F.SilkS))
    (fp_text value 0 (at 0 1.8 180) (layer F.Fab))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 370 /fpga/adc/3V0))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 188 "Net-(R93-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer F.Cu) (tedit 5870D8B0)
    (at 128.75 83.325 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R92 (at 1.96 -0.025 180) (layer F.SilkS))
    (fp_text value DNP (at 0 1.8 180) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 104 "Net-(R91-Pad2)"))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer F.Cu) (tedit 5870D8BE)
    (at 128.8 84.225)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R91 (at -1.76 0.055) (layer F.SilkS))
    (fp_text value 0 (at 0 1.8) (layer F.Fab))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 104 "Net-(R91-Pad2)"))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 370 /fpga/adc/3V0))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer F.Cu) (tedit 5870D95C)
    (at 145.475 53.95 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R88 (at -1.52 -0.085 180) (layer F.SilkS))
    (fp_text value 33 (at 0 1.8 90) (layer F.Fab))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 186 "Net-(R88-Pad2)"))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 187 /fpga/TDI))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer F.Cu) (tedit 5870DA85)
    (at 131.025 113.9 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R68 (at -0.13 -2.095 270) (layer F.SilkS))
    (fp_text value 49.9 (at 0 1.8 270) (layer F.Fab))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 161 "Net-(R68-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer F.Cu) (tedit 5870D960)
    (at 146.675 54 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R84 (at 0.2 1.655 180) (layer F.SilkS))
    (fp_text value 33 (at 0 1.8 90) (layer F.Fab))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 182 "Net-(R84-Pad2)"))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 183 /fpga/TCK))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer F.Cu) (tedit 5870D98B)
    (at 134.575 45.85)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R82 (at -1.665 -0.02) (layer F.SilkS))
    (fp_text value 1k5 (at 0 1.8) (layer F.Fab))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 90 "Net-(R82-Pad2)"))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 181 "Net-(R81-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer F.Cu) (tedit 5870D97D)
    (at 128.475 44.35 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R81 (at -2.085 -0.17 180) (layer F.SilkS))
    (fp_text value 27 (at 0 1.8 180) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 181 "Net-(R81-Pad1)"))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 123 /fpga/usb/USBDP))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer F.Cu) (tedit 5870D97B)
    (at 128.475 43.25 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R80 (at -2.045 0.04 180) (layer F.SilkS))
    (fp_text value 27 (at 0 1.8 180) (layer F.Fab))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 124 /fpga/usb/USBDM))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 180 "Net-(R80-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer B.Cu) (tedit 5870DB53)
    (at 133.075 38.725 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R79 (at 0.925 -1.465) (layer B.SilkS))
    (fp_text value 2k2 (at 0 -1.8 270) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 167 /fpga/usb/DO))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 166 /fpga/usb/EEDATA))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer B.Cu) (tedit 5870DB51)
    (at 133.575 37.325 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R73 (at -1.015 -1.075 180) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.8 180) (layer B.Fab))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 167 /fpga/usb/DO))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 406 /fpga/usb/5V))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer B.Cu) (tedit 5870DB4D)
    (at 142.575 43.05 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R83 (at -0.425 1.61 180) (layer B.SilkS))
    (fp_text value 470 (at 0 -1.8 180) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 406 /fpga/usb/5V))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 382 "Net-(C213-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer B.Cu) (tedit 5870DB98)
    (at 167.159966 93.55524)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R24 (at 0.610034 -1.30524 90) (layer B.SilkS))
    (fp_text value 0 (at 0 -1.8) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 81 "Net-(C125-Pad2)"))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 179 "Net-(C122-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer B.Cu) (tedit 5870DB8C)
    (at 169.859966 94.85524)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R23 (at 1.850034 0.01476) (layer B.SilkS))
    (fp_text value 0 (at 0 -1.8) (layer B.Fab))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 78 /receiver/IF+))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 176 "Net-(C123-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer B.Cu) (tedit 5870DB8B)
    (at 169.909966 93.65524)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R22 (at 1.840034 -0.07524) (layer B.SilkS))
    (fp_text value 0 (at 0 -1.8) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 179 "Net-(C122-Pad2)"))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 77 /receiver/IF-))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer B.Cu) (tedit 5870DB9C)
    (at 167.159966 94.65524)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R28 (at 0.560034 1.37476 90) (layer B.SilkS))
    (fp_text value 0 (at 0 -1.8) (layer B.Fab))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 176 "Net-(C123-Pad2)"))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 177 "Net-(C126-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer B.Cu) (tedit 5870DAD1)
    (at 154.475 115.15 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R10 (at -0.175 -1.19 180) (layer B.SilkS))
    (fp_text value 100 (at 0 -1.8 180) (layer B.Fab))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 143 "Net-(C85-Pad1)"))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 403 "/receiver/RX switch/3V3"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer B.Cu) (tedit 5870DADE)
    (at 151.825 114.25)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R9 (at 1.495 -0.1) (layer B.SilkS))
    (fp_text value 10 (at 0 -1.8) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 202 /RX_SW5))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 142 "Net-(R9-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer F.Cu) (tedit 5870D86D)
    (at 131.425 100.075 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R40 (at 0.895 1.455) (layer F.SilkS))
    (fp_text value 1k (at 0 1.8 270) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 110 "Net-(C144-Pad2)"))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 88 "Net-(C135-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer B.Cu) (tedit 5870DAF2)
    (at 142.875 114.625 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R7 (at -0.055 0.985 270) (layer B.SilkS))
    (fp_text value 100 (at 0 -1.8 180) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 403 "/receiver/RX switch/3V3"))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 144 "Net-(C82-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer B.Cu) (tedit 5870DAD7)
    (at 152.45 116.075)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R8 (at -0.04 1.255) (layer B.SilkS))
    (fp_text value 10 (at 0 -1.8) (layer B.Fab))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 141 "Net-(R8-Pad2)"))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 203 /RX_SW4))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer B.Cu) (tedit 5870DAEE)
    (at 140.375 114.625)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R4 (at -0.425 -1.095 90) (layer B.SilkS))
    (fp_text value 10 (at 0 -1.8) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 213 /RX_SW3))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 44 "Net-(R4-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer B.Cu) (tedit 5870DB07)
    (at 130.26 117.55 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R55 (at -0.03 0.83 180) (layer B.SilkS))
    (fp_text value 100 (at 0 -1.8 180) (layer B.Fab))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 158 "Net-(R55-Pad2)"))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 174 /PORT_SW0))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer B.Cu) (tedit 5870DAA7)
    (at 176.81 113.03)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R54 (at 0.76 -0.78) (layer B.SilkS))
    (fp_text value 100 (at 0 -1.8) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 174 /PORT_SW0))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 155 "Net-(R54-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer F.Cu) (tedit 5870DA38)
    (at 159.09 66.41)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R51 (at 0.18 1.28) (layer F.SilkS))
    (fp_text value 1k (at 0 1.8) (layer F.Fab))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 87 "Net-(R51-Pad2)"))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 173 /PORT_SW1))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer B.Cu) (tedit 5870DAA1)
    (at 178.26 114.06)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R52 (at 1.56 -0.2 90) (layer B.SilkS))
    (fp_text value 100 (at 0 -1.8) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 171 /3V3A))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 156 "Net-(C171-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer B.Cu) (tedit 55A401B2)
    (at 165.825 102.8 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R14 (at 0 1.4 270) (layer B.SilkS))
    (fp_text value 0 (at 0 -1.8 270) (layer B.Fab))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 175 "Net-(R14-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer B.Cu) (tedit 5870DABB)
    (at 162.225 116.5 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R1 (at -1.34 -0.245 180) (layer B.SilkS))
    (fp_text value 10 (at 0 -1.8 90) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 205 /RX_SW0))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 147 "Net-(R1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer B.Cu) (tedit 5870DAE5)
    (at 140.8 116.85)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R2 (at 1.5 0) (layer B.SilkS))
    (fp_text value 10 (at 0 -1.8) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 214 /RX_SW2))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 89 "Net-(R2-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer B.Cu) (tedit 5870DAC5)
    (at 163.08 115.2)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R3 (at -1.43 -0.18 90) (layer B.SilkS))
    (fp_text value 10 (at 0 -1.8) (layer B.Fab))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 148 "Net-(R3-Pad2)"))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 204 /RX_SW1))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer B.Cu) (tedit 5870DAB3)
    (at 165.71 115.39 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R5 (at -0.91 0.91 180) (layer B.SilkS))
    (fp_text value 100 (at 0 -1.8 180) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 403 "/receiver/RX switch/3V3"))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 149 "Net-(C81-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer F.Cu) (tedit 5870D84D)
    (at 129.85 99.975 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R39 (at 1.5 1.205 180) (layer F.SilkS))
    (fp_text value DNP (at 0 1.8 180) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 110 "Net-(C144-Pad2)"))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 91 "Net-(C138-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer B.Cu) (tedit 5870DBCE)
    (at 161.05 66.6)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R50 (at -0.09 1.18) (layer B.SilkS))
    (fp_text value 1k (at 0 -1.8) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 174 /PORT_SW0))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 86 "Net-(R50-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer B.Cu) (tedit 5870DBCD)
    (at 164.4 66.6 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R49 (at -0.13 -1.15 180) (layer B.SilkS))
    (fp_text value 100 (at 0 -1.8 180) (layer B.Fab))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 150 "Net-(C168-Pad1)"))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 171 /3V3A))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer B.Cu) (tedit 5870DAA6)
    (at 174.81 112.73)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R56 (at -1.94 0.03) (layer B.SilkS))
    (fp_text value 100 (at 0 -1.8) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 173 /PORT_SW1))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 154 "Net-(R56-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer F.Cu) (tedit 55A401B2)
    (at 157 55.675 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R47 (at 0 -1.4 180) (layer F.SilkS))
    (fp_text value 1k (at 0 1.8 180) (layer F.Fab))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 119 "Net-(C157-Pad2)"))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 117 /tx_amp/OUTP))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer F.Cu) (tedit 5870D83B)
    (at 131.475 92.95 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R46 (at 0.28 1.665) (layer F.SilkS))
    (fp_text value 50 (at 0 1.8 270) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 170 /ADC+))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 385 "Net-(R46-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer B.Cu) (tedit 5870DB0D)
    (at 129.275 115.075 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R53 (at 1.635 -0.005 180) (layer B.SilkS))
    (fp_text value 100 (at 0 -1.8 180) (layer B.Fab))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 157 "Net-(C172-Pad1)"))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 415 3V3A_RX))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer F.Cu) (tedit 5870D861)
    (at 132.825 98 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R44 (at -1.955 0.38 180) (layer F.SilkS))
    (fp_text value 3.3k (at 0 1.8 180) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 101 "Net-(C146-Pad1)"))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 102 "Net-(C146-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer F.Cu) (tedit 5870D875)
    (at 131.075 97.975)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R43 (at -1.735 -0.805) (layer F.SilkS))
    (fp_text value 3.3k (at 0 1.8) (layer F.Fab))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 110 "Net-(C144-Pad2)"))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 115 "Net-(C144-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer F.Cu) (tedit 5870D838)
    (at 132.55 92.925 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R45 (at -0.415 -1.51) (layer F.SilkS))
    (fp_text value 50 (at 0 1.8 270) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 172 /ADC-))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 386 "Net-(R45-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer F.Cu) (tedit 5870D86B)
    (at 132.425 100.05 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R41 (at 0.81 -1.245) (layer F.SilkS))
    (fp_text value 1k (at 0 1.8 270) (layer F.Fab))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 97 "Net-(C135-Pad1)"))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 102 "Net-(C146-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer F.Cu) (tedit 55A401B2)
    (at 156.975 56.575)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R48 (at 0 -1.4) (layer F.SilkS))
    (fp_text value 10k (at 0 1.8) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 119 "Net-(C157-Pad2)"))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer F.Cu) (tedit 5870D863)
    (at 134.025 99.9)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R42 (at 1.005 -0.98) (layer F.SilkS))
    (fp_text value 1k (at 0 1.8) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 102 "Net-(C146-Pad2)"))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 92 "Net-(C139-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:SOT-23-6 (layer F.Cu) (tedit 5870D98E)
    (at 133.345 38.2725 270)
    (fp_text reference U32 (at 2.3875 -0.095) (layer F.SilkS))
    (fp_text value 93LC46B (at 0.0635 0 270) (layer F.SilkS))
    (pad 6 smd rect (at -0.9525 -1.27 270) (size 0.70104 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 406 /fpga/usb/5V))
    (pad 5 smd rect (at 0 -1.27 270) (size 0.70104 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 164 /fpga/usb/EECS))
    (pad 4 smd rect (at 0.9525 -1.27 270) (size 0.70104 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 165 /fpga/usb/EESK))
    (pad 3 smd rect (at 0.9525 1.27 270) (size 0.70104 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 166 /fpga/usb/EEDATA))
    (pad 2 smd rect (at 0 1.27 270) (size 0.70104 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.9525 1.27 270) (size 0.70104 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 167 /fpga/usb/DO))
    (model smd/SOT23_6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.11 0.11 0.11))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:TCM1-63AX+ (layer F.Cu) (tedit 5870D72F)
    (at 165.4123 94.0925 180)
    (zone_connect 2)
    (fp_text reference T1 (at 3.2823 0.0025 180) (layer F.SilkS))
    (fp_text value TCM1-63AX+ (at 0 -3.6 180) (layer F.Fab))
    (pad 1 smd rect (at -1.2827 -1.5875 180) (size 0.76 1.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 smd rect (at -0.0127 -1.5875 180) (size 0.76 1.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 3 smd rect (at 1.2573 -1.5875 180) (size 0.76 1.65) (layers F.Cu F.Paste F.Mask)
      (net 162 /receiver/RF_BALUN) (zone_connect 2))
    (pad 4 smd rect (at 1.2573 1.5925 180) (size 0.76 1.65) (layers F.Cu F.Paste F.Mask)
      (net 163 "Net-(C7-Pad1)") (zone_connect 2))
    (pad 5 smd rect (at -0.0127 1.5925 180) (size 0.76 1.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 6 smd rect (at -1.2827 1.5925 180) (size 0.76 1.65) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(C52-Pad2)") (zone_connect 2))
  )
  (module VNA:USB_MICRO (layer F.Cu) (tedit 5870D96F)
    (at 125.52 40.635 180)
    (fp_text reference U31 (at -0.24 5.645 180) (layer F.SilkS))
    (fp_text value USB-MICRO (at 0.1 7.3 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.3 0 180) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 122 /fpga/usb/USB_5V))
    (pad 5 smd rect (at 1.3 0 180) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 0 0 180) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 123 /fpga/usb/USBDP))
    (pad 2 smd rect (at -0.65 0 180) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 124 /fpga/usb/USBDM))
    (pad 4 smd rect (at 0.65 0 180) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 125 "Net-(U31-Pad4)"))
    (pad ~ smd rect (at -3.1 0.12 180) (size 2.1 1.6) (layers F.Cu F.Paste F.Mask))
    (pad ~ smd rect (at 3.1 0.12 180) (size 2.1 1.6) (layers F.Cu F.Paste F.Mask))
    (pad SH smd rect (at 3.8 2.675 180) (size 1.8 1.9) (layers F.Cu F.Paste F.Mask)
      (net 126 "Net-(U31-PadSH)"))
    (pad ~ smd rect (at -3.8 2.675 180) (size 1.8 1.9) (layers F.Cu F.Paste F.Mask))
    (pad ~ smd rect (at 1.2 2.675 180) (size 1.9 1.9) (layers F.Cu F.Paste F.Mask))
    (pad ~ smd rect (at -1.2 2.675 180) (size 1.9 1.9) (layers F.Cu F.Paste F.Mask))
  )
  (module VNA:VFQFN-16 (layer F.Cu) (tedit 584D6891)
    (at 156.8 59.125 180)
    (zone_connect 2)
    (fp_text reference U24 (at 0 2.7 180) (layer F.SilkS))
    (fp_text value HMC713LP3E (at 0 -3.3 180) (layer F.Fab))
    (pad EP smd rect (at 0 0 270) (size 1.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad EP smd rect (at 0 0 180) (size 1.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad EP thru_hole circle (at 0.4 0.4 180) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad EP thru_hole circle (at -0.4 0.4 180) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad EP thru_hole circle (at 0.4 -0.4 180) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad EP thru_hole circle (at -0.4 -0.4 180) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad EP smd rect (at 0 0 180) (size 1.6 1.6) (layers F.Cu F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 16 smd oval (at -0.75 -1.35 180) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 171 /3V3A) (zone_connect 2))
    (pad 15 smd oval (at -0.25 -1.35 180) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 171 /3V3A) (zone_connect 2))
    (pad 14 smd oval (at 0.25 -1.35 180) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 363 "Net-(R94-Pad1)") (zone_connect 2))
    (pad 13 smd oval (at 0.75 -1.35 180) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 117 /tx_amp/OUTP) (zone_connect 2))
    (pad 8 smd oval (at 0.75 1.35 180) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 118 "Net-(C166-Pad1)") (zone_connect 2))
    (pad 7 smd oval (at 0.25 1.35 180) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 119 "Net-(C157-Pad2)") (zone_connect 2))
    (pad 6 smd oval (at -0.25 1.35 180) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 171 /3V3A) (zone_connect 2))
    (pad 9 smd oval (at 1.35 0.75 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 10 smd oval (at 1.35 0.25 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 11 smd oval (at 1.35 -0.25 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 12 smd oval (at 1.35 -0.75 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 5 smd oval (at -0.75 1.35 180) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 4 smd oval (at -1.35 0.75 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 120 "Net-(U24-Pad4)") (zone_connect 2))
    (pad 3 smd oval (at -1.35 0.25 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 412 "Net-(C255-Pad1)") (zone_connect 2))
    (pad 2 smd oval (at -1.35 -0.25 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 1 smd oval (at -1.35 -0.75 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 121 "Net-(U24-Pad1)") (zone_connect 2))
  )
  (module VNA:VFQFN-16 (layer F.Cu) (tedit 5870D878)
    (at 132.025 95.65 90)
    (fp_text reference U21 (at -0.96 3.295 180) (layer F.SilkS))
    (fp_text value ADA4940-1 (at 0 -3.3 90) (layer F.Fab))
    (pad 1 smd oval (at -1.35 -0.75 180) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 115 "Net-(C144-Pad1)"))
    (pad 2 smd oval (at -1.35 -0.25 180) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 110 "Net-(C144-Pad2)"))
    (pad 3 smd oval (at -1.35 0.25 180) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 102 "Net-(C146-Pad2)"))
    (pad 4 smd oval (at -1.35 0.75 180) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 101 "Net-(C146-Pad1)"))
    (pad 5 smd oval (at -0.75 1.35 90) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 415 3V3A_RX))
    (pad 12 smd oval (at 1.35 -0.75 180) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 415 3V3A_RX))
    (pad 11 smd oval (at 1.35 -0.25 180) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 385 "Net-(R46-Pad2)"))
    (pad 10 smd oval (at 1.35 0.25 180) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 386 "Net-(R45-Pad2)"))
    (pad 9 smd oval (at 1.35 0.75 180) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 116 /ADC_VCM))
    (pad 6 smd oval (at -0.25 1.35 90) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 415 3V3A_RX))
    (pad 7 smd oval (at 0.25 1.35 90) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 415 3V3A_RX))
    (pad 8 smd oval (at 0.75 1.35 90) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 415 3V3A_RX))
    (pad 13 smd oval (at 0.75 -1.35 90) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 14 smd oval (at 0.25 -1.35 90) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 15 smd oval (at -0.25 -1.35 90) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 16 smd oval (at -0.75 -1.35 90) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad EP smd rect (at 0 0 90) (size 1.6 1.6) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad EP thru_hole circle (at -0.4 -0.4 90) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad EP thru_hole circle (at 0.4 -0.4 90) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad EP thru_hole circle (at -0.4 0.4 90) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad EP thru_hole circle (at 0.4 0.4 90) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad EP smd rect (at 0 0 90) (size 1.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad EP smd rect (at 0 0 180) (size 1.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module VNA:VQFN-24 (layer F.Cu) (tedit 587D06F4)
    (at 162.27 51.24 180)
    (fp_text reference U3 (at -3.91 0.51 180) (layer F.SilkS))
    (fp_text value PE43711 (at 0 3.25 180) (layer F.SilkS))
    (pad 1 smd rect (at -1.25 1.9 180) (size 0.25 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -0.75 1.9 180) (size 0.25 0.7) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(C11-Pad1)"))
    (pad 3 smd rect (at -0.25 1.9 180) (size 0.25 0.7) (layers F.Cu F.Paste F.Mask)
      (net 171 /3V3A))
    (pad 4 smd rect (at 0.25 1.9 180) (size 0.25 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 0.75 1.9 180) (size 0.25 0.7) (layers F.Cu F.Paste F.Mask)
      (net 98 /tx_amp/RF_IN))
    (pad 6 smd rect (at 1.25 1.9 180) (size 0.25 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 13 smd rect (at 1.25 -1.9 180) (size 0.25 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 14 smd rect (at 0.75 -1.9 180) (size 0.25 0.7) (layers F.Cu F.Paste F.Mask)
      (net 106 "Net-(C152-Pad2)"))
    (pad 15 smd rect (at 0.25 -1.9 180) (size 0.25 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 16 smd rect (at -0.25 -1.9 180) (size 0.25 0.7) (layers F.Cu F.Paste F.Mask)
      (net 328 /ATTEN_LE))
    (pad 17 smd rect (at -0.75 -1.9 180) (size 0.25 0.7) (layers F.Cu F.Paste F.Mask)
      (net 111 /SPI_CLK))
    (pad 18 smd rect (at -1.25 -1.9 180) (size 0.25 0.7) (layers F.Cu F.Paste F.Mask)
      (net 320 /ATTEN_SPI_DATA))
    (pad 19 smd rect (at -1.9 -1.25 270) (size 0.25 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 20 smd rect (at -1.9 -0.75 270) (size 0.25 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 21 smd rect (at -1.9 -0.25 270) (size 0.25 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 22 smd rect (at -1.9 0.25 270) (size 0.25 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 23 smd rect (at -1.9 0.75 270) (size 0.25 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 7 smd rect (at 1.9 1.25 270) (size 0.25 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 8 smd rect (at 1.9 0.76 270) (size 0.25 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd rect (at 1.9 0.25 270) (size 0.25 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 10 smd rect (at 1.9 -0.25 270) (size 0.25 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 11 smd rect (at 1.9 -0.75 270) (size 0.25 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 12 smd rect (at 1.9 -1.25 270) (size 0.25 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 24 smd rect (at -1.9 1.25 270) (size 0.25 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad EP smd rect (at 0 0 180) (size 2.7 2.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.15))
    (pad EP thru_hole circle (at 0 0 180) (size 0.3 0.3) (drill 0.3) (layers *.Cu F.SilkS F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad EP thru_hole circle (at -0.5 -0.5 180) (size 0.3 0.3) (drill 0.3) (layers *.Cu F.SilkS F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad EP thru_hole circle (at -1 -1 180) (size 0.3 0.3) (drill 0.3) (layers *.Cu F.SilkS F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad EP thru_hole circle (at 0 -1 180) (size 0.3 0.3) (drill 0.3) (layers *.Cu F.SilkS F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad EP thru_hole circle (at 1 -1 180) (size 0.3 0.3) (drill 0.3) (layers *.Cu F.SilkS F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad EP thru_hole circle (at 0.5 -0.5 180) (size 0.3 0.3) (drill 0.3) (layers *.Cu F.SilkS F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad EP thru_hole circle (at -1 0 180) (size 0.3 0.3) (drill 0.3) (layers *.Cu F.SilkS F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad EP thru_hole circle (at 1 0 180) (size 0.3 0.3) (drill 0.3) (layers *.Cu F.SilkS F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad EP thru_hole circle (at -0.5 0.5 180) (size 0.3 0.3) (drill 0.3) (layers *.Cu F.SilkS F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad EP thru_hole circle (at 0.5 0.5 180) (size 0.3 0.3) (drill 0.3) (layers *.Cu F.SilkS F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad EP thru_hole circle (at -1 1 180) (size 0.3 0.3) (drill 0.3) (layers *.Cu F.SilkS F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad EP thru_hole circle (at 0 1 180) (size 0.3 0.3) (drill 0.3) (layers *.Cu F.SilkS F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad EP thru_hole circle (at 1 1 180) (size 0.3 0.3) (drill 0.3) (layers *.Cu F.SilkS F.Mask)
      (net 1 GND) (zone_connect 2))
  )
  (module VNA:EJ508A (layer F.Cu) (tedit 56ADBA23)
    (at 112.458 53.087 270)
    (fp_text reference CON1 (at -4.4 3.5 270) (layer F.SilkS))
    (fp_text value BARREL_JACK (at -0.7 -7.6 270) (layer F.Fab))
    (pad 3 thru_hole circle (at 0 -3 270) (size 4.2 4.2) (drill 3.05) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole circle (at -5.9 -6 270) (size 4.6 4.6) (drill 3.56) (layers *.Cu *.Mask F.SilkS)
      (net 96 /power/12V_IN) (zone_connect 2))
    (pad 2 thru_hole circle (at -5.9 0 270) (size 4.2 4.2) (drill 3.05) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
  )
  (module VNA:TP_1.00 (layer F.Cu) (tedit 55A404EB)
    (at 161.3 88.66)
    (fp_text reference P3 (at 0.125 0.05) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 -0.5) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 14 /receiver/DETO))
  )
  (module VNA:SOT-23-5 (layer F.Cu) (tedit 56A67093)
    (at 169.05 37.68 270)
    (fp_text reference U4 (at 0.91 -1.47 270) (layer F.SilkS))
    (fp_text value LP5907-3V3 (at 0 -4.05 270) (layer F.SilkS))
    (pad 1 smd rect (at 0 0 270) (size 0.6 1.05) (layers F.Cu F.Paste F.Mask)
      (net 168 /3V6))
    (pad 2 smd rect (at 0.95 0 270) (size 0.6 1.05) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.9 0 270) (size 0.6 1.05) (layers F.Cu F.Paste F.Mask)
      (net 168 /3V6))
    (pad 4 smd rect (at 1.9 -2.6 270) (size 0.6 1.25) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 0 -2.6 270) (size 0.6 1.25) (layers F.Cu F.Paste F.Mask)
      (net 93 /transmitter/3V3_RF))
  )
  (module VNA:VFQFN-24 (layer F.Cu) (tedit 587D0722)
    (at 165.375 86.625 180)
    (fp_text reference U7 (at -0.075 -0.095) (layer F.SilkS))
    (fp_text value ADL5801 (at 0 -5 180) (layer F.SilkS))
    (pad 1 smd oval (at -1.25 1.8 180) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd oval (at -0.75 1.8 180) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd oval (at -0.25 1.8 180) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(C37-Pad2)"))
    (pad 4 smd oval (at 0.25 1.8 180) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(C38-Pad1)"))
    (pad 5 smd oval (at 0.75 1.8 180) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd oval (at 1.25 1.8 180) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 13 smd oval (at 1.25 -1.8 180) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 95 /receiver/5VF))
    (pad 14 smd oval (at 0.75 -1.8 180) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 15 smd oval (at 0.25 -1.8 180) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 112 "Net-(C7-Pad2)"))
    (pad 16 smd oval (at -0.25 -1.8 180) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 113 "Net-(C52-Pad1)"))
    (pad 17 smd oval (at -0.75 -1.8 180) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 18 smd oval (at -1.25 -1.8 180) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 95 /receiver/5VF))
    (pad 19 smd oval (at -1.8 -1.25 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 20 smd oval (at -1.8 -0.75 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C46-Pad2)"))
    (pad 21 smd oval (at -1.8 -0.25 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C44-Pad2)"))
    (pad 22 smd oval (at -1.8 0.25 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 114 "Net-(U7-Pad22)"))
    (pad 23 smd oval (at -1.8 0.75 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 7 smd oval (at 1.8 1.25 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 95 /receiver/5VF))
    (pad 8 smd oval (at 1.8 0.76 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd oval (at 1.8 0.25 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 215 /MIXER_ENABLE))
    (pad 10 smd oval (at 1.8 -0.25 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C45-Pad1)"))
    (pad 11 smd oval (at 1.8 -0.75 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 14 /receiver/DETO))
    (pad 12 smd oval (at 1.8 -1.25 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 24 smd oval (at -1.8 1.25 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 95 /receiver/5VF))
    (pad PAD smd rect (at 0 0 180) (size 2.5 2.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.15))
    (pad PAD thru_hole circle (at 0 0 180) (size 0.3 0.3) (drill 0.3) (layers *.Cu F.SilkS F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad PAD thru_hole circle (at 0 -0.65 180) (size 0.3 0.3) (drill 0.3) (layers *.Cu F.SilkS F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad PAD thru_hole circle (at 0.65 0.65 180) (size 0.3 0.3) (drill 0.3) (layers *.Cu F.SilkS F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad PAD thru_hole circle (at 0 0.65 180) (size 0.3 0.3) (drill 0.3) (layers *.Cu F.SilkS F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad PAD thru_hole circle (at 0.65 0 180) (size 0.3 0.3) (drill 0.3) (layers *.Cu F.SilkS F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad PAD thru_hole circle (at 0.65 -0.65 180) (size 0.3 0.3) (drill 0.3) (layers *.Cu F.SilkS F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad PAD thru_hole circle (at -0.65 -0.65 180) (size 0.3 0.3) (drill 0.3) (layers *.Cu F.SilkS F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad PAD thru_hole circle (at -0.65 0 180) (size 0.3 0.3) (drill 0.3) (layers *.Cu F.SilkS F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad PAD thru_hole circle (at -0.65 0.65 180) (size 0.3 0.3) (drill 0.3) (layers *.Cu F.SilkS F.Mask)
      (net 1 GND) (zone_connect 2))
  )
  (module VNA:SOT-23-5 (layer F.Cu) (tedit 56A8FCBE)
    (at 158 91.18)
    (fp_text reference U8 (at 1.175 -1.2) (layer F.SilkS))
    (fp_text value LP5907-3V3 (at 0 -4.05) (layer F.SilkS))
    (pad 1 smd rect (at 0 0) (size 0.6 1.05) (layers F.Cu F.Paste F.Mask)
      (net 168 /3V6))
    (pad 2 smd rect (at 0.95 0) (size 0.6 1.05) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.9 0) (size 0.6 1.05) (layers F.Cu F.Paste F.Mask)
      (net 168 /3V6))
    (pad 4 smd rect (at 1.9 -2.6) (size 0.6 1.25) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 0 -2.6) (size 0.6 1.25) (layers F.Cu F.Paste F.Mask)
      (net 94 /receiver/lo_synth/3V3_RF))
  )
  (module VNA:SRR6040A (layer F.Cu) (tedit 56A6711D)
    (at 113.045 90.765 90)
    (fp_text reference L4 (at -0.19 -0.115 90) (layer F.SilkS))
    (fp_text value "33u (SRR6040A-330M)" (at -0.25 -4.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.25 -2.9 90) (size 7.3 1.4) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at -0.25 2.9 90) (size 7.3 1.4) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(C110-Pad1)"))
    (pad 1 smd rect (at -3.575 -1.7 90) (size 0.65 1) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(D2-Pad1)"))
    (pad 1 smd rect (at 3.075 -1.7 90) (size 0.65 1) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at -3.575 1.7 90) (size 0.65 1) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(C110-Pad1)"))
    (pad 2 smd rect (at 3.075 1.7 90) (size 0.65 1) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(C110-Pad1)"))
  )
  (module VNA:SRR6040A (layer F.Cu) (tedit 56A66FB5)
    (at 113.555 110.495 90)
    (fp_text reference L5 (at -0.45 0.275 180) (layer F.SilkS))
    (fp_text value "33u (SRR6040A-330M)" (at -0.25 -4.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.25 -2.9 90) (size 7.3 1.4) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(D3-Pad1)"))
    (pad 2 smd rect (at -0.25 2.9 90) (size 7.3 1.4) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(C111-Pad1)"))
    (pad 1 smd rect (at -3.575 -1.7 90) (size 0.65 1) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(D3-Pad1)"))
    (pad 1 smd rect (at 3.075 -1.7 90) (size 0.65 1) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(D3-Pad1)"))
    (pad 2 smd rect (at -3.575 1.7 90) (size 0.65 1) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(C111-Pad1)"))
    (pad 2 smd rect (at 3.075 1.7 90) (size 0.65 1) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(C111-Pad1)"))
  )
  (module Housings_DFN_QFN:DFN-8-1EP_3x3mm_Pitch0.5mm (layer F.Cu) (tedit 54130A77)
    (at 115.09 97.185)
    (descr "DD Package; 8-Lead Plastic DFN (3mm x 3mm) (see Linear Technology DFN_8_05-08-1698.pdf)")
    (tags "DFN 0.5")
    (attr smd)
    (fp_text reference U19 (at 0 -2.55) (layer F.SilkS))
    (fp_text value L7980 (at 0 2.55) (layer F.Fab))
    (pad 1 smd rect (at -1.4 -0.75) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at -1.4 -0.25) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 76 /power/SYNC_3V3))
    (pad 3 smd rect (at -1.4 0.25) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 199 /1V8))
    (pad 4 smd rect (at -1.4 0.75) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(C105-Pad1)"))
    (pad 5 smd rect (at 1.4 0.75) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(C101-Pad2)"))
    (pad 6 smd rect (at 1.4 0.25) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 74 "Net-(R32-Pad1)"))
    (pad 7 smd rect (at 1.4 -0.25) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 8 smd rect (at 1.4 -0.75) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 56 /power/12V))
    (pad 9 smd rect (at 0.415 0.595) (size 0.83 1.19) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (pad 9 smd rect (at 0.415 -0.595) (size 0.83 1.19) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (pad 9 smd rect (at -0.415 0.595) (size 0.83 1.19) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (pad 9 smd rect (at -0.415 -0.595) (size 0.83 1.19) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (model Housings_DFN_QFN.3dshapes/DFN-8-1EP_3x3mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DFN_QFN:DFN-8-1EP_3x3mm_Pitch0.5mm (layer F.Cu) (tedit 5870D819)
    (at 115.07 105.065)
    (descr "DD Package; 8-Lead Plastic DFN (3mm x 3mm) (see Linear Technology DFN_8_05-08-1698.pdf)")
    (tags "DFN 0.5")
    (attr smd)
    (fp_text reference U20 (at 3.9 -2.765) (layer F.SilkS))
    (fp_text value L7980 (at 0 2.55) (layer F.Fab))
    (pad 1 smd rect (at -1.4 -0.75) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(D3-Pad1)"))
    (pad 2 smd rect (at -1.4 -0.25) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 76 /power/SYNC_3V3))
    (pad 3 smd rect (at -1.4 0.25) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 56 /power/12V))
    (pad 4 smd rect (at -1.4 0.75) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(C106-Pad1)"))
    (pad 5 smd rect (at 1.4 0.75) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(C104-Pad2)"))
    (pad 6 smd rect (at 1.4 0.25) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 75 "Net-(R34-Pad1)"))
    (pad 7 smd rect (at 1.4 -0.25) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 8 smd rect (at 1.4 -0.75) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 56 /power/12V))
    (pad 9 smd rect (at 0.415 0.595) (size 0.83 1.19) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (pad 9 smd rect (at 0.415 -0.595) (size 0.83 1.19) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (pad 9 smd rect (at -0.415 0.595) (size 0.83 1.19) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (pad 9 smd rect (at -0.415 -0.595) (size 0.83 1.19) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (model Housings_DFN_QFN.3dshapes/DFN-8-1EP_3x3mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:SOT-23-5 (layer F.Cu) (tedit 56A671D1)
    (at 142.395 90.38)
    (fp_text reference U22 (at 1.02 -1.34) (layer F.SilkS))
    (fp_text value TSV911 (at 0 -4.05) (layer F.SilkS))
    (pad 1 smd rect (at 0 0) (size 0.6 1.05) (layers F.Cu F.Paste F.Mask)
      (net 388 "Net-(C132-Pad1)"))
    (pad 2 smd rect (at 0.95 0) (size 0.6 1.05) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.9 0) (size 0.6 1.05) (layers F.Cu F.Paste F.Mask)
      (net 85 "Net-(C133-Pad1)"))
    (pad 4 smd rect (at 1.9 -2.6) (size 0.6 1.25) (layers F.Cu F.Paste F.Mask)
      (net 388 "Net-(C132-Pad1)"))
    (pad 5 smd rect (at 0 -2.6) (size 0.6 1.25) (layers F.Cu F.Paste F.Mask)
      (net 415 3V3A_RX))
  )
  (module VNA:SOD-123F (layer F.Cu) (tedit 5870D822)
    (at 110.59 97.465 270)
    (fp_text reference D2 (at 3.015 -0.14 180) (layer F.SilkS))
    (fp_text value SS13FL (at -0.3 -2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1.5 -0.1 270) (size 1.34 1.8) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at 1.36 -0.1 270) (size 1.34 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module VNA:SOD-123F (layer F.Cu) (tedit 5870D813)
    (at 110.92 104.665 90)
    (fp_text reference D3 (at 2.815 -0.13 180) (layer F.SilkS))
    (fp_text value SS13FL (at -0.3 -2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.5 -0.1 90) (size 1.34 1.8) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(D3-Pad1)"))
    (pad 2 smd rect (at 1.36 -0.1 90) (size 1.34 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module VNA:DFN-8-1EP_2x2mm_Pitch0.5mm (layer F.Cu) (tedit 56A1373B)
    (at 162.12 56.305 270)
    (descr "DFN8 2x2, 0.5P; CASE 506CN (see ON Semiconductor 506CN.PDF)")
    (tags "DFN 0.5")
    (attr smd)
    (fp_text reference U26 (at -0.05 -2.075 270) (layer F.SilkS))
    (fp_text value TRF37A75 (at -0.05 2.075 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 -0.75 270) (size 0.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 99 "Net-(C142-Pad1)"))
    (pad 2 smd rect (at -0.95 -0.25 270) (size 0.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 105 "Net-(C152-Pad1)"))
    (pad 3 smd rect (at -0.95 0.25 270) (size 0.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at -0.95 0.75 270) (size 0.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 0.95 0.75 270) (size 0.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 108 "Net-(R97-Pad1)"))
    (pad 6 smd rect (at 0.95 0.25 270) (size 0.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 7 smd rect (at 0.95 -0.25 270) (size 0.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 107 "Net-(C151-Pad2)"))
    (pad 8 smd rect (at 0.95 -0.75 270) (size 0.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd rect (at 0 0.44 270) (size 1.06 0.88) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (pad 9 smd rect (at 0 -0.44 270) (size 1.06 0.88) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (model Housings_DFN_QFN.3dshapes/DFN-8-1EP_2x2mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:TP_1.00 (layer F.Cu) (tedit 56A145A8)
    (at 161.34 90.96)
    (fp_text reference P5 (at 0.125 0.05) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 -0.5) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 5870D9F1)
    (at 181.01 63.63)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C1 (at 1.43 0) (layer F.SilkS))
    (fp_text value 1u (at 0 1.7) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 389 /1V8_OSC))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 5870D9EC)
    (at 182.45 65.47 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C2 (at -1.18 0.01) (layer F.SilkS))
    (fp_text value 100n (at 0 1.7 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 171 /3V3A))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 5870D9B4)
    (at 174.82 44.09)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C5 (at 0.816 -1.014 180) (layer F.SilkS))
    (fp_text value 1n (at 0 1.7) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 22 /filter_bank/RF_IN))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 /transmitter/RF_OUT_P))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 56A8FAD1)
    (at 176.09 45.29)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C6 (at -0.03 -0.82) (layer F.SilkS))
    (fp_text value 1n (at 0 1.7) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C6-Pad1)"))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 4 /transmitter/RF_OUT_N))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 56A8FAE4)
    (at 163.52 48.31)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C11 (at -0.04 -0.97) (layer F.SilkS))
    (fp_text value 100n (at 0 1.7) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(C11-Pad1)"))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0603b (layer F.Cu) (tedit 5870D9A7)
    (at 167.62 38.48 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C13 (at 0.04 1.29 270) (layer F.SilkS))
    (fp_text value 1u (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 168 /3V6))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0603b (layer F.Cu) (tedit 56A8FAD5)
    (at 173.06 38.56 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C14 (at -0.12 -1.2 270) (layer F.SilkS))
    (fp_text value 1u (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 93 /transmitter/3V3_RF))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0603b (layer B.Cu) (tedit 56A8FBFE)
    (at 173.135 53.355 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C15 (at 0.375 -1.165 180) (layer B.SilkS))
    (fp_text value 1u (at 0 -1.9 180) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 25 "Net-(C15-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer B.Cu) (tedit 56A8FBEE)
    (at 179.78 51.01 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C16 (at 0.62 -1.21 180) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.7 90) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(C16-Pad1)"))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0603b (layer B.Cu) (tedit 56A8FC15)
    (at 173.06 51.33 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C17 (at -0.75 1.23 180) (layer B.SilkS))
    (fp_text value 1u (at 0 -1.9 180) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 26 "Net-(C17-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 5870D9F6)
    (at 177.995 56.205 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C18 (at 0.645 0.875 90) (layer F.SilkS))
    (fp_text value 10n (at 0 1.7 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(C18-Pad1)"))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 184 /CLK_SOURCE))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0603b (layer B.Cu) (tedit 56A8FBF8)
    (at 175.985 54.655)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C19 (at 2.305 -0.085) (layer B.SilkS))
    (fp_text value 1u (at 0 -1.9) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 28 "Net-(C19-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer B.Cu) (tedit 56A8FC0A)
    (at 177.74 49.06 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C20 (at -1.84 0.37 90) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.7 270) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(C16-Pad1)"))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer B.Cu) (tedit 56A8FC04)
    (at 175.385 49.98 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C21 (at 0.03 -1.145 270) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.7 270) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(C21-Pad1)"))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer B.Cu) (tedit 56A8FA9D)
    (at 178.75 47.65 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C22 (at 0.16 0.94 180) (layer B.SilkS))
    (fp_text value 100p (at 0 -1.7 90) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(C16-Pad1)"))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 56A8FA73)
    (at 173.835 49.38 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C23 (at 0.645 -1.62 180) (layer F.SilkS))
    (fp_text value 100n (at 0 1.7 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C21-Pad1)"))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer B.Cu) (tedit 56A8FBE8)
    (at 181.24 50.65 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C24 (at 1.86 -0.23 180) (layer B.SilkS))
    (fp_text value 100p (at 0 -1.7 90) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(C16-Pad1)"))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 56A8FA74)
    (at 173.635 50.255 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C25 (at 0.475 -1.465 180) (layer F.SilkS))
    (fp_text value 100p (at 0 1.7 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C21-Pad1)"))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 5870D9FB)
    (at 176.7 55.74 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C26 (at 0.98 -0.92) (layer F.SilkS))
    (fp_text value 100n (at 0 1.7 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 340 /3V3D))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 5870D9F4)
    (at 179.57 56.155 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C27 (at -0.015 -1.71 270) (layer F.SilkS))
    (fp_text value 100n (at 0 1.7 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 340 /3V3D))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0603b (layer F.Cu) (tedit 56A8FCD5)
    (at 160.9 80.92)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C29 (at -1.05 -1.475) (layer F.SilkS))
    (fp_text value DNP (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 341 /5V))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 55A40188)
    (at 181.385 50.355 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C30 (at 0 -1.7 90) (layer F.SilkS))
    (fp_text value 100n (at 0 1.7 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C30-Pad1)"))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C30-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 55A40188)
    (at 180.835 49.13 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C31 (at 0 -1.7 180) (layer F.SilkS))
    (fp_text value 12n (at 0 1.7 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C30-Pad2)"))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 56A8FAA3)
    (at 180.535 47.155)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C32 (at 0.335 -0.635) (layer F.SilkS))
    (fp_text value 820p (at 0 1.7) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C32-Pad1)"))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 56A8FAA6)
    (at 178.81 46.92 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C33 (at -1.13 -1.46) (layer F.SilkS))
    (fp_text value 100p (at 0 1.7 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 93 /transmitter/3V3_RF))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 56A8FA8D)
    (at 175.91 47.72 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C34 (at -1.47 0.3) (layer F.SilkS))
    (fp_text value 100p (at 0 1.7 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 93 /transmitter/3V3_RF))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 56A46985)
    (at 165.82 83.25 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C37 (at 0.115 -1.03 270) (layer F.SilkS))
    (fp_text value 1n (at 0 1.7 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 131 /receiver/LON))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(C37-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 5870D766)
    (at 165.04 83.26 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C38 (at 0.045 -0.915 270) (layer F.SilkS))
    (fp_text value 1n (at 0 1.7 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(C38-Pad1)"))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 130 /receiver/LOP))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer B.Cu) (tedit 5870DBAF)
    (at 168.895 85.205)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C39 (at 2.125 0.075 180) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.7) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 95 /receiver/5VF))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 56A4697D)
    (at 168.845 85.305)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C40 (at -0.17 -0.635) (layer F.SilkS))
    (fp_text value 100p (at 0 1.7) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 95 /receiver/5VF))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer B.Cu) (tedit 56A8FBB6)
    (at 161.595 85.205)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C41 (at -2.3 -0.145) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.7) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 95 /receiver/5VF))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 5870D73E)
    (at 170.51 88.91)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C42 (at 1.23 1.36 90) (layer F.SilkS))
    (fp_text value 100n (at 0 1.7) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 95 /receiver/5VF))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 5870D75E)
    (at 163.045 83.905 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C43 (at -0.355 1.005 270) (layer F.SilkS))
    (fp_text value 100p (at 0 1.7 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 95 /receiver/5VF))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 5870D742)
    (at 170.9 87.16 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C44 (at -1.43 1.24 270) (layer F.SilkS))
    (fp_text value 100n (at 0 1.7 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 77 /receiver/IF-))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C44-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer B.Cu) (tedit 56A8FBB9)
    (at 161.345 87.205 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C45 (at 2.16 0.275 180) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.7 180) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(C45-Pad1)"))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 5870D740)
    (at 170.885 87.96 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C46 (at -1.575 -0.7 270) (layer F.SilkS))
    (fp_text value 100n (at 0 1.7 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 78 /receiver/IF+))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C46-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 5870D753)
    (at 160.995 85.905 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C47 (at -0.035 0.605 180) (layer F.SilkS))
    (fp_text value 100p (at 0 1.7 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C45-Pad1)"))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 5870D743)
    (at 170.535 86.185)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C48 (at 0.525 -1.055) (layer F.SilkS))
    (fp_text value 100n (at 0 1.7) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 95 /receiver/5VF))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 5870D734)
    (at 162.745 89.705 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C49 (at -0.065 -1.085 180) (layer F.SilkS))
    (fp_text value 100n (at 0 1.7 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 95 /receiver/5VF))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 5870D750)
    (at 162.345 88.055 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C50 (at -0.195 1.285) (layer F.SilkS))
    (fp_text value 1n (at 0 1.7 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 14 /receiver/DETO))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 5870D73C)
    (at 167.845 89.505 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C51 (at 0.875 -1.605) (layer F.SilkS))
    (fp_text value 100n (at 0 1.7 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 95 /receiver/5VF))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 5870D73A)
    (at 165.875 90.35 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C52 (at -0.25 -0.995 90) (layer F.SilkS))
    (fp_text value 1n (at 0 1.7 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 113 "Net-(C52-Pad1)"))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(C52-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0805b (layer F.Cu) (tedit 56A8FCEC)
    (at 169.405 83.435)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C53 (at 0.09 -0.005 90) (layer F.SilkS))
    (fp_text value DNP (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 95 /receiver/5VF))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0603b (layer F.Cu) (tedit 5870D758)
    (at 158.22 86.4 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C56 (at 1.51 0.5 180) (layer F.SilkS))
    (fp_text value 1u (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 94 /receiver/lo_synth/3V3_RF))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0603b (layer B.Cu) (tedit 5870DBBD)
    (at 170.355 75.94)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C57 (at 2.055 -0.19 90) (layer B.SilkS))
    (fp_text value 1u (at 0 -1.9) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 32 "Net-(C57-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer B.Cu) (tedit 5870DBE1)
    (at 161.295 76.555 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C58 (at 0.965 1.065 90) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.7 90) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(C58-Pad1)"))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0603b (layer B.Cu) (tedit 5870DBB5)
    (at 170.005 77.93)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C59 (at 1.435 1.14) (layer B.SilkS))
    (fp_text value 1u (at 0 -1.9) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 33 "Net-(C59-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 5870D78A)
    (at 165.245 72.51 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C60 (at 0.46 -1.475 180) (layer F.SilkS))
    (fp_text value 10n (at 0 1.7 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(C60-Pad1)"))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 185 /CLK_LO))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0603b (layer B.Cu) (tedit 55A401E5)
    (at 168.495 73.78 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C61 (at 0 1.425 90) (layer B.SilkS))
    (fp_text value 1u (at 0 -1.9 90) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 35 "Net-(C61-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 55A40188)
    (at 161.545 78.055 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C62 (at 0 -1.7 180) (layer F.SilkS))
    (fp_text value 100n (at 0 1.7 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C58-Pad1)"))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer B.Cu) (tedit 5870DBB9)
    (at 168.795 80.13)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C63 (at -0.415 0.85) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.7) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 16 "Net-(C63-Pad1)"))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 56A8FCC7)
    (at 161.645 76.555 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C64 (at 0.375 -1.7 180) (layer F.SilkS))
    (fp_text value 100p (at 0 1.7 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C58-Pad1)"))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 5870D79E)
    (at 168.72 79.705)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C65 (at 2.46 -0.405) (layer F.SilkS))
    (fp_text value 100n (at 0 1.7) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C63-Pad1)"))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 5870D763)
    (at 163.295 80.73 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C66 (at 0.155 0.77) (layer F.SilkS))
    (fp_text value 100p (at 0 1.7 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C58-Pad1)"))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 5870D79A)
    (at 169.37 79.055)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C67 (at 0.58 -1.115) (layer F.SilkS))
    (fp_text value 100p (at 0 1.7) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C63-Pad1)"))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 56A8FDBE)
    (at 166.695 72.955)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C68 (at 0.2 -1.025) (layer F.SilkS))
    (fp_text value 100n (at 0 1.7) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 340 /3V3D))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 5870D788)
    (at 163.495 73.655)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C69 (at -0.185 -0.935) (layer F.SilkS))
    (fp_text value 100n (at 0 1.7) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 340 /3V3D))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0805b (layer F.Cu) (tedit 56A8FCD7)
    (at 158.67 81.07 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C70 (at 0.07 0.055 180) (layer F.SilkS))
    (fp_text value 10u (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 341 /5V))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0805b (layer F.Cu) (tedit 55A401FA)
    (at 118.29 94.165 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C71 (at 0 -1.675 90) (layer F.SilkS))
    (fp_text value 10u (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 56 /power/12V))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 55A40188)
    (at 161.595 79.005)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C72 (at 0 -1.7) (layer F.SilkS))
    (fp_text value 100n (at 0 1.7) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(C72-Pad1)"))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(C72-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 56A8FCD4)
    (at 161.47 79.73 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C73 (at 0.025 -1.15 180) (layer F.SilkS))
    (fp_text value 12n (at 0 1.7 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(C72-Pad2)"))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer B.Cu) (tedit 5870DBDE)
    (at 166.995 75.805 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C74 (at -1.415 -0.105) (layer B.SilkS))
    (fp_text value 820p (at 0 -1.7 270) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 19 "Net-(C74-Pad1)"))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 56A8FCDF)
    (at 162.775 81.9)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C75 (at -0.025 0) (layer F.SilkS))
    (fp_text value 100p (at 0 1.7) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 94 /receiver/lo_synth/3V3_RF))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 5870D783)
    (at 168.075 82.1 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C76 (at -1.915 0.08 180) (layer F.SilkS))
    (fp_text value 100p (at 0 1.7 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 94 /receiver/lo_synth/3V3_RF))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0805b (layer B.Cu) (tedit 56A8FB44)
    (at 114.72 89.865)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C79 (at -2.56 -1.75 90) (layer B.SilkS))
    (fp_text value DNP (at 0 -2.1) (layer B.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 56 /power/12V))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0805b (layer B.Cu) (tedit 5870DB21)
    (at 115.37 102.84 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C86 (at -0.05 1.31 180) (layer B.SilkS))
    (fp_text value DNP (at 0 -2.1 180) (layer B.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 56 /power/12V))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 56A6706C)
    (at 170.854 48.55)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C92 (at -0.354 -0.92) (layer F.SilkS))
    (fp_text value 10p (at 0 1.7) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(C92-Pad1)"))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(C92-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 56A6709E)
    (at 169.33 42.708)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C93 (at -0.01 0.892) (layer F.SilkS))
    (fp_text value 10p (at 0 1.7) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(C93-Pad1)"))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(C93-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 56A670D8)
    (at 170.092 46.772)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C94 (at -0.782 -1.452) (layer F.SilkS))
    (fp_text value 100p (at 0 1.7) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(C94-Pad1)"))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(C94-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 56A67097)
    (at 171.145 42.03 315)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C95 (at 0.03182 -1.120764 315) (layer F.SilkS))
    (fp_text value 1n (at 0 1.7 315) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 315) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(C95-Pad1)"))
    (pad 2 smd rect (at 0.55 0 315) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(C95-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 56A670E8)
    (at 164.27 42.85 45)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C96 (at -0.898026 -1.619275 45) (layer F.SilkS))
    (fp_text value 1n (at 0 1.7 45) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 45) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(C96-Pad1)"))
    (pad 2 smd rect (at 0.55 0 45) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(C96-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 56A670E3)
    (at 165.71 43.71 45)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C97 (at 0.13435 -0.827315 45) (layer F.SilkS))
    (fp_text value 10p (at 0 1.7 45) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 45) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(C97-Pad1)"))
    (pad 2 smd rect (at 0.55 0 45) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(C97-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 56A670DC)
    (at 165.61 46.13)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C98 (at 0.25 -0.94) (layer F.SilkS))
    (fp_text value 100p (at 0 1.7) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(C98-Pad1)"))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(C98-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 56A670C4)
    (at 166.11 47.84 322.5)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C99 (at -0.084755 1.022994 322.5) (layer F.SilkS))
    (fp_text value 10p (at 0 1.7 322.5) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 322.5) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(C99-Pad1)"))
    (pad 2 smd rect (at 0.55 0 322.5) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(C99-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0805b (layer F.Cu) (tedit 5870D81C)
    (at 115.295 102.79 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C100 (at -0.025 1.41 180) (layer F.SilkS))
    (fp_text value 10u (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 56 /power/12V))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer B.Cu) (tedit 56A8FB67)
    (at 114.62 99.745 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C101 (at -0.09 1.83 90) (layer B.SilkS))
    (fp_text value 10n (at 0 -1.7 90) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 57 "Net-(C101-Pad1)"))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 58 "Net-(C101-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0805b (layer F.Cu) (tedit 5870D949)
    (at 120.51 51.675 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C102 (at -0.035 -1.72 90) (layer F.SilkS))
    (fp_text value 10u (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 96 /power/12V_IN))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0805b (layer B.Cu) (tedit 56A8FB3F)
    (at 114.695 88.24)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C103 (at -2.715 1.645 90) (layer B.SilkS))
    (fp_text value 10u (at 0 -2.1) (layer B.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 56 /power/12V))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer B.Cu) (tedit 5870DB16)
    (at 113.67 108.065)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C104 (at -0.22 1.895) (layer B.SilkS))
    (fp_text value 10n (at 0 -1.7) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 60 "Net-(C104-Pad1)"))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 61 "Net-(C104-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer B.Cu) (tedit 56A8FB65)
    (at 115.57 99.765 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C105 (at -0.13 1.7 90) (layer B.SilkS))
    (fp_text value 100p (at 0 -1.7 90) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 62 "Net-(C105-Pad1)"))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 58 "Net-(C101-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer B.Cu) (tedit 5870DB19)
    (at 113.67 107.215)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C106 (at -0.13 1.995 180) (layer B.SilkS))
    (fp_text value 68p (at 0 -1.7) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 63 "Net-(C106-Pad1)"))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 61 "Net-(C104-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0805b (layer F.Cu) (tedit 5870D9F3)
    (at 178.41 62.73 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C107 (at -2.01 -0.1) (layer F.SilkS))
    (fp_text value DNP (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 171 /3V3A))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer B.Cu) (tedit 5870DB26)
    (at 115.17 93.315 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C108 (at 0.06 0.965 180) (layer B.SilkS))
    (fp_text value 4.7n (at 0 -1.7 180) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 64 "Net-(C108-Pad1)"))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 58 "Net-(C101-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer B.Cu) (tedit 55A40188)
    (at 116.52 107.065 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C109 (at 0 1.7 90) (layer B.SilkS))
    (fp_text value 4.7n (at 0 -1.7 90) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 65 "Net-(C109-Pad1)"))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 61 "Net-(C104-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0805b (layer F.Cu) (tedit 56A8FC96)
    (at 117.91 88.965 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C110 (at -2.88 0.31 180) (layer F.SilkS))
    (fp_text value 10u (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(C110-Pad1)"))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0805b (layer F.Cu) (tedit 56A8FC94)
    (at 119.07 88.965 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C112 (at -2.19 -0.96 180) (layer F.SilkS))
    (fp_text value 10u (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(C110-Pad1)"))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0805b (layer F.Cu) (tedit 5870D825)
    (at 120.15 96.95)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C116 (at 0.03 1.63) (layer F.SilkS))
    (fp_text value 10u (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 168 /3V6))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0805b (layer F.Cu) (tedit 5870D80D)
    (at 119.86 108.08 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C117 (at 2.92 -0.18 180) (layer F.SilkS))
    (fp_text value 10u (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 341 /5V))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0805b (layer F.Cu) (tedit 56A8FCA7)
    (at 121.63 85.1 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C118 (at 2.75 -1.35 270) (layer F.SilkS))
    (fp_text value 10u (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 168 /3V6))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0805b (layer F.Cu) (tedit 5870D80E)
    (at 118.64 108.08 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C119 (at 2.24 0.99 180) (layer F.SilkS))
    (fp_text value 10u (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 341 /5V))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer B.Cu) (tedit 56A8FC36)
    (at 140.02 88.805)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C129 (at -0.605 -1.745) (layer B.SilkS))
    (fp_text value 100p (at 0 -1.7) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 82 "Net-(C129-Pad1)"))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer B.Cu) (tedit 56A8FC38)
    (at 140.055 89.82 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C130 (at 0.69 2.06 180) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.7 180) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 83 "Net-(C130-Pad1)"))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 82 "Net-(C129-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 5870D892)
    (at 141.33 92.1 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C131 (at 0.31 -2.2 180) (layer F.SilkS))
    (fp_text value 100n (at 0 1.7 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 116 /ADC_VCM))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 5870D895)
    (at 145.595 88.03 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C132 (at 0.06 -0.985 270) (layer F.SilkS))
    (fp_text value 100p (at 0 1.7 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 388 "Net-(C132-Pad1)"))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 84 "Net-(C132-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer B.Cu) (tedit 56A8FC3F)
    (at 144.27 87.48)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C133 (at 2.025 0.47) (layer B.SilkS))
    (fp_text value 100p (at 0 -1.7) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 85 "Net-(C133-Pad1)"))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer B.Cu) (tedit 56A8FC47)
    (at 140.995 87.68)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C134 (at 1.49 -0.07 90) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.7) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 415 3V3A_RX))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 5870D979)
    (at 124.24 46.44 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C136 (at 0.3 1.1 270) (layer F.SilkS))
    (fp_text value 100n (at 0 1.7 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 168 /3V6))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0805b (layer F.Cu) (tedit 5870D96A)
    (at 129.43 47.09 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C137 (at -0.17 -1.59 90) (layer F.SilkS))
    (fp_text value 10u (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 340 /3V3D))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 55A40188)
    (at 164.86 54.56 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C141 (at 0 -1.7 90) (layer F.SilkS))
    (fp_text value 100n (at 0 1.7 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 341 /5V))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 55A40188)
    (at 163.74 54.8 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C142 (at 0 -1.7 90) (layer F.SilkS))
    (fp_text value 100n (at 0 1.7 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 99 "Net-(C142-Pad1)"))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0805b (layer F.Cu) (tedit 5870DA15)
    (at 167.25 55.16 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C143 (at 0.06 2.01 90) (layer F.SilkS))
    (fp_text value 10u (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 99 "Net-(C142-Pad1)"))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 55A40188)
    (at 163.71 56.81 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C145 (at 0 -1.7 90) (layer F.SilkS))
    (fp_text value 10p (at 0 1.7 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 100 "Net-(C145-Pad1)"))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer F.Cu) (tedit 5870D9D3)
    (at 161.87 54.38 135)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C152 (at 0.056569 -0.042426 135) (layer F.SilkS))
    (fp_text value 1n (at 0 1.7 135) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 135) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 105 "Net-(C152-Pad1)"))
    (pad 2 smd rect (at 0.55 0 135) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 106 "Net-(C152-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0603b (layer B.Cu) (tedit 56A8FD6F)
    (at 181.22 46.53 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference FB1 (at -2.52 0.095 270) (layer B.SilkS))
    (fp_text value BLM18PG181SN1D (at 0 -1.9 270) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 93 /transmitter/3V3_RF))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(C16-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0603b (layer B.Cu) (tedit 56A8FD70)
    (at 175.11 45.69 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference FB2 (at -2.47 0.075 270) (layer B.SilkS))
    (fp_text value BLM18PG181SN1D (at 0 -1.9 270) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 93 /transmitter/3V3_RF))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(C21-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0603b (layer F.Cu) (tedit 5870D7AB)
    (at 159.445 75.155)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference FB3 (at -1.735 0.055 90) (layer F.SilkS))
    (fp_text value BLM18PG181SN1D (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 94 /receiver/lo_synth/3V3_RF))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C58-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0603b (layer F.Cu) (tedit 5870D7AE)
    (at 159.445 73.705)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference FB4 (at -1.795 -0.105 90) (layer F.SilkS))
    (fp_text value BLM18PG181SN1D (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 94 /receiver/lo_synth/3V3_RF))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C63-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer F.Cu) (tedit 56A8FA7D)
    (at 174.22 45.77 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R6 (at 0.53 0.97 270) (layer F.SilkS))
    (fp_text value 49.9 (at 0 1.8 270) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C6-Pad1)"))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer F.Cu) (tedit 56A8FA69)
    (at 174 52.88 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R11 (at 0.97 -0.68 180) (layer F.SilkS))
    (fp_text value 5.1k (at 0 1.8 180) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(R11-Pad1)"))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer B.Cu) (tedit 56A8FC0E)
    (at 173.91 47.63)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R12 (at -0.77 -1.01) (layer B.SilkS))
    (fp_text value 0 (at 0 -1.8) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 93 /transmitter/3V3_RF))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 70 "Net-(R12-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer B.Cu) (tedit 56A8FC12)
    (at 173.8 48.52)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R13 (at -1.36 -0.82 90) (layer B.SilkS))
    (fp_text value 0 (at 0 -1.8) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 93 /transmitter/3V3_RF))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 71 "Net-(R13-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer B.Cu) (tedit 56A8FBF1)
    (at 179.86 52.48)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R15 (at 0.16 1.15) (layer B.SilkS))
    (fp_text value 90.9 (at 0 -1.8) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(R15-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer B.Cu) (tedit 5870DB59)
    (at 165.1 49.22)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R16 (at 0.86 1.01) (layer B.SilkS))
    (fp_text value 33 (at 0 -1.8) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 59 "Net-(C11-Pad1)"))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 171 /3V3A))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer F.Cu) (tedit 56A8FA58)
    (at 181.385 51.93 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R17 (at 1.82 0.015 270) (layer F.SilkS))
    (fp_text value 30.1 (at 0 1.8 270) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C30-Pad1)"))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(R15-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer F.Cu) (tedit 56A8FAAB)
    (at 180.76 48.13 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R18 (at 1.33 0.08 270) (layer F.SilkS))
    (fp_text value 240 (at 0 1.8 180) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C30-Pad2)"))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C32-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer F.Cu) (tedit 56A8FABA)
    (at 178.39 48.28 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R19 (at -1.2 -0.89 270) (layer F.SilkS))
    (fp_text value 49.9 (at 0 1.8 180) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 93 /transmitter/3V3_RF))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 /transmitter/RF_OUT_P))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer F.Cu) (tedit 56A8FA90)
    (at 176.94 48.27)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R20 (at -0.19 -1.35 270) (layer F.SilkS))
    (fp_text value 49.9 (at 0 1.8) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 93 /transmitter/3V3_RF))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 /transmitter/RF_OUT_N))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer F.Cu) (tedit 5870D746)
    (at 169.235 86.635 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R25 (at -0.085 -1.035 90) (layer F.SilkS))
    (fp_text value 49.9 (at 0 1.8 90) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C44-Pad2)"))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 95 /receiver/5VF))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer F.Cu) (tedit 5870D749)
    (at 169.235 88.485 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R26 (at 0.255 -0.875 90) (layer F.SilkS))
    (fp_text value 49.9 (at 0 1.8 90) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 95 /receiver/5VF))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C46-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer F.Cu) (tedit 5870D755)
    (at 161.145 86.755)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R27 (at -1.565 0.165 90) (layer F.SilkS))
    (fp_text value 1k (at 0 1.8) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 95 /receiver/5VF))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C45-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer F.Cu) (tedit 5870D796)
    (at 169.795 76.355)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R29 (at 1.905 -0.525) (layer F.SilkS))
    (fp_text value 5.1k (at 0 1.8) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(R29-Pad1)"))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer F.Cu) (tedit 5870D780)
    (at 168.545 81.28 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R30 (at -1.695 0.38 180) (layer F.SilkS))
    (fp_text value 0 (at 0 1.8 180) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 94 /receiver/lo_synth/3V3_RF))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(R30-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer F.Cu) (tedit 5870D79F)
    (at 168.545 80.505 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R31 (at -2.385 0.475 180) (layer F.SilkS))
    (fp_text value 0 (at 0 1.8 180) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 94 /receiver/lo_synth/3V3_RF))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(R31-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer F.Cu) (tedit 5870D820)
    (at 117.32 98.065 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R32 (at 1.555 -0.24) (layer F.SilkS))
    (fp_text value 68k (at 0 1.8 270) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 74 "Net-(R32-Pad1)"))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer F.Cu) (tedit 5870D7A8)
    (at 160.445 77.105 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R33 (at 1.705 -0.455 180) (layer F.SilkS))
    (fp_text value 90.9 (at 0 1.8 180) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(R33-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer F.Cu) (tedit 5870D816)
    (at 117.47 105.015 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R34 (at 1.445 0.93 180) (layer F.SilkS))
    (fp_text value 59k (at 0 1.8 90) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 75 "Net-(R34-Pad1)"))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer F.Cu) (tedit 56A8FCD0)
    (at 160.045 78.555 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R35 (at -0.125 -1.05 90) (layer F.SilkS))
    (fp_text value 30.1 (at 0 1.8 90) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(C72-Pad1)"))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(R33-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer B.Cu) (tedit 5870DBDB)
    (at 165.245 75.08)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R36 (at -0.015 -0.82) (layer B.SilkS))
    (fp_text value 240 (at 0 -1.8) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(C72-Pad2)"))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 19 "Net-(C74-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer F.Cu) (tedit 56A8FCDC)
    (at 164.575 81.7)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R37 (at -0.025 -1.05) (layer F.SilkS))
    (fp_text value 49.9 (at 0 1.8) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 94 /receiver/lo_synth/3V3_RF))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 130 /receiver/LOP))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer F.Cu) (tedit 5870D76A)
    (at 166.275 81.7 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R38 (at -0.545 0.94) (layer F.SilkS))
    (fp_text value 49.9 (at 0 1.8 180) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 94 /receiver/lo_synth/3V3_RF))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 131 /receiver/LON))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer B.Cu) (tedit 56A8FB5F)
    (at 113.34 99.645 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R57 (at -0.17 0.96 270) (layer B.SilkS))
    (fp_text value 6.8k (at 0 -1.8 270) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 62 "Net-(C105-Pad1)"))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 57 "Net-(C101-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer B.Cu) (tedit 55A401B2)
    (at 112.07 107.665 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R58 (at 0 1.4 270) (layer B.SilkS))
    (fp_text value 8.2k (at 0 -1.8 270) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 63 "Net-(C106-Pad1)"))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 60 "Net-(C104-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer B.Cu) (tedit 56A8FB54)
    (at 113.62 94.815 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R60 (at -0.17 1.04 270) (layer B.SilkS))
    (fp_text value 4.99k (at 0 -1.8 270) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 66 "Net-(C110-Pad1)"))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 58 "Net-(C101-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer B.Cu) (tedit 56A8FB52)
    (at 114.57 95.615 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R61 (at 0.74 1.16 270) (layer B.SilkS))
    (fp_text value 1k (at 0 -1.8 270) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 58 "Net-(C101-Pad2)"))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer B.Cu) (tedit 56A8FB8C)
    (at 115.062 108.119 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R62 (at -1.816 0.138 90) (layer B.SilkS))
    (fp_text value 4.99k (at 0 -1.8 90) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 67 "Net-(C111-Pad1)"))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 61 "Net-(C104-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer B.Cu) (tedit 56A8FB79)
    (at 115.07 106.715 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R63 (at 0.77 -1.11 270) (layer B.SilkS))
    (fp_text value 680 (at 0 -1.8 90) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 61 "Net-(C104-Pad2)"))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer B.Cu) (tedit 56A8FB58)
    (at 115.72 94.79 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R64 (at -0.085 -0.86 270) (layer B.SilkS))
    (fp_text value 100 (at 0 -1.8 270) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 66 "Net-(C110-Pad1)"))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 64 "Net-(C108-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer B.Cu) (tedit 56A8FB85)
    (at 116.18 108.395)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R65 (at 0.22 1.17) (layer B.SilkS))
    (fp_text value 100 (at 0 -1.8) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 67 "Net-(C111-Pad1)"))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 65 "Net-(C109-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer B.Cu) (tedit 56A8FC43)
    (at 140.63 91.02 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R76 (at 0.09 1.1 90) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.8 90) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 116 /ADC_VCM))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 83 "Net-(C130-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer B.Cu) (tedit 56A8FC4B)
    (at 141.97 89.655 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R77 (at 1.565 0.235 270) (layer B.SilkS))
    (fp_text value 16k (at 0 -1.8 270) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 84 "Net-(C132-Pad2)"))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 83 "Net-(C130-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer B.Cu) (tedit 56A8FC3C)
    (at 144.17 88.955)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R78 (at 1.595 1.195 90) (layer B.SilkS))
    (fp_text value 16k (at 0 -1.8) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 85 "Net-(C133-Pad1)"))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 84 "Net-(C132-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer F.Cu) (tedit 5870D915)
    (at 112.59 71.68 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R86 (at 0.99 -0.1) (layer F.SilkS))
    (fp_text value DNP (at 0 1.8 270) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 387 /power/fpga_power/SYNC_1V0))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 76 /power/SYNC_3V3))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer F.Cu) (tedit 55A401B2)
    (at 161.875 58.9 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R90 (at 0 -1.4 180) (layer F.SilkS))
    (fp_text value 100 (at 0 1.8 180) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 107 "Net-(C151-Pad2)"))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 364 /tx_amp/DET_IN))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:R_0402b (layer F.Cu) (tedit 5870D9D1)
    (at 159.32 54.105 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R97 (at -0.12 0.885 180) (layer F.SilkS))
    (fp_text value 100 (at 0 1.8 180) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 108 "Net-(R97-Pad1)"))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 189 /PWDN))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:MLPD-10 (layer F.Cu) (tedit 5884C504)
    (at 171.524 44.646)
    (fp_text reference U13 (at 0.056 0.034 90) (layer F.SilkS))
    (fp_text value SKY13322-375LF (at 0.2 -2.1) (layer F.Fab))
    (pad 1 smd rect (at -0.875 -1) (size 0.55 0.25) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(C93-Pad2)"))
    (pad 2 smd rect (at -0.875 -0.5) (size 0.55 0.25) (layers F.Cu F.Paste F.Mask)
      (net 195 /FILTER_V2))
    (pad 3 smd rect (at -0.875 0) (size 0.55 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at -0.875 0.5) (size 0.55 0.25) (layers F.Cu F.Paste F.Mask)
      (net 194 /FILTER_V1))
    (pad 5 smd rect (at -0.875 1) (size 0.55 0.25) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(C94-Pad2)"))
    (pad 6 smd rect (at 0.875 1) (size 0.55 0.25) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(C92-Pad2)"))
    (pad 7 smd rect (at 0.875 0.5) (size 0.55 0.25) (layers F.Cu F.Paste F.Mask)
      (net 197 /FILTER_V3))
    (pad 8 smd rect (at 0.875 0) (size 0.55 0.25) (layers F.Cu F.Paste F.Mask)
      (net 22 /filter_bank/RF_IN))
    (pad 9 smd rect (at 0.875 -0.5) (size 0.55 0.25) (layers F.Cu F.Paste F.Mask)
      (net 196 /FILTER_V4))
    (pad 10 smd rect (at 0.875 -1) (size 0.55 0.25) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(C95-Pad2)"))
    (pad EP smd rect (at 0 0) (size 0.76 2.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.15))
    (pad EP thru_hole circle (at 0 0) (size 0.55 0.55) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
    (pad EP thru_hole circle (at 0 -0.9) (size 0.55 0.55) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
    (pad EP thru_hole circle (at 0 0.9) (size 0.55 0.55) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module VNA:MLPD-10 (layer F.Cu) (tedit 5884C4FC)
    (at 163.34 45.12 180)
    (fp_text reference U18 (at -0.04 0.21 270) (layer F.SilkS))
    (fp_text value SKY13322-375LF (at 0.2 -2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -0.875 -1 180) (size 0.55 0.25) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(C98-Pad1)"))
    (pad 2 smd rect (at -0.875 -0.5 180) (size 0.55 0.25) (layers F.Cu F.Paste F.Mask)
      (net 194 /FILTER_V1))
    (pad 3 smd rect (at -0.875 0 180) (size 0.55 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at -0.875 0.5 180) (size 0.55 0.25) (layers F.Cu F.Paste F.Mask)
      (net 195 /FILTER_V2))
    (pad 5 smd rect (at -0.875 1 180) (size 0.55 0.25) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(C97-Pad1)"))
    (pad 6 smd rect (at 0.875 1 180) (size 0.55 0.25) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(C96-Pad1)"))
    (pad 7 smd rect (at 0.875 0.5 180) (size 0.55 0.25) (layers F.Cu F.Paste F.Mask)
      (net 196 /FILTER_V4))
    (pad 8 smd rect (at 0.875 0 180) (size 0.55 0.25) (layers F.Cu F.Paste F.Mask)
      (net 23 /filter_bank/RF_OUT))
    (pad 9 smd rect (at 0.875 -0.5 180) (size 0.55 0.25) (layers F.Cu F.Paste F.Mask)
      (net 197 /FILTER_V3))
    (pad 10 smd rect (at 0.875 -1 180) (size 0.55 0.25) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(C99-Pad1)"))
    (pad EP smd rect (at 0 0 180) (size 0.76 2.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.15))
    (pad EP thru_hole circle (at 0 0 180) (size 0.55 0.55) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
    (pad EP thru_hole circle (at 0 -0.9 180) (size 0.55 0.55) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
    (pad EP thru_hole circle (at 0 0.9 180) (size 0.55 0.55) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module VNA:C_0805b (layer F.Cu) (tedit 5870D791)
    (at 170.18 73.98 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C158 (at -0.28 1.98 90) (layer F.SilkS))
    (fp_text value DNP (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 341 /5V))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0805b (layer F.Cu) (tedit 5870D898)
    (at 140.145 88.69 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C159 (at 0 -1.675 90) (layer F.SilkS))
    (fp_text value DNP (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 415 3V3A_RX))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer B.Cu) (tedit 55A40188)
    (at 167.56 54.39)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C161 (at 0 1.7) (layer B.SilkS))
    (fp_text value DNP (at 0 -1.7) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 341 /5V))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0402b (layer B.Cu) (tedit 5870DBC4)
    (at 167.63 71.14 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (zone_connect 2)
    (attr smd)
    (fp_text reference C162 (at -0.19 0.91 180) (layer B.SilkS))
    (fp_text value DNP (at 0 -1.7 180) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 341 /5V) (zone_connect 2))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND) (zone_connect 2))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0603b (layer F.Cu) (tedit 55A401E5)
    (at 163.11 58.17 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference L12 (at 0 -1.425 180) (layer F.SilkS))
    (fp_text value AISC-0603HP-R10J (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 100 "Net-(C145-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 107 "Net-(C151-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0603b (layer F.Cu) (tedit 5870DA11)
    (at 165.71 55.61 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference FB6 (at 0.12 -0.09) (layer F.SilkS))
    (fp_text value BLM18PG181SN1D (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 341 /5V))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 99 "Net-(C142-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-353 (layer F.Cu) (tedit 5870D9E9)
    (at 180.666 65.43 180)
    (descr SOT353)
    (attr smd)
    (fp_text reference U23 (at -0.864 -1.83) (layer F.SilkS))
    (fp_text value MIC5366-1.8YC5 (at 0.09906 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.016 -0.635 180) (size 0.508 0.3048) (layers F.Cu F.Paste F.Mask)
      (net 171 /3V3A))
    (pad 3 smd rect (at -1.016 0.635 180) (size 0.508 0.3048) (layers F.Cu F.Paste F.Mask)
      (net 171 /3V3A))
    (pad 5 smd rect (at 1.016 -0.635 180) (size 0.508 0.3048) (layers F.Cu F.Paste F.Mask)
      (net 389 /1V8_OSC))
    (pad 2 smd rect (at -1.016 0 180) (size 0.508 0.3048) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 1.016 0.635 180) (size 0.508 0.3048) (layers F.Cu F.Paste F.Mask))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-353.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.07000000000000001 0.09 0.08))
      (rotate (xyz 0 0 90))
    )
  )
  (module VNA:C_0603b (layer F.Cu) (tedit 5870D75B)
    (at 160.295 83.57)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference FB7 (at 0.215 -1.04) (layer F.SilkS))
    (fp_text value BLM18PG181SN1D (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 341 /5V))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 95 /receiver/5VF))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:5515LP15A730 (layer F.Cu) (tedit 56AC6C5D)
    (at 168.59 48.54)
    (fp_text reference U14 (at 0.225 1.625) (layer F.SilkS))
    (fp_text value 5515LP15A730 (at 0.325 -1.65) (layer F.Fab))
    (pad 1 smd rect (at 0.65 -0.7) (size 0.35 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 smd rect (at 0 -0.7) (size 0.35 0.6) (layers F.Cu F.Paste F.Mask)
      (zone_connect 2))
    (pad 3 smd rect (at -0.65 -0.7) (size 0.35 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 5 smd rect (at -0.65 0.7) (size 0.35 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 6 smd rect (at 0 0.7) (size 0.35 0.6) (layers F.Cu F.Paste F.Mask)
      (zone_connect 2))
    (pad 7 smd rect (at 0.65 0.7) (size 0.35 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 4 smd rect (at -1.12 0 90) (size 0.35 0.6) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(C99-Pad2)") (zone_connect 2))
    (pad 8 smd rect (at 1.12 0 90) (size 0.35 0.6) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(C92-Pad1)") (zone_connect 2))
  )
  (module VNA:LP0603A0902 (layer F.Cu) (tedit 5870D9AC)
    (at 167.298 41.438 180)
    (fp_text reference U15 (at 2.258 1.048 180) (layer F.SilkS))
    (fp_text value LP0603A0902ANTR (at -0.6 -1.375 180) (layer F.Fab))
    (pad 1 smd rect (at -0.6 0.35 180) (size 0.5 0.4) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(C95-Pad1)") (zone_connect 2))
    (pad 2 smd rect (at 0.65 0.35 180) (size 0.5 0.4) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(C96-Pad2)") (zone_connect 2))
    (pad 3 smd rect (at 0.65 -0.35 180) (size 0.5 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 4 smd rect (at -0.6 -0.35 180) (size 0.5 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
  )
  (module VNA:LP0603A0902 (layer F.Cu) (tedit 56AC6C42)
    (at 167.552 46.264 180)
    (fp_text reference U17 (at -0.048 1.284 180) (layer F.SilkS))
    (fp_text value LP0603A1880ANTR (at -0.6 -1.375 180) (layer F.Fab))
    (pad 1 smd rect (at -0.6 0.35 180) (size 0.5 0.4) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(C94-Pad1)") (zone_connect 2))
    (pad 2 smd rect (at 0.65 0.35 180) (size 0.5 0.4) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(C98-Pad2)") (zone_connect 2))
    (pad 3 smd rect (at 0.65 -0.35 180) (size 0.5 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 4 smd rect (at -0.6 -0.35 180) (size 0.5 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
  )
  (module VNA:3550LP14A300 (layer F.Cu) (tedit 5870D9B0)
    (at 167.806 43.724 180)
    (fp_text reference U16 (at 0.346 0.544 180) (layer F.SilkS))
    (fp_text value 3550LP14A300 (at 0.1 -1.1 180) (layer F.Fab))
    (pad 1 smd rect (at 0 0 180) (size 0.55 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 smd rect (at 0 0.5 180) (size 0.55 0.25) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(C93-Pad1)") (zone_connect 2))
    (pad 3 smd rect (at 0 1 180) (size 0.55 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 4 smd rect (at 0.8 1 180) (size 0.55 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 5 smd rect (at 0.8 0.5 180) (size 0.55 0.25) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(C97-Pad2)") (zone_connect 2))
    (pad 6 smd rect (at 0.8 0 180) (size 0.55 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
  )
  (module VNA:C_0805b (layer B.Cu) (tedit 5870DB42)
    (at 120.57 51.685 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C163 (at 0.075 -2.12) (layer B.SilkS))
    (fp_text value DNP (at 0 -2.1 270) (layer B.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 96 /power/12V_IN))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VNA:C_0805b (layer B.Cu) (tedit 5870DB3F)
    (at 119.32 51.675 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C164 (at -0.985 -3.35) (layer B.SilkS))
    (fp_text value DNP (at 0 -2.1 270) (layer B.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 96 /power/12V_IN))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 109.1 36.52) (end 183.01 36.52) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 109.1 122.17) (end 109.1 36.52) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 183.01 122.17) (end 109.1 122.17) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 183.01 36.52) (end 183.01 122.17) (layer Edge.Cuts) (width 0.15))
  (zone (net 96) (net_name /power/12V_IN) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.3))
    (min_thickness 0.18)
    (fill yes (arc_segments 16) (thermal_gap 0.208) (thermal_bridge_width 0.408))
    (polygon
      (pts
        (xy 120.86 43.095) (xy 120.86 51.395) (xy 109.71 51.395) (xy 109.71 43.095) (xy 109.96 43.095)
      )
    )
  )
  (zone (net 95) (net_name /receiver/5VF) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.3))
    (min_thickness 0.18)
    (fill yes (arc_segments 16) (thermal_gap 0.208) (thermal_bridge_width 0.408))
    (polygon
      (pts
        (xy 161.95 83.48) (xy 169.1 83.48) (xy 169.12 85.38) (xy 170.245 86.505) (xy 170.245 89.705)
        (xy 162.12 89.705) (xy 159.82 87.405) (xy 159.82 85.255)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -2.4 -32.7) (xy 297.7 -33.1) (xy 297.7 212.2) (xy -1.4 210.1)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -2.371015 -33.148673) (xy 297.728985 -33.548673) (xy 297.728985 211.751327) (xy -1.371015 209.651327)
      )
    )
  )
  (zone (net 56) (net_name /power/12V) (layer B.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads (clearance 0.35))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 107.73 51.547072) (xy 118.59 51.56) (xy 118.56 104.35) (xy 107.57 104.337072)
      )
    )
  )
  (zone (net 168) (net_name /3V6) (layer B.Cu) (hatch edge 0.508)
    (priority 3)
    (connect_pads (clearance 0.3))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 168.28 35.75) (xy 168.28 38.58) (xy 164.11 38.58) (xy 160.92 41.77) (xy 157.6 41.77)
        (xy 156.61 40.78) (xy 147.63 40.78) (xy 146.32 42.09) (xy 136.4 42.09) (xy 130.21 48.28)
        (xy 130.21 53.57) (xy 123.1 60.68) (xy 123.1 75.45) (xy 125.84 78.19) (xy 125.84 91.12)
        (xy 142.77 91.12) (xy 144.35 91.12) (xy 146.33 91.12) (xy 146.33 95.51) (xy 128.44 95.51)
        (xy 126.09 97.86) (xy 118.75 97.86) (xy 118.75 59.85) (xy 122.86 55.74) (xy 122.86 38.59)
        (xy 125.781516 35.668484)
      )
    )
  )
  (zone (net 199) (net_name /1V8) (layer B.Cu) (hatch edge 0.508)
    (priority 3)
    (connect_pads (clearance 0.2))
    (min_thickness 0.15)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 137.48 71.37) (xy 137.33 71.42) (xy 138.83 71.42) (xy 140.1 70.15) (xy 140.1 67.65)
        (xy 139.27 66.82) (xy 139.27 65.38) (xy 139.83 64.82) (xy 139.83 62.24) (xy 141.61 60.46)
        (xy 141.61 57.96) (xy 137.78 54.13) (xy 134.06 54.13) (xy 134.06 55.34) (xy 137.89 59.17)
        (xy 137.89 64.74) (xy 137.38 65.25) (xy 137.38 66.8) (xy 138.03 67.45) (xy 138.03 68.08)
        (xy 138.03 68.66) (xy 137.58 69.11) (xy 137.58 71.2)
      )
    )
  )
  (zone (net 199) (net_name /1V8) (layer B.Cu) (hatch edge 0.508)
    (priority 6)
    (connect_pads (clearance 0.25))
    (min_thickness 0.15)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 123.33 74.68) (xy 126.8 74.61) (xy 126.88 61.65) (xy 131.39 57.43) (xy 131.39 55.26)
        (xy 134.04 55.26) (xy 134.04 54.15) (xy 129.89 54.15) (xy 123.34 60.72)
      )
    )
  )
  (zone (net 368) (net_name /1V0) (layer B.Cu) (hatch edge 0.508)
    (priority 4)
    (connect_pads (clearance 0.2))
    (min_thickness 0.15)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 131.48 55.3) (xy 133.95 55.3) (xy 137.83 59.18) (xy 137.83 65.24) (xy 135.25 65.24)
        (xy 134.59 65.9) (xy 134.59 67.08) (xy 137.28 67.08) (xy 137.76 67.56) (xy 137.76 70.84)
        (xy 136.91 71.69) (xy 134.2 71.69) (xy 132.76 70.25) (xy 132.76 65.53) (xy 134.1 64.19)
        (xy 135.29 64.19) (xy 135.64 63.84) (xy 135.64 62.93) (xy 135.1 62.39) (xy 135.1 59.53)
        (xy 134.57 59) (xy 131.57 59)
      )
    )
  )
  (zone (net 368) (net_name /1V0) (layer In2.Cu) (hatch edge 0.508)
    (priority 3)
    (connect_pads (clearance 0.2))
    (min_thickness 0.15)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 134.11 63.7) (xy 140.17 63.7) (xy 140.17 67.48) (xy 135.99 71.66) (xy 135.18 71.66)
        (xy 132.96 69.44) (xy 132.96 63.67)
      )
    )
  )
  (zone (net 368) (net_name /1V0) (layer In2.Cu) (hatch edge 0.508)
    (priority 3)
    (connect_pads (clearance 0.2))
    (min_thickness 0.15)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 125.33 52.36) (xy 133.08 52.36) (xy 133.08 59.88) (xy 136.75 63.55) (xy 136.75 69.24)
        (xy 135.52 70.47) (xy 128.11 70.47) (xy 128.11 56.87) (xy 124.73 56.87) (xy 122.76 58.84)
        (xy 115.79 58.84) (xy 115.79 55.74) (xy 119.1 52.43)
      )
    )
  )
  (zone (net 368) (net_name /1V0) (layer F.Cu) (hatch edge 0.508)
    (priority 3)
    (connect_pads (clearance 0.25))
    (min_thickness 0.15)
    (fill yes (arc_segments 16) (thermal_gap 0.25) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 132.79 52.38) (xy 132.79 55.77) (xy 125.74 55.77) (xy 122.99 58.52) (xy 115.68 58.52)
        (xy 115.68 56.26) (xy 121.92 56.26) (xy 122.95 55.23) (xy 122.95 52.4)
      )
    )
  )
  (zone (net 341) (net_name /5V) (layer F.Cu) (hatch edge 0.508)
    (priority 3)
    (connect_pads yes (clearance 0.25))
    (min_thickness 0.15)
    (fill yes (arc_segments 16) (thermal_gap 0.25) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 154.4 99.26) (xy 154.41 102.84) (xy 148.09 102.82) (xy 144.35 106.56) (xy 132.94 106.56)
        (xy 131.28 106.56) (xy 129.25 104.53) (xy 126.27 104.53) (xy 124.72 109.84) (xy 123.18 109.85)
        (xy 121.1 111.93) (xy 117.69 111.93) (xy 117.69 108.02) (xy 120.01 108.02) (xy 127.21 100.82)
        (xy 129.91 100.82) (xy 132.6 103.51) (xy 143.29 103.53) (xy 147.86 99.26)
      )
    )
  )
  (zone (net 341) (net_name /5V) (layer In2.Cu) (hatch edge 0.508)
    (priority 3)
    (connect_pads (clearance 0.25))
    (min_thickness 0.15)
    (fill yes (arc_segments 16) (thermal_gap 0.25) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 172.3 78.51) (xy 172.3 84.5) (xy 161.58 84.5) (xy 161.58 87.58) (xy 159.1 90.06)
        (xy 156.96 90.06) (xy 156.96 81.09) (xy 158.13 79.92) (xy 170.48 79.92) (xy 170.47 78.52)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -2.788853 -31.575358) (xy 297.311147 -31.975358) (xy 297.311147 213.324642) (xy -1.788853 211.224642)
      )
    )
  )
  (zone (net 341) (net_name /5V) (layer F.Cu) (hatch edge 0.508)
    (priority 3)
    (connect_pads (clearance 0.2))
    (min_thickness 0.15)
    (fill yes (arc_segments 16) (thermal_gap 0.25) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 166.57 58.63) (xy 170.47 58.65) (xy 170.51 68.12) (xy 168.49 68.1) (xy 166.46 68.14)
        (xy 166.58 67.11) (xy 166.62 65.47) (xy 166.57 62.41) (xy 166.58 61.26)
      )
    )
  )
  (zone (net 341) (net_name /5V) (layer B.Cu) (hatch edge 0.508)
    (priority 3)
    (connect_pads (clearance 0.25))
    (min_thickness 0.15)
    (fill yes (arc_segments 16) (thermal_gap 0.25) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 153.72 100.59) (xy 153.72 101.57) (xy 167.81 101.57) (xy 169.1 102.86) (xy 171.57 102.86)
        (xy 171.57 98.2) (xy 160.01 98.2) (xy 160.01 95.89) (xy 159.47 95.35) (xy 159.47 84.9)
        (xy 161.41 83.32) (xy 169.56 83.32) (xy 172.92 79.6) (xy 171.3 78.29) (xy 169.91 79.68)
        (xy 157.89 80.14) (xy 156.96 81.07) (xy 156.96 95.54) (xy 153.75 99.17)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.15)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 163.775 94.85) (xy 164.525 94.85) (xy 164.525 96.5) (xy 163.775 96.5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.15)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 163.775 91.66) (xy 164.525 91.66) (xy 164.525 93.31) (xy 163.775 93.31)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.15)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 166.325 91.66) (xy 167.075 91.66) (xy 167.075 93.31) (xy 166.325 93.31)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.15))
    (min_thickness 0.15)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 111.075 59.025) (xy 116.85 59.025) (xy 116.85 65.75) (xy 110.975 65.75)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.15))
    (min_thickness 0.15)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 110.675 107.4) (xy 116.45 107.4) (xy 116.45 114.125) (xy 110.575 114.125)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.15))
    (min_thickness 0.15)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 122.35 123.14) (xy 122.35 117.84) (xy 124.85 117.84) (xy 124.85 123.14)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.15))
    (min_thickness 0.15)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 134.544023 123.15) (xy 134.544023 117.85) (xy 137.044023 117.85) (xy 137.044023 123.15)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.15))
    (min_thickness 0.15)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 145.740081 123.14) (xy 145.740081 117.84) (xy 148.240081 117.84) (xy 148.240081 123.14)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.15))
    (min_thickness 0.15)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 157.02 123.142979) (xy 157.02 117.842979) (xy 159.52 117.842979) (xy 159.52 123.142979)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.15))
    (min_thickness 0.15)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 167.742628 123.13) (xy 167.742628 117.83) (xy 170.242628 117.83) (xy 170.242628 123.13)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.15))
    (min_thickness 0.15)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 178.01 123.13) (xy 178.01 117.83) (xy 180.51 117.83) (xy 180.51 123.13)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.5))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -3.401567 -32.500301) (xy 296.698433 -32.900301) (xy 296.698433 212.399699) (xy -2.401567 210.299699)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (priority 9)
    (connect_pads yes (clearance 0.5))
    (min_thickness 0.15)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 120 125.9) (xy 120 117.7) (xy 184 117.7) (xy 183.9 125.9)
      )
    )
  )
  (zone (net 341) (net_name /5V) (layer In2.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads (clearance 0.25))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 124.89 103.42) (xy 127.49 100.82) (xy 129.11 100.82) (xy 129.54 101.25) (xy 129.54 102.89)
        (xy 127.21 105.22) (xy 125.18 105.22)
      )
    )
  )
  (zone (net 341) (net_name /5V) (layer B.Cu) (hatch edge 0.508)
    (priority 4)
    (connect_pads (clearance 0.25))
    (min_thickness 0.15)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 172.9 79.64) (xy 172.9 74.1) (xy 170.75 71.95) (xy 169.81 71.92544) (xy 169.22 71.31)
        (xy 169.22 67.47) (xy 168.85 67.1) (xy 166.69 67.1) (xy 166.46 67.33) (xy 166.46 68.41)
        (xy 167.02 68.97) (xy 167.37 69.32) (xy 167.37 72.3) (xy 168.74 72.3) (xy 168.74 77.72)
        (xy 170.66 77.72) (xy 171.25 78.31)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads (clearance 0.25))
    (min_thickness 0.15)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 132.92 106.46) (xy 134.09 107.63) (xy 144.93 107.63) (xy 146.86 105.7) (xy 150.93 105.7)
        (xy 154.83 109.6) (xy 154.83 102.49) (xy 148.38 102.48) (xy 144.55 106.48) (xy 133 106.48)
      )
    )
  )
  (zone (net 171) (net_name /3V3A) (layer F.Cu) (hatch edge 0.508)
    (priority 3)
    (connect_pads (clearance 0.2))
    (min_thickness 0.15)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 183.4 107.29) (xy 180.44 107.29) (xy 180.44 72.27) (xy 181.1 71.61) (xy 181.1 64.12)
        (xy 183.4 64.12)
      )
    )
  )
  (zone (net 171) (net_name /3V3A) (layer In2.Cu) (hatch edge 0.508)
    (priority 3)
    (connect_pads (clearance 0.2))
    (min_thickness 0.15)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 181.3 70.31) (xy 183.67 70.31) (xy 183.67 62.01) (xy 177.24 62.01) (xy 174.1 58.87)
        (xy 174.1 55.96) (xy 173.29 55.15) (xy 161.18 55.15) (xy 159.72 53.69) (xy 159.72 43.42)
        (xy 156.93 43.42) (xy 156.93 56.69) (xy 159.46 59.22) (xy 166.62 59.22) (xy 167.89 57.95)
        (xy 172.32 57.95) (xy 172.32 60.75) (xy 174.07 62.5) (xy 175.36 62.5) (xy 181.07 68.21)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer In1.Cu) (hatch edge 0.508)
    (priority 10)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.15)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 134.7 116.48) (xy 136.77 116.48) (xy 136.77 117.97) (xy 134.7 117.97) (xy 134.69 117.77)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer In1.Cu) (hatch edge 0.508)
    (priority 10)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.15)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 146.02 116.5) (xy 148.09 116.5) (xy 148.09 118.08) (xy 146.02 118.08) (xy 146.016089 117.77)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer In1.Cu) (hatch edge 0.508)
    (priority 10)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.15)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 143.953911 113.46) (xy 147.09 113.37) (xy 147.09 114.95) (xy 144.36 115.16) (xy 143.95 114.73)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer In1.Cu) (hatch edge 0.508)
    (priority 10)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.15)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 135.003911 113.69) (xy 138.35 113.65) (xy 138.35 115.23) (xy 136.28 115.23) (xy 135 114.96)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer In1.Cu) (hatch edge 0.508)
    (priority 10)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.15)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 157.25 116.44) (xy 159.32 116.44) (xy 159.32 118.02) (xy 157.25 118.02) (xy 157.246089 117.71)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer In1.Cu) (hatch edge 0.508)
    (priority 10)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.15)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 167.573911 116.59) (xy 170.27 116.58) (xy 170.27 118.16) (xy 167.96 118.1) (xy 167.57 117.86)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer In1.Cu) (hatch edge 0.508)
    (priority 10)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.15)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 166.888269 113.46) (xy 170.26 113.46) (xy 170.26 115.04) (xy 166.888269 115.04) (xy 166.884358 114.73)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer In1.Cu) (hatch edge 0.508)
    (priority 10)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.15)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 158.468269 113.41) (xy 161.84 113.41) (xy 161.84 114.99) (xy 158.468269 114.99) (xy 158.464358 114.68)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer In1.Cu) (hatch edge 0.508)
    (priority 10)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.15)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 149.26 109.05) (xy 156.056089 108.96) (xy 156.08 114.15) (xy 149.785468 114.155489) (xy 149.25 114.16)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer In1.Cu) (hatch edge 0.508)
    (priority 10)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.15)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 157.01 103.16) (xy 160.381731 103.16) (xy 160.39 106.83) (xy 157.018269 106.83) (xy 157.035514 105.2)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer In1.Cu) (hatch edge 0.508)
    (priority 10)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.15)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 139.725401 107.97) (xy 143.097132 107.97) (xy 143.105401 111.64) (xy 139.73367 111.64) (xy 139.750915 110.01)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer In1.Cu) (hatch edge 0.508)
    (priority 10)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.15)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 126.15 108.09) (xy 129.521731 108.09) (xy 129.53 111.76) (xy 126.158269 111.76) (xy 126.175514 110.13)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer In1.Cu) (hatch edge 0.508)
    (priority 10)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.15)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 157.86 62.09) (xy 166.58 62.14) (xy 166.588269 65.81) (xy 157.868269 65.76) (xy 157.885514 64.13)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer In1.Cu) (hatch edge 0.508)
    (priority 10)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.15)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 176.248269 106.97) (xy 179.62 106.97) (xy 179.62 108.55) (xy 176.248269 108.55) (xy 176.244358 108.24)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (priority 10)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.15)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 126.08514 108.120992) (xy 129.456871 108.120992) (xy 129.46514 111.790992) (xy 126.093409 111.790992) (xy 126.110654 110.160992)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (priority 10)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.15)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 157.9 62.07) (xy 160.001731 62.06) (xy 160.01 65.73) (xy 157.95 65.69) (xy 157.89 64.05)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (priority 10)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.15)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 164.55479 62.22555) (xy 166.656521 62.21555) (xy 166.66479 65.88555) (xy 164.60479 65.84555) (xy 164.54479 64.20555)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (priority 10)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.15)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 176.81 105.58) (xy 179.61 105.71) (xy 179.618269 109.38) (xy 176.88 109.39) (xy 176.82 107.75)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (priority 10)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.15)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 167.563911 116.5) (xy 170.26 116.49) (xy 170.26 118.07) (xy 167.95 118.01) (xy 167.56 117.77)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (priority 10)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.15)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 156.999912 116.453598) (xy 159.696001 116.443598) (xy 159.696001 118.023598) (xy 157.386001 117.963598) (xy 156.996001 117.723598)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (priority 10)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.15)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 145.766632 116.562126) (xy 148.462721 116.552126) (xy 148.462721 118.132126) (xy 146.152721 118.072126) (xy 145.762721 117.832126)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (priority 10)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.15)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 134.446461 116.389416) (xy 137.14255 116.379416) (xy 137.14255 117.959416) (xy 134.83255 117.899416) (xy 134.44255 117.659416)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (priority 10)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.15)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 135.005047 113.657192) (xy 138.351136 113.617192) (xy 138.351136 115.197192) (xy 136.281136 115.197192) (xy 135.001136 114.927192)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (priority 10)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.15)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 143.682426 113.54231) (xy 147.028515 113.50231) (xy 147.028515 115.08231) (xy 144.958515 115.08231) (xy 143.678515 114.81231)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (priority 10)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.15)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 158.463911 113.47) (xy 161.81 113.43) (xy 161.81 115.01) (xy 159.74 115.01) (xy 158.46 114.74)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (priority 10)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.15)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 166.513911 113.54) (xy 169.86 113.5) (xy 169.86 115.08) (xy 167.79 115.08) (xy 166.51 114.81)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (priority 10)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.15)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 151.283911 109.04) (xy 153.98 109.03) (xy 153.98 110.61) (xy 151.67 110.55) (xy 151.28 110.31)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (priority 10)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.15)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 157.333911 103.75) (xy 160.03 103.74) (xy 160.01 106.24) (xy 157.7 106.18) (xy 157.33 105.02)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (priority 10)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.15)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 139.423911 109.68) (xy 143.12 109.66) (xy 143.12 111.24) (xy 140.326409 111.204746) (xy 139.42 110.95)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (priority 10)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.15)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 162.31 109.08) (xy 166.006089 109.06) (xy 165.99 111.48) (xy 163.196409 111.444746) (xy 162.34 111.47)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer In1.Cu) (hatch edge 0.508)
    (priority 10)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.15)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 162.47 109.09) (xy 165.841731 109.09) (xy 165.83 111.58) (xy 162.458269 111.58) (xy 162.464358 110.77)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (priority 10)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.15)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 154.45671 111.0581) (xy 156.77 110.52) (xy 156.74 114.16) (xy 155.35 114.22) (xy 154.493591 114.245254)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (priority 10)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.15)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 148.403786 111.116112) (xy 150.717076 110.578012) (xy 150.687076 114.218012) (xy 149.297076 114.278012) (xy 148.440667 114.303266)
      )
    )
  )
  (zone (net 340) (net_name /3V3D) (layer B.Cu) (hatch edge 0.508)
    (priority 5)
    (connect_pads (clearance 0.25))
    (min_thickness 0.15)
    (fill yes (arc_segments 16) (thermal_gap 0.25) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 136.23 48.99) (xy 137.96 47.07) (xy 147.369996 47.09) (xy 147.36 72.32) (xy 145.18 74.5)
        (xy 145.18 77.36) (xy 144.84 77.7) (xy 144.84 79.37) (xy 146.37 79.37) (xy 146.37 80.38)
        (xy 141.27 80.38) (xy 138.62 83.03) (xy 133.31 83.03) (xy 132.64 82.36) (xy 132.64 80.86)
        (xy 128.51 76.73) (xy 128.51 60.3) (xy 130.6 58.21) (xy 131.43 58.21) (xy 131.43 59.11)
        (xy 134 59.11) (xy 134 61.42) (xy 135.4 62.82) (xy 135.4 63.84) (xy 134.24 63.84)
        (xy 132.59 65.49) (xy 132.59 70.2) (xy 134.23 71.84) (xy 139.13 71.84) (xy 140.25 70.72)
        (xy 140.25 62.19) (xy 141.85 60.59) (xy 141.85 57.74) (xy 136.55 52.44)
      )
    )
  )
)
