(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(grid_origin 27 24.25)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "GND")
	(net 2 "VCC")
	(net 3 "/SDA")
	(net 4 "/SCL")
	(net 5 "/INT")
	(net 6 "/ADD0")
	(net 7 "unconnected-(U1-EXP-Pad7)")
	(net 8 "unconnected-(U1-EXP-Pad7)_0")
	(net 9 "unconnected-(U1-EXP-Pad7)_1")
	(net 10 "unconnected-(U1-EXP-Pad7)_2")
	(net 11 "unconnected-(U1-EXP-Pad7)_3")
	(net 12 "unconnected-(U1-EXP-Pad7)_4")
	(net 13 "unconnected-(U1-EXP-Pad7)_5")
	(net 14 "unconnected-(U1-EXP-Pad7)_6")
	(footprint "Connector_Wire:SolderWirePad_1x01_SMD_1x2mm"
		(layer "F.Cu")
		(at 20 26.25 -90)
		(descr "Wire Pad, Square, SMD Pad,  1mm x 2mm,")
		(tags "MesurementPoint Square SMDPad 1mmx2mm ")
		(property "Reference" "J4"
			(at 0 -2.54 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x01_Pin"
			(at 0 2.54 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Connector_Wire:SolderWirePad_1x01_SMD_1x2mm"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "project-tmp117.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at 0 0 270)
			(size 1 2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "/INT")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 40 19.75 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C2"
			(at 0 -1.68 270)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "4.7uF"
			(at 0 1.68 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "project-tmp117.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Wire:SolderWirePad_1x01_SMD_1x2mm"
		(layer "F.Cu")
		(at 20 28.25 -90)
		(descr "Wire Pad, Square, SMD Pad,  1mm x 2mm,")
		(tags "MesurementPoint Square SMDPad 1mmx2mm ")
		(property "Reference" "J5"
			(at 0 -2.54 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x01_Pin"
			(at 0 2.54 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Connector_Wire:SolderWirePad_1x01_SMD_1x2mm"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "project-tmp117.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at 0 0 270)
			(size 1 2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 32.5 24.25 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R4"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10k"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "project-tmp117.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "/SCL")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "SM04B-SRSS-TB(LF)(SN):JST_SM04B-SRSS-TB(LF)(SN)"
		(layer "F.Cu")
		(at 27 26)
		(property "Reference" "J7"
			(at -0.545095 -1.767685 360)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SM04B-SRSS-TB(LF)(SN)"
			(at 12.17039 5.74055 360)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "JST_SM04B-SRSS-TB(LF)(SN)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Manufacturer recommendations"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "JST"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "project-tmp117.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at -1.5 0)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.5 0)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "VCC")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 0.5 0)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "/SDA")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 1.5 0)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "/SCL")
			(pinfunction "4")
			(pintype "passive")
		)
		(pad "S1" smd rect
			(at -2.8 3.875)
			(size 1.2 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "SHIELD")
			(pintype "passive")
		)
		(pad "S2" smd rect
			(at 2.8 3.875)
			(size 1.2 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "SHIELD")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/kicad-library/SM04B-SRSS-TB(LF)(SN)/SM04B-SRSS-TB_LF__SN_.step"
			(offset
				(xyz 0 -0.5 -0.3)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "Connector_Wire:SolderWirePad_1x01_SMD_1x2mm"
		(layer "F.Cu")
		(at 20 20.25 -90)
		(descr "Wire Pad, Square, SMD Pad,  1mm x 2mm,")
		(tags "MesurementPoint Square SMDPad 1mmx2mm ")
		(property "Reference" "J1"
			(at 0 -2.54 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x01_Pin"
			(at 0 2.54 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Connector_Wire:SolderWirePad_1x01_SMD_1x2mm"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "project-tmp117.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at 0 0 270)
			(size 1 2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "VCC")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
	)
	(footprint "TMP117AIDRVR:SON65P200X200X80-7N"
		(layer "F.Cu")
		(at 56 24.25 90)
		(property "Reference" "U1"
			(at 0.532 -1.9064 270)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TMP117AIDRVR"
			(at 6.2216 1.9064 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "TMP117AIDRVR:SON65P200X200X80-7N"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" "Texas Instruments"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" "0.8 mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" "WSON-6 Texas Instruments"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price" "None"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Check_prices" "https://www.snapeda.com/parts/TMP117AIDRVR/Texas+Instruments/view-part/?ref=eda"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" "IPC 7351B"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" "B"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" "https://www.snapeda.com/parts/TMP117AIDRVR/Texas+Instruments/view-part/?ref=snap"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MP" "TMP117AIDRVR"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Purchase-URL" "https://www.snapeda.com/api/url_track_click_mouser/?unipart_id=3214034&manufacturer=Texas Instruments&part_name=TMP117AIDRVR&search_term=None"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" "\n0.1°C digital temperature sensor, 48-bit EEPROM, PT100/PT1000 RTD replacement\n"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Availability" "In Stock"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Texas Instruments"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "project-tmp117.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -1.02 -0.65 90)
			(size 0.69 0.32)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.04)
			(net 4 "/SCL")
			(pinfunction "SCL")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -1.02 0 90)
			(size 0.69 0.32)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.04)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at -1.02 0.65 90)
			(size 0.69 0.32)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.04)
			(net 5 "/INT")
			(pinfunction "ALERT")
			(pintype "output")
		)
		(pad "4" smd roundrect
			(at 1.02 0.65 90)
			(size 0.69 0.32)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.04)
			(net 6 "/ADD0")
			(pinfunction "ADD0")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at 1.02 0 90)
			(size 0.69 0.32)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.04)
			(net 2 "VCC")
			(pinfunction "V+")
			(pintype "power_in")
		)
		(pad "6" smd roundrect
			(at 1.02 -0.65 90)
			(size 0.69 0.32)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.04)
			(net 3 "/SDA")
			(pinfunction "SDA")
			(pintype "bidirectional")
		)
		(pad "7" thru_hole circle
			(at -0.2 -0.5 180)
			(size 0.508 0.508)
			(drill 0.254)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "unconnected-(U1-EXP-Pad7)_3")
			(pinfunction "EXP")
			(pintype "power_in+no_connect")
		)
		(pad "7" thru_hole circle
			(at -0.2 0 180)
			(size 0.508 0.508)
			(drill 0.254)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "unconnected-(U1-EXP-Pad7)_5")
			(pinfunction "EXP")
			(pintype "power_in+no_connect")
		)
		(pad "7" thru_hole circle
			(at -0.2 0.5 180)
			(size 0.508 0.508)
			(drill 0.254)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "unconnected-(U1-EXP-Pad7)_4")
			(pinfunction "EXP")
			(pintype "power_in+no_connect")
		)
		(pad "7" smd rect
			(at 0 0 180)
			(size 1.6 1)
			(layers "F.Cu" "F.Mask")
			(net 9 "unconnected-(U1-EXP-Pad7)_1")
			(pinfunction "EXP")
			(pintype "power_in+no_connect")
		)
		(pad "7" smd rect
			(at 0 0 180)
			(size 1.6 1)
			(layers "B.Cu" "B.Mask")
			(net 14 "unconnected-(U1-EXP-Pad7)_6")
			(pinfunction "EXP")
			(pintype "power_in+no_connect")
		)
		(pad "7" thru_hole circle
			(at 0.2 -0.5 180)
			(size 0.508 0.508)
			(drill 0.254)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "unconnected-(U1-EXP-Pad7)_2")
			(pinfunction "EXP")
			(pintype "power_in+no_connect")
		)
		(pad "7" thru_hole circle
			(at 0.2 0 180)
			(size 0.508 0.508)
			(drill 0.254)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "unconnected-(U1-EXP-Pad7)")
			(pinfunction "EXP")
			(pintype "power_in+no_connect")
		)
		(pad "7" thru_hole circle
			(at 0.2 0.5 180)
			(size 0.508 0.508)
			(drill 0.254)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "unconnected-(U1-EXP-Pad7)_0")
			(pinfunction "EXP")
			(pintype "power_in+no_connect")
		)
		(model "${KIPRJMOD}/kicad-library/TMP117AIDRVR/TMP117AIDRVR.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm"
		(layer "F.Cu")
		(at 40.5 29.25 90)
		(descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
		(tags "solder jumper open")
		(property "Reference" "JP3"
			(at 0 -1.8 270)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "4B"
			(at 2.25 0 0)
			(layer "F.SilkS")
		)
		(property "Footprint" "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Solder Jumper, 2-pole, open"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Open*")
		(sheetname "Root")
		(sheetfile "project-tmp117.kicad_sch")
		(zone_connect 1)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "1" smd custom
			(at -0.65 0 90)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 6 "/ADD0")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0.5 0.75) (xy 0 0.75) (xy 0 -0.75) (xy 0.5 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" smd custom
			(at 0.65 0 90)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 4 "/SCL")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
	)
	(footprint "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm"
		(layer "F.Cu")
		(at 35.5 29.25 90)
		(descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
		(tags "solder jumper open")
		(property "Reference" "JP1"
			(at 0 -1.8 270)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "49"
			(at 2.25 0 180)
			(layer "F.SilkS")
		)
		(property "Footprint" "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Solder Jumper, 2-pole, open"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Open*")
		(sheetname "Root")
		(sheetfile "project-tmp117.kicad_sch")
		(zone_connect 1)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "1" smd custom
			(at -0.65 0 90)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 6 "/ADD0")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0.5 0.75) (xy 0 0.75) (xy 0 -0.75) (xy 0.5 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" smd custom
			(at 0.65 0 90)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 2 "VCC")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
	)
	(footprint "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm"
		(layer "F.Cu")
		(at 38 29.25 90)
		(descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
		(tags "solder jumper open")
		(property "Reference" "JP2"
			(at 0 -1.8 270)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "4A"
			(at 2.25 0 180)
			(layer "F.SilkS")
		)
		(property "Footprint" "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Solder Jumper, 2-pole, open"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Open*")
		(sheetname "Root")
		(sheetfile "project-tmp117.kicad_sch")
		(zone_connect 1)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "1" smd custom
			(at -0.65 0 90)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 6 "/ADD0")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0.5 0.75) (xy 0 0.75) (xy 0 -0.75) (xy 0.5 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" smd custom
			(at 0.65 0 90)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 3 "/SDA")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 54 24.25 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C1"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0.1uF"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "project-tmp117.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 34 24.25 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R2"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10k"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "project-tmp117.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "/SDA")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "SM04B-SRSS-TB(LF)(SN):JST_SM04B-SRSS-TB(LF)(SN)"
		(layer "F.Cu")
		(at 27 22.5 180)
		(property "Reference" "J8"
			(at -0.545095 -1.767685 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SM04B-SRSS-TB(LF)(SN)"
			(at 12.17039 5.74055 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "JST_SM04B-SRSS-TB(LF)(SN)"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Manufacturer recommendations"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "JST"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "project-tmp117.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at -1.5 0 180)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.5 0 180)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "VCC")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 0.5 0 180)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "/SDA")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 1.5 0 180)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "/SCL")
			(pinfunction "4")
			(pintype "passive")
		)
		(pad "S1" smd rect
			(at -2.8 3.875 180)
			(size 1.2 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "SHIELD")
			(pintype "passive")
		)
		(pad "S2" smd rect
			(at 2.8 3.875 180)
			(size 1.2 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "SHIELD")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/kicad-library/SM04B-SRSS-TB(LF)(SN)/SM04B-SRSS-TB_LF__SN_.step"
			(offset
				(xyz 0 -0.5 -0.3)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "Connector_Wire:SolderWirePad_1x01_SMD_1x2mm"
		(layer "F.Cu")
		(at 20 22.25 -90)
		(descr "Wire Pad, Square, SMD Pad,  1mm x 2mm,")
		(tags "MesurementPoint Square SMDPad 1mmx2mm ")
		(property "Reference" "J2"
			(at 0 -2.54 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x01_Pin"
			(at 0 2.54 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Connector_Wire:SolderWirePad_1x01_SMD_1x2mm"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "project-tmp117.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at 0 0 270)
			(size 1 2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "/SDA")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
	)
	(footprint "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm"
		(layer "F.Cu")
		(at 33 29.25 90)
		(descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
		(tags "solder jumper open")
		(property "Reference" "JP4"
			(at 0 -1.8 270)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "48"
			(at 2.25 0 180)
			(layer "F.SilkS")
		)
		(property "Footprint" "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Solder Jumper, 2-pole, open"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Open*")
		(sheetname "Root")
		(sheetfile "project-tmp117.kicad_sch")
		(zone_connect 1)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "1" smd custom
			(at -0.65 0 90)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 6 "/ADD0")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0.5 0.75) (xy 0 0.75) (xy 0 -0.75) (xy 0.5 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" smd custom
			(at 0.65 0 90)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 1 "GND")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
	)
	(footprint "Connector_Wire:SolderWirePad_1x01_SMD_1x2mm"
		(layer "F.Cu")
		(at 20 24.25 -90)
		(descr "Wire Pad, Square, SMD Pad,  1mm x 2mm,")
		(tags "MesurementPoint Square SMDPad 1mmx2mm ")
		(property "Reference" "J3"
			(at 0 -2.54 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x01_Pin"
			(at 0 2.54 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Connector_Wire:SolderWirePad_1x01_SMD_1x2mm"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "project-tmp117.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at 0 0 270)
			(size 1 2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "/SCL")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
	)
	(gr_line
		(start 58 26.25)
		(end 58 22.25)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 41 17.25)
		(end 19.5 17.25)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 57 21.25)
		(mid 57.707107 21.542893)
		(end 58 22.25)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 19.5 31.25)
		(end 41 31.25)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 45 27.25)
		(end 57 27.25)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 19.5 31.25)
		(mid 18.085786 30.664214)
		(end 17.5 29.25)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 41 17.25)
		(mid 42.414214 17.835786)
		(end 43 19.25)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 17.5 19.25)
		(end 17.5 29.25)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 17.5 19.25)
		(mid 18.085786 17.835786)
		(end 19.5 17.25)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 43 29.25)
		(mid 42.414214 30.664214)
		(end 41 31.25)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 43 29.25)
		(mid 43.585786 27.835786)
		(end 45 27.25)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 45 21.25)
		(mid 43.585786 20.664214)
		(end 43 19.25)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 45 21.25)
		(end 57 21.25)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 58 26.25)
		(mid 57.707107 26.957107)
		(end 57 27.25)
		(layer "Edge.Cuts")
	)
	(gr_text "François Gervais\n2 avril 2024\nv1.0.0"
		(at 41.5 24.75 0)
		(layer "B.SilkS")
	)
	(gr_text "Sda"
		(at 21 22.25 0)
		(layer "F.SilkS")
	)
	(gr_text "Vcc"
		(at 21 20.25 0)
		(layer "F.SilkS")
	)
	(gr_text "Gnd"
		(at 21 28.25 0)
		(layer "F.SilkS")
	)
	(gr_text "Int"
		(at 21 26.25 0)
		(layer "F.SilkS")
	)
	(gr_text "Scl"
		(at 21 24.25 0)
		(layer "F.SilkS")
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 17.5 31.25) (xy 17.5 17.25) (xy 58 17.25) (xy 58 31.25)
			)
		)
	)
)