(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (aux_axis_origin 122.301 132.334)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "+12V")
  (net 2 "GND")
  (net 3 "Net-(J2-Pad2)")
  (net 4 "Net-(J4-Pad2)")
  (net 5 "Net-(J5-Pad2)")
  (net 6 "Net-(R1-Pad2)")
  (net 7 "Net-(R2-Pad2)")
  (net 8 "Net-(R3-Pad2)")
  (net 9 "Net-(R4-Pad2)")
  (net 10 "Net-(R5-Pad2)")
  (net 11 "Net-(R6-Pad2)")
  (net 12 "Net-(R7-Pad2)")
  (net 13 "Net-(R8-Pad2)")
  (net 14 "Net-(J1-Pad5)")
  (net 15 "Net-(U1-Pad4)")
  (net 16 "+3V3")
  (net 17 "Net-(J1-Pad4)")
  (net 18 "Net-(U16-Pad1)")
  (net 19 "Net-(J1-Pad3)")
  (net 20 "Net-(U20-Pad1)")
  (net 21 "Net-(J1-Pad2)")
  (net 22 "Net-(U4-Pad4)")
  (net 23 "Net-(J2-Pad3)")
  (net 24 "Net-(J3-Pad3)")
  (net 25 "Net-(J4-Pad3)")
  (net 26 "Net-(J5-Pad3)")
  (net 27 "Net-(J3-Pad2)")
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 134.0855 68.199 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Switch_Driver.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C6" (at 2.6405 0) (layer "F.SilkS"))
    (fp_text value "C" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0 180) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+12V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 180) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23_Handsoldering" (layer "F.Cu")
    (tedit 5A0AB76C)
    (at 135.1806 81.961)
    (descr "SOT-23, Handsoldering")
    (tags "SOT-23")
    (property "Sheetfile" "Switch_Driver.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U16" (at 0 -2.5) (layer "F.SilkS"))
    (fp_text value "NMOS_0_2A" (at 0 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.5 -0.95) (size 1.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "Net-(U16-Pad1)") (pinfunction "Gate") (pintype "input"))
    (pad "2" smd rect (at -1.5 0.95) (size 1.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "Drain") (pintype "output"))
    (pad "3" smd rect (at 1.5 0) (size 1.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "Net-(R7-Pad2)") (pinfunction "Source") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x03_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5A19A429)
    (at 158.8266 101.976)
    (descr "Through hole straight socket strip, 1x03, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x03 2.54mm single row")
    (property "Sheetfile" "Switch_Driver.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J5" (at 0 -2.77) (layer "F.SilkS"))
    (fp_text value "Conn_01x03" (at 0 7.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J5-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(J5-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23_Handsoldering" (layer "F.Cu")
    (tedit 5A0AB76C)
    (at 135.2286 99.553)
    (descr "SOT-23, Handsoldering")
    (tags "SOT-23")
    (property "Sheetfile" "Switch_Driver.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U20" (at -1.294 -2.794) (layer "F.SilkS"))
    (fp_text value "NMOS_0_2A" (at 0 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.5 -0.95) (size 1.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 20 "Net-(U20-Pad1)") (pinfunction "Gate") (pintype "input"))
    (pad "2" smd rect (at -1.5 0.95) (size 1.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "Drain") (pintype "output"))
    (pad "3" smd rect (at 1.5 0) (size 1.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "Net-(R8-Pad2)") (pinfunction "Source") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2_DIN965_Pad" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 126.238 127.635)
    (descr "Mounting Hole 2.2mm, M2, DIN965")
    (tags "mounting hole 2.2mm m2 din965")
    (property "Sheetfile" "Switch_Driver.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H1" (at 0 -2.9) (layer "F.SilkS"))
    (fp_text value "MountingHole_Pad" (at 0 2.9) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 3.8 3.8) (drill 2.2) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input"))
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2_DIN965_Pad" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 126.238 64.77)
    (descr "Mounting Hole 2.2mm, M2, DIN965")
    (tags "mounting hole 2.2mm m2 din965")
    (property "Sheetfile" "Switch_Driver.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H2" (at -1.27 2.921) (layer "F.SilkS"))
    (fp_text value "MountingHole_Pad" (at 0 2.9) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 3.8 3.8) (drill 2.2) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input"))
  )
  (footprint "Package_TO_SOT_SMD:TO-252-2" (layer "F.Cu")
    (tedit 5A70A390)
    (at 143.6216 83.7464)
    (descr "TO-252 / DPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO252/PG-TO252-3-1/")
    (tags "DPAK TO-252 DPAK-3 TO-252-3 SOT-428")
    (property "Sheetfile" "Switch_Driver.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U15" (at 0 -4.5) (layer "F.SilkS"))
    (fp_text value "PMOS_4A" (at 0 4.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" smd rect (at 3.775 1.525) (size 3.05 2.75) (layers "F.Paste"))
    (pad "" smd rect (at 3.775 -1.525) (size 3.05 2.75) (layers "F.Paste"))
    (pad "" smd rect (at 0.425 1.525) (size 3.05 2.75) (layers "F.Paste"))
    (pad "" smd rect (at 0.425 -1.525) (size 3.05 2.75) (layers "F.Paste"))
    (pad "1" smd rect (at -4.2 -2.28) (size 2.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "Net-(R7-Pad2)") (pinfunction "Gate") (pintype "input"))
    (pad "2" smd rect (at 2.1 0) (size 6.4 5.8) (layers "F.Cu" "F.Mask")
      (net 4 "Net-(J4-Pad2)") (pinfunction "Drain") (pintype "output"))
    (pad "3" smd rect (at -4.2 2.28) (size 2.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "+12V") (pinfunction "Source") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/TO-252-2.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23_Handsoldering" (layer "F.Cu")
    (tedit 5A0AB76C)
    (at 135.2286 107.173)
    (descr "SOT-23, Handsoldering")
    (tags "SOT-23")
    (property "Sheetfile" "Switch_Driver.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U18" (at -2.6406 2.555) (layer "F.SilkS"))
    (fp_text value "NMOS_0_2A" (at 0 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.5 -0.95) (size 1.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 19 "Net-(J1-Pad3)") (pinfunction "Gate") (pintype "input"))
    (pad "2" smd rect (at -1.5 0.95) (size 1.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "Drain") (pintype "output"))
    (pad "3" smd rect (at 1.5 0) (size 1.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "Net-(R5-Pad2)") (pinfunction "Source") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23_Handsoldering" (layer "F.Cu")
    (tedit 5A0AB76C)
    (at 135.2046 70.978)
    (descr "SOT-23, Handsoldering")
    (tags "SOT-23")
    (property "Sheetfile" "Switch_Driver.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U10" (at -1.905 2.413) (layer "F.SilkS"))
    (fp_text value "NMOS_0_2A" (at 0 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.5 -0.95) (size 1.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "Net-(J1-Pad5)") (pinfunction "Gate") (pintype "input"))
    (pad "2" smd rect (at -1.5 0.95) (size 1.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "Drain") (pintype "output"))
    (pad "3" smd rect (at 1.5 0) (size 1.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "Net-(R3-Pad2)") (pinfunction "Source") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric_Pad0.72x0.64mm_HandSolder" (layer "F.Cu")
    (tedit 5F6BB9E0)
    (at 137.3636 73.9885 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Switch_Driver.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R3" (at -1.9575 -0.2036 180) (layer "F.SilkS"))
    (fp_text value "100k" (at 0 1.17 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.5975 0 90) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+12V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.5975 0 90) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(R3-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-353_SC-70-5_Handsoldering" (layer "F.Cu")
    (tedit 5C9ED275)
    (at 130.8866 100.188 90)
    (descr "SOT-353, SC-70-5, Handsoldering")
    (tags "SOT-353 SC-70-5 Handsoldering")
    (property "Sheetfile" "Switch_Driver.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U3" (at 3.287 0.0504 180) (layer "F.SilkS"))
    (fp_text value "74LVC1G04" (at 0 2 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -1.33 -0.65 90) (size 1.5 0.4) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "2" smd rect (at -1.33 0 90) (size 1.5 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 19 "Net-(J1-Pad3)") (pinfunction "A") (pintype "input"))
    (pad "3" smd rect (at -1.33 0.65 90) (size 1.5 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "Gnd") (pintype "output"))
    (pad "4" smd rect (at 1.33 0.65 90) (size 1.5 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 20 "Net-(U20-Pad1)") (pinfunction "Y") (pintype "output"))
    (pad "5" smd rect (at 1.33 -0.65 90) (size 1.5 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "+3V3") (pinfunction "Vcc") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-353_SC-70-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric_Pad0.72x0.64mm_HandSolder" (layer "F.Cu")
    (tedit 5F6BB9E0)
    (at 136.7286 110.1835 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Switch_Driver.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R5" (at -1.9575 -0.0766 180) (layer "F.SilkS"))
    (fp_text value "100k" (at 0 1.17 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.5975 0 90) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+12V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.5975 0 90) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "Net-(R5-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 133.8315 86.233 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Switch_Driver.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C7" (at 2.6405 -0.127) (layer "F.SilkS"))
    (fp_text value "C" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0 180) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+12V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 180) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2_DIN965_Pad" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 156.6672 96.1136)
    (descr "Mounting Hole 2.2mm, M2, DIN965")
    (tags "mounting hole 2.2mm m2 din965")
    (property "Sheetfile" "Switch_Driver.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H3" (at 0 -2.9) (layer "F.SilkS"))
    (fp_text value "MountingHole_Pad" (at 0 2.9) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 3.8 3.8) (drill 2.2) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input"))
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder" (layer "F.Cu")
    (tedit 5F6BB22C)
    (at 128.143 61.976 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Switch_Driver.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C2" (at 2.286 0 180) (layer "F.SilkS"))
    (fp_text value "C" (at 0 1.16) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.5675 0 180) (size 0.735 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.5675 0 180) (size 0.735 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x07_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 124.46 103.505 180)
    (descr "Through hole straight pin header, 1x07, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x07 2.54mm single row")
    (property "Sheetfile" "Switch_Driver.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at 0 -2.33) (layer "F.SilkS"))
    (fp_text value "Conn_01x07" (at 0 17.57) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 7.62 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(J1-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(J1-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(J1-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J1-Pad5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "+3V3") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "+12V") (pinfunction "Pin_7") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x07_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-353_SC-70-5_Handsoldering" (layer "F.Cu")
    (tedit 5C9ED275)
    (at 130.8866 82.662 90)
    (descr "SOT-353, SC-70-5, Handsoldering")
    (tags "SOT-353 SC-70-5 Handsoldering")
    (property "Sheetfile" "Switch_Driver.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U2" (at 3.287 -0.0766 180) (layer "F.SilkS"))
    (fp_text value "74LVC1G04" (at 0 2 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -1.33 -0.65 90) (size 1.5 0.4) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "2" smd rect (at -1.33 0 90) (size 1.5 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "Net-(J1-Pad4)") (pinfunction "A") (pintype "input"))
    (pad "3" smd rect (at -1.33 0.65 90) (size 1.5 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "Gnd") (pintype "output"))
    (pad "4" smd rect (at 1.33 0.65 90) (size 1.5 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "Net-(U16-Pad1)") (pinfunction "Y") (pintype "output"))
    (pad "5" smd rect (at 1.33 -0.65 90) (size 1.5 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "+3V3") (pinfunction "Vcc") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-353_SC-70-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23_Handsoldering" (layer "F.Cu")
    (tedit 5A0AB76C)
    (at 135.0172 125.587)
    (descr "SOT-23, Handsoldering")
    (tags "SOT-23")
    (property "Sheetfile" "Switch_Driver.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U6" (at -1.8446 2.541) (layer "F.SilkS"))
    (fp_text value "NMOS_0_2A" (at 0 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.5 -0.95) (size 1.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "Net-(J1-Pad2)") (pinfunction "Gate") (pintype "input"))
    (pad "2" smd rect (at -1.5 0.95) (size 1.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "Drain") (pintype "output"))
    (pad "3" smd rect (at 1.5 0) (size 1.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "Net-(R1-Pad2)") (pinfunction "Source") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:TO-252-2" (layer "F.Cu")
    (tedit 5A70A390)
    (at 143.6216 72.756)
    (descr "TO-252 / DPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO252/PG-TO252-3-1/")
    (tags "DPAK TO-252 DPAK-3 TO-252-3 SOT-428")
    (property "Sheetfile" "Switch_Driver.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U9" (at -0.3148 4.2568) (layer "F.SilkS"))
    (fp_text value "PMOS_4A" (at 0 4.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" smd rect (at 3.775 -1.525) (size 3.05 2.75) (layers "F.Paste"))
    (pad "" smd rect (at 0.425 1.525) (size 3.05 2.75) (layers "F.Paste"))
    (pad "" smd rect (at 0.425 -1.525) (size 3.05 2.75) (layers "F.Paste"))
    (pad "" smd rect (at 3.775 1.525) (size 3.05 2.75) (layers "F.Paste"))
    (pad "1" smd rect (at -4.2 -2.28) (size 2.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "Net-(R3-Pad2)") (pinfunction "Gate") (pintype "input"))
    (pad "2" smd rect (at 2.1 0) (size 6.4 5.8) (layers "F.Cu" "F.Mask")
      (net 24 "Net-(J3-Pad3)") (pinfunction "Drain") (pintype "output"))
    (pad "3" smd rect (at -4.2 2.28) (size 2.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "+12V") (pinfunction "Source") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/TO-252-2.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:TO-252-2" (layer "F.Cu")
    (tedit 5A70A390)
    (at 143.6216 90.874666)
    (descr "TO-252 / DPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO252/PG-TO252-3-1/")
    (tags "DPAK TO-252 DPAK-3 TO-252-3 SOT-428")
    (property "Sheetfile" "Switch_Driver.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U13" (at 0.0916 4.273734) (layer "F.SilkS"))
    (fp_text value "PMOS_4A" (at 0 4.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" smd rect (at 3.775 1.525) (size 3.05 2.75) (layers "F.Paste"))
    (pad "" smd rect (at 0.425 1.525) (size 3.05 2.75) (layers "F.Paste"))
    (pad "" smd rect (at 3.775 -1.525) (size 3.05 2.75) (layers "F.Paste"))
    (pad "" smd rect (at 0.425 -1.525) (size 3.05 2.75) (layers "F.Paste"))
    (pad "1" smd rect (at -4.2 -2.28) (size 2.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "Net-(R4-Pad2)") (pinfunction "Gate") (pintype "input"))
    (pad "2" smd rect (at 2.1 0) (size 6.4 5.8) (layers "F.Cu" "F.Mask")
      (net 25 "Net-(J4-Pad3)") (pinfunction "Drain") (pintype "output"))
    (pad "3" smd rect (at -4.2 2.28) (size 2.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "+12V") (pinfunction "Source") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/TO-252-2.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder" (layer "F.Cu")
    (tedit 5F6BB22C)
    (at 128.778 82.7365 -90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Switch_Driver.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C3" (at 0 1.524 180) (layer "F.SilkS"))
    (fp_text value "C" (at 0 1.16 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.5675 0 270) (size 0.735 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.5675 0 270) (size 0.735 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-353_SC-70-5_Handsoldering" (layer "F.Cu")
    (tedit 5C9ED275)
    (at 130.9016 64.561 90)
    (descr "SOT-353, SC-70-5, Handsoldering")
    (tags "SOT-353 SC-70-5 Handsoldering")
    (property "Sheetfile" "Switch_Driver.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U1" (at 3.22 1.1784 180) (layer "F.SilkS"))
    (fp_text value "74LVC1G04" (at 0 2 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -1.33 -0.65 90) (size 1.5 0.4) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "2" smd rect (at -1.33 0 90) (size 1.5 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "Net-(J1-Pad5)") (pinfunction "A") (pintype "input"))
    (pad "3" smd rect (at -1.33 0.65 90) (size 1.5 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "Gnd") (pintype "output"))
    (pad "4" smd rect (at 1.33 0.65 90) (size 1.5 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "Net-(U1-Pad4)") (pinfunction "Y") (pintype "output"))
    (pad "5" smd rect (at 1.33 -0.65 90) (size 1.5 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "+3V3") (pinfunction "Vcc") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-353_SC-70-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x03_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5A19A429)
    (at 158.8266 120.015)
    (descr "Through hole straight socket strip, 1x03, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x03 2.54mm single row")
    (property "Sheetfile" "Switch_Driver.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at 0 -2.77) (layer "F.SilkS"))
    (fp_text value "Conn_01x03" (at 0 7.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J2-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(J2-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x03_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5A19A429)
    (at 158.8266 65.898)
    (descr "Through hole straight socket strip, 1x03, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x03 2.54mm single row")
    (property "Sheetfile" "Switch_Driver.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J3" (at 0 -2.77) (layer "F.SilkS"))
    (fp_text value "Conn_01x03" (at 0 7.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(J3-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(J3-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric_Pad0.72x0.64mm_HandSolder" (layer "F.Cu")
    (tedit 5F6BB9E0)
    (at 136.7661 101.966)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Switch_Driver.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R8" (at -2.5775 0.254) (layer "F.SilkS"))
    (fp_text value "100k" (at 0 1.17) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.5975 0) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+12V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.5975 0) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "Net-(R8-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric_Pad0.72x0.64mm_HandSolder" (layer "F.Cu")
    (tedit 5F6BB9E0)
    (at 136.7661 84.694)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Switch_Driver.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R7" (at -2.4505 0) (layer "F.SilkS"))
    (fp_text value "100k" (at 0 1.17) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.5975 0) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+12V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.5975 0) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "Net-(R7-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric_Pad0.72x0.64mm_HandSolder" (layer "F.Cu")
    (tedit 5F6BB9E0)
    (at 136.7286 66.533)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Switch_Driver.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R6" (at -2.3626 0.015) (layer "F.SilkS"))
    (fp_text value "100k" (at 0 1.17) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.5975 0) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+12V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.5975 0) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "Net-(R6-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 134.2125 104.14 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Switch_Driver.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C8" (at 2.7675 -0.127) (layer "F.SilkS"))
    (fp_text value "C" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0 180) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+12V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 180) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23_Handsoldering" (layer "F.Cu")
    (tedit 5A0AB76C)
    (at 135.1806 89.073)
    (descr "SOT-23, Handsoldering")
    (tags "SOT-23")
    (property "Sheetfile" "Switch_Driver.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U14" (at -1.627 2.606) (layer "F.SilkS"))
    (fp_text value "NMOS_0_2A" (at 0 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.5 -0.95) (size 1.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "Net-(J1-Pad4)") (pinfunction "Gate") (pintype "input"))
    (pad "2" smd rect (at -1.5 0.95) (size 1.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "Drain") (pintype "output"))
    (pad "3" smd rect (at 1.5 0) (size 1.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "Net-(R4-Pad2)") (pinfunction "Source") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:TO-252-2" (layer "F.Cu")
    (tedit 5A70A390)
    (at 143.6216 127.112)
    (descr "TO-252 / DPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO252/PG-TO252-3-1/")
    (tags "DPAK TO-252 DPAK-3 TO-252-3 SOT-428")
    (property "Sheetfile" "Switch_Driver.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U5" (at 1.1584 4.333) (layer "F.SilkS"))
    (fp_text value "PMOS_4A" (at 0 4.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" smd rect (at 3.775 -1.525) (size 3.05 2.75) (layers "F.Paste"))
    (pad "" smd rect (at 3.775 1.525) (size 3.05 2.75) (layers "F.Paste"))
    (pad "" smd rect (at 0.425 1.525) (size 3.05 2.75) (layers "F.Paste"))
    (pad "" smd rect (at 0.425 -1.525) (size 3.05 2.75) (layers "F.Paste"))
    (pad "1" smd rect (at -4.2 -2.28) (size 2.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "Net-(R1-Pad2)") (pinfunction "Gate") (pintype "input"))
    (pad "2" smd rect (at 2.1 0) (size 6.4 5.8) (layers "F.Cu" "F.Mask")
      (net 23 "Net-(J2-Pad3)") (pinfunction "Drain") (pintype "output"))
    (pad "3" smd rect (at -4.2 2.28) (size 2.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "+12V") (pinfunction "Source") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/TO-252-2.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric_Pad0.72x0.64mm_HandSolder" (layer "F.Cu")
    (tedit 5F6BB9E0)
    (at 137.2366 92.1495 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Switch_Driver.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R4" (at -1.8305 -0.2036 180) (layer "F.SilkS"))
    (fp_text value "100k" (at 0 1.17 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.5975 0 90) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+12V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.5975 0 90) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "Net-(R4-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:TO-252-2" (layer "F.Cu")
    (tedit 5A70A390)
    (at 143.6216 65.645)
    (descr "TO-252 / DPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO252/PG-TO252-3-1/")
    (tags "DPAK TO-252 DPAK-3 TO-252-3 SOT-428")
    (property "Sheetfile" "Switch_Driver.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U11" (at 1.1584 -4.5) (layer "F.SilkS"))
    (fp_text value "PMOS_4A" (at 0 4.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" smd rect (at 0.425 -1.525) (size 3.05 2.75) (layers "F.Paste"))
    (pad "" smd rect (at 3.775 -1.525) (size 3.05 2.75) (layers "F.Paste"))
    (pad "" smd rect (at 0.425 1.525) (size 3.05 2.75) (layers "F.Paste"))
    (pad "" smd rect (at 3.775 1.525) (size 3.05 2.75) (layers "F.Paste"))
    (pad "1" smd rect (at -4.2 -2.28) (size 2.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "Net-(R6-Pad2)") (pinfunction "Gate") (pintype "input"))
    (pad "2" smd rect (at 2.1 0) (size 6.4 5.8) (layers "F.Cu" "F.Mask")
      (net 27 "Net-(J3-Pad2)") (pinfunction "Drain") (pintype "output"))
    (pad "3" smd rect (at -4.2 2.28) (size 2.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "+12V") (pinfunction "Source") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/TO-252-2.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:TO-252-2" (layer "F.Cu")
    (tedit 5A70A390)
    (at 143.6216 101.8478)
    (descr "TO-252 / DPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO252/PG-TO252-3-1/")
    (tags "DPAK TO-252 DPAK-3 TO-252-3 SOT-428")
    (property "Sheetfile" "Switch_Driver.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U19" (at 0 -4.5) (layer "F.SilkS"))
    (fp_text value "PMOS_4A" (at 0 4.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" smd rect (at 3.775 -1.525) (size 3.05 2.75) (layers "F.Paste"))
    (pad "" smd rect (at 0.425 -1.525) (size 3.05 2.75) (layers "F.Paste"))
    (pad "" smd rect (at 3.775 1.525) (size 3.05 2.75) (layers "F.Paste"))
    (pad "" smd rect (at 0.425 1.525) (size 3.05 2.75) (layers "F.Paste"))
    (pad "1" smd rect (at -4.2 -2.28) (size 2.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "Net-(R8-Pad2)") (pinfunction "Gate") (pintype "input"))
    (pad "2" smd rect (at 2.1 0) (size 6.4 5.8) (layers "F.Cu" "F.Mask")
      (net 5 "Net-(J5-Pad2)") (pinfunction "Drain") (pintype "output"))
    (pad "3" smd rect (at -4.2 2.28) (size 2.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "+12V") (pinfunction "Source") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/TO-252-2.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23_Handsoldering" (layer "F.Cu")
    (tedit 5A0AB76C)
    (at 135.2698 118.1702)
    (descr "SOT-23, Handsoldering")
    (tags "SOT-23")
    (property "Sheetfile" "Switch_Driver.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U8" (at -1.0812 -2.5) (layer "F.SilkS"))
    (fp_text value "NMOS_0_2A" (at 0 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.5 -0.95) (size 1.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "Net-(U4-Pad4)") (pinfunction "Gate") (pintype "input"))
    (pad "2" smd rect (at -1.5 0.95) (size 1.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "Drain") (pintype "output"))
    (pad "3" smd rect (at 1.5 0) (size 1.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "Net-(R2-Pad2)") (pinfunction "Source") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric_Pad0.72x0.64mm_HandSolder" (layer "F.Cu")
    (tedit 5F6BB9E0)
    (at 136.7831 120.6594)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Switch_Driver.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R2" (at -2.2135 0.1026) (layer "F.SilkS"))
    (fp_text value "100k" (at 0 1.17) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.5975 0) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+12V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.5975 0) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "Net-(R2-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 134.2655 122.301 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Switch_Driver.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C5" (at 2.5665 0) (layer "F.SilkS"))
    (fp_text value "C" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0 180) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+12V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 180) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:TO-252-2" (layer "F.Cu")
    (tedit 5A70A390)
    (at 143.6216 119.9492)
    (descr "TO-252 / DPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO252/PG-TO252-3-1/")
    (tags "DPAK TO-252 DPAK-3 TO-252-3 SOT-428")
    (property "Sheetfile" "Switch_Driver.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U7" (at 0 -4.5) (layer "F.SilkS"))
    (fp_text value "PMOS_4A" (at 0 4.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" smd rect (at 0.425 -1.525) (size 3.05 2.75) (layers "F.Paste"))
    (pad "" smd rect (at 3.775 1.525) (size 3.05 2.75) (layers "F.Paste"))
    (pad "" smd rect (at 3.775 -1.525) (size 3.05 2.75) (layers "F.Paste"))
    (pad "" smd rect (at 0.425 1.525) (size 3.05 2.75) (layers "F.Paste"))
    (pad "1" smd rect (at -4.2 -2.28) (size 2.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "Net-(R2-Pad2)") (pinfunction "Gate") (pintype "input"))
    (pad "2" smd rect (at 2.1 0) (size 6.4 5.8) (layers "F.Cu" "F.Mask")
      (net 3 "Net-(J2-Pad2)") (pinfunction "Drain") (pintype "output"))
    (pad "3" smd rect (at -4.2 2.28) (size 2.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "+12V") (pinfunction "Source") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/TO-252-2.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23_Handsoldering" (layer "F.Cu")
    (tedit 5A0AB76C)
    (at 135.2046 63.866)
    (descr "SOT-23, Handsoldering")
    (tags "SOT-23")
    (property "Sheetfile" "Switch_Driver.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U12" (at 1.3204 -2.5) (layer "F.SilkS"))
    (fp_text value "NMOS_0_2A" (at 0 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.5 -0.95) (size 1.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "Net-(U1-Pad4)") (pinfunction "Gate") (pintype "input"))
    (pad "2" smd rect (at -1.5 0.95) (size 1.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "Drain") (pintype "output"))
    (pad "3" smd rect (at 1.5 0) (size 1.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "Net-(R6-Pad2)") (pinfunction "Source") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x03_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5A19A429)
    (at 158.8266 83.937)
    (descr "Through hole straight socket strip, 1x03, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x03 2.54mm single row")
    (property "Sheetfile" "Switch_Driver.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J4" (at 0 -2.77) (layer "F.SilkS"))
    (fp_text value "Conn_01x03" (at 0 7.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J4-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(J4-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder" (layer "F.Cu")
    (tedit 5F6BB22C)
    (at 128.905 118.872 -90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Switch_Driver.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C1" (at -1.905 0.508 180) (layer "F.SilkS"))
    (fp_text value "C" (at 0 1.16 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.5675 0 270) (size 0.735 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.5675 0 270) (size 0.735 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric_Pad0.72x0.64mm_HandSolder" (layer "F.Cu")
    (tedit 5F6BB9E0)
    (at 137.2524 128.9011 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Switch_Driver.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R1" (at -1.7819 0.0346 180) (layer "F.SilkS"))
    (fp_text value "100k" (at 0 1.17 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.5975 0 90) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+12V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.5975 0 90) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(R1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder" (layer "F.Cu")
    (tedit 5F6BB22C)
    (at 128.778 100.0085 -90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Switch_Driver.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C4" (at 3.1155 0 180) (layer "F.SilkS"))
    (fp_text value "C" (at 0 1.16 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.5675 0 270) (size 0.735 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.5675 0 270) (size 0.735 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:TO-252-2" (layer "F.Cu")
    (tedit 5A70A390)
    (at 143.6216 108.993332)
    (descr "TO-252 / DPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO252/PG-TO252-3-1/")
    (tags "DPAK TO-252 DPAK-3 TO-252-3 SOT-428")
    (property "Sheetfile" "Switch_Driver.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U17" (at 0.219 4.402668) (layer "F.SilkS"))
    (fp_text value "PMOS_4A" (at 0 4.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" smd rect (at 3.775 -1.525) (size 3.05 2.75) (layers "F.Paste"))
    (pad "" smd rect (at 0.425 1.525) (size 3.05 2.75) (layers "F.Paste"))
    (pad "" smd rect (at 3.775 1.525) (size 3.05 2.75) (layers "F.Paste"))
    (pad "" smd rect (at 0.425 -1.525) (size 3.05 2.75) (layers "F.Paste"))
    (pad "1" smd rect (at -4.2 -2.28) (size 2.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "Net-(R5-Pad2)") (pinfunction "Gate") (pintype "input"))
    (pad "2" smd rect (at 2.1 0) (size 6.4 5.8) (layers "F.Cu" "F.Mask")
      (net 26 "Net-(J5-Pad3)") (pinfunction "Drain") (pintype "output"))
    (pad "3" smd rect (at -4.2 2.28) (size 2.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "+12V") (pinfunction "Source") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/TO-252-2.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-353_SC-70-5_Handsoldering" (layer "F.Cu")
    (tedit 5C9ED275)
    (at 130.8866 118.857 90)
    (descr "SOT-353, SC-70-5, Handsoldering")
    (tags "SOT-353 SC-70-5 Handsoldering")
    (property "Sheetfile" "Switch_Driver.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U4" (at 3.16 -0.0766 180) (layer "F.SilkS"))
    (fp_text value "74LVC1G04" (at 0 2 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -1.33 -0.65 90) (size 1.5 0.4) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "2" smd rect (at -1.33 0 90) (size 1.5 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "Net-(J1-Pad2)") (pinfunction "A") (pintype "input"))
    (pad "3" smd rect (at -1.33 0.65 90) (size 1.5 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "Gnd") (pintype "output"))
    (pad "4" smd rect (at 1.33 0.65 90) (size 1.5 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "Net-(U4-Pad4)") (pinfunction "Y") (pintype "output"))
    (pad "5" smd rect (at 1.33 -0.65 90) (size 1.5 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "+3V3") (pinfunction "Vcc") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-353_SC-70-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_rect (start 122.301 59.944) (end 160.909 132.334) (layer "Edge.Cuts") (width 0.1) (fill none))
  (gr_text "12V" (at 128.016 88.138) (layer "F.SilkS"))
  (gr_text "SW 1" (at 155.8544 122.4788 90) (layer "F.SilkS"))
  (gr_text "4" (at 126.746 93.3196) (layer "F.SilkS"))
  (gr_text "SW 4" (at 155.8544 68.326 90) (layer "F.SilkS"))
  (gr_text "SW 2" (at 155.8544 104.2416 90) (layer "F.SilkS"))
  (gr_text "SW 3" (at 155.8544 86.3092 90) (layer "F.SilkS"))
  (gr_text "3" (at 126.746 96.012) (layer "F.SilkS"))
  (gr_text "2" (at 126.746 98.552) (layer "F.SilkS"))
  (gr_text "1" (at 126.746 100.9396) (layer "F.SilkS"))
  (gr_text "3.3V" (at 128.373143 90.932) (layer "F.SilkS"))
  (zone (net 2) (net_name "GND") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 161.036 59.817)
        (xy 161.036 132.461)
        (xy 122.047 132.715)
        (xy 122.047 59.69)
      )
    )
  )
)
