(kicad_pcb (version 20171130) (host pcbnew "(5.0.0)")
  (general
    (thickness 1.6)
    (drawings 28)
    (tracks 167)
    (zones 0)
    (modules 41)
    (nets 17)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.1778)
    (user_trace_width 0.254)
    (user_trace_width 0.3048)
    (user_trace_width 0.381)
    (user_trace_width 0.508)
    (user_trace_width 0.635)
    (user_trace_width 0.762)
    (user_trace_width 1.016)
    (user_trace_width 1.27)
    (user_trace_width 1.524)
    (user_trace_width 2.54)
    (user_trace_width 6.35)
    (trace_clearance 0.2)
    (zone_clearance 0.254)
    (zone_45_only yes)
    (trace_min 0.1778)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (user_via 0.6858 0.3302)
    (user_via 0.8636 0.508)
    (user_via 1.1176 0.762)
    (user_via 1.3716 1.016)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 0.635 0.635)
    (mod_text_width 0.15875)
    (pad_size 1.7272 1.7272)
    (pad_drill 1.016)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 83.185 146.05)
    (grid_origin 83.185 146.05)
    (visible_elements 7FFDDF7F)
    (pcbplotparams
      (layerselection 0x010fc_80000001)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "Gerber/"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(C1-Pad1)")
  (net 3 "Net-(C3-Pad2)")
  (net 4 "Net-(C3-Pad1)")
  (net 5 "Net-(C4-Pad1)")
  (net 6 "Net-(C4-Pad2)")
  (net 7 "Net-(C5-Pad1)")
  (net 8 "Net-(C6-Pad1)")
  (net 9 "Net-(D1-Pad2)")
  (net 10 "Net-(D2-Pad2)")
  (net 11 "Net-(R1-Pad2)")
  (net 12 "Net-(R3-Pad2)")
  (net 13 "Net-(R5-Pad1)")
  (net 14 "Net-(R5-Pad2)")
  (net 15 "Net-(R6-Pad2)")
  (net 16 "Net-(R10-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C4-Pad2)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R10-Pad1)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(R5-Pad1)")
    (add_net "Net-(R5-Pad2)")
    (add_net "Net-(R6-Pad2)")
  )
  (module PJS-pth-parts:Stewart_USB_SS-52100-001 (layer F.Cu) (tedit 5B7A1462)
    (at 137.16 146.05 270)
    (fp_text reference J13 (at -14.605 -5.08) (layer F.SilkS))
    (fp_text value SS-52100-001 (at -7 9.5 270) (layer F.Fab))
    (pad 1 thru_hole rect (at -13 3.5 270) (size 1.3 1.3) (drill 0.92) (layers *.Cu *.Mask)
      (net 8 "Net-(C6-Pad1)"))
    (pad 2 thru_hole circle (at -13 1 270) (size 1.3 1.3) (drill 0.92) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at -13 -1 270) (size 1.3 1.3) (drill 0.92) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at -13 -3.5 270) (size 1.3 1.3) (drill 0.92) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole circle (at -10.28 6.57 270) (size 3 3) (drill 2.3) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole circle (at -10.28 -6.57 270) (size 3 3) (drill 2.3) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module PJS-pth-parts:Stewart_USB_SS-52100-001 (layer F.Cu) (tedit 5B7A1462)
    (at 128.27 100.33 90)
    (fp_text reference J8 (at -14.605 5.715 180) (layer F.SilkS))
    (fp_text value SS-52100-001 (at -7 9.5 90) (layer F.Fab))
    (pad 5 thru_hole circle (at -10.28 -6.57 90) (size 3 3) (drill 2.3) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole circle (at -10.28 6.57 90) (size 3 3) (drill 2.3) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole circle (at -13 -3.5 90) (size 1.3 1.3) (drill 0.92) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole circle (at -13 -1 90) (size 1.3 1.3) (drill 0.92) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at -13 1 90) (size 1.3 1.3) (drill 0.92) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at -13 3.5 90) (size 1.3 1.3) (drill 0.92) (layers *.Cu *.Mask)
      (net 7 "Net-(C5-Pad1)"))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 106.68 116.84 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at -1.905 0) (layer F.SilkS))
    (fp_text value 59k (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R5-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R5-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 111.76 120.65 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 0 -1.5 180) (layer F.SilkS))
    (fp_text value 22uF (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 180) (layer F.Fab))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 123.19 125.73)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 0 -1.5) (layer F.SilkS))
    (fp_text value 22uF (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.5) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 109.855 113.03 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at 1.905 0 270) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C3-Pad2)"))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 125.095 133.35)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at 1.905 0 90) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C4-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 121.92 116.205)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C5 (at 0 1.905) (layer F.SilkS))
    (fp_text value 22uF (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.5) (layer F.Fab))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C5-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 113.03 130.175 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C6 (at 0 1.905 180) (layer F.SilkS))
    (fp_text value 22uF (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C6-Pad1)"))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57FE93A5)
    (at 127 116.205)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D1 (at 0 1.27) (layer F.SilkS))
    (fp_text value LED_red (at 0 1.35) (layer F.Fab))
    (pad 2 smd rect (at 0.8 0 180) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -0.8 0 180) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57FE93A5)
    (at 108.585 130.175 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D2 (at 0 1.27 180) (layer F.SilkS))
    (fp_text value LED_red (at 0 1.35 180) (layer F.Fab))
    (pad 1 smd rect (at -0.8 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.8 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module PJS-icons:metroid (layer F.Cu) (tedit 5A0106A6)
    (at 93.345 143.51)
    (fp_text reference icon1 (at 0 2.54) (layer F.Fab) hide)
    (fp_text value Metroid (at 0 -2.54) (layer F.SilkS) hide)
    (pad "" smd circle (at -0.635 0) (size 0.635 0.635) (layers F.Cu F.Paste F.Mask))
    (pad "" smd circle (at 0.635 0) (size 0.635 0.635) (layers F.Cu F.Paste F.Mask))
    (pad "" smd circle (at 0 -0.635) (size 0.635 0.635) (layers F.Cu F.Paste F.Mask))
  )
  (module PJS-pth-parts:CUI_PJ-102BH (layer F.Cu) (tedit 5B7A1129)
    (at 83.185 123.19 180)
    (fp_text reference J1 (at -6 -5.5 180) (layer F.SilkS))
    (fp_text value PJ-102BH (at -9 5.5 180) (layer F.Fab))
    (pad 1 thru_hole rect (at -13.7 0 180) (size 3.81 3.81) (drill 2.032) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at -7.7 0 180) (size 3.81 3.81) (drill 2.032) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole circle (at -10.7 -4.7 180) (size 3.81 3.81) (drill 2.032) (layers *.Cu *.Mask))
  )
  (module PJS-pth-parts:CUI_PJ-102BH (layer F.Cu) (tedit 5B7A1129)
    (at 152.4 123.19)
    (fp_text reference J2 (at -6 -5.5) (layer F.SilkS))
    (fp_text value PJ-102BH (at -9 5.5) (layer F.Fab))
    (pad 1 thru_hole rect (at -13.7 0) (size 3.81 3.81) (drill 2.032) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at -7.7 0) (size 3.81 3.81) (drill 2.032) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole circle (at -10.7 -4.7) (size 3.81 3.81) (drill 2.032) (layers *.Cu *.Mask))
  )
  (module Degson:DG301-5.002P-12 (layer F.Cu) (tedit 5B7B6EA0)
    (at 86.36 136.485 270)
    (tags terminal)
    (fp_text reference J3 (at -4.405 -5.715 270) (layer F.SilkS))
    (fp_text value Screw (at 12.74 6.35 270) (layer F.SilkS) hide)
    (pad 2 thru_hole circle (at 2.5 0 270) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole rect (at -2.5 0 270) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(C1-Pad1)"))
  )
  (module Degson:DG301-5.002P-12 (layer F.Cu) (tedit 5B7B6ECD)
    (at 134.62 103.505 180)
    (tags terminal)
    (fp_text reference J4 (at -4.445 -5.08 180) (layer F.SilkS))
    (fp_text value Screw (at 7.62 10.795 180) (layer F.SilkS) hide)
    (pad 2 thru_hole circle (at 2.5 0 180) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole rect (at -2.5 0 180) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(C5-Pad1)"))
  )
  (module Degson:DG301-5.002P-12 (layer F.Cu) (tedit 5B7B6ED3)
    (at 104.935 103.505 180)
    (tags terminal)
    (fp_text reference J5 (at -1.745 -5.08 180) (layer F.SilkS))
    (fp_text value Screw (at -11.905 8.255 180) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -2.5 0 180) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(C5-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
  )
  (module Degson:DG301-5.002P-12 (layer F.Cu) (tedit 5B7B6ED0)
    (at 114.935 103.505 180)
    (tags terminal)
    (fp_text reference J6 (at -3.81 -5.08 180) (layer F.SilkS))
    (fp_text value Screw (at -6.35 10.16 180) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -2.5 0 180) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(C5-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
  )
  (module PJS-pth-parts:Stewart_USB_SS-52100-001 (layer F.Cu) (tedit 5B7A1462)
    (at 98.425 100.33 90)
    (fp_text reference J7 (at -14.605 -5.715 180) (layer F.SilkS))
    (fp_text value SS-52100-001 (at -7 9.5 90) (layer F.Fab))
    (pad 1 thru_hole rect (at -13 3.5 90) (size 1.3 1.3) (drill 0.92) (layers *.Cu *.Mask)
      (net 7 "Net-(C5-Pad1)"))
    (pad 2 thru_hole circle (at -13 1 90) (size 1.3 1.3) (drill 0.92) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at -13 -1 90) (size 1.3 1.3) (drill 0.92) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at -13 -3.5 90) (size 1.3 1.3) (drill 0.92) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole circle (at -10.28 6.57 90) (size 3 3) (drill 2.3) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole circle (at -10.28 -6.57 90) (size 3 3) (drill 2.3) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Degson:DG301-5.002P-12 (layer F.Cu) (tedit 5B7B6EA3)
    (at 100.965 142.875)
    (tags terminal)
    (fp_text reference J9 (at -4.445 -5.08) (layer F.SilkS))
    (fp_text value Screw (at -14.605 8.89) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -2.5 0) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(C6-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
  )
  (module Degson:DG301-5.002P-12 (layer F.Cu) (tedit 5B7B6EAA)
    (at 120.69 142.875)
    (tags terminal)
    (fp_text reference J10 (at -3.85 -5.08) (layer F.SilkS))
    (fp_text value Screw (at -7.025 7.62) (layer F.SilkS) hide)
    (pad 2 thru_hole circle (at 2.5 0) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole rect (at -2.5 0) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(C6-Pad1)"))
  )
  (module Degson:DG301-5.002P-12 (layer F.Cu) (tedit 5B7B6EB5)
    (at 130.69 142.875)
    (tags terminal)
    (fp_text reference J11 (at -1.785 -5.08) (layer F.SilkS))
    (fp_text value Screw (at -3.055 6.985) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -2.5 0) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(C6-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
  )
  (module PJS-pth-parts:Stewart_USB_SS-52100-001 (layer F.Cu) (tedit 5B7A1462)
    (at 107.315 146.05 270)
    (fp_text reference J12 (at -14.605 5.715) (layer F.SilkS))
    (fp_text value SS-52100-001 (at -7 9.5 270) (layer F.Fab))
    (pad 5 thru_hole circle (at -10.28 -6.57 270) (size 3 3) (drill 2.3) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole circle (at -10.28 6.57 270) (size 3 3) (drill 2.3) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole circle (at -13 -3.5 270) (size 1.3 1.3) (drill 0.92) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole circle (at -13 -1 270) (size 1.3 1.3) (drill 0.92) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at -13 1 270) (size 1.3 1.3) (drill 0.92) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at -13 3.5 270) (size 1.3 1.3) (drill 0.92) (layers *.Cu *.Mask)
      (net 8 "Net-(C6-Pad1)"))
  )
  (module Yuden:Yuden_Inductor_4.9x4.9 (layer F.Cu) (tedit 5B7A1681)
    (at 116.84 114.935 180)
    (zone_connect 2)
    (fp_text reference L1 (at 0 -3.175 180) (layer F.SilkS))
    (fp_text value 6.5uH (at 0 4 180) (layer F.Fab))
    (pad 1 smd rect (at -1.8 0 180) (size 1.5 4) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C5-Pad1)") (zone_connect 2))
    (pad 2 smd rect (at 1.8 0 180) (size 1.5 4) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad1)") (zone_connect 2))
  )
  (module Yuden:Yuden_Inductor_4.9x4.9 (layer F.Cu) (tedit 5B7A1681)
    (at 118.11 131.445)
    (zone_connect 2)
    (fp_text reference L2 (at 0 -3.175) (layer F.SilkS))
    (fp_text value 6.5uH (at 0 4) (layer F.Fab))
    (pad 2 smd rect (at 1.8 0) (size 1.5 4) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C4-Pad1)") (zone_connect 2))
    (pad 1 smd rect (at -1.8 0) (size 1.5 4) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C6-Pad1)") (zone_connect 2))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 103.505 120.015 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 0 -1.45 90) (layer F.SilkS))
    (fp_text value 499k (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(R1-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 103.505 116.205 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 0 -1.45 90) (layer F.SilkS))
    (fp_text value 100k (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(R1-Pad2)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 131.445 126.365 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 0 -1.45 270) (layer F.SilkS))
    (fp_text value 499k (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(R3-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 131.445 130.175 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 0 -1.45 270) (layer F.SilkS))
    (fp_text value 100k (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(R3-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 128.27 129.54 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at -1.905 0 180) (layer F.SilkS))
    (fp_text value 59k (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(R6-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(R10-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 109.855 111.125 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at 1.905 0 270) (layer F.SilkS))
    (fp_text value 40.2k (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R5-Pad1)"))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C5-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 109.855 109.22)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R8 (at -1.905 0 90) (layer F.SilkS))
    (fp_text value 7.68k (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R5-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 125.095 135.255)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R9 (at 1.905 0 90) (layer F.SilkS))
    (fp_text value 40.2k (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C6-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(R10-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 125.095 137.16 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R10 (at -1.905 0 270) (layer F.SilkS))
    (fp_text value 7.68k (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(R10-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 130.175 116.205 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R11 (at 0 -1.27 180) (layer F.SilkS))
    (fp_text value 499 (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C5-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 105.41 130.175)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R12 (at 0 -1.45) (layer F.SilkS))
    (fp_text value 499 (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C6-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-6 (layer F.Cu) (tedit 58CE4E7E)
    (at 109.855 116.84 180)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference U1 (at -2.54 -1.905 180) (layer F.SilkS))
    (fp_text value AP65111 (at 0 2.9 180) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at -1.1 0 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.1 0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 4 smd rect (at 1.1 0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C3-Pad2)"))
    (pad 6 smd rect (at 1.1 -0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R5-Pad2)"))
    (pad 5 smd rect (at 1.1 0 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(R1-Pad2)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-6 (layer F.Cu) (tedit 58CE4E7E)
    (at 125.095 129.54)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference U2 (at -2.54 -1.905) (layer F.SilkS))
    (fp_text value AP65111 (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 5 smd rect (at 1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(R3-Pad2)"))
    (pad 6 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(R6-Pad2)"))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C4-Pad2)"))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_2.7mm_M2.5_Pad (layer F.Cu) (tedit 5B7B68FA)
    (at 147.955 141.605)
    (descr "Mounting Hole 2.7mm, M2.5")
    (tags "mounting hole 2.7mm m2.5")
    (attr virtual)
    (fp_text reference REF** (at 8.255 -3.175) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.7mm_M2.5_Pad (at 0 3.7) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.4 5.4) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.7mm_M2.5_Pad (layer F.Cu) (tedit 5B7B6844)
    (at 87.63 104.775)
    (descr "Mounting Hole 2.7mm, M2.5")
    (tags "mounting hole 2.7mm m2.5")
    (attr virtual)
    (fp_text reference REF** (at -5.715 -5.715) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.7mm_M2.5_Pad (at 0 3.7) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.4 5.4) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.7mm_M2.5_Pad (layer F.Cu) (tedit 5B7B68AF)
    (at 147.955 104.775)
    (descr "Mounting Hole 2.7mm, M2.5")
    (tags "mounting hole 2.7mm m2.5")
    (attr virtual)
    (fp_text reference REF** (at 0 -6.35) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.7mm_M2.5_Pad (at 0 3.7) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.4 5.4) (drill 2.7) (layers *.Cu *.Mask))
  )
  (gr_text "Vin\n6-18V" (at 93.345 136.525 270) (layer F.SilkS))
  (gr_text "Vin 6 to 18V" (at 144.78 128.905) (layer F.SilkS))
  (gr_text "Vin 6 to 18V" (at 90.805 117.475) (layer F.SilkS))
  (gr_text - (at 88.9 139.065) (layer B.SilkS))
  (gr_text + (at 88.9 133.985) (layer B.SilkS))
  (gr_text - (at 133.35 140.335) (layer B.SilkS))
  (gr_text - (at 123.19 140.335) (layer B.SilkS))
  (gr_text - (at 103.505 140.335) (layer B.SilkS))
  (gr_text - (at 102.235 106.045) (layer B.SilkS))
  (gr_text - (at 112.395 106.045) (layer B.SilkS))
  (gr_text - (at 132.08 106.045) (layer B.SilkS))
  (gr_text + (at 137.16 106.045) (layer B.SilkS))
  (gr_text + (at 117.475 106.045) (layer B.SilkS))
  (gr_text + (at 107.315 106.045) (layer B.SilkS))
  (gr_text + (at 128.27 140.335) (layer B.SilkS))
  (gr_text + (at 118.11 140.335) (layer B.SilkS))
  (gr_text + (at 98.425 140.335) (layer B.SilkS))
  (gr_text "Use R8 and R10 to set the voltage \non each half independently\n7.68k = 5V\n8.66k = 4.5V\n13k = 3.3V\n14.7k = 3V" (at 116.84 126.365) (layer B.SilkS))
  (gr_text "Dual 1.5A badge power supply board\nPJS 20Aug2018 MIT License." (at 116.205 116.84) (layer B.SilkS))
  (gr_text "R8 and R10\n7.68k = 5V\n8.66k = 4.5V\n13k = 3.3V\n14.7k = 3V" (at 105.41 125.095) (layer F.SilkS))
  (gr_line (start 152.4 100.33) (end 152.4 123.19) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 83.185 100.33) (end 152.4 100.33) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 83.185 123.19) (end 83.185 100.33) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 152.4 146.05) (end 83.185 146.05) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 152.4 146.05) (end 152.4 123.19) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 83.185 123.19) (end 83.185 146.05) (layer Edge.Cuts) (width 0.15))
  (gr_text "Copyright (c) 2018 Peter Shabino\n\nPermission is hereby granted, free of charge, to any person obtaining a copy of this hardware, software, and associated documentation files \n(the \"Product\"), to deal in the Product without restriction, including without limitation the rights to use, copy, modify, merge, publish, \ndistribute, sublicense, and/or sell copies of the Product, and to permit persons to whom the Product is furnished to do so, subject to the \nfollowing conditions:\n\nThe above copyright notice and this permission notice shall be included in all copies or substantial portions of the Product.\n\nTHE PRODUCT IS PROVIDED \"AS IS\", WITHOUT WARRANTY OF ANY KIND, EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF \nMERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT. IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT HOLDERS BE LIABLE \nFOR ANY CLAIM, DAMAGES OR OTHER LIABILITY, WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING FROM, OUT OF OR IN CONNECTION \nWITH THE PRODUCT OR THE USE OR OTHER DEALINGS IN THE PRODUCT." (at 178.054 173.863) (layer F.SilkS))
  (gr_text "Copyright (c) 2018 Peter Shabino\n\nPermission is hereby granted, free of charge, to any person obtaining a copy of this hardware, software, and associated documentation files \n(the \"Product\"), to deal in the Product without restriction, including without limitation the rights to use, copy, modify, merge, publish, \ndistribute, sublicense, and/or sell copies of the Product, and to permit persons to whom the Product is furnished to do so, subject to the \nfollowing conditions:\n\nThe above copyright notice and this permission notice shall be included in all copies or substantial portions of the Product.\n\nTHE PRODUCT IS PROVIDED \"AS IS\", WITHOUT WARRANTY OF ANY KIND, EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF \nMERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT. IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT HOLDERS BE LIABLE \nFOR ANY CLAIM, DAMAGES OR OTHER LIABILITY, WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING FROM, OUT OF OR IN CONNECTION \nWITH THE PRODUCT OR THE USE OR OTHER DEALINGS IN THE PRODUCT." (at 178.054 173.863) (layer F.Cu))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (priority 6)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 1.016))
    (polygon
      (pts
        (xy 83.185 100.33) (xy 152.4 100.33) (xy 152.4 146.05) (xy 83.185 146.05)
      )
    )
  )
  (zone (net 4) (net_name "Net-(C3-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 7)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 109.855 112.395) (xy 116.205 112.395) (xy 116.205 117.475) (xy 113.665 117.475) (xy 113.665 116.205)
        (xy 109.855 116.205)
      )
    )
  )
  (zone (net 5) (net_name "Net-(C4-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 7)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 118.745 128.905) (xy 121.285 128.905) (xy 121.285 130.175) (xy 125.095 130.175) (xy 125.095 133.985)
        (xy 118.745 133.985)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (priority 3)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 1.016))
    (polygon
      (pts
        (xy 83.185 100.33) (xy 152.4 100.33) (xy 152.4 146.05) (xy 83.185 146.05)
      )
    )
  )
)
