(kicad_pcb (version 20171130) (host pcbnew "(5.1.2-1)-1")
  (general
    (thickness 1.6)
    (drawings 68)
    (tracks 111)
    (zones 0)
    (modules 55)
    (nets 28)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.3)
    (user_trace_width 0.5)
    (user_trace_width 0.8)
    (user_trace_width 1)
    (user_trace_width 1.5)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.6)
    (via_drill 0.3)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.5 2.5)
    (pad_drill 1.3)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (grid_origin 133 71.5)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(C1-Pad1)")
  (net 3 "Net-(D1-Pad1)")
  (net 4 "Net-(D1-Pad2)")
  (net 5 "Net-(D2-Pad2)")
  (net 6 "Net-(J1-Pad1)")
  (net 7 "Net-(J3-Pad1)")
  (net 8 "Net-(J4-Pad1)")
  (net 9 "Net-(J5-Pad1)")
  (net 10 "Net-(J9-Pad1)")
  (net 11 "Net-(J10-Pad1)")
  (net 12 "Net-(J11-Pad1)")
  (net 13 "Net-(J12-Pad1)")
  (net 14 "Net-(K1-Pad12)")
  (net 15 "Net-(K1-Pad1)")
  (net 16 "Net-(J13-Pad1)")
  (net 17 "Net-(J6-Pad1)")
  (net 18 "Net-(J8-Pad1)")
  (net 19 "Net-(J7-Pad1)")
  (net 20 "Net-(J15-Pad1)")
  (net 21 "Net-(Q4-Pad1)")
  (net 22 "Net-(Q4-Pad2)")
  (net 23 "Net-(J1-Pad3)")
  (net 24 "Net-(J14-Pad1)")
  (net 25 "Net-(J16-Pad1)")
  (net 26 "Net-(Q3-Pad2)")
  (net 27 "Net-(Q3-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.3)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J14-Pad1)")
    (add_net "Net-(J15-Pad1)")
    (add_net "Net-(J16-Pad1)")
    (add_net "Net-(J7-Pad1)")
    (add_net "Net-(Q3-Pad1)")
    (add_net "Net-(Q3-Pad2)")
    (add_net "Net-(Q4-Pad1)")
    (add_net "Net-(Q4-Pad2)")
  )
  (net_class K-coil ""
    (clearance 0.15)
    (trace_width 0.3)
    (via_dia 0.6)
    (via_drill 0.3)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (net_class signal ""
    (clearance 0.2)
    (trace_width 0.6091)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J10-Pad1)")
    (add_net "Net-(J11-Pad1)")
    (add_net "Net-(J12-Pad1)")
    (add_net "Net-(J13-Pad1)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J4-Pad1)")
    (add_net "Net-(J5-Pad1)")
    (add_net "Net-(J6-Pad1)")
    (add_net "Net-(J8-Pad1)")
    (add_net "Net-(J9-Pad1)")
    (add_net "Net-(K1-Pad1)")
    (add_net "Net-(K1-Pad12)")
  )
  (net_class signal-2 ""
    (clearance 0.15)
    (trace_width 0.5)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module In-relay:Relay_DPDT_Kemet_EC2-n (layer F.Cu) (tedit 605E0406)
    (at 161.5 46)
    (descr "Relay Omron G6S-2, see http://omronfs.omron.com/en_US/ecb/products/pdf/en-g6s.pdf")
    (tags "Relay Omron G6S-2")
    (fp_text reference K1 (at 2.5 4) (layer F.SilkS))
    (fp_text value EC2 (at 2.5 12.5) (layer F.SilkS))
    (fp_text user %R (at 2.54 6.35) (layer F.Fab))
    (fp_text user + (at 0 1.9 -90 unlocked) (layer F.SilkS))
    (fp_text user - (at 5.1 1.9 -90 unlocked) (layer F.SilkS))
    (pad 9 thru_hole circle (at 5.08 7.62 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 12 "Net-(J11-Pad1)"))
    (pad 4 thru_hole circle (at 0 7.62 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 13 "Net-(J12-Pad1)"))
    (pad 12 thru_hole circle (at 5.08 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 14 "Net-(K1-Pad12)"))
    (pad 10 thru_hole circle (at 5.08 5.08) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 19 "Net-(J7-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 15 "Net-(K1-Pad1)"))
    (pad 3 thru_hole circle (at 0 5.08) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 9 "Net-(J5-Pad1)"))
    (pad 8 thru_hole circle (at 5.08 10.16) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 11 "Net-(J10-Pad1)"))
    (pad 5 thru_hole circle (at 0 10.16) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 10 "Net-(J9-Pad1)"))
    (model ${KIPRJMOD}/lib/3D/EC2-5SNU.step
      (offset (xyz -1.2 1.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 90))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 122 60.7 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R8 (at 5 0) (layer F.SilkS))
    (fp_text value 1k (at 5.08 2.37) (layer F.Fab))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(Q4-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module In-relay:Relay_DPDT_Kemet_EC2-n (layer F.Cu) (tedit 605E0406)
    (at 99.5 46)
    (descr "Relay Omron G6S-2, see http://omronfs.omron.com/en_US/ecb/products/pdf/en-g6s.pdf")
    (tags "Relay Omron G6S-2")
    (fp_text reference K2 (at 2.5 4) (layer F.SilkS))
    (fp_text value EC2 (at 2.5 12.5) (layer F.SilkS))
    (fp_text user %R (at 2.54 6.35) (layer F.Fab))
    (fp_text user + (at 0 1.9 -90 unlocked) (layer F.SilkS))
    (fp_text user - (at 5.1 1.9 -90 unlocked) (layer F.SilkS))
    (pad 9 thru_hole circle (at 5.08 7.62 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 20 "Net-(J15-Pad1)"))
    (pad 4 thru_hole circle (at 0 7.62 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 25 "Net-(J16-Pad1)"))
    (pad 12 thru_hole circle (at 5.08 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 14 "Net-(K1-Pad12)"))
    (pad 10 thru_hole circle (at 5.08 5.08) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 18 "Net-(J8-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 15 "Net-(K1-Pad1)"))
    (pad 3 thru_hole circle (at 0 5.08) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 17 "Net-(J6-Pad1)"))
    (pad 8 thru_hole circle (at 5.08 10.16) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 24 "Net-(J14-Pad1)"))
    (pad 5 thru_hole circle (at 0 10.16) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 16 "Net-(J13-Pad1)"))
    (model ${KIPRJMOD}/lib/3D/EC2-5SNU.step
      (offset (xyz -1.2 1.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 90))
    )
  )
  (module In-relay:mkds_1,5-3_blank (layer F.Cu) (tedit 606A3716)
    (at 133 37 180)
    (descr "3-way 5mm pitch terminal block, Phoenix MKDS series")
    (fp_text reference J2 (at 0 -6.6) (layer F.SilkS) hide)
    (fp_text value power (at 0 3.4) (layer F.SilkS))
    (pad 2 thru_hole circle (at 0 0 180) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at -5 0 180) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(J1-Pad3)"))
    (pad 3 thru_hole circle (at 5 0 180) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(J1-Pad1)"))
  )
  (module In-relay:IO_Pad_D2.5mm_Drill1.2mm (layer F.Cu) (tedit 5D56008B)
    (at 101.5 67.5)
    (descr "THT pad as test Point, diameter 2.5mm, hole diameter 1.2mm ")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J13 (at 0 -2.148) (layer F.Fab))
    (fp_text value "Rec L" (at 0 -2.5) (layer F.SilkS))
    (fp_text user %R (at 0 -2.15) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 16 "Net-(J13-Pad1)"))
  )
  (module Capacitor_THT:CP_Radial_D5.0mm_P2.00mm (layer F.Cu) (tedit 606A36FD)
    (at 133 57.5 270)
    (descr "CP, Radial series, Radial, pin pitch=2.00mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.00mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C1 (at 4 2 180) (layer F.SilkS))
    (fp_text value 10u (at 1 3.75 90) (layer F.Fab))
    (fp_text user %R (at 1 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 2 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 138.2 47 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 5.08 0) (layer F.SilkS))
    (fp_text value 30k (at 5.08 2.37) (layer F.Fab))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(J1-Pad3)"))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(J4-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 144 51.6)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R9 (at 5.08 0.094999) (layer F.SilkS))
    (fp_text value 137 (at 5.08 2.37) (layer F.Fab))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 "Net-(Q3-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(J1-Pad3)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 121.96 51.6 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R10 (at 5.08 0) (layer F.SilkS))
    (fp_text value 137 (at 5.08 2.37) (layer F.Fab))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(Q4-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 144 54.8)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R5 (at 5 0.044999) (layer F.SilkS))
    (fp_text value 560 (at 5.08 2.37) (layer F.Fab))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(J1-Pad3)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 121.96 54.7 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R6 (at 5.08 0) (layer F.SilkS))
    (fp_text value 560 (at 5.08 2.37) (layer F.Fab))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 138.2 53.2 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R4 (at 5.08 0) (layer F.SilkS))
    (fp_text value 1M (at 5.08 2.37) (layer F.Fab))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(J1-Pad3)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 138.2 50.1 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R3 (at 5.08 0) (layer F.SilkS))
    (fp_text value 560 (at 5.08 2.37) (layer F.Fab))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(J3-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-92_Wide (layer F.Cu) (tedit 5A2795B7)
    (at 112.5 46.4 180)
    (descr "TO-92 leads molded, wide, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q4 (at -0.7 1.9) (layer F.SilkS))
    (fp_text value 2N5551 (at 2.54 2.79) (layer F.Fab))
    (fp_text user %R (at 2.54 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(Q4-Pad1)"))
    (pad 3 thru_hole circle (at 5.08 0 270) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(K1-Pad12)"))
    (pad 2 thru_hole circle (at 2.54 -2.54 270) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(Q4-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92_Wide.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-92_Wide (layer F.Cu) (tedit 5A2795B7)
    (at 153.5 48)
    (descr "TO-92 leads molded, wide, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q3 (at 0.04 -2.84) (layer F.SilkS))
    (fp_text value 2N4403 (at 2.54 2.79) (layer F.Fab))
    (fp_text user %R (at 2.54 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 -2.54 90) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(Q3-Pad2)"))
    (pad 3 thru_hole circle (at 5.08 0 90) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(K1-Pad1)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 "Net-(Q3-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92_Wide.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-92_Wide (layer F.Cu) (tedit 5A2795B7)
    (at 127.5 61 90)
    (descr "TO-92 leads molded, wide, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q1 (at 5 -2.5 180) (layer F.SilkS))
    (fp_text value 2N5551 (at 2.54 2.79 90) (layer F.Fab))
    (fp_text user %R (at 2.54 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole circle (at 5.08 0 180) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 -2.54 180) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(J4-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92_Wide.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-92_Wide (layer F.Cu) (tedit 5A2795B7)
    (at 140 61 90)
    (descr "TO-92 leads molded, wide, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q2 (at 5.24 -2.5 180) (layer F.SilkS))
    (fp_text value 2N7000 (at 2.54 2.79 90) (layer F.Fab))
    (fp_text user %R (at 2.54 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 -2.54 180) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 3 thru_hole circle (at 5.08 0 180) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(D1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92_Wide.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 87.5 37.5 90)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference H1 (at 0 -4.2 90) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4.2 90) (layer F.Fab))
    (fp_text user %R (at 0.3 0 90) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0 90) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 178.5 37.5 270)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference H2 (at 0 -4.2 90) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4.2 90) (layer F.Fab))
    (fp_text user %R (at 0.3 0 90) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0 270) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module In-relay:IO_Pad_D2.5mm_Drill1.2mm (layer F.Cu) (tedit 5D56008B)
    (at 150.5 67.5)
    (descr "THT pad as test Point, diameter 2.5mm, hole diameter 1.2mm ")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J9 (at 0 -2.148) (layer F.Fab))
    (fp_text value "Line R" (at 0 -2.5) (layer F.SilkS))
    (fp_text user %R (at 0 -2.15) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 10 "Net-(J9-Pad1)"))
  )
  (module In-relay:IO_Pad_D2.5mm_Drill1.2mm (layer F.Cu) (tedit 5D56008B)
    (at 164.5 67.5)
    (descr "THT pad as test Point, diameter 2.5mm, hole diameter 1.2mm ")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J10 (at 0 -2.148) (layer F.Fab))
    (fp_text value "Rec R" (at 0 -2.5) (layer F.SilkS))
    (fp_text user %R (at 0 -2.15) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 11 "Net-(J10-Pad1)"))
  )
  (module In-relay:IO_Pad_D2.5mm_Drill1.2mm (layer F.Cu) (tedit 5D56008B)
    (at 164.5 37.5 180)
    (descr "THT pad as test Point, diameter 2.5mm, hole diameter 1.2mm ")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J11 (at 0 -2.148) (layer F.Fab))
    (fp_text value "Rec R" (at 0 -2.25) (layer F.SilkS))
    (fp_text user %R (at 0 -2.15) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 12 "Net-(J11-Pad1)"))
  )
  (module In-relay:IO_Pad_D2.5mm_Drill1.2mm (layer F.Cu) (tedit 5D56008B)
    (at 150.5 37.5 180)
    (descr "THT pad as test Point, diameter 2.5mm, hole diameter 1.2mm ")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J12 (at 0 -2.148) (layer F.Fab))
    (fp_text value "Line R" (at 0 -2.25) (layer F.SilkS))
    (fp_text user %R (at 0 -2.15) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 13 "Net-(J12-Pad1)"))
  )
  (module In-relay:IO_Pad_D2.5mm_Drill1.2mm (layer F.Cu) (tedit 5D56008B)
    (at 115.5 67.5)
    (descr "THT pad as test Point, diameter 2.5mm, hole diameter 1.2mm ")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J14 (at 0 -2.148) (layer F.Fab))
    (fp_text value "Line L" (at 0 -2.5) (layer F.SilkS))
    (fp_text user %R (at 0 -2.15) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 24 "Net-(J14-Pad1)"))
  )
  (module In-relay:IO_Pad_D2.5mm_Drill1.2mm (layer F.Cu) (tedit 5D56008B)
    (at 115.5 37.5 180)
    (descr "THT pad as test Point, diameter 2.5mm, hole diameter 1.2mm ")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J15 (at 0 -2.148) (layer F.Fab))
    (fp_text value "Line L" (at 0 -2.25) (layer F.SilkS))
    (fp_text user %R (at 0 -2.15) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 20 "Net-(J15-Pad1)"))
  )
  (module In-relay:IO_Pad_D2.5mm_Drill1.2mm (layer F.Cu) (tedit 5D56008B)
    (at 101.5 37.5 180)
    (descr "THT pad as test Point, diameter 2.5mm, hole diameter 1.2mm ")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J16 (at 0 -2.148) (layer F.Fab))
    (fp_text value "Rec L" (at 0 -2.25) (layer F.SilkS))
    (fp_text user %R (at 0 -2.15) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 25 "Net-(J16-Pad1)"))
  )
  (module In-relay:mkds_1,5-3 (layer F.Cu) (tedit 606A370B)
    (at 133 66.5)
    (descr "3-way 5mm pitch terminal block, Phoenix MKDS series")
    (fp_text reference J1 (at 0 -5.4) (layer F.Fab))
    (fp_text value power (at 0 3.25) (layer F.SilkS))
    (pad 3 thru_hole circle (at 5 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(J1-Pad3)"))
    (pad 1 thru_hole circle (at -5 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(J1-Pad1)"))
    (pad 2 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (model ${KIPRJMOD}/Lib/3D/pxc_1935174_03_PT-1-5-3-5-0-H_3D.stp
      (offset (xyz -30.09899954795837 -44.70399932861328 -38.86199941635132))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 180 90))
    )
  )
  (module In-relay:IO_Pad_D2.5mm_Drill1.2mm (layer F.Cu) (tedit 5D56008B)
    (at 95.5 67.5)
    (descr "THT pad as test Point, diameter 2.5mm, hole diameter 1.2mm ")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J17 (at 0 -2.148) (layer F.Fab))
    (fp_text value gnd (at 0 -2.5) (layer F.SilkS))
    (fp_text user %R (at 0 -2.15) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module In-relay:IO_Pad_D2.5mm_Drill1.2mm (layer F.Cu) (tedit 5D56008B)
    (at 121.5 37.5 180)
    (descr "THT pad as test Point, diameter 2.5mm, hole diameter 1.2mm ")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J18 (at 0 -2.148) (layer F.Fab))
    (fp_text value gnd (at 0 -2.25) (layer F.SilkS))
    (fp_text user %R (at 0 -2.15) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module In-relay:IO_Pad_D2.5mm_Drill1.2mm (layer F.Cu) (tedit 5D56008B)
    (at 95.5 37.5 180)
    (descr "THT pad as test Point, diameter 2.5mm, hole diameter 1.2mm ")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J19 (at 0 -2.148) (layer F.Fab))
    (fp_text value gnd (at 0 -2.25) (layer F.SilkS))
    (fp_text user %R (at 0 -2.15) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module In-relay:IO_Pad_D2.5mm_Drill1.2mm (layer F.Cu) (tedit 5D56008B)
    (at 144.5 67.5)
    (descr "THT pad as test Point, diameter 2.5mm, hole diameter 1.2mm ")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J20 (at 0 -2.148) (layer F.Fab))
    (fp_text value gnd (at 0 -2.5) (layer F.SilkS))
    (fp_text user %R (at 0 -2.15) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module In-relay:IO_Pad_D2.5mm_Drill1.2mm (layer F.Cu) (tedit 5D56008B)
    (at 144.5 37.5 180)
    (descr "THT pad as test Point, diameter 2.5mm, hole diameter 1.2mm ")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J21 (at 0 -2.148) (layer F.Fab))
    (fp_text value gnd (at 0 -2.25) (layer F.SilkS))
    (fp_text user %R (at 0 -2.15) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module In-relay:IO_Pad_D2.5mm_Drill1.2mm (layer F.Cu) (tedit 5D56008B)
    (at 170.5 67.5)
    (descr "THT pad as test Point, diameter 2.5mm, hole diameter 1.2mm ")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J22 (at 0 -2.148) (layer F.Fab))
    (fp_text value gnd (at 0 -2.5) (layer F.SilkS))
    (fp_text user %R (at 0 -2.15) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module In-relay:IO_Pad_D2.5mm_Drill1.2mm (layer F.Cu) (tedit 5D56008B)
    (at 121.5 67.5)
    (descr "THT pad as test Point, diameter 2.5mm, hole diameter 1.2mm ")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J23 (at 0 -2.148) (layer F.Fab))
    (fp_text value gnd (at 0 -2.5) (layer F.SilkS))
    (fp_text user %R (at 0 -2.15) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module In-relay:IO_Pad_D2.5mm_Drill1.2mm (layer F.Cu) (tedit 5D56008B)
    (at 170.5 37.5 180)
    (descr "THT pad as test Point, diameter 2.5mm, hole diameter 1.2mm ")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J24 (at 0 -2.148) (layer F.Fab))
    (fp_text value gnd (at 0 -2.25) (layer F.SilkS))
    (fp_text user %R (at 0 -2.15) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module In-relay:Oval_Pad_D2.5mm_Drill1.2mm (layer F.Cu) (tedit 5D56DE29)
    (at 107.25 37.5)
    (descr "THT pad as test Point, diameter 2.5mm, hole diameter 1.2mm ")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J25 (at -0.7 -2.3) (layer F.Fab))
    (fp_text value gnd (at 1.25 2.25) (layer F.SilkS))
    (fp_text user %R (at 3.65 -2.4) (layer F.Fab))
    (pad 1 thru_hole oval (at 2.5 0) (size 5 2.5) (drill 1.2 (offset -1.25 0)) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole oval (at 0 0) (size 5 2.5) (drill 1.2 (offset 1.25 0)) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module In-relay:Oval_Pad_D2.5mm_Drill1.2mm (layer F.Cu) (tedit 5D56DE29)
    (at 156.25 37.5)
    (descr "THT pad as test Point, diameter 2.5mm, hole diameter 1.2mm ")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J26 (at -0.7 -2.3) (layer F.Fab))
    (fp_text value gnd (at 1.25 2.25) (layer F.SilkS))
    (fp_text user %R (at 3.65 -2.4) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 5 2.5) (drill 1.2 (offset 1.25 0)) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole oval (at 2.5 0) (size 5 2.5) (drill 1.2 (offset -1.25 0)) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 144 60.7)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R7 (at 5 0) (layer F.SilkS))
    (fp_text value 1k (at 5.08 2.37) (layer F.Fab))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(D1-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(Q3-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 87.5 67)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference H3 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 178.5 67)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference H4 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module In-relay:Oval_Pad_D2.5mm_Drill1.2mm (layer F.Cu) (tedit 5D56DE29)
    (at 107.25 67.5)
    (descr "THT pad as test Point, diameter 2.5mm, hole diameter 1.2mm ")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J27 (at -0.7 -2.3) (layer F.Fab))
    (fp_text value gnd (at 1.25 -2.5) (layer F.SilkS))
    (fp_text user %R (at 3.65 -2.4) (layer F.Fab))
    (pad 1 thru_hole oval (at 2.5 0) (size 5 2.5) (drill 1.2 (offset -1.25 0)) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole oval (at 0 0) (size 5 2.5) (drill 1.2 (offset 1.25 0)) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module In-relay:Oval_Pad_D2.5mm_Drill1.2mm (layer F.Cu) (tedit 5D56DE29)
    (at 156.25 67.5)
    (descr "THT pad as test Point, diameter 2.5mm, hole diameter 1.2mm ")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J28 (at -0.7 -2.3) (layer F.Fab))
    (fp_text value gnd (at 1.25 -2.5) (layer F.SilkS))
    (fp_text user %R (at 3.65 -2.4) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 5 2.5) (drill 1.2 (offset 1.25 0)) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole oval (at 2.5 0) (size 5 2.5) (drill 1.2 (offset -1.25 0)) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 128 43.9)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at 5.08 0) (layer F.SilkS))
    (fp_text value 270 (at 5.08 2.37) (layer F.Fab))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(J4-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-35_SOD27_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE50CD5)
    (at 154.16 57.7 180)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 10.16mm  length 4mm diameter 2mm")
    (fp_text reference D1 (at 5.12 0) (layer F.SilkS))
    (fp_text value BZX79C10 (at 5.08 2.12) (layer F.Fab))
    (fp_text user K (at -1.34 0) (layer F.SilkS))
    (fp_text user K (at 0 -1.8) (layer F.Fab))
    (fp_text user %R (at 5.38 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(D1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-35_SOD27_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-35_SOD27_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE50CD5)
    (at 122 57.7 180)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 10.16mm  length 4mm diameter 2mm")
    (fp_text reference D2 (at 5.62 0) (layer F.SilkS))
    (fp_text value BZX79C10 (at 5.08 2.12) (layer F.Fab))
    (fp_text user %R (at 5.38 0) (layer F.Fab))
    (fp_text user K (at 0 -1.8) (layer F.Fab))
    (fp_text user K (at -1.38 0) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-35_SOD27_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module In-relay:IO_Pad_D2.5mm_Drill1.2mm (layer F.Cu) (tedit 5D56008B)
    (at 177 57.5)
    (descr "THT pad as test Point, diameter 2.5mm, hole diameter 1.2mm ")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J7 (at 0 -2.148) (layer F.Fab))
    (fp_text value Hp (at 0 2.25) (layer F.SilkS))
    (fp_text user %R (at 0 -2.15) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 19 "Net-(J7-Pad1)"))
  )
  (module In-relay:IO_Pad_D2.5mm_Drill1.2mm (layer F.Cu) (tedit 5D56008B)
    (at 177 47.5)
    (descr "THT pad as test Point, diameter 2.5mm, hole diameter 1.2mm ")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J5 (at 0 -2.148) (layer F.Fab))
    (fp_text value vHp (at 0 2.25) (layer F.SilkS))
    (fp_text user %R (at 0 -2.15) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 9 "Net-(J5-Pad1)"))
  )
  (module In-relay:IO_Pad_D2.5mm_Drill1.2mm (layer F.Cu) (tedit 5D56008B)
    (at 89 47.5)
    (descr "THT pad as test Point, diameter 2.5mm, hole diameter 1.2mm ")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J8 (at 0 -2.148) (layer F.Fab))
    (fp_text value vHp (at 0 2.25) (layer F.SilkS))
    (fp_text user %R (at 0 -2.15) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 18 "Net-(J8-Pad1)"))
  )
  (module In-relay:IO_Pad_D2.5mm_Drill1.2mm (layer F.Cu) (tedit 5D56008B)
    (at 89 57.5)
    (descr "THT pad as test Point, diameter 2.5mm, hole diameter 1.2mm ")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J6 (at 0 -2.148) (layer F.Fab))
    (fp_text value Hp (at 0 2.25) (layer F.SilkS))
    (fp_text user %R (at 0 -2.15) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 17 "Net-(J6-Pad1)"))
  )
  (module TestPoint:TestPoint_THTPad_2.0x2.0mm_Drill1.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 144.5 46.5 180)
    (descr "THT rectangular pad as test Point, square 2.0mm_Drill1.0mm  side length, hole diameter 1.0mm")
    (tags "test point THT pad rectangle square")
    (attr virtual)
    (fp_text reference J3 (at 0 -1.998) (layer F.SilkS) hide)
    (fp_text value NO (at 0 2.05) (layer F.SilkS))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J3-Pad1)"))
  )
  (module TestPoint:TestPoint_THTPad_2.0x2.0mm_Drill1.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 121.5 46.5 180)
    (descr "THT rectangular pad as test Point, square 2.0mm_Drill1.0mm  side length, hole diameter 1.0mm")
    (tags "test point THT pad rectangle square")
    (attr virtual)
    (fp_text reference J4 (at 0 -1.998) (layer F.SilkS) hide)
    (fp_text value NC (at 0 2.05) (layer F.SilkS))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J4-Pad1)"))
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 108 51.1 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R14 (at 5.08 0 90) (layer F.SilkS))
    (fp_text value 220k (at 5.08 2.37 90) (layer F.Fab))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(J8-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 170 51.1 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R13 (at 5.08 0 90) (layer F.SilkS))
    (fp_text value 220k (at 5.08 2.37 90) (layer F.Fab))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(J7-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 158 51.1 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R11 (at 5.08 0 90) (layer F.SilkS))
    (fp_text value 220k (at 5.08 2.37 90) (layer F.Fab))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(J5-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 96 51.1 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R12 (at 5.08 0 90) (layer F.SilkS))
    (fp_text value 220k (at 5.08 2.37 90) (layer F.Fab))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(J6-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text vHp (at 177 49.75) (layer B.SilkS))
  (gr_text Hp (at 177 59.75) (layer B.SilkS))
  (gr_text Hp (at 89 59.75) (layer B.SilkS))
  (gr_text vHp (at 89 49.75) (layer B.SilkS))
  (gr_text NC (at 121.5 44.5) (layer B.SilkS))
  (gr_text NO (at 144.5 44.5) (layer B.SilkS))
  (gr_text Outputs (at 157.5 70) (layer B.SilkS))
  (gr_text Outputs (at 108.5 70) (layer B.SilkS))
  (gr_text Inputs (at 157.5 34.75) (layer B.SilkS))
  (gr_text Inputs (at 108.5 34.75) (layer B.SilkS))
  (gr_text "Rec R" (at 164.5 65) (layer B.SilkS))
  (gr_text "Line R" (at 150.5 65) (layer B.SilkS))
  (gr_text "Line L" (at 115.5 65) (layer B.SilkS))
  (gr_text "Rec L" (at 101.5 65) (layer B.SilkS))
  (gr_text "Rec R" (at 164.5 39.75) (layer B.SilkS))
  (gr_text "Line R" (at 150.5 39.75) (layer B.SilkS))
  (gr_text "Line L" (at 115.5 39.75) (layer B.SilkS))
  (gr_text "Rec L" (at 101.5 39.75) (layer B.SilkS))
  (gr_text +15v (at 138 69.75) (layer B.SilkS))
  (gr_text +15v (at 138 34.25) (layer B.SilkS))
  (gr_text -15v (at 128 69.75) (layer B.SilkS))
  (gr_text -15v (at 128 34.25) (layer B.SilkS))
  (gr_text Outputs (at 157.5 70) (layer F.SilkS))
  (gr_text Outputs (at 108.5 70) (layer F.SilkS))
  (gr_text Inputs (at 157.5 34.75) (layer F.SilkS))
  (gr_text Inputs (at 108.5 34.75) (layer F.SilkS))
  (gr_line (start 170.5 33) (end 183 33) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 168 35.5) (end 170.5 33) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 167 35.5) (end 168 35.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 164.5 33) (end 167 35.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 150.5 33) (end 164.5 33) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 148 35.5) (end 150.5 33) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 147 35.5) (end 148 35.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 144.5 33) (end 147 35.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 121.5 33) (end 144.5 33) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 119 35.5) (end 121.5 33) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 118 35.5) (end 119 35.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 115.5 33) (end 118 35.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 101.5 33) (end 115.5 33) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 99 35.5) (end 101.5 33) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 98 35.5) (end 99 35.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 95.5 33) (end 98 35.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 83 33) (end 95.5 33) (layer Edge.Cuts) (width 0.05))
  (gr_text +15v (at 141.4 66.5 90) (layer F.SilkS))
  (gr_text -15v (at 124.8 66.6 90) (layer F.SilkS))
  (gr_text -15v (at 124.8 37 90) (layer F.SilkS))
  (gr_text +15v (at 141.25 37 90) (layer F.SilkS))
  (gr_line (start 83 71.5) (end 83 33) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 183 71.5) (end 83 71.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 183 33) (end 183 71.5) (layer Edge.Cuts) (width 0.05))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 82.5 32.5) (xy 82.5 72) (xy 183.5 72) (xy 183.5 32.5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 83 41) (xy 89 41) (xy 91 39) (xy 91 33) (xy 83 33)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 83 63.5) (xy 89 63.5) (xy 91 65.5) (xy 91 71.5) (xy 83 71.5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 175 71.5) (xy 175 65.5) (xy 177 63.5) (xy 183 63.5) (xy 183 71.5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 183 41) (xy 177 41) (xy 175 39) (xy 175 33) (xy 183 33)
      )
    )
  )
)
