(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "MTA_Egress_Plugboard_Gerber/")
		)
	)
	(net 0 "")
	(net 1 "Net-(J1-Pin_3)")
	(net 2 "Net-(J1-Pin_1)")
	(net 3 "Net-(J1-Pin_6)")
	(net 4 "Net-(J1-Pin_4)")
	(net 5 "Net-(J2-Pin_12)")
	(net 6 "Net-(J2-Pin_8)")
	(net 7 "Net-(J2-Pin_7)")
	(net 8 "Net-(J2-Pin_2)")
	(net 9 "Net-(J2-Pin_10)")
	(net 10 "Net-(J2-Pin_14)")
	(net 11 "Net-(J2-Pin_1)")
	(net 12 "Net-(J2-Pin_3)")
	(net 13 "Net-(J2-Pin_6)")
	(net 14 "Net-(J2-Pin_13)")
	(net 15 "Net-(J2-Pin_11)")
	(net 16 "Net-(J2-Pin_4)")
	(net 17 "Net-(J2-Pin_15)")
	(net 18 "Net-(J2-Pin_9)")
	(net 19 "Net-(J2-Pin_5)")
	(footprint "TerminalBlock_Phoenix:TerminalBlock_Phoenix_MKDS-1,5-6_1x06_P5.00mm_Horizontal"
		(layer "F.Cu")
		(at 81.5 3 -90)
		(descr "Terminal Block Phoenix MKDS-1,5-6, 6 pins, pitch 5mm, size 30x9.8mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/100425.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix")
		(tags "THT Terminal Block Phoenix MKDS-1,5-6 pitch 5mm size 30x9.8mm^2 drill 1.3mm pad 2.6mm")
		(property "Reference" "J1"
			(at 9.5 6 90)
			(layer "F.SilkS")
		)
		(property "Value" "Screw_Terminal_01x06"
			(at 12.5 5.66 90)
			(layer "F.Fab")
		)
		(property "Footprint" "TerminalBlock_Phoenix:TerminalBlock_Phoenix_MKDS-1,5-6_1x06_P5.00mm_Horizontal"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic screw terminal, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(sheetname "Root")
		(sheetfile "MTA_Egress_Plugboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 12.5 3.2 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(J1-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5 0 270)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(J1-Pin_1)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 10 0 270)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "Net-(J1-Pin_3)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 15 0 270)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "Net-(J1-Pin_4)")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at 20 0 270)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "Net-(J1-Pin_3)")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at 25 0 270)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "Net-(J1-Pin_6)")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MKDS-1,5-6_1x06_P5.00mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TerminalBlock_Phoenix:TerminalBlock_Phoenix_MKDS-1,5-15_1x15_P5.00mm_Horizontal"
		(layer "F.Cu")
		(at 3 5.5)
		(descr "Terminal Block Phoenix MKDS-1,5-15, 15 pins, pitch 5mm, size 75x9.8mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/100425.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix")
		(tags "THT Terminal Block Phoenix MKDS-1,5-15 pitch 5mm size 75x9.8mm^2 drill 1.3mm pad 2.6mm")
		(property "Reference" "J3"
			(at 35 -6.26 0)
			(layer "F.SilkS")
		)
		(property "Value" "Screw_Terminal_01x15"
			(at 35 5.66 0)
			(layer "F.Fab")
		)
		(property "Footprint" "TerminalBlock_Phoenix:TerminalBlock_Phoenix_MKDS-1,5-15_1x15_P5.00mm_Horizontal"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.lcsc.com/datasheet/lcsc_datasheet_1912251709_Ningbo-Kangnex-Elec-WJ500V-5-08-3P_C72334.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic screw terminal, single row, 01x15, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Qty" "5"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Website" "https://www.lcsc.com/product-detail/span-style-background-color-ff0-Screw-span-span-style-background-color-ff0-Terminal-span-Blocks_Ningbo-Kangnex-Elec-WJ500V-5-08-3P_C72334.html"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" " WJ500V-5.08-3P"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Vendor" "LCSC"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price" ".14"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(sheetname "Root")
		(sheetfile "MTA_Egress_Plugboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 35 3.2 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "Net-(J2-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5 0)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "Net-(J2-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 10 0)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "Net-(J2-Pin_3)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 15 0)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "Net-(J2-Pin_4)")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at 20 0)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "Net-(J2-Pin_5)")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at 25 0)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "Net-(J2-Pin_6)")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole circle
			(at 30 0)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "Net-(J2-Pin_7)")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole circle
			(at 35 0)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "Net-(J2-Pin_8)")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" thru_hole circle
			(at 40 0)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "Net-(J2-Pin_9)")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" thru_hole circle
			(at 45 0)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "Net-(J2-Pin_10)")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(pad "11" thru_hole circle
			(at 50 0)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "Net-(J2-Pin_11)")
			(pinfunction "Pin_11")
			(pintype "passive")
		)
		(pad "12" thru_hole circle
			(at 55 0)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "Net-(J2-Pin_12)")
			(pinfunction "Pin_12")
			(pintype "passive")
		)
		(pad "13" thru_hole circle
			(at 60 0)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "Net-(J2-Pin_13)")
			(pinfunction "Pin_13")
			(pintype "passive")
		)
		(pad "14" thru_hole circle
			(at 65 0)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "Net-(J2-Pin_14)")
			(pinfunction "Pin_14")
			(pintype "passive")
		)
		(pad "15" thru_hole circle
			(at 70 0)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "Net-(J2-Pin_15)")
			(pinfunction "Pin_15")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MKDS-1,5-15_1x15_P5.00mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Phoenix_MC:PhoenixContact_MCV_1,5_16-G-3.81_1x16_P3.81mm_Vertical"
		(layer "F.Cu")
		(at 3.69 25.5)
		(descr "Generic Phoenix Contact connector footprint for: MCV_1,5/16-G-3.81; number of pins: 16; pin pitch: 3.81mm; Vertical || order number: 1803565 8A 160V")
		(tags "phoenix_contact connector MCV_01x16_G_3.81mm")
		(property "Reference" "J2"
			(at 28.58 -5.45 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x15_Socket"
			(at 28.58 4.2 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_Phoenix_MC:PhoenixContact_MCV_1,5_16-G-3.81_1x16_P3.81mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.lcsc.com/datasheet/lcsc_datasheet_2002271942_Ningbo-Kangnex-Elec-WJ15EDGVC-3-81-15P_C489976.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x15, script generated"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Website" "https://www.lcsc.com/product-detail/Pluggable-System-Terminal-Block_Ningbo-Kangnex-Elec-WJ15EDGVC-3-81-15P_C489976.html"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price" ".11"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" "WJ15EDGVC-3.81-15P"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Vendor" "LCSC"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "MTA_Egress_Plugboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 28.58 -3.55 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.8 3.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.138889)
			(net 11 "Net-(J2-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 3.81 0)
			(size 1.8 3.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "Net-(J2-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 7.62 0)
			(size 1.8 3.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "Net-(J2-Pin_3)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 11.43 0)
			(size 1.8 3.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "Net-(J2-Pin_4)")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 15.24 0)
			(size 1.8 3.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "Net-(J2-Pin_5)")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 19.05 0)
			(size 1.8 3.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "Net-(J2-Pin_6)")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 22.86 0)
			(size 1.8 3.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "Net-(J2-Pin_7)")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at 26.67 0)
			(size 1.8 3.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "Net-(J2-Pin_8)")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" thru_hole oval
			(at 30.48 0)
			(size 1.8 3.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "Net-(J2-Pin_9)")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" thru_hole oval
			(at 34.29 0)
			(size 1.8 3.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "Net-(J2-Pin_10)")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(pad "11" thru_hole oval
			(at 38.1 0)
			(size 1.8 3.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "Net-(J2-Pin_11)")
			(pinfunction "Pin_11")
			(pintype "passive")
		)
		(pad "12" thru_hole oval
			(at 41.91 0)
			(size 1.8 3.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "Net-(J2-Pin_12)")
			(pinfunction "Pin_12")
			(pintype "passive")
		)
		(pad "13" thru_hole oval
			(at 45.72 0)
			(size 1.8 3.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "Net-(J2-Pin_13)")
			(pinfunction "Pin_13")
			(pintype "passive")
		)
		(pad "14" thru_hole oval
			(at 49.53 0)
			(size 1.8 3.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "Net-(J2-Pin_14)")
			(pinfunction "Pin_14")
			(pintype "passive")
		)
		(pad "15" thru_hole oval
			(at 53.34 0)
			(size 1.8 3.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "Net-(J2-Pin_15)")
			(pinfunction "Pin_15")
			(pintype "passive")
		)
		(pad "16" thru_hole oval
			(at 57.15 0)
			(size 1.8 3.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_Phoenix_MC.3dshapes/PhoenixContact_MCV_1,5_16-G-3.81_1x16_P3.81mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TerminalBlock_Phoenix:TerminalBlock_Phoenix_MKDS-1,5-2_1x02_P5.00mm_Horizontal"
		(layer "F.Cu")
		(at 72.5 23.195 180)
		(descr "Terminal Block Phoenix MKDS-1,5-2, 2 pins, pitch 5mm, size 10x9.8mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/100425.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix")
		(tags "THT Terminal Block Phoenix MKDS-1,5-2 pitch 5mm size 10x9.8mm^2 drill 1.3mm pad 2.6mm")
		(property "Reference" "J4"
			(at 1 5.695 180)
			(layer "F.SilkS")
		)
		(property "Value" "Screw_Terminal_01x02"
			(at 2.5 5.66 180)
			(layer "F.Fab")
		)
		(property "Footprint" "TerminalBlock_Phoenix:TerminalBlock_Phoenix_MKDS-1,5-2_1x02_P5.00mm_Horizontal"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.lcsc.com/datasheet/lcsc_datasheet_1912251636_Ningbo-Kangnex-Elec-WJ500V-5-08-2P_C8465.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic screw terminal, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Website" "https://www.lcsc.com/product-detail/span-style-background-color-ff0-Screw-span-span-style-background-color-ff0-Terminal-span-Blocks_Ningbo-Kangnex-Elec-WJ500V-5-08-2P_C8465.html"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Vendor" "LCSC"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price" ".08"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" "WJ500V-5.08-3P"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(sheetname "Root")
		(sheetfile "MTA_Egress_Plugboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 3.2 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "Net-(J1-Pin_6)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5 0 180)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "Net-(J1-Pin_4)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MKDS-1,5-2_1x02_P5.00mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_line
		(start 0 0)
		(end 95.25 0)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 57.15 15.5)
		(end 59.049 15.5)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 95.25 0)
		(end 95.25 38.1)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 0 0)
		(end 0 38.1)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 0 38.1)
		(end 95.25 38.1)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 6.35 15.5)
		(end 8.249 15.5)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_text "7"
		(at 26.6 31 0)
		(layer "F.SilkS")
	)
	(gr_text "IN"
		(at 93 25.9 90)
		(layer "F.SilkS")
	)
	(gr_text "11"
		(at 41.8 31 0)
		(layer "F.SilkS")
	)
	(gr_text "8"
		(at 30.4 31 0)
		(layer "F.SilkS")
	)
	(gr_text "-"
		(at 89 23 90)
		(layer "F.SilkS")
	)
	(gr_text "+"
		(at 89.1 17.9 90)
		(layer "F.SilkS")
	)
	(gr_text "15"
		(at 57 31 0)
		(layer "F.SilkS")
	)
	(gr_text "+"
		(at 89 7.9 90)
		(layer "F.SilkS")
	)
	(gr_text "A"
		(at 67.4 31.1 0)
		(layer "F.SilkS")
	)
	(gr_text "9"
		(at 34.3 31 0)
		(layer "F.SilkS")
	)
	(gr_text "-"
		(at 89 12.9 90)
		(layer "F.SilkS")
	)
	(gr_text "12"
		(at 45.7 31 0)
		(layer "F.SilkS")
	)
	(gr_text "OUT"
		(at 93.2 10.4 90)
		(layer "F.SilkS")
	)
	(gr_text "UNPD\nKS"
		(at 32.5 35.5 0)
		(layer "F.SilkS")
	)
	(gr_text "16"
		(at 60.9 31.1 0)
		(layer "F.SilkS")
	)
	(gr_text "GATE\nOPNR"
		(at 55 35.5 0)
		(layer "F.SilkS")
	)
	(gr_text "14"
		(at 53.1 31 0)
		(layer "F.SilkS")
	)
	(gr_text "3"
		(at 11.5 31 0)
		(layer "F.SilkS")
	)
	(gr_text "10"
		(at 38 31 0)
		(layer "F.SilkS")
	)
	(gr_text "C   NC  NO"
		(at 15.5 33.5 0)
		(layer "F.SilkS")
	)
	(gr_text "B"
		(at 72.2 31.1 0)
		(layer "F.SilkS")
	)
	(gr_text "DSS"
		(at 25 34 0)
		(layer "F.SilkS")
	)
	(gr_text "2"
		(at 7.5 31 0)
		(layer "F.SilkS")
	)
	(gr_text "4"
		(at 15 31 0)
		(layer "F.SilkS")
	)
	(gr_text "13"
		(at 49.5 31 0)
		(layer "F.SilkS")
	)
	(gr_text "1"
		(at 2 5.5 90)
		(layer "F.SilkS")
	)
	(gr_text "+"
		(at 89.1 2.8 90)
		(layer "F.SilkS")
	)
	(gr_text "6"
		(at 22.8 31 0)
		(layer "F.SilkS")
	)
	(gr_text "AFAS\nSGNL"
		(at 47.5 35.5 0)
		(layer "F.SilkS")
	)
	(gr_text "MAG\nSW"
		(at 5.5 35.5 0)
		(layer "F.SilkS")
	)
	(gr_text "+"
		(at 89.1 28.2 90)
		(layer "F.SilkS")
	)
	(gr_text "RTU"
		(at 70 35.7 0)
		(layer "F.SilkS")
	)
	(gr_text "5"
		(at 19 31 0)
		(layer "F.SilkS")
	)
	(gr_text "1"
		(at 4 31 0)
		(layer "F.SilkS")
	)
	(gr_text "PAID\nKS"
		(at 40 35.5 0)
		(layer "F.SilkS")
	)
	(gr_text "T-Bar SW"
		(at 15 36 0)
		(layer "F.SilkS")
	)
)
