(kicad_pcb (version 20171130) (host pcbnew "(5.1.10)-1")
  (general
    (thickness 1.6)
    (drawings 7)
    (tracks 134)
    (zones 0)
    (modules 22)
    (nets 22)
  )
  (page A4)
  (title_block
    (title "Controls - Eurorack Dual Envelope Module")
    (date 2021-12-12)
    (rev 1.1)
    (company "Len Popp")
    (comment 1 "Copyright © 2021 Len Popp CC BY")
    (comment 2 "Eurorack digital ADSR envelope module")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.381)
    (user_trace_width 0.762)
    (trace_clearance 0.1524)
    (zone_clearance 0.2032)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.762)
    (via_drill 0.381)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.8 1.8)
    (pad_drill 0.9)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFF77F)
    (pcbplotparams
      (layerselection 0x01030_ffffffff)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers/controls/"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +5V)
  (net 3 "Net-(J2-PadTN)")
  (net 4 IN-POT-A-1)
  (net 5 IN-GATE-1)
  (net 6 IN-POT-D-1)
  (net 7 OUT-1)
  (net 8 IN-POT-S-1)
  (net 9 LED-1)
  (net 10 IN-POT-R-1)
  (net 11 IN-SW-LOGLIN-1)
  (net 12 IN-SW-LOGLIN-2)
  (net 13 IN-POT-A-2)
  (net 14 LED-2)
  (net 15 IN-POT-D-2)
  (net 16 IN-POT-S-2)
  (net 17 IN-GATE-2)
  (net 18 IN-POT-R-2)
  (net 19 OUT-2)
  (net 20 IN-GATE-BUS)
  (net 21 "Net-(J4-PadTN)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.762)
    (via_drill 0.381)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net GND)
    (add_net IN-GATE-1)
    (add_net IN-GATE-2)
    (add_net IN-GATE-BUS)
    (add_net IN-POT-A-1)
    (add_net IN-POT-A-2)
    (add_net IN-POT-D-1)
    (add_net IN-POT-D-2)
    (add_net IN-POT-R-1)
    (add_net IN-POT-R-2)
    (add_net IN-POT-S-1)
    (add_net IN-POT-S-2)
    (add_net IN-SW-LOGLIN-1)
    (add_net IN-SW-LOGLIN-2)
    (add_net LED-1)
    (add_net LED-2)
    (add_net "Net-(J2-PadTN)")
    (add_net "Net-(J4-PadTN)")
    (add_net OUT-1)
    (add_net OUT-2)
  )
  (module -lmp-synth:Jack_3.5mm_QingPu_WQP-PJ398SM_Vertical (layer F.Cu) (tedit 61B64B5F)
    (at 106.4006 132.334)
    (descr "TS mono 3.5mm, vertical, Thonkiconn, PCB mount, (http://www.qingpu-electronics.com/en/products/WQP-PJ398SM-362.html)")
    (tags "WQP-PJ398SM WQP-PJ301M-12 TS 3.5mm mono vertical jack thonkiconn qingpu")
    (fp_text reference J2 (at -4.03 1.08 180) (layer F.SilkS))
    (fp_text value WQP-PJ398 (at 0 5 180) (layer F.Fab))
    (fp_text user %R (at 0 8 180) (layer F.Fab))
    (pad T thru_hole oval (at 0 11.4 180) (size 2.75 1.75) (drill oval 1.65 0.65) (layers *.Cu *.Mask)
      (net 7 OUT-1))
    (pad TN thru_hole oval (at 0 3.1 180) (size 2.75 1.75) (drill oval 1.65 0.65) (layers *.Cu *.Mask)
      (net 3 "Net-(J2-PadTN)"))
    (pad S thru_hole oval (at 0 0 180) (size 2.75 1.75) (drill oval 1.65 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_Audio.3dshapes/Jack_3.5mm_QingPu_WQP-PJ398SM_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module -lmp-synth:Jack_3.5mm_QingPu_WQP-PJ398SM_Vertical (layer F.Cu) (tedit 61B64B5F)
    (at 134.9756 132.334)
    (descr "TS mono 3.5mm, vertical, Thonkiconn, PCB mount, (http://www.qingpu-electronics.com/en/products/WQP-PJ398SM-362.html)")
    (tags "WQP-PJ398SM WQP-PJ301M-12 TS 3.5mm mono vertical jack thonkiconn qingpu")
    (fp_text reference J4 (at -4.03 1.08 180) (layer F.SilkS))
    (fp_text value WQP-PJ398 (at 0 5 180) (layer F.Fab))
    (fp_text user %R (at 0 8 180) (layer F.Fab))
    (pad T thru_hole oval (at 0 11.4 180) (size 2.75 1.75) (drill oval 1.65 0.65) (layers *.Cu *.Mask)
      (net 19 OUT-2))
    (pad TN thru_hole oval (at 0 3.1 180) (size 2.75 1.75) (drill oval 1.65 0.65) (layers *.Cu *.Mask)
      (net 21 "Net-(J4-PadTN)"))
    (pad S thru_hole oval (at 0 0 180) (size 2.75 1.75) (drill oval 1.65 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_Audio.3dshapes/Jack_3.5mm_QingPu_WQP-PJ398SM_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module -lmp-synth:Jack_3.5mm_QingPu_WQP-PJ398SM_Vertical (layer F.Cu) (tedit 61B64B5F)
    (at 106.4006 118.2878)
    (descr "TS mono 3.5mm, vertical, Thonkiconn, PCB mount, (http://www.qingpu-electronics.com/en/products/WQP-PJ398SM-362.html)")
    (tags "WQP-PJ398SM WQP-PJ301M-12 TS 3.5mm mono vertical jack thonkiconn qingpu")
    (fp_text reference J1 (at -4.03 1.08 180) (layer F.SilkS))
    (fp_text value WQP-PJ398 (at 0 5 180) (layer F.Fab))
    (fp_text user %R (at 0 8 180) (layer F.Fab))
    (pad T thru_hole oval (at 0 11.4 180) (size 2.75 1.75) (drill oval 1.65 0.65) (layers *.Cu *.Mask)
      (net 5 IN-GATE-1))
    (pad TN thru_hole oval (at 0 3.1 180) (size 2.75 1.75) (drill oval 1.65 0.65) (layers *.Cu *.Mask)
      (net 20 IN-GATE-BUS))
    (pad S thru_hole oval (at 0 0 180) (size 2.75 1.75) (drill oval 1.65 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_Audio.3dshapes/Jack_3.5mm_QingPu_WQP-PJ398SM_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module -lmp-synth:Jack_3.5mm_QingPu_WQP-PJ398SM_Vertical (layer F.Cu) (tedit 61B64B5F)
    (at 134.9756 118.2878)
    (descr "TS mono 3.5mm, vertical, Thonkiconn, PCB mount, (http://www.qingpu-electronics.com/en/products/WQP-PJ398SM-362.html)")
    (tags "WQP-PJ398SM WQP-PJ301M-12 TS 3.5mm mono vertical jack thonkiconn qingpu")
    (fp_text reference J3 (at -4.03 1.08 180) (layer F.SilkS))
    (fp_text value WQP-PJ398 (at 0 5 180) (layer F.Fab))
    (fp_text user %R (at 0 8 180) (layer F.Fab))
    (pad T thru_hole oval (at 0 11.4 180) (size 2.75 1.75) (drill oval 1.65 0.65) (layers *.Cu *.Mask)
      (net 17 IN-GATE-2))
    (pad TN thru_hole oval (at 0 3.1 180) (size 2.75 1.75) (drill oval 1.65 0.65) (layers *.Cu *.Mask)
      (net 5 IN-GATE-1))
    (pad S thru_hole oval (at 0 0 180) (size 2.75 1.75) (drill oval 1.65 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_Audio.3dshapes/Jack_3.5mm_QingPu_WQP-PJ398SM_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module -lmp-misc:SW_SPDT_THT_2.54 (layer F.Cu) (tedit 60B83C48)
    (at 132.715 112.649 270)
    (descr "Switch SPDT THT 2.54")
    (tags "SWITCH TOGGLE ILLUM SPDT NKK")
    (fp_text reference SW2 (at 0 8.509 180) (layer F.SilkS))
    (fp_text value SPDT (at 0 7.3 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.2 90) (layer F.Fab))
    (pad 3 thru_hole circle (at 0 5.08 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 0 2.54 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask)
      (net 12 IN-SW-LOGLIN-2))
    (model ${KISYS3DMOD}/Button_Switch_THT.3dshapes/SW_NKK_G1xJP.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module -lmp-synth:Potentiometer_Alpha_RD901F-40-00D_Single_Vertical (layer F.Cu) (tedit 5C6C6C14)
    (at 127.6858 106.68 90)
    (descr "Potentiometer, vertical, 9mm, single, http://www.taiwanalpha.com.tw/downloads?target=products&id=113")
    (tags "potentiometer vertical 9mm single")
    (fp_text reference RV8 (at -2.413 2.4892) (layer F.SilkS))
    (fp_text value 100K (at 0 9.86 270) (layer F.Fab))
    (fp_text user %R (at 7.62 2.54 90) (layer F.Fab))
    (pad "" thru_hole oval (at 7.5 -2.3 180) (size 2.72 3.24) (drill oval 1.1 1.8) (layers *.Cu *.Mask))
    (pad "" thru_hole oval (at 7.5 7.3 180) (size 2.72 3.24) (drill oval 1.1 1.8) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 0 5 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 2 thru_hole circle (at 0 2.5 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 18 IN-POT-R-2))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Potentiometer_THT.3dshapes/Potentiometer_Alpha_RD901F-40-00D_Single_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module -lmp-misc:Logo_OSHW (layer F.Cu) (tedit 60F495A1)
    (at 126.365 142.113)
    (descr "Open Source Hardware logo")
    (tags "Open Source Hardware logo")
    (attr virtual)
    (fp_text reference G4 (at 0 0) (layer F.SilkS) hide)
    (fp_text value Logo_OSHW (at 0.75 0) (layer F.SilkS) hide)
  )
  (module -lmp-synth:Potentiometer_Alpha_RD901F-40-00D_Single_Vertical (layer F.Cu) (tedit 5C6C6C14)
    (at 108.6358 68.58 90)
    (descr "Potentiometer, vertical, 9mm, single, http://www.taiwanalpha.com.tw/downloads?target=products&id=113")
    (tags "potentiometer vertical 9mm single")
    (fp_text reference RV2 (at -2.286 2.4892) (layer F.SilkS))
    (fp_text value 100K (at 0 9.86 270) (layer F.Fab))
    (fp_text user %R (at 7.62 2.54 90) (layer F.Fab))
    (pad "" thru_hole oval (at 7.5 -2.3 180) (size 2.72 3.24) (drill oval 1.1 1.8) (layers *.Cu *.Mask))
    (pad "" thru_hole oval (at 7.5 7.3 180) (size 2.72 3.24) (drill oval 1.1 1.8) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 0 5 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 2 thru_hole circle (at 0 2.5 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 6 IN-POT-D-1))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Potentiometer_THT.3dshapes/Potentiometer_Alpha_RD901F-40-00D_Single_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module -lmp-misc:SW_SPDT_THT_2.54 (layer F.Cu) (tedit 60B83C48)
    (at 113.665 112.649 270)
    (descr "Switch SPDT THT 2.54")
    (tags "SWITCH TOGGLE ILLUM SPDT NKK")
    (fp_text reference SW1 (at 0 8.509 180) (layer F.SilkS))
    (fp_text value SPDT (at 0 7.3 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.2 90) (layer F.Fab))
    (pad 3 thru_hole circle (at 0 5.08 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 0 2.54 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask)
      (net 11 IN-SW-LOGLIN-1))
    (model ${KISYS3DMOD}/Button_Switch_THT.3dshapes/SW_NKK_G1xJP.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D5.0mm (layer F.Cu) (tedit 5995936A)
    (at 115.8875 130.5814 270)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D3 (at 5.461 0.0635 180) (layer F.SilkS))
    (fp_text value LED_5mm_Blue (at 1.27 3.96 90) (layer F.Fab))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 9 LED-1))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module -lmp-synth:Potentiometer_Alpha_RD901F-40-00D_Single_Vertical (layer F.Cu) (tedit 5C6C6C14)
    (at 108.6358 106.68 90)
    (descr "Potentiometer, vertical, 9mm, single, http://www.taiwanalpha.com.tw/downloads?target=products&id=113")
    (tags "potentiometer vertical 9mm single")
    (fp_text reference RV4 (at -2.413 2.4892) (layer F.SilkS))
    (fp_text value 100K (at 0 9.86 270) (layer F.Fab))
    (fp_text user %R (at 7.62 2.54 90) (layer F.Fab))
    (pad "" thru_hole oval (at 7.5 -2.3 180) (size 2.72 3.24) (drill oval 1.1 1.8) (layers *.Cu *.Mask))
    (pad "" thru_hole oval (at 7.5 7.3 180) (size 2.72 3.24) (drill oval 1.1 1.8) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 0 5 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 2 thru_hole circle (at 0 2.5 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 10 IN-POT-R-1))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Potentiometer_THT.3dshapes/Potentiometer_Alpha_RD901F-40-00D_Single_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module -lmp-synth:Potentiometer_Alpha_RD901F-40-00D_Single_Vertical (layer F.Cu) (tedit 5C6C6C14)
    (at 108.6358 87.63 90)
    (descr "Potentiometer, vertical, 9mm, single, http://www.taiwanalpha.com.tw/downloads?target=products&id=113")
    (tags "potentiometer vertical 9mm single")
    (fp_text reference RV3 (at -2.286 2.4892) (layer F.SilkS))
    (fp_text value 100K (at 0 9.86 270) (layer F.Fab))
    (fp_text user %R (at 7.62 2.54 90) (layer F.Fab))
    (pad "" thru_hole oval (at 7.5 -2.3 180) (size 2.72 3.24) (drill oval 1.1 1.8) (layers *.Cu *.Mask))
    (pad "" thru_hole oval (at 7.5 7.3 180) (size 2.72 3.24) (drill oval 1.1 1.8) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 0 5 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 2 thru_hole circle (at 0 2.5 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 8 IN-POT-S-1))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Potentiometer_THT.3dshapes/Potentiometer_Alpha_RD901F-40-00D_Single_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D5.0mm (layer F.Cu) (tedit 5995936A)
    (at 125.4125 130.5814 270)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D5 (at 5.461 0.0635 180) (layer F.SilkS))
    (fp_text value LED_5mm_Blue (at 1.27 3.96 90) (layer F.Fab))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 14 LED-2))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module -lmp-synth:Potentiometer_Alpha_RD901F-40-00D_Single_Vertical (layer F.Cu) (tedit 5C6C6C14)
    (at 108.6358 49.53 90)
    (descr "Potentiometer, vertical, 9mm, single, http://www.taiwanalpha.com.tw/downloads?target=products&id=113")
    (tags "potentiometer vertical 9mm single")
    (fp_text reference RV1 (at -2.286 2.4892) (layer F.SilkS))
    (fp_text value 100K (at 0 9.86 270) (layer F.Fab))
    (fp_text user %R (at 7.62 2.54 90) (layer F.Fab))
    (pad "" thru_hole oval (at 7.5 -2.3 180) (size 2.72 3.24) (drill oval 1.1 1.8) (layers *.Cu *.Mask))
    (pad "" thru_hole oval (at 7.5 7.3 180) (size 2.72 3.24) (drill oval 1.1 1.8) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 0 5 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 2 thru_hole circle (at 0 2.5 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 4 IN-POT-A-1))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Potentiometer_THT.3dshapes/Potentiometer_Alpha_RD901F-40-00D_Single_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module -lmp-synth:Potentiometer_Alpha_RD901F-40-00D_Single_Vertical (layer F.Cu) (tedit 5C6C6C14)
    (at 127.6858 68.58 90)
    (descr "Potentiometer, vertical, 9mm, single, http://www.taiwanalpha.com.tw/downloads?target=products&id=113")
    (tags "potentiometer vertical 9mm single")
    (fp_text reference RV6 (at -2.286 2.4892) (layer F.SilkS))
    (fp_text value 100K (at 0 9.86 270) (layer F.Fab))
    (fp_text user %R (at 7.62 2.54 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 0 2.5 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 15 IN-POT-D-2))
    (pad 3 thru_hole circle (at 0 5 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad "" thru_hole oval (at 7.5 7.3 180) (size 2.72 3.24) (drill oval 1.1 1.8) (layers *.Cu *.Mask))
    (pad "" thru_hole oval (at 7.5 -2.3 180) (size 2.72 3.24) (drill oval 1.1 1.8) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Potentiometer_THT.3dshapes/Potentiometer_Alpha_RD901F-40-00D_Single_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module -lmp-synth:Potentiometer_Alpha_RD901F-40-00D_Single_Vertical (layer F.Cu) (tedit 5C6C6C14)
    (at 127.6858 87.63 90)
    (descr "Potentiometer, vertical, 9mm, single, http://www.taiwanalpha.com.tw/downloads?target=products&id=113")
    (tags "potentiometer vertical 9mm single")
    (fp_text reference RV7 (at -2.286 2.4892) (layer F.SilkS))
    (fp_text value 100K (at 0 9.86 270) (layer F.Fab))
    (fp_text user %R (at 7.62 2.54 90) (layer F.Fab))
    (pad "" thru_hole oval (at 7.5 -2.3 180) (size 2.72 3.24) (drill oval 1.1 1.8) (layers *.Cu *.Mask))
    (pad "" thru_hole oval (at 7.5 7.3 180) (size 2.72 3.24) (drill oval 1.1 1.8) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 0 5 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 2 thru_hole circle (at 0 2.5 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 16 IN-POT-S-2))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Potentiometer_THT.3dshapes/Potentiometer_Alpha_RD901F-40-00D_Single_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module -lmp-misc:Logo_CC_BY (layer F.Cu) (tedit 0)
    (at 117.348 142.24)
    (fp_text reference G2 (at 0 0) (layer F.SilkS) hide)
    (fp_text value Logo_CC_BY (at 0.75 0) (layer F.SilkS) hide)
  )
  (module -lmp-synth:Potentiometer_Alpha_RD901F-40-00D_Single_Vertical (layer F.Cu) (tedit 5C6C6C14)
    (at 127.6858 49.53 90)
    (descr "Potentiometer, vertical, 9mm, single, http://www.taiwanalpha.com.tw/downloads?target=products&id=113")
    (tags "potentiometer vertical 9mm single")
    (fp_text reference RV5 (at -2.286 2.4892) (layer F.SilkS))
    (fp_text value 100K (at 0 9.86 270) (layer F.Fab))
    (fp_text user %R (at 7.62 2.54 90) (layer F.Fab))
    (pad "" thru_hole oval (at 7.5 -2.3 180) (size 2.72 3.24) (drill oval 1.1 1.8) (layers *.Cu *.Mask))
    (pad "" thru_hole oval (at 7.5 7.3 180) (size 2.72 3.24) (drill oval 1.1 1.8) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 0 5 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 2 thru_hole circle (at 0 2.5 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 13 IN-POT-A-2))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Potentiometer_THT.3dshapes/Potentiometer_Alpha_RD901F-40-00D_Single_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module -lmp-holes:MountingHole_PCB_3.2mm_M3 (layer F.Cu) (tedit 61A52D67)
    (at 137.836 53.34)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (clearance 1.15)
    (attr virtual)
    (fp_text reference H2 (at 0 0) (layer F.SilkS) hide)
    (fp_text value MountingHole_M3 (at 0 0.009) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module -lmp-holes:MountingHole_PCB_3.2mm_M3 (layer F.Cu) (tedit 61A52D67)
    (at 103.124 53.34)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (clearance 1.15)
    (attr virtual)
    (fp_text reference H1 (at 0 0) (layer F.SilkS) hide)
    (fp_text value MountingHole_M3 (at 0 0.009) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x11_P2.54mm_Vertical (layer B.Cu) (tedit 5A19A42E)
    (at 101.6 60.96 180)
    (descr "Through hole straight socket strip, 1x11, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x11 2.54mm single row")
    (fp_text reference J5 (at 0 2.77) (layer B.SilkS))
    (fp_text value Conn_Front_Left_Top (at 0 -28.17) (layer B.Fab))
    (fp_text user %R (at 0 -12.7 270) (layer B.Fab))
    (pad 11 thru_hole oval (at 0 -25.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 IN-GATE-BUS))
    (pad 10 thru_hole oval (at 0 -22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 OUT-1))
    (pad 9 thru_hole oval (at 0 -20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 8 thru_hole oval (at 0 -17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 IN-POT-S-1))
    (pad 7 thru_hole oval (at 0 -15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 IN-POT-A-1))
    (pad 6 thru_hole oval (at 0 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 IN-POT-D-1))
    (pad 5 thru_hole oval (at 0 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 IN-POT-A-2))
    (pad 4 thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 IN-POT-D-2))
    (pad 3 thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 IN-POT-R-2))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 IN-POT-R-1))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 IN-GATE-1))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x11_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x08_P2.54mm_Vertical (layer B.Cu) (tedit 5A19A420)
    (at 139.36 96.52 180)
    (descr "Through hole straight socket strip, 1x08, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x08 2.54mm single row")
    (fp_text reference J7 (at 0 2.77) (layer B.SilkS))
    (fp_text value Conn_Front_Right (at 0 -20.55) (layer B.Fab))
    (fp_text user %R (at 0 -8.89 270) (layer B.Fab))
    (pad 8 thru_hole oval (at 0 -17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 OUT-2))
    (pad 7 thru_hole oval (at 0 -15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 LED-2))
    (pad 6 thru_hole oval (at 0 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 IN-SW-LOGLIN-2))
    (pad 5 thru_hole oval (at 0 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 IN-GATE-2))
    (pad 3 thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 LED-1))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 IN-SW-LOGLIN-1))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 IN-POT-S-2))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "rev 1.1" (at 120.65 122.809) (layer F.SilkS))
  (gr_text "© 2021 Len Popp" (at 112.903 138.43) (layer F.SilkS))
  (gr_text 2Shapes (at 120.65 119.38) (layer F.SilkS))
  (gr_line (start 140.63 36.83) (end 140.63 145.034) (layer Edge.Cuts) (width 0.3556))
  (gr_line (start 100.33 145.034) (end 100.33 36.83) (layer Edge.Cuts) (width 0.3556))
  (gr_line (start 100.33 36.83) (end 140.63 36.83) (layer Edge.Cuts) (width 0.3556))
  (gr_line (start 140.63 145.034) (end 100.33 145.034) (layer Edge.Cuts) (width 0.3556))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2032))
    (min_thickness 0.2032)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 141.605 145.415) (xy 99.695 145.415) (xy 99.695 36.195) (xy 141.605 36.195)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2032))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 134.9756 140.311) (xy 135.4391 140.2376) (xy 135.8573 140.0245) (xy 136.1891 139.6927) (xy 136.4022 139.2745)
        (xy 136.4756 138.811) (xy 136.4022 138.3475) (xy 136.1891 137.9293) (xy 135.8573 137.5975) (xy 135.4391 137.3844)
        (xy 134.9756 137.311) (xy 134.5121 137.3844) (xy 134.0939 137.5975) (xy 133.7621 137.9293) (xy 133.549 138.3475)
        (xy 133.4756 138.811) (xy 133.549 139.2745) (xy 133.7621 139.6927) (xy 134.0939 140.0245) (xy 134.5121 140.2376)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2032))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 106.3992 140.311) (xy 106.8627 140.2376) (xy 107.2809 140.0245) (xy 107.6127 139.6927) (xy 107.8258 139.2745)
        (xy 107.8992 138.811) (xy 107.8258 138.3475) (xy 107.6127 137.9293) (xy 107.2809 137.5975) (xy 106.8627 137.3844)
        (xy 106.3992 137.311) (xy 105.9357 137.3844) (xy 105.5175 137.5975) (xy 105.1857 137.9293) (xy 104.9726 138.3475)
        (xy 104.8992 138.811) (xy 104.9726 139.2745) (xy 105.1857 139.6927) (xy 105.5175 140.0245) (xy 105.9357 140.2376)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2032))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 134.9813 126.2721) (xy 135.4448 126.1987) (xy 135.863 125.9856) (xy 136.1948 125.6538) (xy 136.4079 125.2356)
        (xy 136.4813 124.7721) (xy 136.4079 124.3086) (xy 136.1948 123.8904) (xy 135.863 123.5586) (xy 135.4448 123.3455)
        (xy 134.9813 123.2721) (xy 134.5178 123.3455) (xy 134.0996 123.5586) (xy 133.7678 123.8904) (xy 133.5547 124.3086)
        (xy 133.4813 124.7721) (xy 133.5547 125.2356) (xy 133.7678 125.6538) (xy 134.0996 125.9856) (xy 134.5178 126.1987)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2032))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 106.3695 126.2467) (xy 106.833 126.1733) (xy 107.2512 125.9602) (xy 107.583 125.6284) (xy 107.7961 125.2102)
        (xy 107.8695 124.7467) (xy 107.7961 124.2832) (xy 107.583 123.865) (xy 107.2512 123.5332) (xy 106.833 123.3201)
        (xy 106.3695 123.2467) (xy 105.906 123.3201) (xy 105.4878 123.5332) (xy 105.156 123.865) (xy 104.9429 124.2832)
        (xy 104.8695 124.7467) (xy 104.9429 125.2102) (xy 105.156 125.6284) (xy 105.4878 125.9602) (xy 105.906 126.1733)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2032))
    (min_thickness 0.2032)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 141.605 145.415) (xy 99.695 145.415) (xy 99.695 36.195) (xy 141.605 36.195)
      )
    )
  )
)
