(kicad_pcb (version 20171130) (host pcbnew "(5.0.0)")
  (general
    (thickness 1.6)
    (drawings 10)
    (tracks 6)
    (zones 0)
    (modules 4)
    (nets 4)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.254)
    (user_trace_width 0.381)
    (user_trace_width 0.635)
    (user_trace_width 1.016)
    (user_trace_width 1.27)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 5 5)
    (pad_drill 2.75)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad1)")
  (net 2 "Net-(J1-Pad2)")
  (net 3 "Net-(J1-Pad3)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
  )
  (module modules:CK_MINI_SLIDE_SWITCH (layer F.Cu) (tedit 5BDA6A30)
    (at 147 104 270)
    (fp_text reference SW1 (at 0.1 -1.3 270) (layer F.SilkS) hide)
    (fp_text value SW_SPDT (at 0 -3.4 270) (layer F.Fab) hide)
    (pad "" thru_hole oval (at -4.1 0 270) (size 2 4) (drill 1.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -2 0 270) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad 3 thru_hole circle (at 2 0 270) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad3)"))
    (pad 2 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad "" thru_hole oval (at 4.1 0 270) (size 2 4) (drill 1.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.5mm_Pad (layer F.Cu) (tedit 5BDA7CD8)
    (at 145.5 113)
    (descr "Mounting Hole 2.5mm")
    (tags "mounting hole 2.5mm")
    (attr virtual)
    (fp_text reference "" (at 0 -3.5) (layer F.SilkS))
    (fp_text value "" (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 2.75) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.5mm_Pad (layer F.Cu) (tedit 5BDA7CCB)
    (at 145.5 95)
    (descr "Mounting Hole 2.5mm")
    (tags "mounting hole 2.5mm")
    (attr virtual)
    (fp_text reference "" (at 0 -3.5) (layer F.SilkS))
    (fp_text value "" (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 2.75) (layers *.Cu *.Mask))
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 5BDA68A1)
    (at 142 101.5)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J1 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value Conn_01x03 (at 0 7.41) (layer F.Fab) hide)
    (fp_text user %R (at 0 2.54 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad3)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (dimension 1.5 (width 0.3) (layer Cmts.User)
    (gr_text "1.500 mm" (at 146.25 87.3) (layer Cmts.User))
    (feature1 (pts (xy 145.5 99.9) (xy 145.5 88.813579)))
    (feature2 (pts (xy 147 99.9) (xy 147 88.813579)))
    (crossbar (pts (xy 147 89.4) (xy 145.5 89.4)))
    (arrow1a (pts (xy 145.5 89.4) (xy 146.626504 88.813579)))
    (arrow1b (pts (xy 145.5 89.4) (xy 146.626504 89.986421)))
    (arrow2a (pts (xy 147 89.4) (xy 145.873496 88.813579)))
    (arrow2b (pts (xy 147 89.4) (xy 145.873496 89.986421)))
  )
  (dimension 4.3 (width 0.3) (layer Cmts.User)
    (gr_text "4.300 mm" (at 146.95 118) (layer Cmts.User))
    (feature1 (pts (xy 149.1 108.3) (xy 149.1 116.486421)))
    (feature2 (pts (xy 144.8 108.3) (xy 144.8 116.486421)))
    (crossbar (pts (xy 144.8 115.9) (xy 149.1 115.9)))
    (arrow1a (pts (xy 149.1 115.9) (xy 147.973496 116.486421)))
    (arrow1b (pts (xy 149.1 115.9) (xy 147.973496 115.313579)))
    (arrow2a (pts (xy 144.8 115.9) (xy 145.926504 116.486421)))
    (arrow2b (pts (xy 144.8 115.9) (xy 145.926504 115.313579)))
  )
  (dimension 8.6 (width 0.3) (layer Cmts.User)
    (gr_text "8.600 mm" (at 152.7 103.9 270) (layer Cmts.User))
    (feature1 (pts (xy 149.2 108.2) (xy 151.186421 108.2)))
    (feature2 (pts (xy 149.2 99.6) (xy 151.186421 99.6)))
    (crossbar (pts (xy 150.6 99.6) (xy 150.6 108.2)))
    (arrow1a (pts (xy 150.6 108.2) (xy 150.013579 107.073496)))
    (arrow1b (pts (xy 150.6 108.2) (xy 151.186421 107.073496)))
    (arrow2a (pts (xy 150.6 99.6) (xy 150.013579 100.726504)))
    (arrow2b (pts (xy 150.6 99.6) (xy 151.186421 100.726504)))
  )
  (dimension 24 (width 0.3) (layer Cmts.User)
    (gr_text "24.000 mm" (at 155.7 104 90) (layer Cmts.User))
    (feature1 (pts (xy 150.6 92) (xy 154.186421 92)))
    (feature2 (pts (xy 150.6 116) (xy 154.186421 116)))
    (crossbar (pts (xy 153.6 116) (xy 153.6 92)))
    (arrow1a (pts (xy 153.6 92) (xy 154.186421 93.126504)))
    (arrow1b (pts (xy 153.6 92) (xy 153.013579 93.126504)))
    (arrow2a (pts (xy 153.6 116) (xy 154.186421 114.873496)))
    (arrow2b (pts (xy 153.6 116) (xy 153.013579 114.873496)))
  )
  (dimension 10 (width 0.3) (layer Cmts.User)
    (gr_text "10.000 mm" (at 145.6 121.5) (layer Cmts.User))
    (feature1 (pts (xy 140.6 116) (xy 140.6 119.986421)))
    (feature2 (pts (xy 150.6 116) (xy 150.6 119.986421)))
    (crossbar (pts (xy 150.6 119.4) (xy 140.6 119.4)))
    (arrow1a (pts (xy 140.6 119.4) (xy 141.726504 118.813579)))
    (arrow1b (pts (xy 140.6 119.4) (xy 141.726504 119.986421)))
    (arrow2a (pts (xy 150.6 119.4) (xy 149.473496 118.813579)))
    (arrow2b (pts (xy 150.6 119.4) (xy 149.473496 119.986421)))
  )
  (dimension 18 (width 0.3) (layer Cmts.User)
    (gr_text "18.000 mm" (at 134.9 104 270) (layer Cmts.User))
    (feature1 (pts (xy 145 113) (xy 136.413579 113)))
    (feature2 (pts (xy 145 95) (xy 136.413579 95)))
    (crossbar (pts (xy 137 95) (xy 137 113)))
    (arrow1a (pts (xy 137 113) (xy 136.413579 111.873496)))
    (arrow1b (pts (xy 137 113) (xy 137.586421 111.873496)))
    (arrow2a (pts (xy 137 95) (xy 136.413579 96.126504)))
    (arrow2b (pts (xy 137 95) (xy 137.586421 96.126504)))
  )
  (gr_line (start 140.5 92) (end 150.5 92) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 140.5 116) (end 140.5 92) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 150.5 116) (end 140.5 116) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 150.5 92) (end 150.5 116) (angle 90) (layer Edge.Cuts) (width 0.15))
)
