(kicad_pcb (version 4) (host pcbnew 4.0.2-stable)
  (general
    (links 24)
    (no_connects 0)
    (area 139.624999 27.864999 180.415001 129.615001)
    (thickness 1.6)
    (drawings 4)
    (tracks 55)
    (zones 0)
    (modules 7)
    (nets 14)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /r+)
  (net 2 /r-)
  (net 3 +24V)
  (net 4 GNDPWR)
  (net 5 "Net-(350ma1-Pad5)")
  (net 6 GND)
  (net 7 /g+)
  (net 8 /g-)
  (net 9 "Net-(350ma2-Pad5)")
  (net 10 /b+)
  (net 11 /b-)
  (net 12 "Net-(350ma3-Pad5)")
  (net 13 VCC)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(350ma1-Pad5)")
    (add_net "Net-(350ma2-Pad5)")
    (add_net "Net-(350ma3-Pad5)")
    (add_net VCC)
  )
  (net_class led ""
    (clearance 0.2)
    (trace_width 1)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /b+)
    (add_net /b-)
    (add_net /g+)
    (add_net /g-)
    (add_net /r+)
    (add_net /r-)
  )
  (net_class power ""
    (clearance 0.2)
    (trace_width 1)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +24V)
    (add_net GNDPWR)
  )
  (module "lighting:350ma constant current xl4001" (layer F.Cu) (tedit 576E5BAE)
    (at 175.26 48.26 90)
    (fp_text reference 350ma1 (at 5.08 -12.7 90) (layer F.SilkS))
    (fp_text value Led_Driver (at 5.08 -15.24 90) (layer F.Fab))
    (pad 3 thru_hole rect (at 0 0 90) (size 4 4) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 1 /r+))
    (pad 4 thru_hole rect (at 12.7 0 90) (size 4 4) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 2 /r-))
    (pad 1 thru_hole rect (at 0 -30.48 90) (size 4 4) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 3 +24V))
    (pad 2 thru_hole rect (at 12.7 -30.48 90) (size 4 4) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 4 GNDPWR))
    (pad 5 thru_hole circle (at 0 -22.86 90) (size 2 2) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(350ma1-Pad5)"))
    (pad 6 thru_hole circle (at 0 -20.32 90) (size 2 2) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
  )
  (module "lighting:350ma constant current xl4001" (layer F.Cu) (tedit 576E5BAE)
    (at 175.26 76.2 90)
    (fp_text reference 350ma2 (at 5.08 -12.7 90) (layer F.SilkS))
    (fp_text value Led_Driver (at 5.08 -15.24 90) (layer F.Fab))
    (pad 3 thru_hole rect (at 0 0 90) (size 4 4) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 7 /g+))
    (pad 4 thru_hole rect (at 12.7 0 90) (size 4 4) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 8 /g-))
    (pad 1 thru_hole rect (at 0 -30.48 90) (size 4 4) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 3 +24V))
    (pad 2 thru_hole rect (at 12.7 -30.48 90) (size 4 4) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 4 GNDPWR))
    (pad 5 thru_hole circle (at 0 -22.86 90) (size 2 2) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(350ma2-Pad5)"))
    (pad 6 thru_hole circle (at 0 -20.32 90) (size 2 2) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
  )
  (module "lighting:350ma constant current xl4001" (layer F.Cu) (tedit 576E5BAE)
    (at 175.26 106.68 90)
    (fp_text reference 350ma3 (at 5.08 -12.7 90) (layer F.SilkS))
    (fp_text value Led_Driver (at 5.08 -15.24 90) (layer F.Fab))
    (pad 3 thru_hole rect (at 0 0 90) (size 4 4) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 10 /b+))
    (pad 4 thru_hole rect (at 12.7 0 90) (size 4 4) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 11 /b-))
    (pad 1 thru_hole rect (at 0 -30.48 90) (size 4 4) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 3 +24V))
    (pad 2 thru_hole rect (at 12.7 -30.48 90) (size 4 4) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 4 GNDPWR))
    (pad 5 thru_hole circle (at 0 -22.86 90) (size 2 2) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(350ma3-Pad5)"))
    (pad 6 thru_hole circle (at 0 -20.32 90) (size 2 2) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 56648415)
    (at 161.29 54.61 180)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R1 (at 5.32892 -3.50012 180) (layer F.SilkS))
    (fp_text value 10k (at 5.08 3.81 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 13 VCC))
    (pad 2 thru_hole circle (at 10.16 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 5 "Net-(350ma1-Pad5)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 56648415)
    (at 161.29 85.09 180)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R2 (at 5.32892 -3.50012 180) (layer F.SilkS))
    (fp_text value 10k (at 5.08 3.81 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 13 VCC))
    (pad 2 thru_hole circle (at 10.16 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 9 "Net-(350ma2-Pad5)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 56648415)
    (at 161.29 113.03 180)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R3 (at 5.32892 -3.50012 180) (layer F.SilkS))
    (fp_text value 10k (at 5.08 3.81 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 13 VCC))
    (pad 2 thru_hole circle (at 10.16 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 12 "Net-(350ma3-Pad5)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module lighting:rgb.breakout (layer F.Cu) (tedit 57764A8B)
    (at 150.114 124.206)
    (fp_text reference U1 (at 15.24 -5.08) (layer F.SilkS))
    (fp_text value rgb.breakout (at 5.08 -5.08) (layer F.Fab))
    (fp_text user b+ (at 19.05 -2.54 270) (layer F.SilkS))
    (fp_text user b- (at 19.05 0 270) (layer F.SilkS))
    (fp_text user g- (at 16.51 0 270) (layer F.SilkS))
    (fp_text user g+ (at 16.51 -2.54 270) (layer F.SilkS))
    (fp_text user r+ (at 13.97 -2.54 270) (layer F.SilkS))
    (fp_text user r- (at 13.97 0 270) (layer F.SilkS))
    (fp_text user vcc (at 6.35 0 90) (layer F.SilkS))
    (fp_text user gnd (at 3.81 0 90) (layer F.SilkS))
    (fp_text user V- (at 0 0) (layer F.SilkS))
    (fp_text user V+ (at 0 -2.54) (layer F.SilkS))
    (fp_text user b (at 8.89 -2.54) (layer F.SilkS))
    (fp_text user g (at 6.35 -2.54) (layer F.SilkS))
    (fp_text user r (at 3.81 -2.54) (layer F.SilkS))
    (pad 1 thru_hole rect (at -2.54 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 3 +24V))
    (pad 3 thru_hole circle (at 2.54 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 13 VCC))
    (pad 4 thru_hole circle (at 5.08 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
    (pad "" thru_hole circle (at 7.62 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
    (pad 9 thru_hole circle (at 12.7 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 2 /r-))
    (pad 11 thru_hole circle (at 15.24 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 8 /g-))
    (pad 13 thru_hole circle (at 17.78 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 11 /b-))
    (pad 2 thru_hole circle (at -2.54 -2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 4 GNDPWR))
    (pad 5 thru_hole circle (at 2.54 -2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(350ma1-Pad5)"))
    (pad 6 thru_hole circle (at 5.08 -2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(350ma2-Pad5)"))
    (pad 7 thru_hole circle (at 7.62 -2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(350ma3-Pad5)"))
    (pad 8 thru_hole circle (at 12.7 -2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 1 /r+))
    (pad 10 thru_hole circle (at 15.24 -2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 7 /g+))
    (pad 12 thru_hole circle (at 17.78 -2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 10 /b+))
  )
  (gr_line (start 180.34 27.94) (end 139.7 27.94) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 180.34 127) (end 180.34 27.94) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 139.7 127) (end 180.34 127) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 139.7 27.94) (end 139.7 127) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 3) (net_name +24V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 140.97 127) (xy 149.86 127) (xy 149.86 119.38) (xy 148.59 119.38) (xy 148.59 31.75)
        (xy 140.97 31.75)
      )
    )
  )
  (zone (net 4) (net_name GNDPWR) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 140.97 127) (xy 149.86 127) (xy 149.86 119.38) (xy 148.59 119.38) (xy 148.59 31.75)
        (xy 140.97 31.75)
      )
    )
  )
)
