<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.4.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="-0.635" x2="35.54" y2="-0.635" width="0" layer="20"/>
<wire x1="35.54" y1="-0.635" x2="35.54" y2="10.795" width="0" layer="20"/>
<wire x1="35.54" y1="10.795" x2="0" y2="10.795" width="0" layer="20"/>
<wire x1="0" y1="10.795" x2="0" y2="-0.635" width="0" layer="20"/>
<text>DALI power injector</text>
<text>16V</text>
<text>DALI</text>
<text>DALI</text>
<text>LM317 + 5R/1W + SS14 + 1M

SS14+1M protect when power
is supplied to bus elsewhere.</text>
<text>GND</text>
</plain>
<libraries>
<library name="MikesParts">
<packages>
<package name="1X04/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="2512">
</package>
<package name="TO263-3">
</package>
<package name="SMA">
</package>
<package name="0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP1" library="MikesParts" package="1X04/90" value="PINHD-1X4/90"/>
<element name="R1" library="MikesParts" package="2512" value="5R1">
<attribute name="SMT" value="2"/>
<attribute name="NAME"/>
</element>
<element name="U3" library="MikesParts" package="TO263-3" value="LM317TO263"/>
<element name="D1" library="MikesParts" package="SMA" value="SS14">
<attribute name="NAME"/>
</element>
<element name="R2" library="MikesParts" package="0603" value="10M">
<attribute name="SMT" value="2"/>
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="DALIP+">
<contactref element="JP1" pad="1"/>
<contactref element="D1" pad="C"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="R1" pad="1"/>
<contactref element="U3" pad="2"/>
<contactref element="U3" pad="6"/>
</signal>
<signal name="N$1">
<contactref element="U3" pad="3"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="N$2">
<contactref element="JP1" pad="3"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="D1" pad="A"/>
<contactref element="U3" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="R2" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
