(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 85)
    (no_connects 0)
    (area 153.823599 103.429999 253.075001 153.440201)
    (thickness 1.6)
    (drawings 37)
    (tracks 328)
    (zones 0)
    (modules 20)
    (nets 49)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user hide)
    (37 F.SilkS user hide)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.1524)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3.2 3.2)
    (pad_drill 3.2)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "/home/spencer/Documents/KiCad/2016/RC2014/Dimension Template/"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 VCC)
  (net 3 A7)
  (net 4 A6)
  (net 5 A5)
  (net 6 A4)
  (net 7 A3)
  (net 8 A2)
  (net 9 A1)
  (net 10 A0)
  (net 11 /M1)
  (net 12 /RST)
  (net 13 CLK)
  (net 14 /WR)
  (net 15 /RD)
  (net 16 /IORQ)
  (net 17 D0)
  (net 18 D1)
  (net 19 D2)
  (net 20 D3)
  (net 21 D4)
  (net 22 D5)
  (net 23 D6)
  (net 24 D7)
  (net 25 "Net-(D1-Pad2)")
  (net 26 "Net-(D2-Pad2)")
  (net 27 "Net-(J3-Pad1)")
  (net 28 "Net-(U1-Pad17)")
  (net 29 "Net-(U1-Pad19)")
  (net 30 "Net-(D3-Pad2)")
  (net 31 "Net-(J4-Pad2)")
  (net 32 "Net-(J4-Pad3)")
  (net 33 "Net-(J4-Pad4)")
  (net 34 "Net-(J4-Pad5)")
  (net 35 "Net-(J4-Pad6)")
  (net 36 "Net-(J4-Pad7)")
  (net 37 "Net-(J4-Pad8)")
  (net 38 "Net-(R3-Pad1)")
  (net 39 "Net-(R4-Pad1)")
  (net 40 "Net-(J4-Pad1)")
  (net 41 "Net-(J1-Pad37)")
  (net 42 "Net-(J1-Pad38)")
  (net 43 SDA)
  (net 44 "Net-(J3-Pad9)")
  (net 45 "Net-(J3-Pad3)")
  (net 46 "Net-(J3-Pad5)")
  (net 47 "Net-(J5-Pad2)")
  (net 48 SCL)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (add_net /IORQ)
    (add_net /M1)
    (add_net /RD)
    (add_net /RST)
    (add_net /WR)
    (add_net A0)
    (add_net A1)
    (add_net A2)
    (add_net A3)
    (add_net A4)
    (add_net A5)
    (add_net A6)
    (add_net A7)
    (add_net CLK)
    (add_net D0)
    (add_net D1)
    (add_net D2)
    (add_net D3)
    (add_net D4)
    (add_net D5)
    (add_net D6)
    (add_net D7)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(J1-Pad37)")
    (add_net "Net-(J1-Pad38)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J3-Pad3)")
    (add_net "Net-(J3-Pad5)")
    (add_net "Net-(J3-Pad9)")
    (add_net "Net-(J4-Pad1)")
    (add_net "Net-(J4-Pad2)")
    (add_net "Net-(J4-Pad3)")
    (add_net "Net-(J4-Pad4)")
    (add_net "Net-(J4-Pad5)")
    (add_net "Net-(J4-Pad6)")
    (add_net "Net-(J4-Pad7)")
    (add_net "Net-(J4-Pad8)")
    (add_net "Net-(J5-Pad2)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(R4-Pad1)")
    (add_net "Net-(U1-Pad17)")
    (add_net "Net-(U1-Pad19)")
    (add_net SCL)
    (add_net SDA)
  )
  (net_class Power ""
    (clearance 0.1524)
    (trace_width 0.3302)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (add_net GND)
    (add_net VCC)
  )
  (module Pin_Headers:Pin_Header_Straight_1x08_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 243.205 140.97 180)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (fp_text reference J4 (at 0 -2.33 180) (layer F.SilkS))
    (fp_text value Conn_01x08_Male (at 0 20.11 180) (layer F.Fab))
    (fp_text user %R (at 0 8.89 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 "Net-(J4-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(J4-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(J4-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(J4-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(J4-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(J4-Pad6)"))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(J4-Pad7)"))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 "Net-(J4-Pad8)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x08_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 218.44 125.095 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R5 (at 3.81 -0.635 180) (layer F.SilkS))
    (fp_text value 150 (at 3.81 2.31 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 "Net-(J5-Pad2)"))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 "Net-(D3-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x39_Pitch2.54mm (layer F.Cu) (tedit 592844A9)
    (at 155.702 151.613 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J1 (at 2.388 2.413 180) (layer F.SilkS))
    (fp_text value CONN_01X39 (at -3.8354 -7.874 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 A7))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 A6))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 A5))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 A4))
    (pad 13 thru_hole oval (at 0 30.48 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 A3))
    (pad 14 thru_hole oval (at 0 33.02 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 A2))
    (pad 15 thru_hole oval (at 0 35.56 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 A1))
    (pad 16 thru_hole oval (at 0 38.1 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 A0))
    (pad 17 thru_hole oval (at 0 40.64 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 18 thru_hole oval (at 0 43.18 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (pad 19 thru_hole oval (at 0 45.72 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 /M1))
    (pad 20 thru_hole oval (at 0 48.26 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 /RST))
    (pad 21 thru_hole oval (at 0 50.8 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 CLK))
    (pad 22 thru_hole oval (at 0 53.34 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 23 thru_hole oval (at 0 55.88 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 24 thru_hole oval (at 0 58.42 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 /WR))
    (pad 25 thru_hole oval (at 0 60.96 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 /RD))
    (pad 26 thru_hole oval (at 0 63.5 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 /IORQ))
    (pad 27 thru_hole oval (at 0 66.04 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 D0))
    (pad 28 thru_hole oval (at 0 68.58 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 D1))
    (pad 29 thru_hole oval (at 0 71.12 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 D2))
    (pad 30 thru_hole oval (at 0 73.66 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 D3))
    (pad 31 thru_hole oval (at 0 76.2 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 D4))
    (pad 32 thru_hole oval (at 0 78.74 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 D5))
    (pad 33 thru_hole oval (at 0 81.28 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 D6))
    (pad 34 thru_hole oval (at 0 83.82 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 D7))
    (pad 35 thru_hole oval (at 0 86.36 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 36 thru_hole oval (at 0 88.9 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 37 thru_hole oval (at 0 91.44 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 41 "Net-(J1-Pad37)"))
    (pad 38 thru_hole oval (at 0 93.98 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 42 "Net-(J1-Pad38)"))
    (pad 39 thru_hole oval (at 0 96.52 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x39.wrl
      (at (xyz 0 -1.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 locked (layer F.Cu) (tedit 59284471)
    (at 158.928 120.244)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference MNT0 (at 2.6162 -2.3876) (layer F.SilkS) hide)
    (fp_text value "" (at 2.3368 -73.0631 90) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask F.SilkS))
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 215.9 107.95 270)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D1 (at 1.27 -2.96 270) (layer F.SilkS))
    (fp_text value LED (at 1.27 2.96 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 25 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 208.915 107.95 270)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D2 (at 1.27 -2.96 270) (layer F.SilkS))
    (fp_text value LED (at 1.27 2.96 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 26 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 210.82 140.335)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R4 (at 3.81 0.635) (layer F.SilkS))
    (fp_text value 150 (at 3.81 2.31) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 "Net-(R4-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Sockets:PLCC44 (layer F.Cu) (tedit 0)
    (at 177.8 130.81 270)
    (descr "Support Plcc 44 pins, pads ronds")
    (tags PLCC)
    (fp_text reference U2 (at 13.97 -1.27 360) (layer F.SilkS))
    (fp_text value ATF1504AS-PLCC44 (at -2.54 0 360) (layer F.Fab))
    (pad 1 thru_hole rect (at -6.35 -1.27 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 12 /RST))
    (pad 2 thru_hole circle (at -8.89 1.27 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at -6.35 1.27 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 2 VCC))
    (pad 4 thru_hole circle (at -8.89 3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 39 "Net-(R4-Pad1)"))
    (pad 5 thru_hole circle (at -6.35 3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at -8.89 6.35 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 38 "Net-(R3-Pad1)"))
    (pad 7 thru_hole circle (at -6.35 8.89 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 44 "Net-(J3-Pad9)"))
    (pad 8 thru_hole circle (at -6.35 6.35 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 9 thru_hole circle (at -3.81 8.89 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 10 thru_hole circle (at -3.81 6.35 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 11 thru_hole circle (at -1.27 8.89 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 12 thru_hole circle (at -1.27 6.35 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 13 thru_hole circle (at 1.27 8.89 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 46 "Net-(J3-Pad5)"))
    (pad 14 thru_hole circle (at 1.27 6.35 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 15 thru_hole circle (at 3.81 8.89 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 2 VCC))
    (pad 16 thru_hole circle (at 3.81 6.35 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 17 thru_hole circle (at 6.35 8.89 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 16 /IORQ))
    (pad 18 thru_hole circle (at 8.89 6.35 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 19 thru_hole circle (at 6.35 6.35 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 3 A7))
    (pad 20 thru_hole circle (at 8.89 3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 4 A6))
    (pad 21 thru_hole circle (at 6.35 3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 5 A5))
    (pad 22 thru_hole circle (at 8.89 1.27 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 23 thru_hole circle (at 6.35 1.27 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 2 VCC))
    (pad 24 thru_hole circle (at 8.89 -1.27 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 6 A4))
    (pad 25 thru_hole circle (at 6.35 -1.27 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 7 A3))
    (pad 26 thru_hole circle (at 8.89 -3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 8 A2))
    (pad 27 thru_hole circle (at 6.35 -3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 9 A1))
    (pad 28 thru_hole circle (at 8.89 -6.35 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 10 A0))
    (pad 29 thru_hole circle (at 6.35 -8.89 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 11 /M1))
    (pad 30 thru_hole circle (at 6.35 -6.35 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 31 thru_hole circle (at 3.81 -8.89 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 32 thru_hole circle (at 3.81 -6.35 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 27 "Net-(J3-Pad1)"))
    (pad 33 thru_hole circle (at 1.27 -8.89 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 34 thru_hole circle (at 1.27 -6.35 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 35 thru_hole circle (at -1.27 -8.89 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 2 VCC))
    (pad 36 thru_hole circle (at -1.27 -6.35 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 17 D0))
    (pad 37 thru_hole circle (at -3.81 -8.89 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 15 /RD))
    (pad 38 thru_hole circle (at -3.81 -6.35 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 45 "Net-(J3-Pad3)"))
    (pad 39 thru_hole circle (at -6.35 -8.89 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 14 /WR))
    (pad 40 thru_hole circle (at -8.89 -6.35 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 28 "Net-(U1-Pad17)"))
    (pad 41 thru_hole circle (at -6.35 -6.35 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 29 "Net-(U1-Pad19)"))
    (pad 42 thru_hole circle (at -8.89 -3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 43 thru_hole circle (at -6.35 -3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 44 thru_hole circle (at -8.89 -1.27 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (model /Users/sam/Downloads/walter/pth_plcc/plcc44_pth-skt.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 210.82 136.525)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R3 (at 3.81 0.635) (layer F.SilkS))
    (fp_text value 150 (at 3.81 2.31) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 "Net-(R3-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D3.0mm_W2.0mm_P2.50mm (layer F.Cu) (tedit 597BC7C2)
    (at 200.66 117.475 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3*2mm^2, Capacitor")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3mm width 2mm Capacitor")
    (fp_text reference C1 (at 1.25 1.905 180) (layer F.SilkS))
    (fp_text value 0.1µF (at 1.25 2.31 180) (layer F.Fab))
    (fp_text user %R (at 1.25 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 VCC))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D3.0mm_W2.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D3.0mm_W2.0mm_P2.50mm (layer F.Cu) (tedit 597BC7C2)
    (at 231.775 117.475 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3*2mm^2, Capacitor")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3mm width 2mm Capacitor")
    (fp_text reference C2 (at 1.25 1.905 180) (layer F.SilkS))
    (fp_text value 0.1µF (at 1.25 2.31 180) (layer F.Fab))
    (fp_text user %R (at 1.25 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 VCC))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D3.0mm_W2.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D3.0mm_W2.0mm_P2.50mm (layer F.Cu) (tedit 597BC7C2)
    (at 163.83 132.715 90)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3*2mm^2, Capacitor")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3mm width 2mm Capacitor")
    (fp_text reference C3 (at 1.25 -2.31 90) (layer F.SilkS))
    (fp_text value 0.1µF (at 1.25 2.31 90) (layer F.Fab))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 VCC))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D3.0mm_W2.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 201.295 107.95 270)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D3 (at 1.27 -2.96 270) (layer F.SilkS))
    (fp_text value LED (at 1.27 2.96 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 30 "Net-(D3-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 210.82 128.905)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 3.81 0.635) (layer F.SilkS))
    (fp_text value 10k (at 3.81 2.31) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 VCC))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 SDA))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 218.44 132.715 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at 3.81 -0.635 180) (layer F.SilkS))
    (fp_text value 10k (at 3.81 2.31 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 VCC))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 48 SCL))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-20_W7.62mm_Socket_LongPads (layer F.Cu) (tedit 59C78D6B)
    (at 195.58 120.65)
    (descr "20-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket, LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket LongPads")
    (fp_text reference U1 (at 0 -2.54) (layer F.SilkS))
    (fp_text value PCF8584 (at 3.81 25.19) (layer F.Fab))
    (fp_text user %R (at 3.81 11.43) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 CLK))
    (pad 11 thru_hole oval (at 7.62 22.86) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 D3))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 SDA))
    (pad 12 thru_hole oval (at 7.62 20.32) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 D4))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 48 SCL))
    (pad 13 thru_hole oval (at 7.62 17.78) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 D5))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 14 thru_hole oval (at 7.62 15.24) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 D6))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 15 thru_hole oval (at 7.62 12.7) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 D7))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 A0))
    (pad 16 thru_hole oval (at 7.62 10.16) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 /RD))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 D0))
    (pad 17 thru_hole oval (at 7.62 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "Net-(U1-Pad17)"))
    (pad 8 thru_hole oval (at 0 17.78) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 D1))
    (pad 18 thru_hole oval (at 7.62 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 /WR))
    (pad 9 thru_hole oval (at 0 20.32) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 D2))
    (pad 19 thru_hole oval (at 7.62 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(U1-Pad19)"))
    (pad 10 thru_hole oval (at 0 22.86) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 20 thru_hole oval (at 7.62 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 VCC))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-20_W7.62mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-18_W7.62mm_Socket_LongPads (layer F.Cu) (tedit 59C78D6B)
    (at 226.695 120.65)
    (descr "18-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket, LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket LongPads")
    (fp_text reference U3 (at -0.635 -2.33) (layer F.SilkS))
    (fp_text value MCP23008 (at 3.81 22.65) (layer F.Fab))
    (fp_text user %R (at 3.81 10.16) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 48 SCL))
    (pad 10 thru_hole oval (at 7.62 20.32) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 "Net-(J4-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 SDA))
    (pad 11 thru_hole oval (at 7.62 17.78) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 "Net-(J4-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 VCC))
    (pad 12 thru_hole oval (at 7.62 15.24) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 "Net-(J4-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 VCC))
    (pad 13 thru_hole oval (at 7.62 12.7) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 "Net-(J4-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 VCC))
    (pad 14 thru_hole oval (at 7.62 10.16) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(J4-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(U1-Pad19)"))
    (pad 15 thru_hole oval (at 7.62 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 "Net-(J4-Pad6)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 16 thru_hole oval (at 7.62 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 "Net-(J4-Pad7)"))
    (pad 8 thru_hole oval (at 0 17.78) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 17 thru_hole oval (at 7.62 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 "Net-(J4-Pad8)"))
    (pad 9 thru_hole oval (at 0 20.32) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 18 thru_hole oval (at 7.62 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 VCC))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-18_W7.62mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_conn_strip:vasch_strip_5x2 (layer F.Cu) (tedit 53DE0503)
    (at 179.07 110.49 180)
    (descr "Box header 5x2pin 2.54mm")
    (tags "CONN DEV")
    (fp_text reference J3 (at 0 -5.7 180) (layer F.SilkS))
    (fp_text value ATDH1150USB_JTAG (at 0 5.7 180) (layer F.SilkS) hide)
    (pad 9 thru_hole oval (at 5.08 1.27 180) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 44 "Net-(J3-Pad9)"))
    (pad 10 thru_hole oval (at 5.08 -1.27 180) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 8 thru_hole oval (at 2.54 -1.27 180) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS))
    (pad 7 thru_hole oval (at 2.54 1.27 180) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole rect (at -5.08 1.27 180) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(J3-Pad1)"))
    (pad 2 thru_hole oval (at -5.08 -1.27 180) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 3 thru_hole oval (at -2.54 1.27 180) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 45 "Net-(J3-Pad3)"))
    (pad 4 thru_hole oval (at -2.54 -1.27 180) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (pad 5 thru_hole oval (at 0 1.27 180) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 46 "Net-(J3-Pad5)"))
    (pad 6 thru_hole oval (at 0 -1.27 180) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS))
    (model walter/conn_strip/vasch_strip_5x2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x01_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 243.205 109.855 180)
    (descr "Through hole straight pin header, 2x01, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x01 2.54mm double row")
    (fp_text reference J5 (at 5.715 0.635 180) (layer F.SilkS))
    (fp_text value Conn_02x01 (at 1.27 2.33 180) (layer F.Fab))
    (fp_text user %R (at 1.27 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 "Net-(J4-Pad8)"))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 "Net-(J5-Pad2)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x02_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 243.205 114.935 180)
    (descr "Through hole straight pin header, 2x02, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x02 2.54mm double row")
    (fp_text reference J2 (at 5.715 -0.635 180) (layer F.SilkS))
    (fp_text value Conn_02x02_Odd_Even (at 1.27 4.87 180) (layer F.Fab))
    (fp_text user %R (at 1.27 1.27 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 "Net-(J1-Pad38)"))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 SDA))
    (pad 3 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 "Net-(J1-Pad37)"))
    (pad 4 thru_hole oval (at 2.54 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 SCL))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text SCL (at 247.015 147.32 90) (layer F.SilkS))
  (gr_text SDA (at 249.555 147.32 90) (layer F.SilkS))
  (gr_text "I2C v1.0" (at 245.11 106.68) (layer F.SilkS))
  (gr_text TEST (at 201.295 105.41) (layer F.SilkS))
  (gr_text RST (at 208.915 105.41) (layer F.SilkS))
  (gr_text "ERR\n" (at 215.9 105.41) (layer F.SilkS))
  (gr_text "Pin 1" (at 155.68168 146.60118 90) (layer F.SilkS))
  (target plus (at 153.8986 153.3652) (size 5) (width 0.15) (layer Edge.Cuts))
  (gr_text "M3 Mounting Hole" (at 155.56992 118.91264 45) (layer F.CrtYd))
  (dimension 1.714568 (width 0.3) (layer F.CrtYd)
    (gr_text "1.715 mm" (at 256.222742 152.44727 270.5092824) (layer F.CrtYd))
    (feature1 (pts (xy 249.67438 151.64816) (xy 257.565069 151.578021)))
    (feature2 (pts (xy 249.68962 153.36266) (xy 257.580309 153.292521)))
    (crossbar (pts (xy 254.880416 153.31652) (xy 254.865176 151.60202)))
    (arrow1a (pts (xy 254.865176 151.60202) (xy 255.461587 152.723267)))
    (arrow1b (pts (xy 254.865176 151.60202) (xy 254.288791 152.733692)))
    (arrow2a (pts (xy 254.880416 153.31652) (xy 255.456801 152.184848)))
    (arrow2b (pts (xy 254.880416 153.31652) (xy 254.284005 152.195273)))
  )
  (dimension 3.398129 (width 0.3) (layer F.CrtYd)
    (gr_text "3.2 mm" (at 166.13124 113.10112 315) (layer F.CrtYd))
    (feature1 (pts (xy 160.13176 121.44756) (xy 166.797097 114.782223)))
    (feature2 (pts (xy 157.72892 119.04472) (xy 164.394257 112.379383)))
    (crossbar (pts (xy 162.485069 114.288571) (xy 164.887909 116.691411)))
    (arrow1a (pts (xy 164.887909 116.691411) (xy 163.676688 116.309515)))
    (arrow1b (pts (xy 164.887909 116.691411) (xy 164.506013 115.48019)))
    (arrow2a (pts (xy 162.485069 114.288571) (xy 162.866965 115.499792)))
    (arrow2b (pts (xy 162.485069 114.288571) (xy 163.69629 114.670467)))
  )
  (gr_text "5.1mm\nradius" (at 245.2878 108.4326) (layer F.CrtYd))
  (gr_text "135 deg" (at 172.15104 107.60964) (layer F.CrtYd))
  (dimension 15.0114 (width 0.3) (layer F.CrtYd)
    (gr_text "15.011 mm" (at 161.4043 99.06636) (layer F.CrtYd))
    (feature1 (pts (xy 153.8986 103.505) (xy 153.8986 97.71636)))
    (feature2 (pts (xy 168.91 103.505) (xy 168.91 97.71636)))
    (crossbar (pts (xy 168.91 100.41636) (xy 153.8986 100.41636)))
    (arrow1a (pts (xy 153.8986 100.41636) (xy 155.025104 99.829939)))
    (arrow1b (pts (xy 153.8986 100.41636) (xy 155.025104 101.002781)))
    (arrow2a (pts (xy 168.91 100.41636) (xy 167.783496 99.829939)))
    (arrow2b (pts (xy 168.91 100.41636) (xy 167.783496 101.002781)))
  )
  (dimension 5.0292 (width 0.3) (layer F.CrtYd)
    (gr_text "5.029 mm" (at 156.4132 128.7564) (layer F.CrtYd))
    (feature1 (pts (xy 153.8986 120.2436) (xy 153.8986 130.1064)))
    (feature2 (pts (xy 158.9278 120.2436) (xy 158.9278 130.1064)))
    (crossbar (pts (xy 158.9278 127.4064) (xy 153.8986 127.4064)))
    (arrow1a (pts (xy 153.8986 127.4064) (xy 155.025104 126.819979)))
    (arrow1b (pts (xy 153.8986 127.4064) (xy 155.025104 127.992821)))
    (arrow2a (pts (xy 158.9278 127.4064) (xy 157.801296 126.819979)))
    (arrow2b (pts (xy 158.9278 127.4064) (xy 157.801296 127.992821)))
  )
  (dimension 33.1216 (width 0.3) (layer F.CrtYd)
    (gr_text "33.122 mm" (at 165.9928 136.8044 270) (layer F.CrtYd))
    (feature1 (pts (xy 158.9278 153.3652) (xy 167.3428 153.3652)))
    (feature2 (pts (xy 158.9278 120.2436) (xy 167.3428 120.2436)))
    (crossbar (pts (xy 164.6428 120.2436) (xy 164.6428 153.3652)))
    (arrow1a (pts (xy 164.6428 153.3652) (xy 164.056379 152.238696)))
    (arrow1b (pts (xy 164.6428 153.3652) (xy 165.229221 152.238696)))
    (arrow2a (pts (xy 164.6428 120.2436) (xy 164.056379 121.370104)))
    (arrow2b (pts (xy 164.6428 120.2436) (xy 165.229221 121.370104)))
  )
  (dimension 34.8488 (width 0.3) (layer F.CrtYd)
    (gr_text "34.849 mm" (at 146.3129 135.9408 90) (layer F.CrtYd))
    (feature1 (pts (xy 153.8986 118.5164) (xy 144.9629 118.5164)))
    (feature2 (pts (xy 153.8986 153.3652) (xy 144.9629 153.3652)))
    (crossbar (pts (xy 147.6629 153.3652) (xy 147.6629 118.5164)))
    (arrow1a (pts (xy 147.6629 118.5164) (xy 148.249321 119.642904)))
    (arrow1b (pts (xy 147.6629 118.5164) (xy 147.076479 119.642904)))
    (arrow2a (pts (xy 147.6629 153.3652) (xy 148.249321 152.238696)))
    (arrow2b (pts (xy 147.6629 153.3652) (xy 147.076479 152.238696)))
  )
  (dimension 49.8602 (width 0.3) (layer F.CrtYd)
    (gr_text "49.860 mm" (at 137.969 128.4351 90) (layer F.CrtYd))
    (feature1 (pts (xy 179.8955 103.505) (xy 136.619 103.505)))
    (feature2 (pts (xy 179.8955 153.3652) (xy 136.619 153.3652)))
    (crossbar (pts (xy 139.319 153.3652) (xy 139.319 103.505)))
    (arrow1a (pts (xy 139.319 103.505) (xy 139.905421 104.631504)))
    (arrow1b (pts (xy 139.319 103.505) (xy 138.732579 104.631504)))
    (arrow2a (pts (xy 139.319 153.3652) (xy 139.905421 152.238696)))
    (arrow2b (pts (xy 139.319 153.3652) (xy 138.732579 152.238696)))
  )
  (dimension 99.10572 (width 0.3) (layer F.CrtYd)
    (gr_text "99.106 mm" (at 203.45146 162.7035) (layer F.CrtYd))
    (feature1 (pts (xy 253.00432 149.86254) (xy 253.00432 164.0535)))
    (feature2 (pts (xy 153.8986 149.86254) (xy 153.8986 164.0535)))
    (crossbar (pts (xy 153.8986 161.3535) (xy 253.00432 161.3535)))
    (arrow1a (pts (xy 253.00432 161.3535) (xy 251.877816 161.939921)))
    (arrow1b (pts (xy 253.00432 161.3535) (xy 251.877816 160.767079)))
    (arrow2a (pts (xy 153.8986 161.3535) (xy 155.025104 161.939921)))
    (arrow2b (pts (xy 153.8986 161.3535) (xy 155.025104 160.767079)))
  )
  (dimension 5.034511 (width 0.3) (layer F.CrtYd)
    (gr_text "5.035 mm" (at 156.801297 161.017316 0.5492363601) (layer F.CrtYd))
    (feature1 (pts (xy 153.89352 120.29186) (xy 154.297098 162.391384)))
    (feature2 (pts (xy 158.9278 120.2436) (xy 159.331378 162.343124)))
    (crossbar (pts (xy 159.305496 159.643248) (xy 154.271216 159.691508)))
    (arrow1a (pts (xy 154.271216 159.691508) (xy 155.392047 159.094316)))
    (arrow1b (pts (xy 154.271216 159.691508) (xy 155.403289 160.267103)))
    (arrow2a (pts (xy 159.305496 159.643248) (xy 158.173423 159.067653)))
    (arrow2b (pts (xy 159.305496 159.643248) (xy 158.184665 160.24044)))
  )
  (gr_line (start 253 108.685) (end 253 153.3652) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 247.8184 103.505) (end 168.91 103.505) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 247.8184 108.685) (end 247.8184 103.505) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 153.8986 118.5164) (end 153.8986 153.3652) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 168.91 103.505) (end 153.8986 118.5164) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 153.8986 153.3652) (end 253 153.3652) (angle 90) (layer Edge.Cuts) (width 0.15))
)
