(kicad_pcb (version 4) (host pcbnew 4.0.4-stable)
  (general
    (links 32)
    (no_connects 0)
    (area 136.830999 97.460999 157.809001 113.359001)
    (thickness 1.6002)
    (drawings 21)
    (tracks 88)
    (zones 0)
    (modules 3)
    (nets 17)
  )
  (page A4)
  (layers
    (0 Top signal)
    (31 Bottom signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.3048)
    (user_trace_width 0.2032)
    (user_trace_width 0.3048)
    (user_trace_width 0.381)
    (user_trace_width 0.508)
    (trace_clearance 0.1524)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.28702)
    (uvia_size 0.762)
    (uvia_drill 0.6858)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0127)
    (aux_axis_origin 0 0)
    (visible_elements FFFFF77F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask true)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory Gerbers/))
  )
  (net 0 "")
  (net 1 "Net-(P1-Pad9)")
  (net 2 "Net-(P1-Pad11)")
  (net 3 "Net-(P1-Pad10)")
  (net 4 "Net-(P1-Pad12)")
  (net 5 "Net-(P1-Pad5)")
  (net 6 "Net-(P1-Pad3)")
  (net 7 "Net-(P1-Pad4)")
  (net 8 "Net-(P1-Pad1)")
  (net 9 "Net-(P1-Pad7)")
  (net 10 "Net-(P1-Pad6)")
  (net 11 "Net-(P1-Pad2)")
  (net 12 "Net-(P1-Pad8)")
  (net 13 "Net-(P1-Pad15)")
  (net 14 "Net-(P1-Pad14)")
  (net 15 "Net-(P1-Pad13)")
  (net 16 "Net-(P1-Pad16)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.6858)
    (add_net "Net-(P1-Pad1)")
    (add_net "Net-(P1-Pad10)")
    (add_net "Net-(P1-Pad11)")
    (add_net "Net-(P1-Pad12)")
    (add_net "Net-(P1-Pad13)")
    (add_net "Net-(P1-Pad14)")
    (add_net "Net-(P1-Pad15)")
    (add_net "Net-(P1-Pad16)")
    (add_net "Net-(P1-Pad2)")
    (add_net "Net-(P1-Pad3)")
    (add_net "Net-(P1-Pad4)")
    (add_net "Net-(P1-Pad5)")
    (add_net "Net-(P1-Pad6)")
    (add_net "Net-(P1-Pad7)")
    (add_net "Net-(P1-Pad8)")
    (add_net "Net-(P1-Pad9)")
  )
  (module Purple_Frog_Breakouts:BO_BOARD_16 (layer Top) (tedit 57D08C03)
    (at 147.32 105.41)
    (descr BO_Board_16_Pin)
    (tags Breakout,16,pin,SOIC)
    (fp_text reference P1 (at -0.1 -2.7) (layer F.SilkS) hide)
    (fp_text value Connector_8x2 (at 0 0) (layer F.SilkS) hide)
    (fp_text user 16 (at -8.9 -4.6) (layer F.SilkS))
    (fp_text user 15 (at -6.3 -4.6) (layer F.SilkS))
    (fp_text user 14 (at -3.8 -4.6) (layer F.SilkS))
    (fp_text user 13 (at -1.2 -4.6) (layer F.SilkS))
    (fp_text user 12 (at 1.3 -4.6) (layer F.SilkS))
    (fp_text user 9 (at 8.9 -4.6) (layer F.SilkS))
    (fp_text user 10 (at 6.4 -4.6) (layer F.SilkS))
    (fp_text user 11 (at 3.8 -4.6) (layer F.SilkS))
    (fp_text user 6 (at 3.8 4.6) (layer F.SilkS))
    (fp_text user 7 (at 6.4 4.6) (layer F.SilkS))
    (fp_text user 8 (at 8.9 4.6) (layer F.SilkS))
    (fp_text user 5 (at 1.3 4.6) (layer F.SilkS))
    (fp_text user 4 (at -1.2 4.6) (layer F.SilkS))
    (fp_text user 3 (at -3.8 4.6) (layer F.SilkS))
    (fp_text user 2 (at -6.3 4.6) (layer F.SilkS))
    (pad 9 thru_hole circle (at 8.89 -6.35) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(P1-Pad9)"))
    (pad 11 thru_hole circle (at 3.81 -6.35) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(P1-Pad11)"))
    (pad 10 thru_hole circle (at 6.35 -6.35) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(P1-Pad10)"))
    (pad 12 thru_hole circle (at 1.27 -6.35) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(P1-Pad12)"))
    (pad 5 thru_hole circle (at 1.27 6.35) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(P1-Pad5)"))
    (pad 3 thru_hole circle (at -3.81 6.35) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(P1-Pad3)"))
    (pad 4 thru_hole circle (at -1.27 6.35) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(P1-Pad4)"))
    (pad 1 thru_hole rect (at -8.89 6.35) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(P1-Pad1)"))
    (pad 7 thru_hole circle (at 6.35 6.35) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(P1-Pad7)"))
    (pad 6 thru_hole circle (at 3.81 6.35) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(P1-Pad6)"))
    (pad 2 thru_hole circle (at -6.35 6.35) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(P1-Pad2)"))
    (pad 8 thru_hole circle (at 8.89 6.35) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(P1-Pad8)"))
    (pad 15 thru_hole circle (at -6.35 -6.35) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(P1-Pad15)"))
    (pad 14 thru_hole circle (at -3.81 -6.35) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(P1-Pad14)"))
    (pad 13 thru_hole circle (at -1.27 -6.35) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(P1-Pad13)"))
    (pad 16 thru_hole circle (at -8.89 -6.35) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(P1-Pad16)"))
  )
  (module Purple_Frog_SMD:SOIC_16 (layer Top) (tedit 57D0E22C)
    (at 147.32 105.41)
    (descr SOIC_16)
    (fp_text reference U1 (at 0 -0.381) (layer F.SilkS) hide)
    (fp_text value MCP3x08 (at 0 0) (layer F.SilkS) hide)
    (pad 16 smd rect (at -4.445 -2.794) (size 0.635 1.27) (layers Top F.Paste F.Mask)
      (net 16 "Net-(P1-Pad16)"))
    (pad 15 smd rect (at -3.175 -2.794) (size 0.635 1.27) (layers Top F.Paste F.Mask)
      (net 13 "Net-(P1-Pad15)"))
    (pad 8 smd rect (at 4.445 2.794) (size 0.635 1.27) (layers Top F.Paste F.Mask)
      (net 12 "Net-(P1-Pad8)"))
    (pad 1 smd rect (at -4.445 2.794) (size 0.635 1.27) (layers Top F.Paste F.Mask)
      (net 8 "Net-(P1-Pad1)"))
    (pad 2 smd rect (at -3.175 2.794) (size 0.635 1.27) (layers Top F.Paste F.Mask)
      (net 11 "Net-(P1-Pad2)"))
    (pad 3 smd rect (at -1.905 2.794) (size 0.635 1.27) (layers Top F.Paste F.Mask)
      (net 6 "Net-(P1-Pad3)"))
    (pad 4 smd rect (at -0.635 2.794) (size 0.635 1.27) (layers Top F.Paste F.Mask)
      (net 7 "Net-(P1-Pad4)"))
    (pad 5 smd rect (at 0.635 2.794) (size 0.635 1.27) (layers Top F.Paste F.Mask)
      (net 5 "Net-(P1-Pad5)"))
    (pad 6 smd rect (at 1.905 2.794) (size 0.635 1.27) (layers Top F.Paste F.Mask)
      (net 10 "Net-(P1-Pad6)"))
    (pad 7 smd rect (at 3.175 2.794) (size 0.635 1.27) (layers Top F.Paste F.Mask)
      (net 9 "Net-(P1-Pad7)"))
    (pad 9 smd rect (at 4.445 -2.794) (size 0.635 1.27) (layers Top F.Paste F.Mask)
      (net 1 "Net-(P1-Pad9)"))
    (pad 10 smd rect (at 3.175 -2.794) (size 0.635 1.27) (layers Top F.Paste F.Mask)
      (net 3 "Net-(P1-Pad10)"))
    (pad 11 smd rect (at 1.905 -2.794) (size 0.635 1.27) (layers Top F.Paste F.Mask)
      (net 2 "Net-(P1-Pad11)"))
    (pad 12 smd rect (at 0.635 -2.794) (size 0.635 1.27) (layers Top F.Paste F.Mask)
      (net 4 "Net-(P1-Pad12)"))
    (pad 13 smd rect (at -0.635 -2.794) (size 0.635 1.27) (layers Top F.Paste F.Mask)
      (net 15 "Net-(P1-Pad13)"))
    (pad 14 smd rect (at -1.905 -2.794) (size 0.635 1.27) (layers Top F.Paste F.Mask)
      (net 14 "Net-(P1-Pad14)"))
    (model smd/smd_dil/so-14.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Purple_Frog_SMD:SSOP_16 (layer Bottom) (tedit 57D0E31E)
    (at 147.32 105.41 270)
    (descr "16-Lead Plastic Shrink Small Outline Narrow Body (QR)-.150\" Body [QSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.635")
    (attr smd)
    (fp_text reference U2 (at 0 0 540) (layer B.SilkS) hide)
    (fp_text value MCP3x08 (at 0 -3.5 270) (layer B.SilkS) hide)
    (pad 1 smd rect (at -2.6543 2.2225 270) (size 1.6 0.41) (layers Bottom B.Paste B.Mask)
      (net 16 "Net-(P1-Pad16)"))
    (pad 2 smd rect (at -2.6543 1.5875 270) (size 1.6 0.41) (layers Bottom B.Paste B.Mask)
      (net 13 "Net-(P1-Pad15)"))
    (pad 3 smd rect (at -2.6543 0.9525 270) (size 1.6 0.41) (layers Bottom B.Paste B.Mask)
      (net 14 "Net-(P1-Pad14)"))
    (pad 4 smd rect (at -2.6543 0.3175 270) (size 1.6 0.41) (layers Bottom B.Paste B.Mask)
      (net 15 "Net-(P1-Pad13)"))
    (pad 5 smd rect (at -2.6543 -0.3175 270) (size 1.6 0.41) (layers Bottom B.Paste B.Mask)
      (net 4 "Net-(P1-Pad12)"))
    (pad 6 smd rect (at -2.6543 -0.9525 270) (size 1.6 0.41) (layers Bottom B.Paste B.Mask)
      (net 2 "Net-(P1-Pad11)"))
    (pad 7 smd rect (at -2.6543 -1.5875 270) (size 1.6 0.41) (layers Bottom B.Paste B.Mask)
      (net 3 "Net-(P1-Pad10)"))
    (pad 8 smd rect (at -2.6543 -2.2225 270) (size 1.6 0.41) (layers Bottom B.Paste B.Mask)
      (net 1 "Net-(P1-Pad9)"))
    (pad 9 smd rect (at 2.6543 -2.2225 270) (size 1.6 0.41) (layers Bottom B.Paste B.Mask)
      (net 12 "Net-(P1-Pad8)"))
    (pad 10 smd rect (at 2.6543 -1.5875 270) (size 1.6 0.41) (layers Bottom B.Paste B.Mask)
      (net 9 "Net-(P1-Pad7)"))
    (pad 11 smd rect (at 2.6543 -0.9525 270) (size 1.6 0.41) (layers Bottom B.Paste B.Mask)
      (net 10 "Net-(P1-Pad6)"))
    (pad 12 smd rect (at 2.6543 -0.3175 270) (size 1.6 0.41) (layers Bottom B.Paste B.Mask)
      (net 5 "Net-(P1-Pad5)"))
    (pad 13 smd rect (at 2.6543 0.3175 270) (size 1.6 0.41) (layers Bottom B.Paste B.Mask)
      (net 7 "Net-(P1-Pad4)"))
    (pad 14 smd rect (at 2.6543 0.9525 270) (size 1.6 0.41) (layers Bottom B.Paste B.Mask)
      (net 6 "Net-(P1-Pad3)"))
    (pad 15 smd rect (at 2.6543 1.5875 270) (size 1.6 0.41) (layers Bottom B.Paste B.Mask)
      (net 11 "Net-(P1-Pad2)"))
    (pad 16 smd rect (at 2.6543 2.2225 270) (size 1.6 0.41) (layers Bottom B.Paste B.Mask)
      (net 8 "Net-(P1-Pad1)"))
    (model Housings_SSOP.3dshapes/QSOP-16_3.9x4.9mm_Pitch0.635mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 136.906 97.536) (end 137.033 97.536) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 136.906 113.284) (end 136.906 97.536) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 157.734 113.284) (end 136.906 113.284) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 157.734 97.536) (end 157.734 113.284) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 136.906 97.536) (end 157.734 97.536) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text 16 (at 138.43 110.109 180) (layer B.SilkS))
  (gr_text 15 (at 140.97 110.109 180) (layer B.SilkS))
  (gr_text 14 (at 143.51 110.109 180) (layer B.SilkS))
  (gr_text 13 (at 146.05 110.109 180) (layer B.SilkS))
  (gr_text 12 (at 148.717 110.109 180) (layer B.SilkS))
  (gr_text 11 (at 151.13 110.109 180) (layer B.SilkS))
  (gr_text 10 (at 153.67 110.109 180) (layer B.SilkS))
  (gr_text 9 (at 156.21 110.109 180) (layer B.SilkS))
  (gr_text 8 (at 156.21 100.838 180) (layer B.SilkS))
  (gr_text 7 (at 153.67 100.838 180) (layer B.SilkS))
  (gr_text 6 (at 151.257 100.838 180) (layer B.SilkS))
  (gr_text 5 (at 148.59 100.838 180) (layer B.SilkS))
  (gr_text 4 (at 146.05 100.838 180) (layer B.SilkS))
  (gr_text 3 (at 143.51 100.838 180) (layer B.SilkS))
  (gr_text 2 (at 140.97 100.838 180) (layer B.SilkS))
)
