(kicad_pcb (version 4) (host pcbnew 4.0.5)
  (general
    (links 0)
    (no_connects 0)
    (area 118.924999 92.923 154.075001 117.129)
    (thickness 1.6)
    (drawings 14)
    (tracks 18)
    (zones 0)
    (modules 5)
    (nets 6)
  )
  (page USLetter)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.4064)
    (user_trace_width 0.6096)
    (trace_clearance 0.254)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 4.064 4.064)
    (pad_drill 3.048)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (grid_origin 119 116)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 /R_OUT)
  (net 3 /L_OUT)
  (net 4 /R_IN)
  (net 5 /L_IN)
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /L_IN)
    (add_net /L_OUT)
    (add_net /R_IN)
    (add_net /R_OUT)
    (add_net GND)
  )
  (module machadolab:AUDIO_POT_SWITCH (layer F.Cu) (tedit 58956403)
    (at 148.5011 105.0036)
    (fp_text reference RV1 (at 2 6) (layer F.SilkS) hide)
    (fp_text value POT_Dual (at -4 -6) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 0) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 /R_OUT))
    (pad 1 thru_hole circle (at 0 2.5) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole circle (at 0 -2.5) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 4 /R_IN))
    (pad 5 thru_hole circle (at -5 0) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 3 /L_OUT))
    (pad 6 thru_hole circle (at -5 -2.5) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 5 /L_IN))
    (pad 4 thru_hole circle (at -5 2.5) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 7 thru_hole circle (at -11.5 2.5) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at -11.5 -2.5) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask))
  )
  (module Pin_Headers:Pin_Header_Straight_1x06_Pitch2.54mm (layer F.Cu) (tedit 589563FE)
    (at 130 111 180)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (fp_text reference P1 (at 0 -2.39 180) (layer F.SilkS) hide)
    (fp_text value CONN_01X06 (at 0 15.09 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /R_OUT))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /L_OUT))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /R_IN))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /L_IN))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x06_Pitch2.54mm.wrl
      (at (xyz 0 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Connectors:1pin (layer F.Cu) (tedit 589565F8)
    (at 122 97)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 3) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask))
  )
  (module Connectors:1pin (layer F.Cu) (tedit 589565FD)
    (at 122 113)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 3) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask))
  )
  (module machadolab:mhq_logo_small (layer B.Cu) (tedit 0)
    (at 123 105 90)
    (fp_text reference G*** (at 0 0 90) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 90) (layer B.SilkS) hide)
  )
  (gr_text GND (at 127.75 111) (layer F.SilkS))
  (gr_text R_OUT (at 127.75 108.5) (layer F.SilkS))
  (gr_text L_OUT (at 127.75 106) (layer F.SilkS))
  (gr_text GND (at 127.75 103.5) (layer F.SilkS))
  (gr_text R_IN (at 127.75 101) (layer F.SilkS))
  (gr_text L_IN (at 127.75 98.25) (layer F.SilkS))
  (gr_line (start 119 94) (end 119 116) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 133 94) (end 119 94) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 136 97) (end 133 94) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 154 97) (end 136 97) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 133 116) (end 119 116) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 136 113) (end 133 116) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 154 113) (end 136 113) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 154 97) (end 154 113) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 136 97) (xy 154 97) (xy 154 113) (xy 136 113) (xy 133 116)
        (xy 119 116) (xy 119 94) (xy 133 94)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 136 97) (xy 154 97) (xy 154 113) (xy 136 113) (xy 133 116)
        (xy 119 116) (xy 119 94) (xy 133 94)
      )
    )
  )
)
