(kicad_pcb (version 20171130) (host pcbnew "(5.1.2-1)-1")
  (general
    (thickness 1.6)
    (drawings 8)
    (tracks 584)
    (zones 0)
    (modules 38)
    (nets 51)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.1524)
    (user_trace_width 0.2032)
    (user_trace_width 0.254)
    (user_trace_width 0.3048)
    (user_trace_width 0.635)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.4064)
    (via_drill 0.2032)
    (via_min_size 0.4064)
    (via_min_drill 0.2032)
    (uvia_size 0.4064)
    (uvia_drill 0.2032)
    (uvias_allowed no)
    (uvia_min_size 0.4064)
    (uvia_min_drill 0.2032)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(D1-Pad1)")
  (net 2 /HT16K33_COM0_AD)
  (net 3 "Net-(D2-Pad1)")
  (net 4 /HT16K33_COM1_KS0)
  (net 5 "Net-(D3-Pad1)")
  (net 6 /HT16K33_COM2_KS1)
  (net 7 "Net-(D4-Pad1)")
  (net 8 /HT16K33_COM3_KS2)
  (net 9 GND)
  (net 10 /P5V0_INT)
  (net 11 /I2C_SDA_5V5)
  (net 12 /I2C_SCL_5V5)
  (net 13 /HT16K33_COM4)
  (net 14 /HT16K33_COM5)
  (net 15 /HT16K33_COM6)
  (net 16 /HT16K33_COM7)
  (net 17 /HT16K33_ROW15_K13_INT)
  (net 18 /HT16K33_ROW14_K12)
  (net 19 /HT16K33_ROW13_K11)
  (net 20 /HT16K33_ROW12_K10)
  (net 21 /HT16K33_ROW11_K9)
  (net 22 /HT16K33_ROW10_K8)
  (net 23 /HT16K33_ROW9_K7)
  (net 24 /HT16K33_ROW8_K6)
  (net 25 /HT16K33_ROW7_K5)
  (net 26 /HT16K33_ROW6_K4)
  (net 27 /HT16K33_ROW5_K3)
  (net 28 /HT16K33_ROW4_K2)
  (net 29 /HT16K33_ROW3_K1)
  (net 30 /HT16K33_ROW2_A0)
  (net 31 /HT16K33_ROW1_A1)
  (net 32 /HT16K33_ROW0_A2)
  (net 33 /P5V0)
  (net 34 /P5V0_EXT)
  (net 35 "Net-(J8-Pad1)")
  (net 36 "Net-(J8-Pad2)")
  (net 37 "Net-(J8-Pad3)")
  (net 38 "Net-(J8-Pad4)")
  (net 39 "Net-(J8-Pad5)")
  (net 40 "Net-(J8-Pad6)")
  (net 41 "Net-(J8-Pad7)")
  (net 42 "Net-(J8-Pad8)")
  (net 43 "Net-(J8-Pad9)")
  (net 44 "Net-(J8-Pad10)")
  (net 45 "Net-(J8-Pad11)")
  (net 46 "Net-(J8-Pad12)")
  (net 47 "Net-(J8-Pad13)")
  (net 48 "Net-(JP2-Pad2)")
  (net 49 "Net-(JP3-Pad2)")
  (net 50 "Net-(JP4-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.4064)
    (via_drill 0.2032)
    (uvia_dia 0.4064)
    (uvia_drill 0.2032)
    (add_net /HT16K33_COM0_AD)
    (add_net /HT16K33_COM1_KS0)
    (add_net /HT16K33_COM2_KS1)
    (add_net /HT16K33_COM3_KS2)
    (add_net /HT16K33_COM4)
    (add_net /HT16K33_COM5)
    (add_net /HT16K33_COM6)
    (add_net /HT16K33_COM7)
    (add_net /HT16K33_ROW0_A2)
    (add_net /HT16K33_ROW10_K8)
    (add_net /HT16K33_ROW11_K9)
    (add_net /HT16K33_ROW12_K10)
    (add_net /HT16K33_ROW13_K11)
    (add_net /HT16K33_ROW14_K12)
    (add_net /HT16K33_ROW15_K13_INT)
    (add_net /HT16K33_ROW1_A1)
    (add_net /HT16K33_ROW2_A0)
    (add_net /HT16K33_ROW3_K1)
    (add_net /HT16K33_ROW4_K2)
    (add_net /HT16K33_ROW5_K3)
    (add_net /HT16K33_ROW6_K4)
    (add_net /HT16K33_ROW7_K5)
    (add_net /HT16K33_ROW8_K6)
    (add_net /HT16K33_ROW9_K7)
    (add_net /I2C_SCL_5V5)
    (add_net /I2C_SDA_5V5)
    (add_net /P5V0)
    (add_net /P5V0_EXT)
    (add_net /P5V0_INT)
    (add_net GND)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(J8-Pad1)")
    (add_net "Net-(J8-Pad10)")
    (add_net "Net-(J8-Pad11)")
    (add_net "Net-(J8-Pad12)")
    (add_net "Net-(J8-Pad13)")
    (add_net "Net-(J8-Pad2)")
    (add_net "Net-(J8-Pad3)")
    (add_net "Net-(J8-Pad4)")
    (add_net "Net-(J8-Pad5)")
    (add_net "Net-(J8-Pad6)")
    (add_net "Net-(J8-Pad7)")
    (add_net "Net-(J8-Pad8)")
    (add_net "Net-(J8-Pad9)")
    (add_net "Net-(JP2-Pad2)")
    (add_net "Net-(JP3-Pad2)")
    (add_net "Net-(JP4-Pad2)")
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 95.25 99.314 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference JP4 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value I2C_AD_SEL_A2 (at 0 4.87 90) (layer F.Fab))
    (fp_text user %R (at 0 1.27) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 /HT16K33_ROW0_A2))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 50 "Net-(JP4-Pad2)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 101.6 68.58 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference JP1 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value PWR_SELECT (at 0 7.41 90) (layer F.Fab))
    (fp_text user %R (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /P5V0_INT))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 /P5V0))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 /P5V0_EXT))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:Barrel_Jack_CUI_PJ-102AH (layer F.Cu) (tedit 59BC552D)
    (at 106.68 63.5 180)
    (descr "Thin-pin DC Barrel Jack, https://cdn-shop.adafruit.com/datasheets/21mmdcjackDatasheet.pdf")
    (tags "Power Jack")
    (fp_text reference J3 (at 5.75 8.45 90) (layer F.SilkS))
    (fp_text value P5V0_EXT (at -5.5 6.2 90) (layer F.Fab))
    (fp_text user %R (at 0 6.5) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.6 2.6) (drill 1.6) (layers *.Cu *.Mask)
      (net 34 /P5V0_EXT))
    (pad 2 thru_hole circle (at 0 6 180) (size 2.6 2.6) (drill 1.6) (layers *.Cu *.Mask)
      (net 9 GND))
    (pad 3 thru_hole circle (at 4.7 3 180) (size 2.6 2.6) (drill 1.6) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connectors.3dshapes/Barrel_Jack_CUI_PJ-102AH.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 95.25 103.632 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference JP3 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value I2C_AD_SEL_A1 (at 0 4.87 90) (layer F.Fab))
    (fp_text user %R (at 0 1.27) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 /HT16K33_ROW1_A1))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 "Net-(JP3-Pad2)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 95.25 107.95 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference JP2 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value I2C_AD_SEL_A0 (at 0 4.87 90) (layer F.Fab))
    (fp_text user %R (at 0 1.27) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 /HT16K33_ROW2_A0))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 "Net-(JP2-Pad2)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_PH_S16B-PH-K_16x2.00mm_Angled (layer F.Cu) (tedit 58D3FE32)
    (at 84.06 127)
    (descr "JST PH series connector, S16B-PH-K, side entry type, through hole, Datasheet: http://www.jst-mfg.com/product/pdf/eng/ePH.pdf")
    (tags "connector jst ph")
    (fp_text reference J8 (at -3.669 -1.397) (layer F.SilkS))
    (fp_text value KS_Matrix (at 15 7.25) (layer F.Fab))
    (fp_text user %R (at 15 2.5) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 35 "Net-(J8-Pad1)"))
    (pad 2 thru_hole oval (at 2 0) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 36 "Net-(J8-Pad2)"))
    (pad 3 thru_hole oval (at 4 0) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 37 "Net-(J8-Pad3)"))
    (pad 4 thru_hole oval (at 6 0) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 38 "Net-(J8-Pad4)"))
    (pad 5 thru_hole oval (at 8 0) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 39 "Net-(J8-Pad5)"))
    (pad 6 thru_hole oval (at 10 0) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 40 "Net-(J8-Pad6)"))
    (pad 7 thru_hole oval (at 12 0) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 41 "Net-(J8-Pad7)"))
    (pad 8 thru_hole oval (at 14 0) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 42 "Net-(J8-Pad8)"))
    (pad 9 thru_hole oval (at 16 0) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 43 "Net-(J8-Pad9)"))
    (pad 10 thru_hole oval (at 18 0) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 44 "Net-(J8-Pad10)"))
    (pad 11 thru_hole oval (at 20 0) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 45 "Net-(J8-Pad11)"))
    (pad 12 thru_hole oval (at 22 0) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 46 "Net-(J8-Pad12)"))
    (pad 13 thru_hole oval (at 24 0) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 47 "Net-(J8-Pad13)"))
    (pad 14 thru_hole oval (at 26 0) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 3 "Net-(D2-Pad1)"))
    (pad 15 thru_hole oval (at 28 0) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 5 "Net-(D3-Pad1)"))
    (pad 16 thru_hole oval (at 30 0) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 7 "Net-(D4-Pad1)"))
    (model ${KISYS3DMOD}/Connectors_JST.3dshapes/JST_PH_S16B-PH-K_16x2.00mm_Angled.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_PH_S12B-PH-K_12x2.00mm_Angled (layer F.Cu) (tedit 58D3FE32)
    (at 121.92 119.32 90)
    (descr "JST PH series connector, S12B-PH-K, side entry type, through hole, Datasheet: http://www.jst-mfg.com/product/pdf/eng/ePH.pdf")
    (tags "connector jst ph")
    (fp_text reference J7 (at 1.5 -2.45 90) (layer F.SilkS))
    (fp_text value LED_PORT_D (at 11 7.25 90) (layer F.Fab))
    (fp_text user %R (at 11 2.5 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 24 /HT16K33_ROW8_K6))
    (pad 2 thru_hole oval (at 2 0 90) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 23 /HT16K33_ROW9_K7))
    (pad 3 thru_hole oval (at 4 0 90) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 22 /HT16K33_ROW10_K8))
    (pad 4 thru_hole oval (at 6 0 90) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 21 /HT16K33_ROW11_K9))
    (pad 5 thru_hole oval (at 8 0 90) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 20 /HT16K33_ROW12_K10))
    (pad 6 thru_hole oval (at 10 0 90) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 19 /HT16K33_ROW13_K11))
    (pad 7 thru_hole oval (at 12 0 90) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 18 /HT16K33_ROW14_K12))
    (pad 8 thru_hole oval (at 14 0 90) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 17 /HT16K33_ROW15_K13_INT))
    (pad 9 thru_hole oval (at 16 0 90) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 13 /HT16K33_COM4))
    (pad 10 thru_hole oval (at 18 0 90) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 14 /HT16K33_COM5))
    (pad 11 thru_hole oval (at 20 0 90) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 15 /HT16K33_COM6))
    (pad 12 thru_hole oval (at 22 0 90) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 16 /HT16K33_COM7))
    (model ${KISYS3DMOD}/Connectors_JST.3dshapes/JST_PH_S12B-PH-K_12x2.00mm_Angled.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_PH_S12B-PH-K_12x2.00mm_Angled (layer F.Cu) (tedit 58D3FE32)
    (at 76.2 96.52 270)
    (descr "JST PH series connector, S12B-PH-K, side entry type, through hole, Datasheet: http://www.jst-mfg.com/product/pdf/eng/ePH.pdf")
    (tags "connector jst ph")
    (fp_text reference J6 (at 1.5 -2.45 90) (layer F.SilkS))
    (fp_text value LED_PORT_B (at 11 7.25 90) (layer F.Fab))
    (fp_text user %R (at 11 2.5 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 32 /HT16K33_ROW0_A2))
    (pad 2 thru_hole oval (at 2 0 270) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 31 /HT16K33_ROW1_A1))
    (pad 3 thru_hole oval (at 4 0 270) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 30 /HT16K33_ROW2_A0))
    (pad 4 thru_hole oval (at 6 0 270) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 29 /HT16K33_ROW3_K1))
    (pad 5 thru_hole oval (at 8 0 270) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 28 /HT16K33_ROW4_K2))
    (pad 6 thru_hole oval (at 10 0 270) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 27 /HT16K33_ROW5_K3))
    (pad 7 thru_hole oval (at 12 0 270) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 26 /HT16K33_ROW6_K4))
    (pad 8 thru_hole oval (at 14 0 270) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 25 /HT16K33_ROW7_K5))
    (pad 9 thru_hole oval (at 16 0 270) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 13 /HT16K33_COM4))
    (pad 10 thru_hole oval (at 18 0 270) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 14 /HT16K33_COM5))
    (pad 11 thru_hole oval (at 20 0 270) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 15 /HT16K33_COM6))
    (pad 12 thru_hole oval (at 22 0 270) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 16 /HT16K33_COM7))
    (model ${KISYS3DMOD}/Connectors_JST.3dshapes/JST_PH_S12B-PH-K_12x2.00mm_Angled.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_PH_S12B-PH-K_12x2.00mm_Angled (layer F.Cu) (tedit 58D3FE32)
    (at 121.92 88.1 90)
    (descr "JST PH series connector, S12B-PH-K, side entry type, through hole, Datasheet: http://www.jst-mfg.com/product/pdf/eng/ePH.pdf")
    (tags "connector jst ph")
    (fp_text reference J5 (at 1.5 -2.45 90) (layer F.SilkS))
    (fp_text value LED_PORT_C (at 11 7.25 90) (layer F.Fab))
    (fp_text user %R (at 11 2.5 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 24 /HT16K33_ROW8_K6))
    (pad 2 thru_hole oval (at 2 0 90) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 23 /HT16K33_ROW9_K7))
    (pad 3 thru_hole oval (at 4 0 90) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 22 /HT16K33_ROW10_K8))
    (pad 4 thru_hole oval (at 6 0 90) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 21 /HT16K33_ROW11_K9))
    (pad 5 thru_hole oval (at 8 0 90) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 20 /HT16K33_ROW12_K10))
    (pad 6 thru_hole oval (at 10 0 90) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 19 /HT16K33_ROW13_K11))
    (pad 7 thru_hole oval (at 12 0 90) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 18 /HT16K33_ROW14_K12))
    (pad 8 thru_hole oval (at 14 0 90) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 17 /HT16K33_ROW15_K13_INT))
    (pad 9 thru_hole oval (at 16 0 90) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 2 /HT16K33_COM0_AD))
    (pad 10 thru_hole oval (at 18 0 90) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 4 /HT16K33_COM1_KS0))
    (pad 11 thru_hole oval (at 20 0 90) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 6 /HT16K33_COM2_KS1))
    (pad 12 thru_hole oval (at 22 0 90) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 8 /HT16K33_COM3_KS2))
    (model ${KISYS3DMOD}/Connectors_JST.3dshapes/JST_PH_S12B-PH-K_12x2.00mm_Angled.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_PH_S12B-PH-K_12x2.00mm_Angled (layer F.Cu) (tedit 58D3FE32)
    (at 76.2 65.7 270)
    (descr "JST PH series connector, S12B-PH-K, side entry type, through hole, Datasheet: http://www.jst-mfg.com/product/pdf/eng/ePH.pdf")
    (tags "connector jst ph")
    (fp_text reference J4 (at 1.5 -2.45 90) (layer F.SilkS))
    (fp_text value LED_PORT_A (at 11 7.25 90) (layer F.Fab))
    (fp_text user %R (at 11 2.5 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 32 /HT16K33_ROW0_A2))
    (pad 2 thru_hole oval (at 2 0 270) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 31 /HT16K33_ROW1_A1))
    (pad 3 thru_hole oval (at 4 0 270) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 30 /HT16K33_ROW2_A0))
    (pad 4 thru_hole oval (at 6 0 270) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 29 /HT16K33_ROW3_K1))
    (pad 5 thru_hole oval (at 8 0 270) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 28 /HT16K33_ROW4_K2))
    (pad 6 thru_hole oval (at 10 0 270) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 27 /HT16K33_ROW5_K3))
    (pad 7 thru_hole oval (at 12 0 270) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 26 /HT16K33_ROW6_K4))
    (pad 8 thru_hole oval (at 14 0 270) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 25 /HT16K33_ROW7_K5))
    (pad 9 thru_hole oval (at 16 0 270) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 2 /HT16K33_COM0_AD))
    (pad 10 thru_hole oval (at 18 0 270) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 4 /HT16K33_COM1_KS0))
    (pad 11 thru_hole oval (at 20 0 270) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 6 /HT16K33_COM2_KS1))
    (pad 12 thru_hole oval (at 22 0 270) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 8 /HT16K33_COM3_KS2))
    (model ${KISYS3DMOD}/Connectors_JST.3dshapes/JST_PH_S12B-PH-K_12x2.00mm_Angled.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 108.077 122.598 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R18 (at 3.440191 0 90) (layer F.SilkS))
    (fp_text value 47K (at 0 1.55 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(J8-Pad13)"))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 17 /HT16K33_ROW15_K13_INT))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 106.07675 122.588 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R17 (at 3.430191 -0.03175 90) (layer F.SilkS))
    (fp_text value 47K (at 0 1.55 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(J8-Pad12)"))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 18 /HT16K33_ROW14_K12))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 104.0765 122.588 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R16 (at 3.430191 0.0635 90) (layer F.SilkS))
    (fp_text value 47K (at 0 1.55 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(J8-Pad11)"))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 19 /HT16K33_ROW13_K11))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 102.07625 122.588 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R15 (at 3.430191 0.03175 90) (layer F.SilkS))
    (fp_text value 47K (at 0 1.55 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(J8-Pad10)"))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 20 /HT16K33_ROW12_K10))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 100.076 122.588 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R14 (at 3.430191 0 90) (layer F.SilkS))
    (fp_text value 47K (at 0 1.55 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(J8-Pad9)"))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 21 /HT16K33_ROW11_K9))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 98.07575 122.588 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R13 (at 3.430191 -0.03175 90) (layer F.SilkS))
    (fp_text value 47K (at 0 1.55 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(J8-Pad8)"))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 22 /HT16K33_ROW10_K8))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 96.0755 122.588 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R12 (at 3.430191 -0.0635 90) (layer F.SilkS))
    (fp_text value 47K (at 0 1.55 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(J8-Pad7)"))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 23 /HT16K33_ROW9_K7))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 94.07525 122.588 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R11 (at 3.430191 0.03175 90) (layer F.SilkS))
    (fp_text value 47K (at 0 1.55 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(J8-Pad6)"))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 24 /HT16K33_ROW8_K6))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 92.075 122.588 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R10 (at 3.430191 0 90) (layer F.SilkS))
    (fp_text value 47K (at 0 1.55 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(J8-Pad5)"))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 25 /HT16K33_ROW7_K5))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 90.07475 122.588 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R9 (at 2.954 -0.03175 90) (layer F.SilkS))
    (fp_text value 47K (at 0 1.55 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(J8-Pad4)"))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 26 /HT16K33_ROW6_K4))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 88.0745 122.588 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R8 (at 2.954 0.0635 90) (layer F.SilkS))
    (fp_text value 47K (at 0 1.55 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(J8-Pad3)"))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 27 /HT16K33_ROW5_K3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 86.07425 122.588 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at 2.954 0.03175 90) (layer F.SilkS))
    (fp_text value 47K (at 0 1.55 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(J8-Pad2)"))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 28 /HT16K33_ROW4_K2))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 84.074 122.588 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at 2.954 0 90) (layer F.SilkS))
    (fp_text value 47K (at 0 1.55 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(J8-Pad1)"))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 29 /HT16K33_ROW3_K1))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 103.56832 99.23526 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at 0 1.45) (layer B.SilkS))
    (fp_text value 47K (at 0 -1.55) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 50 "Net-(JP4-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 103.53566 103.51262 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 0 1.45) (layer B.SilkS))
    (fp_text value 47K (at 0 -1.55) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 49 "Net-(JP3-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 103.39814 107.90682 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 0 1.45) (layer B.SilkS))
    (fp_text value 47K (at 0 -1.55) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 48 "Net-(JP2-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 91.61 74.422)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at -2.964 0) (layer B.SilkS))
    (fp_text value DNP (at 0 -1.55) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 33 /P5V0))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 11 /I2C_SDA_5V5))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 91.59476 76.2)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at -2.94876 0.0762) (layer B.SilkS))
    (fp_text value DNP (at 0 -1.55) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 33 /P5V0))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 12 /I2C_SCL_5V5))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SOIC-28 (layer B.Cu) (tedit 0)
    (at 99.06 81.915 270)
    (descr "Module CMS SOJ 28 pins large")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference J2 (at 0 1.26238 270) (layer B.SilkS))
    (fp_text value HT16K33 (at 0 -1.27 270) (layer B.Fab))
    (pad 1 smd rect (at -8.255 -3.556 270) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 9 GND))
    (pad 2 smd rect (at -6.985 -3.556 270) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 2 /HT16K33_COM0_AD))
    (pad 3 smd rect (at -5.715 -3.556 270) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 4 /HT16K33_COM1_KS0))
    (pad 4 smd rect (at -4.445 -3.556 270) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 6 /HT16K33_COM2_KS1))
    (pad 5 smd rect (at -3.175 -3.556 270) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 8 /HT16K33_COM3_KS2))
    (pad 6 smd rect (at -1.905 -3.556 270) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 13 /HT16K33_COM4))
    (pad 7 smd rect (at -0.635 -3.556 270) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 14 /HT16K33_COM5))
    (pad 8 smd rect (at 0.635 -3.556 270) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 15 /HT16K33_COM6))
    (pad 9 smd rect (at 1.905 -3.556 270) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 16 /HT16K33_COM7))
    (pad 10 smd rect (at 3.175 -3.556 270) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 17 /HT16K33_ROW15_K13_INT))
    (pad 11 smd rect (at 4.445 -3.556 270) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 18 /HT16K33_ROW14_K12))
    (pad 12 smd rect (at 5.715 -3.556 270) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 19 /HT16K33_ROW13_K11))
    (pad 13 smd rect (at 6.985 -3.556 270) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 20 /HT16K33_ROW12_K10))
    (pad 14 smd rect (at 8.255 -3.556 270) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 21 /HT16K33_ROW11_K9))
    (pad 15 smd rect (at 8.255 3.556 270) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 22 /HT16K33_ROW10_K8))
    (pad 16 smd rect (at 6.985 3.556 270) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 23 /HT16K33_ROW9_K7))
    (pad 17 smd rect (at 5.715 3.556 270) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 24 /HT16K33_ROW8_K6))
    (pad 18 smd rect (at 4.445 3.556 270) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 25 /HT16K33_ROW7_K5))
    (pad 19 smd rect (at 3.175 3.556 270) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 26 /HT16K33_ROW6_K4))
    (pad 20 smd rect (at 1.905 3.556 270) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 27 /HT16K33_ROW5_K3))
    (pad 21 smd rect (at 0.635 3.556 270) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 28 /HT16K33_ROW4_K2))
    (pad 22 smd rect (at -0.635 3.556 270) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 29 /HT16K33_ROW3_K1))
    (pad 23 smd rect (at -1.905 3.556 270) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 30 /HT16K33_ROW2_A0))
    (pad 24 smd rect (at -3.175 3.556 270) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 31 /HT16K33_ROW1_A1))
    (pad 25 smd rect (at -4.445 3.556 270) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 32 /HT16K33_ROW0_A2))
    (pad 26 smd rect (at -5.715 3.556 270) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 12 /I2C_SCL_5V5))
    (pad 27 smd rect (at -6.985 3.556 270) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 11 /I2C_SDA_5V5))
    (pad 28 smd rect (at -8.255 3.556 270) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 33 /P5V0))
  )
  (module Connectors_JST:JST_PH_S4B-PH-K_04x2.00mm_Angled (layer F.Cu) (tedit 58D3FE32)
    (at 91.44 58.42 180)
    (descr "JST PH series connector, S4B-PH-K, side entry type, through hole, Datasheet: http://www.jst-mfg.com/product/pdf/eng/ePH.pdf")
    (tags "connector jst ph")
    (fp_text reference J1 (at 1.5 -2.45) (layer F.SilkS))
    (fp_text value Conn_01x04 (at 3 7.25) (layer F.Fab))
    (fp_text user %R (at 3 2.5) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 10 /P5V0_INT))
    (pad 2 thru_hole oval (at 2 0 180) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 11 /I2C_SDA_5V5))
    (pad 3 thru_hole oval (at 4 0 180) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 12 /I2C_SCL_5V5))
    (pad 4 thru_hole oval (at 6 0 180) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 9 GND))
    (model ${KISYS3DMOD}/Connectors_JST.3dshapes/JST_PH_S4B-PH-K_04x2.00mm_Angled.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_Pad_Via (layer F.Cu) (tedit 56DDBCCA)
    (at 124.46 129.54)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference H4 (at 0 -4.2) (layer F.SilkS))
    (fp_text value X4 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 9 GND))
    (pad 1 thru_hole circle (at 2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 9 GND))
    (pad 1 thru_hole circle (at 1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 9 GND))
    (pad 1 thru_hole circle (at 0 2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 9 GND))
    (pad 1 thru_hole circle (at -1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 9 GND))
    (pad 1 thru_hole circle (at -2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 9 GND))
    (pad 1 thru_hole circle (at -1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 9 GND))
    (pad 1 thru_hole circle (at 0 -2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 9 GND))
    (pad 1 thru_hole circle (at 1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 9 GND))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_Pad_Via (layer F.Cu) (tedit 56DDBCCA)
    (at 124.46 55.88)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference H3 (at 0 -4.2) (layer F.SilkS))
    (fp_text value X2 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 9 GND))
    (pad 1 thru_hole circle (at 2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 9 GND))
    (pad 1 thru_hole circle (at 1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 9 GND))
    (pad 1 thru_hole circle (at 0 2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 9 GND))
    (pad 1 thru_hole circle (at -1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 9 GND))
    (pad 1 thru_hole circle (at -2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 9 GND))
    (pad 1 thru_hole circle (at -1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 9 GND))
    (pad 1 thru_hole circle (at 0 -2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 9 GND))
    (pad 1 thru_hole circle (at 1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 9 GND))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_Pad_Via (layer F.Cu) (tedit 56DDBCCA)
    (at 73.66 55.88)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference H2 (at 0 -4.2) (layer F.SilkS))
    (fp_text value X3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 9 GND))
    (pad 1 thru_hole circle (at 2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 9 GND))
    (pad 1 thru_hole circle (at 1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 9 GND))
    (pad 1 thru_hole circle (at 0 2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 9 GND))
    (pad 1 thru_hole circle (at -1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 9 GND))
    (pad 1 thru_hole circle (at -2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 9 GND))
    (pad 1 thru_hole circle (at -1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 9 GND))
    (pad 1 thru_hole circle (at 0 -2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 9 GND))
    (pad 1 thru_hole circle (at 1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 9 GND))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_Pad_Via (layer F.Cu) (tedit 56DDBCCA)
    (at 73.66 129.54)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference H1 (at 0 -4.2) (layer F.SilkS))
    (fp_text value X1 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 9 GND))
    (pad 1 thru_hole circle (at 2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 9 GND))
    (pad 1 thru_hole circle (at 1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 9 GND))
    (pad 1 thru_hole circle (at 0 2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 9 GND))
    (pad 1 thru_hole circle (at -1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 9 GND))
    (pad 1 thru_hole circle (at -2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 9 GND))
    (pad 1 thru_hole circle (at -1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 9 GND))
    (pad 1 thru_hole circle (at 0 -2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 9 GND))
    (pad 1 thru_hole circle (at 1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 9 GND))
  )
  (module Diodes_SMD:D_SOD-123 (layer F.Cu) (tedit 58645DC7)
    (at 115.189 117.856 90)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D4 (at 0 -2 90) (layer F.SilkS))
    (fp_text value 1N4148W (at 0 2.1 90) (layer F.Fab))
    (fp_text user %R (at 0 -2 90) (layer F.Fab))
    (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D4-Pad1)"))
    (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 8 /HT16K33_COM3_KS2))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SOD-123 (layer F.Cu) (tedit 58645DC7)
    (at 112.522 117.857 90)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D3 (at 3.556 0 90) (layer F.SilkS))
    (fp_text value 1N4148W (at 0 2.1 90) (layer F.Fab))
    (fp_text user %R (at 0 -2 90) (layer F.Fab))
    (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D3-Pad1)"))
    (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 6 /HT16K33_COM2_KS1))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SOD-123 (layer F.Cu) (tedit 58645DC7)
    (at 109.855 117.857 90)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D2 (at 3.556 0 90) (layer F.SilkS))
    (fp_text value 1N4148W (at 0 2.1 90) (layer F.Fab))
    (fp_text user %R (at 0 -2 90) (layer F.Fab))
    (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 4 /HT16K33_COM1_KS0))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SOD-123 (layer B.Cu) (tedit 58645DC7)
    (at 109.46538 103.48722)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D1 (at 0 2) (layer B.SilkS))
    (fp_text value 1N4148W (at 0 -2.1) (layer B.Fab))
    (fp_text user %R (at 0 2) (layer B.Fab))
    (pad 1 smd rect (at -1.65 0) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 1.65 0) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask)
      (net 2 /HT16K33_COM0_AD))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_arc (start 73.66 129.54) (end 73.66 134.54) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 124.46 129.54) (end 129.46 129.54) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 73.66 55.88) (end 68.66 55.88) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 124.46 55.88) (end 124.46 50.88) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 124.46 134.54) (end 73.66 134.54) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 129.46 55.88) (end 129.46 129.54) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 124.46 50.88) (end 73.66 50.88) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.66 129.54) (end 68.66 55.88) (layer Edge.Cuts) (width 0.1))
  (zone (net 9) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 129.56794 134.44728) (xy 129.56794 50.72888) (xy 68.44284 51.2064) (xy 68.83908 134.5565) (xy 129.56794 134.5565)
      )
    )
  )
  (zone (net 9) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 68.64096 51.2064) (xy 129.56794 50.90668) (xy 129.56794 134.85622) (xy 68.64096 134.6581) (xy 68.64096 51.1048)
      )
    )
  )
)
