(kicad_pcb (version 20230410) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (pdf_front_fp_property_popups true)
      (pdf_back_fp_property_popups true)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "Net-(J1-Pin_4)")
  (net 2 "Net-(J1-Pin_6)")
  (net 3 "Net-(J2-Pin_1)")
  (net 4 "Net-(J2-Pin_2)")
  (net 5 "Net-(J2-Pin_3)")
  (net 6 "Net-(J2-Pin_4)")
  (net 7 "Net-(J2-Pin_5)")
  (net 8 "Net-(J2-Pin_6)")
  (net 9 "Net-(J1-Pin_5)")
  (net 10 "Net-(J1-Pin_1)")
  (net 11 "Net-(J1-Pin_2)")
  (net 12 "Net-(J1-Pin_3)")
  (net 13 "Net-(U1-A1)")
  (net 14 "Net-(U1-A0)")
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 111.75 93.3125 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "TPL0102BreakOut.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R3" (at 0 -1.43 -90) (layer "F.SilkS") hide)
    (fp_text value "R_US" (at 0 1.43 -90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "Net-(J1-Pin_4)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "Net-(U1-A0)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 111.75 82.1625 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "TPL0102BreakOut.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R4" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "R_US" (at 0 1.43 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "Net-(J1-Pin_4)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "Net-(U1-A1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Vertical" (layer "F.Cu")
    (at 116.84 93.98 180)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (property "Sheetfile" "TPL0102BreakOut.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J2" (at 0 -2.33 -180) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x06_Pin" (at 0 15.03 -180) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 6.35 -90) (layer "F.Fab") hide)
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(J2-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(J2-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(J2-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(J2-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(J2-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(J2-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SON:Texas_Instruments-RUC0014A-0-0-IPC_A" (layer "F.Cu")
    (at 113.05 87.701248 180)
    (property "Sheetfile" "TPL0102BreakOut.kicad_sch")
    (property "Sheetname" "")
    (property "ambient temperature range high" "+85°C")
    (property "ambient temperature range low" "-40°C")
    (property "automotive" "No")
    (property "category" "IC")
    (property "ciiva ids" "2913819")
    (property "device class L1" "Integrated Circuits (ICs)")
    (property "device class L2" "Data Converter ICs")
    (property "device class L3" "Digital Potentiometers")
    (property "digikey description" "IC DGT POT 100KOHM 256TAP 14QFN")
    (property "digikey part number" "296-28379-1-ND")
    (property "height" "0.4mm")
    (property "interface" "I2C")
    (property "ki_description" "TPL0102-100RUCR")
    (property "lead free" "Yes")
    (property "library id" "31eba2481818470a")
    (property "manufacturer" "Texas Instruments")
    (property "max supply voltage" "5.5V")
    (property "memory type" "EEPROM")
    (property "min supply voltage" "2.7V")
    (property "mouser description" "TEXAS INSTRUMENTS - TPL0102-100RUCR - DGTL POT, 256POS, 100K, DL, 14QFN")
    (property "mouser part number" "595-TPL0102-100RUCR")
    (property "nominal resistance" "100kΩ")
    (property "nominal supply current" "200uA")
    (property "number of circuits" "2")
    (property "number of taps" "256")
    (property "package" "QFN14")
    (property "release date" "1386908063")
    (property "rohs" "Yes")
    (property "standoff height" "0mm")
    (property "temperature coefficient" "92ppm/°C")
    (property "temperature range high" "+85°C")
    (property "temperature range low" "-40°C")
    (property "tolerance" "20%")
    (attr through_hole)
    (fp_text reference "U1" (at -2.456066 -3.156066 -180) (layer "F.SilkS") hide)
    (fp_text value "TPL0102-100RUCR" (at 0 0 -180) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.951247 -0.8 180) (size 1.009637 0.192474) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "Net-(J2-Pin_1)") (pinfunction "HA") (pintype "passive"))
    (pad "2" smd roundrect (at -0.951247 -0.4 180) (size 1.009637 0.192474) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
      (net 4 "Net-(J2-Pin_2)") (pinfunction "LA") (pintype "passive"))
    (pad "3" smd roundrect (at -0.951247 0 180) (size 1.009637 0.192474) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
      (net 5 "Net-(J2-Pin_3)") (pinfunction "WA") (pintype "passive"))
    (pad "4" smd roundrect (at -0.951247 0.4 180) (size 1.009637 0.192474) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
      (net 6 "Net-(J2-Pin_4)") (pinfunction "HB") (pintype "passive"))
    (pad "5" smd roundrect (at -0.951247 0.8 180) (size 1.009637 0.192474) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
      (net 7 "Net-(J2-Pin_5)") (pinfunction "LB") (pintype "passive"))
    (pad "6" smd roundrect (at -0.2 0.951248 180) (size 0.192474 1.009637) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
      (net 8 "Net-(J2-Pin_6)") (pinfunction "WB") (pintype "passive"))
    (pad "7" smd roundrect (at 0.2 0.951248 180) (size 0.192474 1.009637) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
      (net 9 "Net-(J1-Pin_5)") (pinfunction "A2") (pintype "input"))
    (pad "8" smd roundrect (at 0.951248 0.8 180) (size 1.009637 0.192474) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
      (net 10 "Net-(J1-Pin_1)") (pinfunction "VSS") (pintype "power_in"))
    (pad "9" smd roundrect (at 0.951248 0.4 180) (size 1.009637 0.192474) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
      (net 11 "Net-(J1-Pin_2)") (pinfunction "SDA") (pintype "bidirectional"))
    (pad "10" smd roundrect (at 0.951248 0 180) (size 1.009637 0.192474) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
      (net 12 "Net-(J1-Pin_3)") (pinfunction "SCL") (pintype "input"))
    (pad "11" smd roundrect (at 0.951248 -0.4 180) (size 1.009637 0.192474) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
      (net 1 "Net-(J1-Pin_4)") (pinfunction "GND") (pintype "power_in"))
    (pad "12" smd roundrect (at 0.951248 -0.8 180) (size 1.009637 0.192474) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
      (net 13 "Net-(U1-A1)") (pinfunction "A1") (pintype "input"))
    (pad "13" smd roundrect (at 0.2 -0.951247 180) (size 0.192474 1.009637) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
      (net 14 "Net-(U1-A0)") (pinfunction "A0") (pintype "input"))
    (pad "14" smd roundrect (at -0.2 -0.951247 180) (size 0.192474 1.009637) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
      (net 2 "Net-(J1-Pin_6)") (pinfunction "VDD") (pintype "power_in"))
    (model "eec.models/Texas_Instruments_-_TPL0102-100RUCR.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Vertical" (layer "F.Cu")
    (at 109.22 81.28)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (property "Sheetfile" "TPL0102BreakOut.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J1" (at 0 -2.33) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x06_Pin" (at 0 15.03) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 6.35 90) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(J1-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(J1-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 12 "Net-(J1-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "Net-(J1-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(J1-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "Net-(J1-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 114.25 82.1625 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "TPL0102BreakOut.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R1" (at 0 -1.43 -90) (layer "F.SilkS") hide)
    (fp_text value "R_US" (at 0 1.43 -90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "Net-(U1-A1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "Net-(J1-Pin_6)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 114.25 93.3125 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "TPL0102BreakOut.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R2" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "R_US" (at 0 1.43 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "Net-(U1-A0)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "Net-(J1-Pin_6)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_rect (start 107.5 79.5) (end 118.5 95.75)
    (fill none) (layer "Edge.Cuts"))
)
