(kicad_pcb (version 20171130) (host pcbnew 5.0.2-bee76a0~70~ubuntu18.04.1)
  (general
    (thickness 1.6)
    (drawings 7)
    (tracks 916)
    (zones 0)
    (modules 73)
    (nets 92)
  )
  (page A4)
  (title_block
    (title "Skyfire PCB")
    (date 2019-02-22)
    (rev v03)
    (company "UAH Space Hardware Club")
    (comment 2 "Zac Faudi")
    (comment 3 "Noah Schwalb")
    (comment 4 "Alex Spaulding")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.2032)
    (user_trace_width 0.2032)
    (user_trace_width 0.5588)
    (trace_clearance 0.1524)
    (zone_clearance 0.1525)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3.2 3.2)
    (pad_drill 3.2)
    (pad_to_mask_clearance 0.0508)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFF77F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +6V)
  (net 2 GND)
  (net 3 +3V3)
  (net 4 "Net-(C4-Pad1)")
  (net 5 "Net-(C7-Pad2)")
  (net 6 /MCU_VCC)
  (net 7 /MCU_AVCC)
  (net 8 "Net-(D1-Pad1)")
  (net 9 "Net-(D1-Pad2)")
  (net 10 "Net-(D2-Pad2)")
  (net 11 "Net-(D3-Pad2)")
  (net 12 "Net-(D4-PadA)")
  (net 13 /PDI_DATA)
  (net 14 "Net-(J1-Pad3)")
  (net 15 "Net-(J1-Pad4)")
  (net 16 /PDI_CLK)
  (net 17 "Net-(J2-Pad3)")
  (net 18 "Net-(J2-Pad2)")
  (net 19 "Net-(J2-PadSH)")
  (net 20 "Net-(LS1-PadN)")
  (net 21 "Net-(M1-Pad1)")
  (net 22 "Net-(M1-Pad3)")
  (net 23 "Net-(M2-Pad1)")
  (net 24 "Net-(M3-Pad1)")
  (net 25 "Net-(MOD1-Pad2)")
  (net 26 "Net-(MOD1-Pad3)")
  (net 27 /MISO)
  (net 28 "Net-(MOD1-Pad5)")
  (net 29 "Net-(MOD1-Pad6)")
  (net 30 "Net-(MOD1-Pad7)")
  (net 31 "Net-(MOD1-Pad8)")
  (net 32 "Net-(MOD1-Pad9)")
  (net 33 /MOSI)
  (net 34 "Net-(MOD1-Pad12)")
  (net 35 "Net-(MOD1-Pad13)")
  (net 36 "Net-(MOD1-Pad14)")
  (net 37 "Net-(MOD1-Pad15)")
  (net 38 "Net-(MOD1-Pad16)")
  (net 39 /~SS_XBEE)
  (net 40 /SCLK)
  (net 41 "Net-(MOD1-Pad19)")
  (net 42 "Net-(MOD1-Pad20)")
  (net 43 /CAMERA_DATA)
  (net 44 "Net-(Q1-Pad3)")
  (net 45 /Finn_Power)
  (net 46 /LED_MOS)
  (net 47 /FINN_SERVO_TWO)
  (net 48 /FINN_SERVO_ONE)
  (net 49 /Release_Servo)
  (net 50 /BUZZER_MOS)
  (net 51 /PA6-Therm)
  (net 52 /PA7-Voltage)
  (net 53 "Net-(R7-Pad2)")
  (net 54 /SCL)
  (net 55 /SDA)
  (net 56 "Net-(U2-Pad27)")
  (net 57 "Net-(U2-Pad26)")
  (net 58 "Net-(U2-Pad15)")
  (net 59 /HOST_INTN)
  (net 60 /BNO_NRST)
  (net 61 /BNO_CLOCKSEL0)
  (net 62 /BNO_WAKE)
  (net 63 /BNO_BOOTN)
  (net 64 "Net-(U2-Pad16)")
  (net 65 /~SS_BNO080)
  (net 66 /~SS_5607)
  (net 67 "Net-(U5-Pad1)")
  (net 68 "Net-(U5-Pad2)")
  (net 69 "Net-(U5-Pad3)")
  (net 70 /PA5-Hall_Effect)
  (net 71 /OpenLog_MISO)
  (net 72 /OpenLog_MOSI)
  (net 73 /OpenLog_GRN)
  (net 74 "Net-(U8-Pad1)")
  (net 75 "Net-(U8-Pad2)")
  (net 76 "Net-(U8-Pad3)")
  (net 77 "Net-(U8-Pad4)")
  (net 78 /GPS_MISO)
  (net 79 /GPS_MOSI)
  (net 80 "Net-(U8-Pad9)")
  (net 81 "Net-(U9-Pad4)")
  (net 82 "Net-(U9-Pad5)")
  (net 83 "Net-(U9-Pad6)")
  (net 84 "Net-(U9-Pad7)")
  (net 85 "Net-(U9-Pad25)")
  (net 86 "Net-(U9-Pad26)")
  (net 87 "Net-(U9-Pad27)")
  (net 88 "Net-(U9-Pad28)")
  (net 89 "Net-(U9-Pad29)")
  (net 90 "Net-(U9-Pad36)")
  (net 91 "Net-(U9-Pad37)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.2032)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net /BNO_BOOTN)
    (add_net /BNO_CLOCKSEL0)
    (add_net /BNO_NRST)
    (add_net /BNO_WAKE)
    (add_net /BUZZER_MOS)
    (add_net /CAMERA_DATA)
    (add_net /FINN_SERVO_ONE)
    (add_net /FINN_SERVO_TWO)
    (add_net /Finn_Power)
    (add_net /GPS_MISO)
    (add_net /GPS_MOSI)
    (add_net /HOST_INTN)
    (add_net /LED_MOS)
    (add_net /MCU_AVCC)
    (add_net /MCU_VCC)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /OpenLog_GRN)
    (add_net /OpenLog_MISO)
    (add_net /OpenLog_MOSI)
    (add_net /PA5-Hall_Effect)
    (add_net /PA6-Therm)
    (add_net /PA7-Voltage)
    (add_net /PDI_CLK)
    (add_net /PDI_DATA)
    (add_net /Release_Servo)
    (add_net /SCL)
    (add_net /SCLK)
    (add_net /SDA)
    (add_net /~SS_5607)
    (add_net /~SS_BNO080)
    (add_net /~SS_XBEE)
    (add_net GND)
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C7-Pad2)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-PadA)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-PadSH)")
    (add_net "Net-(LS1-PadN)")
    (add_net "Net-(M1-Pad1)")
    (add_net "Net-(M1-Pad3)")
    (add_net "Net-(M2-Pad1)")
    (add_net "Net-(M3-Pad1)")
    (add_net "Net-(MOD1-Pad12)")
    (add_net "Net-(MOD1-Pad13)")
    (add_net "Net-(MOD1-Pad14)")
    (add_net "Net-(MOD1-Pad15)")
    (add_net "Net-(MOD1-Pad16)")
    (add_net "Net-(MOD1-Pad19)")
    (add_net "Net-(MOD1-Pad2)")
    (add_net "Net-(MOD1-Pad20)")
    (add_net "Net-(MOD1-Pad3)")
    (add_net "Net-(MOD1-Pad5)")
    (add_net "Net-(MOD1-Pad6)")
    (add_net "Net-(MOD1-Pad7)")
    (add_net "Net-(MOD1-Pad8)")
    (add_net "Net-(MOD1-Pad9)")
    (add_net "Net-(Q1-Pad3)")
    (add_net "Net-(R7-Pad2)")
    (add_net "Net-(U2-Pad15)")
    (add_net "Net-(U2-Pad16)")
    (add_net "Net-(U2-Pad26)")
    (add_net "Net-(U2-Pad27)")
    (add_net "Net-(U5-Pad1)")
    (add_net "Net-(U5-Pad2)")
    (add_net "Net-(U5-Pad3)")
    (add_net "Net-(U8-Pad1)")
    (add_net "Net-(U8-Pad2)")
    (add_net "Net-(U8-Pad3)")
    (add_net "Net-(U8-Pad4)")
    (add_net "Net-(U8-Pad9)")
    (add_net "Net-(U9-Pad25)")
    (add_net "Net-(U9-Pad26)")
    (add_net "Net-(U9-Pad27)")
    (add_net "Net-(U9-Pad28)")
    (add_net "Net-(U9-Pad29)")
    (add_net "Net-(U9-Pad36)")
    (add_net "Net-(U9-Pad37)")
    (add_net "Net-(U9-Pad4)")
    (add_net "Net-(U9-Pad5)")
    (add_net "Net-(U9-Pad6)")
    (add_net "Net-(U9-Pad7)")
  )
  (net_class "High Current" ""
    (clearance 0.1524)
    (trace_width 0.5588)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +6V)
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical (layer F.Cu) (tedit 5AE5139B)
    (at 238.76 121.158)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=2.54mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 2.54mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference TH1 (at 1.27 2.286) (layer F.SilkS))
    (fp_text value NTCLE100 (at 1.27 1.92) (layer F.Fab))
    (fp_text user %R (at 1.27 -1.92) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 51 /PA6-Therm))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:MOLEX-1X2_LOCK (layer F.Cu) (tedit 5963E8A8)
    (at 233.172 121.158)
    (descr "MOLEX 2-PIN PLATED THROUGH-HOLE LOCKING FOOTPRINT")
    (tags "MOLEX 2-PIN PLATED THROUGH-HOLE LOCKING FOOTPRINT")
    (attr virtual)
    (fp_text reference BT1 (at 0 -3.556) (layer F.SilkS))
    (fp_text value Battery_Cell (at 0 3.175) (layer F.SilkS))
    (pad 1 thru_hole rect (at -0.127 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 +6V) (solder_mask_margin 0.1016))
    (pad 2 thru_hole circle (at 2.667 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND) (solder_mask_margin 0.1016))
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 214.757 65.532)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C1 (at 2.794 0) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 3 +3V3))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 214.766 67.564)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C2 (at 2.785 0) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 235.712 116.341 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C3 (at 0.009 -2.032 180) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 +6V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 210.693 70.367 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C4 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 4 "Net-(C4-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 210.566 79.257 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C5 (at -2.531 0) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 3 +3V3))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B36C52B)
    (at 241.808 111.506 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C6 (at 2.54 0 180) (layer B.SilkS))
    (fp_text value 1uF (at 0 -1.65 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B36C52B)
    (at 204.225 112.522 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C7 (at 2.803 0 180) (layer B.SilkS))
    (fp_text value 0.1uf (at 0 -1.65 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 5 "Net-(C7-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B36C52B)
    (at 202.692818 62.130703 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C8 (at -2.440703 0.000818) (layer B.SilkS))
    (fp_text value 1uF (at 0 -1.65 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B36C52B)
    (at 204.724 62.130703 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C9 (at -2.440703 0.000818) (layer B.SilkS))
    (fp_text value 47pF (at 0 -1.65 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B36C52B)
    (at 242.062 61.468)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C10 (at 0 -1.651) (layer B.SilkS))
    (fp_text value 1uF (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 1 +6V))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 236.719 108.712)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C11 (at -0.009 -1.651) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 6 /MCU_VCC))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B36C52B)
    (at 218.186 109.22)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C12 (at 0 1.65) (layer B.SilkS))
    (fp_text value 100nF (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 6 /MCU_VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B36C52B)
    (at 218.694 89.653 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C13 (at -2.531 0) (layer B.SilkS))
    (fp_text value 10uF (at 0 -1.65 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 7 /MCU_AVCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B36C52B)
    (at 212.598 102.099 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C14 (at -0.009 2.413 180) (layer B.SilkS))
    (fp_text value 100nF (at 0 -1.65 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 6 /MCU_VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B36C52B)
    (at 215.392 89.653 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C15 (at -2.531 0) (layer B.SilkS))
    (fp_text value 100nF (at 0 -1.65 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 7 /MCU_AVCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B36C52B)
    (at 226.06 98.298)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C16 (at 0 -1.524) (layer B.SilkS))
    (fp_text value 100nF (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 6 /MCU_VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B4B45C9)
    (at 233.567 101.854)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (attr smd)
    (fp_text reference D1 (at 0 -1.43) (layer F.SilkS))
    (fp_text value "Power Status" (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 "Net-(D1-Pad1)"))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B4B45C9)
    (at 233.68 95.758)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (attr smd)
    (fp_text reference D2 (at 0 -1.43) (layer F.SilkS))
    (fp_text value "3V3 Status" (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B4B45C9)
    (at 233.567 98.806)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (attr smd)
    (fp_text reference D3 (at 0 -1.43) (layer F.SilkS))
    (fp_text value "6V Status" (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 "Net-(D3-Pad2)"))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:SOD-123 (layer B.Cu) (tedit 5AD0B3EC)
    (at 215.392 58.674 180)
    (fp_text reference D4 (at -0.01 1.89 180) (layer B.SilkS))
    (fp_text value 1N4148W-TP (at 0.07 -2.05 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad K smd rect (at -2.475 0 180) (size 0.9 0.95) (layers B.Cu B.Paste B.Mask)
      (net 1 +6V))
    (pad A smd rect (at 2.475 0 180) (size 0.9 0.95) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(D4-PadA)"))
  )
  (module Inductor_SMD:L_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B36C52B)
    (at 221.996 89.671 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "inductor handsolder")
    (attr smd)
    (fp_text reference FB1 (at -2.549 0) (layer B.SilkS))
    (fp_text value 220@100MHz (at 0 -1.65 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 7 /MCU_AVCC))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 6 /MCU_VCC))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 203 53)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference H1 (at 0 -4.2) (layer F.SilkS))
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 247 53)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference H2 (at 0 -4.2) (layer F.SilkS))
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 203 122)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference H3 (at -5.642 -0.226) (layer F.SilkS))
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 247 122)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference H4 (at 5.73 -1.496) (layer F.SilkS))
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Connectors:2X3 (layer F.Cu) (tedit 5963E22E)
    (at 224.536 122.174)
    (descr "PLATED THROUGH HOLE - 2X3")
    (tags "PLATED THROUGH HOLE - 2X3")
    (attr virtual)
    (fp_text reference J1 (at 0 -4.445) (layer F.SilkS))
    (fp_text value PDI_Interface (at 0 2.286) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 13 /PDI_DATA) (solder_mask_margin 0.1016))
    (pad 2 thru_hole circle (at 0 -2.54) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 +3V3) (solder_mask_margin 0.1016))
    (pad 3 thru_hole circle (at 2.54 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 14 "Net-(J1-Pad3)") (solder_mask_margin 0.1016))
    (pad 4 thru_hole circle (at 2.54 -2.54) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 15 "Net-(J1-Pad4)") (solder_mask_margin 0.1016))
    (pad 5 thru_hole circle (at 5.08 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 16 /PDI_CLK) (solder_mask_margin 0.1016))
    (pad 6 thru_hole circle (at 5.08 -2.54) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND) (solder_mask_margin 0.1016))
  )
  (module digikey-footprints:USB_Micro_B_Female_10118193-0001LF (layer F.Cu) (tedit 5BD21A05)
    (at 211.512 53.34 180)
    (descr http://portal.fciconnect.com/Comergent//fci/drawing/10118193.pdf)
    (fp_text reference J2 (at 0.184 2.032 180) (layer F.SilkS))
    (fp_text value 10118193-0001LF (at 0 4.5 180) (layer F.Fab))
    (fp_text user %R (at 0.06 1.86 180) (layer F.Fab))
    (pad 3 smd rect (at 0 -2.675 180) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(J2-Pad3)"))
    (pad 4 smd rect (at 0.65 -2.675 180) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at 1.3 -2.675 180) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -0.65 -2.675 180) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(J2-Pad2)"))
    (pad 1 smd rect (at -1.3 -2.675 180) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(D4-PadA)"))
    (pad SH thru_hole oval (at 3.3 0 180) (size 0.9 1.6) (drill oval 0.5 1.2) (layers *.Cu *.Mask)
      (net 19 "Net-(J2-PadSH)"))
    (pad SH thru_hole oval (at -3.3 0 180) (size 0.9 1.6) (drill oval 0.5 1.2) (layers *.Cu *.Mask)
      (net 19 "Net-(J2-PadSH)"))
    (pad SH smd rect (at -3.2 -2.45 180) (size 1.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(J2-PadSH)"))
    (pad SH smd rect (at 3.2 -2.45 180) (size 1.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(J2-PadSH)"))
    (pad SH smd rect (at -1.2 0 180) (size 1.9 1.9) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(J2-PadSH)"))
    (pad SH smd rect (at 1.2 0 180) (size 1.9 1.9) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(J2-PadSH)"))
  )
  (module Inductor_SMD:L_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 235.712 111.769 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "inductor handsolder")
    (attr smd)
    (fp_text reference L1 (at 0.009 -1.778 180) (layer F.SilkS))
    (fp_text value 10uH (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 3 +3V3))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 6 /MCU_VCC))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module CSS-95B30-SMT:CUI_CSS-95B30-SMT (layer F.Cu) (tedit 5C70B2A5)
    (at 213.947 113.618)
    (attr smd)
    (fp_text reference LS1 (at 6.525 2.587) (layer F.SilkS))
    (fp_text value CSS-95B30-SMT (at -1.72768 7.17612) (layer F.SilkS) hide)
    (fp_text user + (at -3.127 6.524) (layer F.SilkS))
    (fp_text user - (at -6.68124 -4.08968) (layer F.SilkS))
    (pad N smd rect (at -3 -5) (size 2.5 2) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(LS1-PadN)"))
    (pad 2 smd rect (at 3 -5) (size 2.5 2) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at 3 5) (size 2.5 2) (layers F.Cu F.Paste F.Mask))
    (pad P smd rect (at -3 5) (size 2.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 +6V))
  )
  (module Connector_JST:JST_XH_B03B-XH-A_1x03_P2.50mm_Vertical (layer F.Cu) (tedit 5B7754C5)
    (at 245.364 72.898 270)
    (descr "JST XH series connector, B03B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST XH side entry")
    (fp_text reference M1 (at 2.5 -3.55 270) (layer F.SilkS))
    (fp_text value Finn_Servo_One (at 2.5 4.6 270) (layer F.Fab))
    (fp_text user %R (at 2.5 2.7 270) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 21 "Net-(M1-Pad1)"))
    (pad 2 thru_hole oval (at 2.5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 1 +6V))
    (pad 3 thru_hole oval (at 5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 22 "Net-(M1-Pad3)"))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_XH_B03B-XH-A_1x03_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_XH_B03B-XH-A_1x03_P2.50mm_Vertical (layer F.Cu) (tedit 5B7754C5)
    (at 232.41 53.34)
    (descr "JST XH series connector, B03B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST XH side entry")
    (fp_text reference M2 (at 6.858 4.953) (layer F.SilkS))
    (fp_text value Finn_Servo_Two (at 2.5 4.6) (layer F.Fab))
    (fp_text user %R (at 2.5 2.7) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 23 "Net-(M2-Pad1)"))
    (pad 2 thru_hole oval (at 2.5 0) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 1 +6V))
    (pad 3 thru_hole oval (at 5 0) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 22 "Net-(M1-Pad3)"))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_XH_B03B-XH-A_1x03_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_XH_B03B-XH-A_1x03_P2.50mm_Vertical (layer F.Cu) (tedit 5B7754C5)
    (at 219.202 53.34)
    (descr "JST XH series connector, B03B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST XH side entry")
    (fp_text reference M3 (at 6.35 4.699) (layer F.SilkS))
    (fp_text value Release_Servo (at 2.5 4.6) (layer F.Fab))
    (fp_text user %R (at 2.5 2.7) (layer F.Fab))
    (pad 3 thru_hole oval (at 5 0) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 2.5 0) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 1 +6V))
    (pad 1 thru_hole roundrect (at 0 0) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 24 "Net-(M3-Pad1)"))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_XH_B03B-XH-A_1x03_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:XBEE_PRO-20_THT (layer F.Cu) (tedit 59947AD9)
    (at 213.614 74.93)
    (fp_text reference MOD1 (at -10.414 -16.51) (layer F.SilkS))
    (fp_text value XBP9B-DMWT-002 (at 0 17.56) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at -11 -9) (size 1.7 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 2 thru_hole circle (at -11 -7) (size 1.7 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 25 "Net-(MOD1-Pad2)"))
    (pad 3 thru_hole circle (at -11 -5) (size 1.7 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 26 "Net-(MOD1-Pad3)"))
    (pad 4 thru_hole circle (at -11 -3) (size 1.7 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 27 /MISO))
    (pad 5 thru_hole circle (at -11 -1) (size 1.7 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 28 "Net-(MOD1-Pad5)"))
    (pad 6 thru_hole circle (at -11 1) (size 1.7 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 29 "Net-(MOD1-Pad6)"))
    (pad 7 thru_hole circle (at -11 3) (size 1.7 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 30 "Net-(MOD1-Pad7)"))
    (pad 8 thru_hole circle (at -11 5) (size 1.7 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 31 "Net-(MOD1-Pad8)"))
    (pad 9 thru_hole circle (at -11 7) (size 1.7 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 32 "Net-(MOD1-Pad9)"))
    (pad 10 thru_hole circle (at -11 9) (size 1.7 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 11 thru_hole circle (at 11 9) (size 1.7 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 33 /MOSI))
    (pad 12 thru_hole circle (at 11 7) (size 1.7 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 34 "Net-(MOD1-Pad12)"))
    (pad 13 thru_hole circle (at 11 5) (size 1.7 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 35 "Net-(MOD1-Pad13)"))
    (pad 14 thru_hole circle (at 11 3) (size 1.7 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 36 "Net-(MOD1-Pad14)"))
    (pad 15 thru_hole circle (at 11 1) (size 1.7 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 37 "Net-(MOD1-Pad15)"))
    (pad 16 thru_hole circle (at 11 -1) (size 1.7 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 38 "Net-(MOD1-Pad16)"))
    (pad 17 thru_hole circle (at 11 -3) (size 1.7 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 39 /~SS_XBEE))
    (pad 18 thru_hole circle (at 11 -5) (size 1.7 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 40 /SCLK))
    (pad 19 thru_hole circle (at 11 -7) (size 1.7 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 41 "Net-(MOD1-Pad19)"))
    (pad 20 thru_hole circle (at 11 -9) (size 1.7 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 42 "Net-(MOD1-Pad20)"))
  )
  (module digikey-footprints:SOT-23-3 (layer F.Cu) (tedit 59D275F3)
    (at 239.361 89.408)
    (fp_text reference Q1 (at 0.025 -3.375) (layer F.SilkS))
    (fp_text value CAMERA_MOS (at 0.025 3.25) (layer F.Fab))
    (fp_text user %R (at -0.125 0.15) (layer F.Fab))
    (pad 1 smd rect (at -1.05 -0.95) (size 1.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 43 /CAMERA_DATA) (solder_mask_margin 0.07))
    (pad 2 smd rect (at -1.05 0.95) (size 1.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.07))
    (pad 3 smd rect (at 1.05 0) (size 1.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(Q1-Pad3)") (solder_mask_margin 0.07))
  )
  (module digikey-footprints:SOT-23-3 (layer F.Cu) (tedit 59D275F3)
    (at 238.345 79.629)
    (fp_text reference Q2 (at 0.025 -3.375) (layer F.SilkS))
    (fp_text value Finn_Power (at 0.025 3.25) (layer F.Fab))
    (fp_text user %R (at -0.125 0.15) (layer F.Fab))
    (pad 3 smd rect (at 1.05 0) (size 1.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(M1-Pad3)") (solder_mask_margin 0.07))
    (pad 2 smd rect (at -1.05 0.95) (size 1.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.07))
    (pad 1 smd rect (at -1.05 -0.95) (size 1.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 45 /Finn_Power) (solder_mask_margin 0.07))
  )
  (module digikey-footprints:SOT-23-3 (layer B.Cu) (tedit 59D275F3)
    (at 238.047712 101.919847 180)
    (fp_text reference Q3 (at 0.049712 2.605847 180) (layer B.SilkS))
    (fp_text value LED_MOS (at 0.025 -3.25 180) (layer B.Fab))
    (fp_text user %R (at -0.125 -0.15 180) (layer B.Fab))
    (pad 3 smd rect (at 1.05 0 180) (size 1.3 0.6) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(D1-Pad1)") (solder_mask_margin 0.07))
    (pad 2 smd rect (at -1.05 -0.95 180) (size 1.3 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND) (solder_mask_margin 0.07))
    (pad 1 smd rect (at -1.05 0.95 180) (size 1.3 0.6) (layers B.Cu B.Paste B.Mask)
      (net 46 /LED_MOS) (solder_mask_margin 0.07))
  )
  (module digikey-footprints:SOT-23-3 (layer F.Cu) (tedit 59D275F3)
    (at 234.569 60.198 90)
    (fp_text reference Q4 (at 0.025 -3.375 90) (layer F.SilkS))
    (fp_text value Finn_Servo_One (at 0.025 3.25 90) (layer F.Fab))
    (fp_text user %R (at -0.125 0.15 90) (layer F.Fab))
    (pad 3 smd rect (at 1.05 0 90) (size 1.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(M2-Pad1)") (solder_mask_margin 0.07))
    (pad 2 smd rect (at -1.05 0.95 90) (size 1.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.07))
    (pad 1 smd rect (at -1.05 -0.95 90) (size 1.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 47 /FINN_SERVO_TWO) (solder_mask_margin 0.07))
  )
  (module digikey-footprints:SOT-23-3 (layer F.Cu) (tedit 59D275F3)
    (at 238.472 73.025)
    (fp_text reference Q5 (at 0.025 -3.375) (layer F.SilkS))
    (fp_text value Finn_Servo_Two (at 0.025 3.25) (layer F.Fab))
    (fp_text user %R (at -0.125 0.15) (layer F.Fab))
    (pad 1 smd rect (at -1.05 -0.95) (size 1.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 48 /FINN_SERVO_ONE) (solder_mask_margin 0.07))
    (pad 2 smd rect (at -1.05 0.95) (size 1.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.07))
    (pad 3 smd rect (at 1.05 0) (size 1.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(M1-Pad1)") (solder_mask_margin 0.07))
  )
  (module digikey-footprints:SOT-23-3 (layer B.Cu) (tedit 59D275F3)
    (at 224.189 60.899)
    (fp_text reference Q6 (at 0.025 3.375) (layer B.SilkS))
    (fp_text value RELEASE_MOS (at 0.025 -3.25) (layer B.Fab))
    (fp_text user %R (at -0.125 -0.15) (layer B.Fab))
    (pad 1 smd rect (at -1.05 0.95) (size 1.3 0.6) (layers B.Cu B.Paste B.Mask)
      (net 49 /Release_Servo) (solder_mask_margin 0.07))
    (pad 2 smd rect (at -1.05 -0.95) (size 1.3 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND) (solder_mask_margin 0.07))
    (pad 3 smd rect (at 1.05 0) (size 1.3 0.6) (layers B.Cu B.Paste B.Mask)
      (net 24 "Net-(M3-Pad1)") (solder_mask_margin 0.07))
  )
  (module digikey-footprints:SOT-23-3 (layer B.Cu) (tedit 59D275F3)
    (at 214.918 113.858)
    (fp_text reference Q7 (at -0.034 -2.733) (layer B.SilkS))
    (fp_text value BUZZER_MOS (at 0.025 -3.25) (layer B.Fab))
    (fp_text user %R (at -0.125 -0.15) (layer B.Fab))
    (pad 3 smd rect (at 1.05 0) (size 1.3 0.6) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(LS1-PadN)") (solder_mask_margin 0.07))
    (pad 2 smd rect (at -1.05 -0.95) (size 1.3 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND) (solder_mask_margin 0.07))
    (pad 1 smd rect (at -1.05 0.95) (size 1.3 0.6) (layers B.Cu B.Paste B.Mask)
      (net 50 /BUZZER_MOS) (solder_mask_margin 0.07))
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B36C52B)
    (at 235.331 89.399 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at -2.531 0) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.65 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 43 /CAMERA_DATA))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B36C52B)
    (at 238.76 117.856 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R2 (at -2.54 0) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.65 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 51 /PA6-Therm))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 225.543 116.586)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R3 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 10k (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 16 /PDI_CLK))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B36C52B)
    (at 205.486 100.33 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R4 (at 2.794 0 180) (layer B.SilkS))
    (fp_text value 30k (at 0 -1.65 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 52 /PA7-Voltage))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 1 +6V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B36C52B)
    (at 205.495 98.171)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R5 (at -2.785 0) (layer B.SilkS))
    (fp_text value 13k (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 52 /PA7-Voltage))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B36C52B)
    (at 202.692 108.195 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R6 (at -2.531 0) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.65 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 3 +3V3))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 5 "Net-(C7-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B36C52B)
    (at 204.978 108.195 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R7 (at -2.549 0) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.65 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 53 "Net-(R7-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B36C52B)
    (at 234.569 79.765 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R8 (at -2.549 0) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.65 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 45 /Finn_Power))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B36C52B)
    (at 233.68 101.854)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R9 (at -0.127 -1.524) (layer B.SilkS))
    (fp_text value 300 (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 9 "Net-(D1-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 1 +6V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B36C52B)
    (at 241.900712 100.969847 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R10 (at 0 1.655847 180) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.65 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 46 /LED_MOS))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B36C52B)
    (at 233.671 95.758)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R11 (at 0.009 -1.524) (layer B.SilkS))
    (fp_text value 165 (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 10 "Net-(D2-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B36C52B)
    (at 233.68 98.806)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R12 (at 0 -1.524) (layer B.SilkS))
    (fp_text value 300 (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 1 +6V))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 11 "Net-(D3-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B36C52B)
    (at 233.816 55.753)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R13 (at 2.54 0 -90) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 23 "Net-(M2-Pad1)"))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 1 +6V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B36C52B)
    (at 242.443 74.041 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R14 (at -2.54 0.009 180) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.65 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 21 "Net-(M1-Pad1)"))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 1 +6V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 228.219 59.826 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R15 (at 2.549 0 180) (layer F.SilkS))
    (fp_text value 10K (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 24 "Net-(M3-Pad1)"))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 +6V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B36C52B)
    (at 234.832 64.008)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R16 (at -2.549 0 90) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 47 /FINN_SERVO_TWO))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B36C52B)
    (at 234.95 73.034 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R17 (at -2.549 0) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.65 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 48 /FINN_SERVO_ONE))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B36C52B)
    (at 220.091 61.078 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R18 (at -2.531 0) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.65 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 49 /Release_Servo))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 206.239 104.394)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R19 (at -3.293 0) (layer F.SilkS))
    (fp_text value 10k (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 55 /SDA))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 206.239 106.426)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R20 (at -3.293 0) (layer F.SilkS))
    (fp_text value 10k (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 3 +3V3))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 54 /SCL))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B36C52B)
    (at 211.074 113.928 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R21 (at -2.676 0) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.65 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 50 /BUZZER_MOS))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_XH_B03B-XH-A_1x03_P2.50mm_Vertical (layer F.Cu) (tedit 5B7754C5)
    (at 245.364 84.328 270)
    (descr "JST XH series connector, B03B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST XH side entry")
    (fp_text reference U1 (at 2.5 -3.55 270) (layer F.SilkS))
    (fp_text value Adafruit_Cam (at 2.5 4.6 270) (layer F.Fab))
    (fp_text user %R (at 2.5 2.7 270) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 3 +3V3))
    (pad 2 thru_hole oval (at 2.5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at 5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 44 "Net-(Q1-Pad3)"))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_XH_B03B-XH-A_1x03_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module BNO080:LGA-28 (layer F.Cu) (tedit 0)
    (at 214.425 72.386)
    (descr "<h3>LGA-28 - LGA-28 package for the BNO080 IMU</h3><p>Specifications:<ul><li>Pin count: 28</li><li>Pin pitch: 0.5mm</li><li>Area: 3.8mm X 5.2mm</li></ul></p><p><a href=”http://www.hillcrestlabs.com/download/5a05f340566d07c196001ec1”>Datasheet referenced for footprint</a></p><p>Example device(s):<ul><li><a href=”https://www.sparkfun.com/products/14618”>BNO080</a></li></ul></p>")
    (attr smd)
    (fp_text reference U2 (at -0.1872 -3.4032) (layer F.SilkS))
    (fp_text value BNO080 (at -0.084 3.1968) (layer F.SilkS))
    (fp_text user Y (at 0.4 -0.5) (layer Edge.Cuts))
    (fp_text user Z (at 0.3 0.6) (layer Edge.Cuts))
    (fp_text user X (at -0.255 0.462) (layer Edge.Cuts))
    (pad 1 smd rect (at 1.7 -2.25 90) (size 0.25 1) (layers F.Cu F.Paste F.Mask))
    (pad 28 smd rect (at 1.7 -1.75 90) (size 0.25 1) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 27 smd rect (at 1.7 -1.25 90) (size 0.25 1) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(U2-Pad27)"))
    (pad 26 smd rect (at 1.7 -0.75 90) (size 0.25 1) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(U2-Pad26)"))
    (pad 25 smd rect (at 1.7 -0.25 90) (size 0.25 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 24 smd rect (at 1.7 0.25 90) (size 0.25 1) (layers F.Cu F.Paste F.Mask))
    (pad 23 smd rect (at 1.7 0.75 90) (size 0.25 1) (layers F.Cu F.Paste F.Mask))
    (pad 22 smd rect (at 1.7 1.25 90) (size 0.25 1) (layers F.Cu F.Paste F.Mask))
    (pad 21 smd rect (at 1.7 1.75 90) (size 0.25 1) (layers F.Cu F.Paste F.Mask))
    (pad 20 smd rect (at 1.7 2.25 90) (size 0.25 1) (layers F.Cu F.Paste F.Mask)
      (net 27 /MISO))
    (pad 15 smd rect (at -1.7 2.25 270) (size 0.25 1) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(U2-Pad15)"))
    (pad 14 smd rect (at -1.7 1.75 270) (size 0.25 1) (layers F.Cu F.Paste F.Mask)
      (net 59 /HOST_INTN))
    (pad 13 smd rect (at -1.7 1.25 270) (size 0.25 1) (layers F.Cu F.Paste F.Mask))
    (pad 12 smd rect (at -1.7 0.75 270) (size 0.25 1) (layers F.Cu F.Paste F.Mask))
    (pad 11 smd rect (at -1.7 0.25 270) (size 0.25 1) (layers F.Cu F.Paste F.Mask)
      (net 60 /BNO_NRST))
    (pad 10 smd rect (at -1.7 -0.25 270) (size 0.25 1) (layers F.Cu F.Paste F.Mask)
      (net 61 /BNO_CLOCKSEL0))
    (pad 9 smd rect (at -1.7 -0.75 270) (size 0.25 1) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C4-Pad1)"))
    (pad 8 smd rect (at -1.7 -1.25 270) (size 0.25 1) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at -1.7 -1.75 270) (size 0.25 1) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at -1.7 -2.25 270) (size 0.25 1) (layers F.Cu F.Paste F.Mask)
      (net 62 /BNO_WAKE))
    (pad 5 smd rect (at -0.75 -2.4 180) (size 0.25 1) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 4 smd rect (at -0.25 -2.4 180) (size 0.25 1) (layers F.Cu F.Paste F.Mask)
      (net 63 /BNO_BOOTN))
    (pad 3 smd rect (at 0.25 -2.4 180) (size 0.25 1) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.75 -2.4 180) (size 0.25 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 16 smd rect (at -0.75 2.4 180) (size 0.25 1) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(U2-Pad16)"))
    (pad 17 smd rect (at -0.25 2.4 180) (size 0.25 1) (layers F.Cu F.Paste F.Mask)
      (net 33 /MOSI))
    (pad 18 smd rect (at 0.25 2.4 180) (size 0.25 1) (layers F.Cu F.Paste F.Mask)
      (net 65 /~SS_BNO080))
    (pad 19 smd rect (at 0.75 2.4 180) (size 0.25 1) (layers F.Cu F.Paste F.Mask)
      (net 40 /SCLK))
  )
  (module MS560702BA03-50:SON125P300X500X100-8N (layer F.Cu) (tedit 0)
    (at 214.7 80.107)
    (attr smd)
    (fp_text reference U3 (at -0.406828 -3.33089) (layer F.SilkS))
    (fp_text value MS560702BA03-50 (at -0.099145 3.35642) (layer F.SilkS))
    (pad 1 smd rect (at -1.2 -1.875) (size 1.31 0.53) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 8 smd rect (at 1.2 -1.875) (size 1.31 0.53) (layers F.Cu F.Paste F.Mask)
      (net 40 /SCLK))
    (pad 2 smd rect (at -1.2 -0.625) (size 1.31 0.53) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -1.2 0.625) (size 1.31 0.53) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at -1.2 1.875) (size 1.31 0.53) (layers F.Cu F.Paste F.Mask)
      (net 66 /~SS_5607))
    (pad 5 smd rect (at 1.2 1.875) (size 1.31 0.53) (layers F.Cu F.Paste F.Mask)
      (net 66 /~SS_5607))
    (pad 6 smd rect (at 1.2 0.625) (size 1.31 0.53) (layers F.Cu F.Paste F.Mask)
      (net 27 /MISO))
    (pad 7 smd rect (at 1.2 -0.625) (size 1.31 0.53) (layers F.Cu F.Paste F.Mask)
      (net 33 /MOSI))
  )
  (module ADP3338AKCZ-3.3RL7:SOT230P700X180-4N (layer F.Cu) (tedit 5C709ADE)
    (at 241.6556 112.776)
    (attr smd)
    (fp_text reference U4 (at -0.1016 -4.572) (layer F.SilkS))
    (fp_text value 6->3V3 (at -0.508485 4.83074) (layer F.SilkS) hide)
    (pad 1 smd rect (at -3.2004 -2.3114) (size 1.6256 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -3.2004 0) (size 1.6256 0.889) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 3 smd rect (at -3.2004 2.3114) (size 1.6256 0.889) (layers F.Cu F.Paste F.Mask)
      (net 1 +6V))
    (pad 4 smd rect (at 3.2004 0) (size 1.6256 3.175) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
  )
  (module digikey-footprints:SOIC-8_W3.9mm (layer F.Cu) (tedit 5ACD0D7F)
    (at 205.613 111.596)
    (fp_text reference U5 (at -4.064 0.037) (layer F.SilkS))
    (fp_text value RTC (at 0.06604 4.80314) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.905 2.45) (size 0.6 2) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(U5-Pad1)"))
    (pad 2 smd rect (at -0.635 2.45) (size 0.6 2) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(U5-Pad2)"))
    (pad 4 smd rect (at 1.905 2.45) (size 0.6 2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at 1.905 -2.45) (size 0.6 2) (layers F.Cu F.Paste F.Mask)
      (net 55 /SDA))
    (pad 6 smd rect (at 0.635 -2.45) (size 0.6 2) (layers F.Cu F.Paste F.Mask)
      (net 54 /SCL))
    (pad 7 smd rect (at -0.635 -2.45) (size 0.6 2) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(R7-Pad2)"))
    (pad 8 smd rect (at -1.905 -2.45) (size 0.6 2) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C7-Pad2)"))
    (pad 3 smd rect (at 0.635 2.45) (size 0.6 2) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(U5-Pad3)"))
  )
  (module Connector_JST:JST_XH_B03B-XH-A_1x03_P2.50mm_Vertical (layer F.Cu) (tedit 5B7754C5)
    (at 245.364 61.468 270)
    (descr "JST XH series connector, B03B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST XH side entry")
    (fp_text reference U6 (at 2.5 -3.55 270) (layer F.SilkS))
    (fp_text value SS49E (at 2.5 4.6 270) (layer F.Fab))
    (fp_text user %R (at 2.5 2.7 270) (layer F.Fab))
    (pad 3 thru_hole oval (at 5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 70 /PA5-Hall_Effect))
    (pad 2 thru_hole oval (at 2.5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole roundrect (at 0 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 1 +6V))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_XH_B03B-XH-A_1x03_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:1X06 (layer F.Cu) (tedit 5963D43D)
    (at 208.28 122.428)
    (descr "PLATED THROUGH HOLE - 6 PIN")
    (tags "PLATED THROUGH HOLE - 6 PIN")
    (attr virtual)
    (fp_text reference U7 (at 0 -1.905) (layer F.SilkS))
    (fp_text value Openlog (at 0 1.905) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND) (solder_mask_margin 0.1016))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND) (solder_mask_margin 0.1016))
    (pad 3 thru_hole circle (at 5.08 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 +3V3) (solder_mask_margin 0.1016))
    (pad 4 thru_hole circle (at 7.62 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 71 /OpenLog_MISO) (solder_mask_margin 0.1016))
    (pad 5 thru_hole circle (at 10.16 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 72 /OpenLog_MOSI) (solder_mask_margin 0.1016))
    (pad 6 thru_hole circle (at 12.7 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 73 /OpenLog_GRN) (solder_mask_margin 0.1016))
  )
  (module Connectors:1X09 (layer F.Cu) (tedit 5963D769)
    (at 247.396 96.266 270)
    (descr "PLATED THROUGH HOLE -9 PIN")
    (tags "PLATED THROUGH HOLE -9 PIN")
    (attr virtual)
    (fp_text reference U8 (at 0 -1.905 270) (layer F.SilkS))
    (fp_text value Adafruit_746 (at 0 1.905 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 74 "Net-(U8-Pad1)") (solder_mask_margin 0.1016))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 75 "Net-(U8-Pad2)") (solder_mask_margin 0.1016))
    (pad 3 thru_hole circle (at 5.08 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 76 "Net-(U8-Pad3)") (solder_mask_margin 0.1016))
    (pad 4 thru_hole circle (at 7.62 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 77 "Net-(U8-Pad4)") (solder_mask_margin 0.1016))
    (pad 5 thru_hole circle (at 10.16 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 78 /GPS_MISO) (solder_mask_margin 0.1016))
    (pad 6 thru_hole circle (at 12.7 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 79 /GPS_MOSI) (solder_mask_margin 0.1016))
    (pad 7 thru_hole circle (at 15.24 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND) (solder_mask_margin 0.1016))
    (pad 8 thru_hole circle (at 17.78 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 +3V3) (solder_mask_margin 0.1016))
    (pad 9 thru_hole circle (at 20.32 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 80 "Net-(U8-Pad9)") (solder_mask_margin 0.1016))
  )
  (module Package_QFP:TQFP-44_10x10mm_P0.8mm (layer F.Cu) (tedit 5A02F146)
    (at 215.392 100.584)
    (descr "44-Lead Plastic Thin Quad Flatpack (PT) - 10x10x1.0 mm Body [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.8")
    (attr smd)
    (fp_text reference U9 (at 0 -7.45) (layer F.SilkS))
    (fp_text value ATxmega128A4U-AU (at 0 7.45) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -5.7 -4) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 70 /PA5-Hall_Effect))
    (pad 2 smd rect (at -5.7 -3.2) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 51 /PA6-Therm))
    (pad 3 smd rect (at -5.7 -2.4) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 52 /PA7-Voltage))
    (pad 4 smd rect (at -5.7 -1.6) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 81 "Net-(U9-Pad4)"))
    (pad 5 smd rect (at -5.7 -0.8) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 82 "Net-(U9-Pad5)"))
    (pad 6 smd rect (at -5.7 0) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 83 "Net-(U9-Pad6)"))
    (pad 7 smd rect (at -5.7 0.8) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 84 "Net-(U9-Pad7)"))
    (pad 8 smd rect (at -5.7 1.6) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 9 smd rect (at -5.7 2.4) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 6 /MCU_VCC))
    (pad 10 smd rect (at -5.7 3.2) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 55 /SDA))
    (pad 11 smd rect (at -5.7 4) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 54 /SCL))
    (pad 12 smd rect (at -4 5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 39 /~SS_XBEE))
    (pad 13 smd rect (at -3.2 5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 65 /~SS_BNO080))
    (pad 14 smd rect (at -2.4 5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 66 /~SS_5607))
    (pad 15 smd rect (at -1.6 5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 33 /MOSI))
    (pad 16 smd rect (at -0.8 5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 27 /MISO))
    (pad 17 smd rect (at 0 5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 40 /SCLK))
    (pad 18 smd rect (at 0.8 5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 19 smd rect (at 1.6 5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 6 /MCU_VCC))
    (pad 20 smd rect (at 2.4 5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 49 /Release_Servo))
    (pad 21 smd rect (at 3.2 5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 48 /FINN_SERVO_ONE))
    (pad 22 smd rect (at 4 5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 47 /FINN_SERVO_TWO))
    (pad 23 smd rect (at 5.7 4) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 46 /LED_MOS))
    (pad 24 smd rect (at 5.7 3.2) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 50 /BUZZER_MOS))
    (pad 25 smd rect (at 5.7 2.4) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 85 "Net-(U9-Pad25)"))
    (pad 26 smd rect (at 5.7 1.6) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 86 "Net-(U9-Pad26)"))
    (pad 27 smd rect (at 5.7 0.8) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 87 "Net-(U9-Pad27)"))
    (pad 28 smd rect (at 5.7 0) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 88 "Net-(U9-Pad28)"))
    (pad 29 smd rect (at 5.7 -0.8) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 89 "Net-(U9-Pad29)"))
    (pad 30 smd rect (at 5.7 -1.6) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 31 smd rect (at 5.7 -2.4) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 6 /MCU_VCC))
    (pad 32 smd rect (at 5.7 -3.2) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 71 /OpenLog_MISO))
    (pad 33 smd rect (at 5.7 -4) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 72 /OpenLog_MOSI))
    (pad 34 smd rect (at 4 -5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 13 /PDI_DATA))
    (pad 35 smd rect (at 3.2 -5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 16 /PDI_CLK))
    (pad 36 smd rect (at 2.4 -5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 90 "Net-(U9-Pad36)"))
    (pad 37 smd rect (at 1.6 -5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 91 "Net-(U9-Pad37)"))
    (pad 38 smd rect (at 0.8 -5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 39 smd rect (at 0 -5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 7 /MCU_AVCC))
    (pad 40 smd rect (at -0.8 -5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 79 /GPS_MOSI))
    (pad 41 smd rect (at -1.6 -5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 78 /GPS_MISO))
    (pad 42 smd rect (at -2.4 -5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 45 /Finn_Power))
    (pad 43 smd rect (at -3.2 -5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 43 /CAMERA_DATA))
    (pad 44 smd rect (at -4 -5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 73 /OpenLog_GRN))
    (model ${KISYS3DMOD}/Package_QFP.3dshapes/TQFP-44_10x10mm_P0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module skyfire_logo:skyfire_logo (layer B.Cu) (tedit 0)
    (at 213.614 69.088 90)
    (fp_text reference G*** (at 0 0 90) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 90) (layer B.SilkS) hide)
  )
  (gr_text "Alex Spaulding\nNoah Schwalb\nZac Faudi" (at 213.741 80.391) (layer B.SilkS))
  (gr_text "February 2019" (at 213.995 77.216) (layer B.SilkS))
  (gr_text "UAH Space Hardware Club\n" (at 213.614 75.565) (layer B.SilkS))
  (gr_line (start 200 125) (end 250 125) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 250 50) (end 250 125) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 200 50) (end 200 125) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 200 50) (end 250 50) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1525))
    (min_thickness 0.1525)
    (fill yes (arc_segments 16) (thermal_gap 0.25) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 194.056 45.974) (xy 256.159 46.228) (xy 257.175 130.175) (xy 192.532 128.778)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1525))
    (min_thickness 0.1525)
    (fill yes (arc_segments 16) (thermal_gap 0.25) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 193.548 45.339) (xy 258.064 45.72) (xy 258.572 130.683) (xy 188.722 130.429)
      )
    )
  )
)
