(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 29)
    (no_connects 0)
    (area 156.794999 99.644999 175.945001 131.495001)
    (thickness 1.6)
    (drawings 15)
    (tracks 121)
    (zones 0)
    (modules 7)
    (nets 28)
  )
  (page A4)
  (title_block
    (title "ZX81 EPROM Adapter (SMD)")
    (date 2018-03-05)
    (rev 1.0)
    (company fatla.eu)
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.254)
    (trace_clearance 0.2032)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2032)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6096)
    (via_drill 0.4064)
    (via_min_size 0.4064)
    (via_min_drill 0.3048)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 VCC)
  (net 2 GND)
  (net 3 A7)
  (net 4 A6)
  (net 5 A5)
  (net 6 A4)
  (net 7 A3)
  (net 8 A2)
  (net 9 A1)
  (net 10 A0)
  (net 11 D0)
  (net 12 D1)
  (net 13 D2)
  (net 14 A8)
  (net 15 A9)
  (net 16 A12)
  (net 17 ~CS~)
  (net 18 A10)
  (net 19 A11)
  (net 20 D7)
  (net 21 D6)
  (net 22 D5)
  (net 23 D4)
  (net 24 D3)
  (net 25 /~CE~)
  (net 26 "Net-(U1-Pad1)")
  (net 27 "Net-(U1-Pad26)")
  (net_class Default "This is the default net class."
    (clearance 0.2032)
    (trace_width 0.254)
    (via_dia 0.6096)
    (via_drill 0.4064)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /~CE~)
    (add_net A0)
    (add_net A1)
    (add_net A10)
    (add_net A11)
    (add_net A12)
    (add_net A2)
    (add_net A3)
    (add_net A4)
    (add_net A5)
    (add_net A6)
    (add_net A7)
    (add_net A8)
    (add_net A9)
    (add_net D0)
    (add_net D1)
    (add_net D2)
    (add_net D3)
    (add_net D4)
    (add_net D5)
    (add_net D6)
    (add_net D7)
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U1-Pad26)")
    (add_net ~CS~)
  )
  (net_class PWR ""
    (clearance 0.2032)
    (trace_width 0.4064)
    (via_dia 0.762)
    (via_drill 0.5588)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net VCC)
  )
  (module Pin_Headers:Pin_Header_Straight_1x12_Pitch2.54mm locked (layer B.Cu) (tedit 59650532)
    (at 173.99 101.6 180)
    (descr "Through hole straight pin header, 1x12, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x12 2.54mm single row")
    (fp_text reference J2 (at 2.54 0 180) (layer B.SilkS))
    (fp_text value ROM2 (at 0 -30.27 180) (layer B.Fab))
    (fp_text user %R (at 0 -13.97 450) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 A8))
    (pad 3 thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 A9))
    (pad 4 thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 A12))
    (pad 5 thru_hole oval (at 0 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 ~CS~))
    (pad 6 thru_hole oval (at 0 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 A10))
    (pad 7 thru_hole oval (at 0 -15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 A11))
    (pad 8 thru_hole oval (at 0 -17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 D7))
    (pad 9 thru_hole oval (at 0 -20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 D6))
    (pad 10 thru_hole oval (at 0 -22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 D5))
    (pad 11 thru_hole oval (at 0 -25.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 D4))
    (pad 12 thru_hole oval (at 0 -27.94 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 D3))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x12_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x12_Pitch2.54mm locked (layer B.Cu) (tedit 59650532)
    (at 158.75 101.6 180)
    (descr "Through hole straight pin header, 1x12, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x12 2.54mm single row")
    (fp_text reference J1 (at -2.54 0 180) (layer B.SilkS))
    (fp_text value ROM1 (at 0 -30.27 180) (layer B.Fab))
    (fp_text user %R (at 0 -13.97 450) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 A7))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 A6))
    (pad 3 thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 A5))
    (pad 4 thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 A4))
    (pad 5 thru_hole oval (at 0 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 A3))
    (pad 6 thru_hole oval (at 0 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 A2))
    (pad 7 thru_hole oval (at 0 -15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 A1))
    (pad 8 thru_hole oval (at 0 -17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 A0))
    (pad 9 thru_hole oval (at 0 -20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 D0))
    (pad 10 thru_hole oval (at 0 -22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 D1))
    (pad 11 thru_hole oval (at 0 -25.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 D2))
    (pad 12 thru_hole oval (at 0 -27.94 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x12_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 163.75 101.6 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0.08 -1.905 360) (layer F.SilkS))
    (fp_text value 1k0 (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 25 /~CE~))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "ZX Speccy:fatla_eu" (layer B.Cu) (tedit 5AA80F6C)
    (at 166.37 129.54 180)
    (fp_text reference G1 (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 168.89 101.6 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 0 -1.75 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "ZX Speccy:logo-speccypl" (layer B.Cu) (tedit 5AA80F74)
    (at 166.37 116.205 90)
    (fp_text reference G2 (at 0 0 90) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 90) (layer B.SilkS) hide)
  )
  (module Housings_SOIC:SOIC-28W_7.5x17.9mm_Pitch1.27mm (layer F.Cu) (tedit 5AD3807B)
    (at 166.37 116.205)
    (descr "28-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U1 (at 0 -10.05) (layer F.SilkS))
    (fp_text value 28C64B (at 0 10.05) (layer F.SilkS))
    (pad 1 smd rect (at -4.7 -8.255) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(U1-Pad1)"))
    (pad 2 smd rect (at -4.7 -6.985) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 A12))
    (pad 3 smd rect (at -4.7 -5.715) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 A7))
    (pad 4 smd rect (at -4.7 -4.445) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 A6))
    (pad 5 smd rect (at -4.7 -3.175) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 A5))
    (pad 6 smd rect (at -4.7 -1.905) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 A4))
    (pad 7 smd rect (at -4.7 -0.635) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 A3))
    (pad 8 smd rect (at -4.7 0.635) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 A2))
    (pad 9 smd rect (at -4.7 1.905) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 A1))
    (pad 10 smd rect (at -4.7 3.175) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 A0))
    (pad 11 smd rect (at -4.7 4.445) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 11 D0))
    (pad 12 smd rect (at -4.7 5.715) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 D1))
    (pad 13 smd rect (at -4.7 6.985) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 D2))
    (pad 14 smd rect (at -4.7 8.255) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 15 smd rect (at 4.7 8.255) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 24 D3))
    (pad 16 smd rect (at 4.7 6.985) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 23 D4))
    (pad 17 smd rect (at 4.7 5.715) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 22 D5))
    (pad 18 smd rect (at 4.7 4.445) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 21 D6))
    (pad 19 smd rect (at 4.7 3.175) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 20 D7))
    (pad 20 smd rect (at 4.7 1.905) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 ~CS~))
    (pad 21 smd rect (at 4.7 0.635) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 18 A10))
    (pad 22 smd rect (at 4.7 -0.635) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 25 /~CE~))
    (pad 23 smd rect (at 4.7 -1.905) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 19 A11))
    (pad 24 smd rect (at 4.7 -3.175) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 A9))
    (pad 25 smd rect (at 4.7 -4.445) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 14 A8))
    (pad 26 smd rect (at 4.7 -5.715) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(U1-Pad26)"))
    (pad 27 smd rect (at 4.7 -6.985) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 28 smd rect (at 4.7 -8.255) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (model Housings_SOIC.3dshapes/SOIC-28_7.5x17.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text v.1.0 (at 171.45 126.365 90) (layer B.Cu))
  (gr_text "ZX81 EEPROM" (at 166.37 129.54) (layer F.SilkS))
  (dimension 19.05 (width 0.3) (layer Dwgs.User)
    (gr_text "0.7500 in" (at 166.37 135.97) (layer Dwgs.User))
    (feature1 (pts (xy 175.895 131.445) (xy 175.895 137.32)))
    (feature2 (pts (xy 156.845 131.445) (xy 156.845 137.32)))
    (crossbar (pts (xy 156.845 134.62) (xy 175.895 134.62)))
    (arrow1a (pts (xy 175.895 134.62) (xy 174.768496 135.206421)))
    (arrow1b (pts (xy 175.895 134.62) (xy 174.768496 134.033579)))
    (arrow2a (pts (xy 156.845 134.62) (xy 157.971504 135.206421)))
    (arrow2b (pts (xy 156.845 134.62) (xy 157.971504 134.033579)))
  )
  (dimension 31.75 (width 0.3) (layer Dwgs.User)
    (gr_text "1.2500 in" (at 151.05 115.57 90) (layer Dwgs.User))
    (feature1 (pts (xy 156.845 99.695) (xy 149.7 99.695)))
    (feature2 (pts (xy 156.845 131.445) (xy 149.7 131.445)))
    (crossbar (pts (xy 152.4 131.445) (xy 152.4 99.695)))
    (arrow1a (pts (xy 152.4 99.695) (xy 152.986421 100.821504)))
    (arrow1b (pts (xy 152.4 99.695) (xy 151.813579 100.821504)))
    (arrow2a (pts (xy 152.4 131.445) (xy 152.986421 130.318496)))
    (arrow2b (pts (xy 152.4 131.445) (xy 151.813579 130.318496)))
  )
  (gr_line (start 156.845 100.965) (end 156.845 131.445) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 158.115 99.695) (end 156.845 100.965) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 175.895 99.695) (end 158.115 99.695) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 175.895 131.445) (end 175.895 99.695) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 156.845 131.445) (end 175.895 131.445) (layer Edge.Cuts) (width 0.1))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 156.845 99.695) (xy 175.895 99.695) (xy 175.895 131.445) (xy 156.845 131.445)
      )
    )
  )
)
