(kicad_pcb (version 20171130) (host pcbnew "(5.0.1-3-g963ef8bb5)")
  (general
    (thickness 1.6)
    (drawings 18)
    (tracks 180)
    (zones 0)
    (modules 225)
    (nets 97)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.5)
    (user_trace_width 0.2)
    (user_trace_width 0.35)
    (user_trace_width 0.5)
    (user_trace_width 0.75)
    (user_trace_width 1)
    (user_trace_width 1.5)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (user_via 0.4 0.3)
    (user_via 0.4 0.3)
    (user_via 0.5 0.3)
    (user_via 0.8 0.5)
    (user_via 1 0.7)
    (user_via 1.5 1)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 5.08 5.08)
    (pad_drill 2.032)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 +VISO)
  (net 3 "Net-(C4-Pad2)")
  (net 4 "Net-(C5-Pad1)")
  (net 5 GNDISO)
  (net 6 "Net-(D1-Pad1)")
  (net 7 "Net-(D1-Pad2)")
  (net 8 "Net-(D2-Pad1)")
  (net 9 "Net-(D3-Pad1)")
  (net 10 /CTRL_A_TTL_FPGA)
  (net 11 /CTRL_A)
  (net 12 /CTRL_B)
  (net 13 /CLK_IN)
  (net 14 /CTRL_B_TTL_FPGA)
  (net 15 /CTRL_A_TTL)
  (net 16 /CTRL_A_TTL_INO)
  (net 17 /CTRL_B_TTL_INO)
  (net 18 /CTRL_B_TTL)
  (net 19 /CTRL_A_NEG)
  (net 20 /CTRL_B_NEG)
  (net 21 /VSEL)
  (net 22 "Net-(U1-Pad1)")
  (net 23 "Net-(U1-Pad2)")
  (net 24 "Net-(U1-Pad3)")
  (net 25 "Net-(U1-Pad4)")
  (net 26 "Net-(U1-Pad8)")
  (net 27 "Net-(U1-Pad11)")
  (net 28 "Net-(U1-Pad13)")
  (net 29 "Net-(U1-Pad9)")
  (net 30 "Net-(U1-Pad10)")
  (net 31 "Net-(U1-Pad24)")
  (net 32 "Net-(U1-Pad22)")
  (net 33 "Net-(U1-Pad19)")
  (net 34 "Net-(U1-Pad21)")
  (net 35 "Net-(U1-Pad17)")
  (net 36 "Net-(U1-Pad23)")
  (net 37 "Net-(U1-Pad25)")
  (net 38 "Net-(U1-Pad29)")
  (net 39 "Net-(U1-Pad27)")
  (net 40 "Net-(U1-Pad30)")
  (net 41 "Net-(U1-Pad28)")
  (net 42 "Net-(U1-Pad32)")
  (net 43 "Net-(U1-Pad31)")
  (net 44 "Net-(U1-Pad26)")
  (net 45 "Net-(U1-Pad33)")
  (net 46 "Net-(U1-Pad37)")
  (net 47 "Net-(U1-Pad35)")
  (net 48 "Net-(U1-Pad38)")
  (net 49 "Net-(U1-Pad40)")
  (net 50 "Net-(U1-Pad39)")
  (net 51 "Net-(U1-Pad34)")
  (net 52 "Net-(U1-Pad43)")
  (net 53 "Net-(U1-Pad45)")
  (net 54 "Net-(U1-Pad48)")
  (net 55 "Net-(U1-Pad46)")
  (net 56 "Net-(U1-Pad50)")
  (net 57 "Net-(U1-Pad49)")
  (net 58 "Net-(U1-Pad41)")
  (net 59 "Net-(U1-Pad44)")
  (net 60 "Net-(U1-Pad42)")
  (net 61 "Net-(U1-Pad61)")
  (net 62 "Net-(U1-Pad65)")
  (net 63 "Net-(U1-Pad66)")
  (net 64 "Net-(U1-Pad64)")
  (net 65 "Net-(U1-Pad76)")
  (net 66 "Net-(U1-Pad72)")
  (net 67 "Net-(U1-Pad71)")
  (net 68 "Net-(U1-Pad73)")
  (net 69 "Net-(U1-Pad70)")
  (net 70 "Net-(U1-Pad53)")
  (net 71 "Net-(U1-Pad55)")
  (net 72 "Net-(U1-Pad58)")
  (net 73 "Net-(U1-Pad56)")
  (net 74 "Net-(U1-Pad59)")
  (net 75 "Net-(U1-Pad54)")
  (net 76 "Net-(U1-Pad84)")
  (net 77 "Net-(U1-Pad80)")
  (net 78 "Net-(U1-Pad82)")
  (net 79 "Net-(U1-Pad79)")
  (net 80 "Net-(U1-Pad81)")
  (net 81 "Net-(U1-Pad78)")
  (net 82 "Net-(U1-Pad83)")
  (net 83 "Net-(U1-Pad77)")
  (net 84 "Net-(U1-Pad60)")
  (net 85 "Net-(U1-Pad57)")
  (net 86 "Net-(U1-Pad52)")
  (net 87 "Net-(U1-Pad85)")
  (net 88 "Net-(U2-Pad5)")
  (net 89 "Net-(U2-Pad6)")
  (net 90 "Net-(U2-Pad7)")
  (net 91 "Net-(U2-Pad8)")
  (net 92 "Net-(U2-Pad17)")
  (net 93 "Net-(U2-Pad19)")
  (net 94 "Net-(U2-Pad20)")
  (net 95 "Net-(U1-Pad36)")
  (net 96 "Net-(J5-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net +VISO)
    (add_net /CLK_IN)
    (add_net /CTRL_A)
    (add_net /CTRL_A_NEG)
    (add_net /CTRL_A_TTL)
    (add_net /CTRL_A_TTL_FPGA)
    (add_net /CTRL_A_TTL_INO)
    (add_net /CTRL_B)
    (add_net /CTRL_B_NEG)
    (add_net /CTRL_B_TTL)
    (add_net /CTRL_B_TTL_FPGA)
    (add_net /CTRL_B_TTL_INO)
    (add_net /VSEL)
    (add_net GNDISO)
    (add_net "Net-(C4-Pad2)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(J5-Pad2)")
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U1-Pad10)")
    (add_net "Net-(U1-Pad11)")
    (add_net "Net-(U1-Pad13)")
    (add_net "Net-(U1-Pad17)")
    (add_net "Net-(U1-Pad19)")
    (add_net "Net-(U1-Pad2)")
    (add_net "Net-(U1-Pad21)")
    (add_net "Net-(U1-Pad22)")
    (add_net "Net-(U1-Pad23)")
    (add_net "Net-(U1-Pad24)")
    (add_net "Net-(U1-Pad25)")
    (add_net "Net-(U1-Pad26)")
    (add_net "Net-(U1-Pad27)")
    (add_net "Net-(U1-Pad28)")
    (add_net "Net-(U1-Pad29)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U1-Pad30)")
    (add_net "Net-(U1-Pad31)")
    (add_net "Net-(U1-Pad32)")
    (add_net "Net-(U1-Pad33)")
    (add_net "Net-(U1-Pad34)")
    (add_net "Net-(U1-Pad35)")
    (add_net "Net-(U1-Pad36)")
    (add_net "Net-(U1-Pad37)")
    (add_net "Net-(U1-Pad38)")
    (add_net "Net-(U1-Pad39)")
    (add_net "Net-(U1-Pad4)")
    (add_net "Net-(U1-Pad40)")
    (add_net "Net-(U1-Pad41)")
    (add_net "Net-(U1-Pad42)")
    (add_net "Net-(U1-Pad43)")
    (add_net "Net-(U1-Pad44)")
    (add_net "Net-(U1-Pad45)")
    (add_net "Net-(U1-Pad46)")
    (add_net "Net-(U1-Pad48)")
    (add_net "Net-(U1-Pad49)")
    (add_net "Net-(U1-Pad50)")
    (add_net "Net-(U1-Pad52)")
    (add_net "Net-(U1-Pad53)")
    (add_net "Net-(U1-Pad54)")
    (add_net "Net-(U1-Pad55)")
    (add_net "Net-(U1-Pad56)")
    (add_net "Net-(U1-Pad57)")
    (add_net "Net-(U1-Pad58)")
    (add_net "Net-(U1-Pad59)")
    (add_net "Net-(U1-Pad60)")
    (add_net "Net-(U1-Pad61)")
    (add_net "Net-(U1-Pad64)")
    (add_net "Net-(U1-Pad65)")
    (add_net "Net-(U1-Pad66)")
    (add_net "Net-(U1-Pad70)")
    (add_net "Net-(U1-Pad71)")
    (add_net "Net-(U1-Pad72)")
    (add_net "Net-(U1-Pad73)")
    (add_net "Net-(U1-Pad76)")
    (add_net "Net-(U1-Pad77)")
    (add_net "Net-(U1-Pad78)")
    (add_net "Net-(U1-Pad79)")
    (add_net "Net-(U1-Pad8)")
    (add_net "Net-(U1-Pad80)")
    (add_net "Net-(U1-Pad81)")
    (add_net "Net-(U1-Pad82)")
    (add_net "Net-(U1-Pad83)")
    (add_net "Net-(U1-Pad84)")
    (add_net "Net-(U1-Pad85)")
    (add_net "Net-(U1-Pad9)")
    (add_net "Net-(U2-Pad17)")
    (add_net "Net-(U2-Pad19)")
    (add_net "Net-(U2-Pad20)")
    (add_net "Net-(U2-Pad5)")
    (add_net "Net-(U2-Pad6)")
    (add_net "Net-(U2-Pad7)")
    (add_net "Net-(U2-Pad8)")
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 88.9 149.86)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 83.82 149.86)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 81.28 149.86)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 86.36 149.86)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 93.98 142.24)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 91.44 144.78)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 96.52 144.78)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 96.52 142.24)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 93.98 144.78)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 91.44 142.24)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 93.98 104.14)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 91.44 134.62)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 93.98 132.08)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 96.52 134.62)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 96.52 132.08)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 93.98 134.62)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 91.44 106.68)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 93.98 121.92)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 91.44 124.46)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 96.52 124.46)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 96.52 121.92)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 93.98 124.46)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 91.44 121.92)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 91.44 114.3)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 93.98 111.76)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 96.52 114.3)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 96.52 111.76)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 93.98 114.3)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 93.98 127)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 91.44 129.54)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 96.52 129.54)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 96.52 127)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 91.44 127)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 93.98 129.54)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 93.98 116.84)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 93.98 147.32)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 91.44 111.76)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 91.44 149.86)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 96.52 149.86)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 96.52 147.32)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 91.44 147.32)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 93.98 149.86)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 91.44 119.38)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 96.52 119.38)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 96.52 116.84)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 91.44 116.84)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 93.98 119.38)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 96.52 106.68)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 96.52 104.14)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 93.98 106.68)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 93.98 109.22)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 91.44 104.14)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 96.52 109.22)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 91.44 109.22)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 91.44 132.08)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 93.98 137.16)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 91.44 139.7)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 96.52 139.7)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 96.52 137.16)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 91.44 137.16)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 93.98 139.7)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 99.06 106.68)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 101.6 104.14)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 111.76 106.68)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 104.14 106.68)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 106.68 106.68)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 104.14 104.14)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 111.76 104.14)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 109.22 106.68)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 106.68 104.14)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 101.6 106.68)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 109.22 109.22)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 101.6 109.22)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 109.22 104.14)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 99.06 104.14)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 104.14 109.22)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 99.06 109.22)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 111.76 109.22)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 106.68 109.22)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 109.22 121.92)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 101.6 121.92)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 99.06 124.46)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 104.14 124.46)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 106.68 124.46)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 104.14 121.92)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 111.76 121.92)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 109.22 124.46)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 114.3 124.46)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 111.76 124.46)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 106.68 121.92)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 101.6 124.46)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 99.06 121.92)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 99.06 114.3)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 101.6 111.76)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 111.76 114.3)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 104.14 114.3)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 106.68 114.3)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 104.14 111.76)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 111.76 111.76)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 109.22 114.3)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 109.22 129.54)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 114.3 129.54)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 111.76 129.54)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 106.68 111.76)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 101.6 114.3)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 109.22 127)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 101.6 127)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 99.06 129.54)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 104.14 129.54)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 106.68 129.54)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 104.14 127)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 99.06 127)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 111.76 127)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 106.68 127)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 101.6 129.54)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 114.3 127)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 109.22 111.76)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 99.06 111.76)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 109.22 119.38)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 111.76 119.38)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 109.22 116.84)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 101.6 116.84)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 99.06 119.38)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 104.14 119.38)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 106.68 119.38)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 104.14 116.84)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 99.06 116.84)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 111.76 116.84)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 106.68 116.84)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 101.6 119.38)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 109.22 132.08)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 101.6 132.08)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 99.06 134.62)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 104.14 134.62)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 106.68 134.62)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 104.14 132.08)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 111.76 132.08)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 109.22 134.62)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 114.3 134.62)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 111.76 134.62)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 106.68 132.08)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 101.6 134.62)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 114.3 132.08)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 99.06 132.08)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 109.22 139.7)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 114.3 139.7)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 111.76 139.7)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 109.22 137.16)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 101.6 137.16)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 99.06 139.7)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 104.14 139.7)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 106.68 139.7)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 104.14 137.16)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 99.06 137.16)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 111.76 137.16)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 106.68 137.16)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 101.6 139.7)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 114.3 137.16)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 109.22 144.78)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 114.3 144.78)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 111.76 144.78)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 109.22 142.24)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 101.6 142.24)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 99.06 144.78)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 104.14 144.78)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 106.68 144.78)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 104.14 142.24)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 99.06 142.24)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 111.76 142.24)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 106.68 142.24)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 101.6 144.78)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 114.3 142.24)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 109.22 147.32)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 114.3 147.32)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 111.76 147.32)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 99.06 147.32)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 104.14 147.32)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 106.68 147.32)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 101.6 147.32)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 109.22 149.86)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 114.3 149.86)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 111.76 149.86)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 104.14 149.86)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 106.68 149.86)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 101.6 149.86)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:SSOP-24_5.3x8.2mm_P0.65mm (layer F.Cu) (tedit 5D1E2818)
    (at 132.08 121.92)
    (attr smd)
    (fp_text reference U2 (at 0 5.08) (layer F.SilkS))
    (fp_text value ADuM6410 (at 0 5.25) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -3.6 -3.575) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at -3.6 -2.925) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 +VISO))
    (pad 3 smd rect (at -3.6 -2.275) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 15 /CTRL_A_TTL))
    (pad 4 smd rect (at -3.6 -1.625) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 18 /CTRL_B_TTL))
    (pad 5 smd rect (at -3.6 -0.975) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 88 "Net-(U2-Pad5)"))
    (pad 6 smd rect (at -3.6 -0.325) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 89 "Net-(U2-Pad6)"))
    (pad 7 smd rect (at -3.6 0.325) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 90 "Net-(U2-Pad7)"))
    (pad 8 smd rect (at -3.6 0.975) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 91 "Net-(U2-Pad8)"))
    (pad 9 smd rect (at -3.6 1.625) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 +VISO))
    (pad 10 smd rect (at -3.6 2.275) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 +VISO))
    (pad 11 smd rect (at -3.6 2.925) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 12 smd rect (at -3.6 3.575) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 +VISO))
    (pad 13 smd rect (at 3.6 3.575) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C4-Pad2)"))
    (pad 14 smd rect (at 3.6 2.925) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C5-Pad1)"))
    (pad 15 smd rect (at 3.6 2.275) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 21 /VSEL))
    (pad 16 smd rect (at 3.6 1.625) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C4-Pad2)"))
    (pad 17 smd rect (at 3.6 0.975) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 92 "Net-(U2-Pad17)"))
    (pad 18 smd rect (at 3.6 0.325) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 +VISO))
    (pad 19 smd rect (at 3.6 -0.325) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 93 "Net-(U2-Pad19)"))
    (pad 20 smd rect (at 3.6 -0.975) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 94 "Net-(U2-Pad20)"))
    (pad 21 smd rect (at 3.6 -1.625) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 20 /CTRL_B_NEG))
    (pad 22 smd rect (at 3.6 -2.275) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 19 /CTRL_A_NEG))
    (pad 23 smd rect (at 3.6 -2.925) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C4-Pad2)"))
    (pad 24 smd rect (at 3.6 -3.575) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 +VISO))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SSOP-24_5.3x8.2mm_P0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RF_Switch_Controller:C_0805_HandSolder (layer B.Cu) (tedit 5D1E325B)
    (at 131.445 118.355 270)
    (attr smd)
    (fp_text reference C1 (at 0 1.905) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.65 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 1 +5V))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 2 +VISO))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RF_Switch_Controller:C_0805_HandSolder (layer B.Cu) (tedit 5D1E325B)
    (at 128.27 125.095 270)
    (attr smd)
    (fp_text reference C2 (at 2.54 0) (layer B.SilkS))
    (fp_text value 10uF (at 0 -1.65 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 1 +5V))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 2 +VISO))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RF_Switch_Controller:C_0805_HandSolder (layer B.Cu) (tedit 5D1E325B)
    (at 131.445 125.095 270)
    (attr smd)
    (fp_text reference C3 (at 2.54 0) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.65 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 2 +VISO))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RF_Switch_Controller:C_0805_HandSolder (layer B.Cu) (tedit 5D1E325B)
    (at 133.35 128.27 90)
    (attr smd)
    (fp_text reference C4 (at -2.54 0 180) (layer B.SilkS))
    (fp_text value 100pF (at 0 -1.65 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 3 "Net-(C4-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 2 +VISO))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RF_Switch_Controller:C_0805_HandSolder (layer B.Cu) (tedit 5D1E325B)
    (at 136.525 127.635 180)
    (attr smd)
    (fp_text reference C5 (at 0 -1.905 180) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.65 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 4 "Net-(C5-Pad1)"))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 3 "Net-(C4-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RF_Switch_Controller:C_0805_HandSolder (layer B.Cu) (tedit 5D1E325B)
    (at 142.875 123.825 90)
    (attr smd)
    (fp_text reference C6 (at -2.54 0 180) (layer B.SilkS))
    (fp_text value 10uF (at 0 -1.65 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 5 GNDISO))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 2 +VISO))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RF_Switch_Controller:LED_0805_HandSolder (layer F.Cu) (tedit 5D1E2D60)
    (at 129.54 92.71 270)
    (attr smd)
    (fp_text reference D1 (at 2.54 0) (layer F.SilkS))
    (fp_text value Amber (at 0 1.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 6 "Net-(D1-Pad1)"))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 7 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RF_Switch_Controller:LED_0805_HandSolder (layer F.Cu) (tedit 5D1E2D60)
    (at 132.08 92.71 270)
    (attr smd)
    (fp_text reference D2 (at 2.54 0) (layer F.SilkS))
    (fp_text value Amber (at 0 1.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 8 "Net-(D2-Pad1)"))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RF_Switch_Controller:LED_0805_HandSolder (layer F.Cu) (tedit 5D1E2D60)
    (at 134.62 92.71 90)
    (attr smd)
    (fp_text reference D3 (at -2.54 0 180) (layer F.SilkS))
    (fp_text value Amber (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 +VISO))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 9 "Net-(D3-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RF_Switch_Controller:FB_0805_HandSolder (layer B.Cu) (tedit 5D1E32A1)
    (at 139.7 125.095 180)
    (attr smd)
    (fp_text reference FB1 (at 3.048 0.127 180) (layer B.SilkS))
    (fp_text value 1.8k (at 0 -1.65 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 4 "Net-(C5-Pad1)"))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 2 +VISO))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RF_Switch_Controller:FB_0805_HandSolder (layer B.Cu) (tedit 5D1E32A1)
    (at 139.7 123.19 180)
    (attr smd)
    (fp_text reference FB2 (at 3.048 0.254 180) (layer B.SilkS))
    (fp_text value 1.8k (at 0 -1.65 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 5 GNDISO))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 3 "Net-(C4-Pad2)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RF_Switch_Controller:MountingHole_80mil (layer F.Cu) (tedit 5D1E2AC0)
    (at 71.755 96.52)
    (attr virtual)
    (fp_text reference H1 (at 3.937 0) (layer F.SilkS))
    (fp_text value Mounting_Hole (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.08 5.08) (drill 2.032) (layers *.Cu *.Mask)
      (net 2 +VISO))
  )
  (module RF_Switch_Controller:MountingHole_80mil (layer F.Cu) (tedit 5D1E2AC0)
    (at 71.755 147.32)
    (attr virtual)
    (fp_text reference H2 (at 3.937 0) (layer F.SilkS))
    (fp_text value Mounting_Hole (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.08 5.08) (drill 2.032) (layers *.Cu *.Mask)
      (net 2 +VISO))
  )
  (module RF_Switch_Controller:MountingHole_80mil (layer F.Cu) (tedit 5D1E2AC0)
    (at 154.305 96.52)
    (attr virtual)
    (fp_text reference H3 (at 4.191 0) (layer F.SilkS))
    (fp_text value Mounting_Hole (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.08 5.08) (drill 2.032) (layers *.Cu *.Mask)
      (net 2 +VISO))
  )
  (module RF_Switch_Controller:MountingHole_80mil (layer F.Cu) (tedit 5D1F8AF0)
    (at 154.305 147.32)
    (attr virtual)
    (fp_text reference H4 (at 4.191 0) (layer F.SilkS))
    (fp_text value Mounting_Hole (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.08 5.08) (drill 2.032) (layers *.Cu *.Mask)
      (net 2 +VISO))
  )
  (module RF_Switch_Controller:PinHeader_1x03_P2.54mm (layer F.Cu) (tedit 5D1E3328)
    (at 127.635 145.415 270)
    (fp_text reference JP1 (at 0 8.255) (layer F.SilkS))
    (fp_text value Jumper_Dual (at 0 7.41 270) (layer F.Fab))
    (fp_text user %R (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /CLK_IN))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 96 "Net-(J5-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /CTRL_A_TTL_FPGA))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RF_Switch_Controller:PinHeader_1x03_P2.54mm (layer F.Cu) (tedit 5D1E3328)
    (at 121.92 118.11 180)
    (fp_text reference JP2 (at 0 7.62 180) (layer F.SilkS))
    (fp_text value Jumper_Dual (at 0 7.41 180) (layer F.Fab))
    (fp_text user %R (at 0 2.54 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /CTRL_A_TTL_FPGA))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /CTRL_A_TTL))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /CTRL_A_TTL_INO))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RF_Switch_Controller:PinHeader_1x03_P2.54mm (layer F.Cu) (tedit 5D1E3328)
    (at 121.92 127 180)
    (fp_text reference JP3 (at 0 -2.54 180) (layer F.SilkS))
    (fp_text value Jumper_Dual (at 0 7.41 180) (layer F.Fab))
    (fp_text user %R (at 0 2.54 270) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /CTRL_B_TTL_INO))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /CTRL_B_TTL))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /CTRL_B_TTL_FPGA))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RF_Switch_Controller:PinHeader_1x03_P2.54mm (layer F.Cu) (tedit 5D1E3328)
    (at 142.24 109.22 180)
    (fp_text reference JP4 (at 0 -2.33 180) (layer F.SilkS))
    (fp_text value Jumper_Dual (at 0 7.41 180) (layer F.Fab))
    (fp_text user %R (at 0 2.54 270) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /CTRL_A_TTL))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /CTRL_A))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /CTRL_A_NEG))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RF_Switch_Controller:PinHeader_1x03_P2.54mm (layer F.Cu) (tedit 5D1E3328)
    (at 142.24 133.985)
    (fp_text reference JP5 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Jumper_Dual (at 0 7.41) (layer F.Fab))
    (fp_text user %R (at 0 2.54 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /CTRL_B_NEG))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /CTRL_B))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /CTRL_B_TTL))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RF_Switch_Controller:R_0805_HandSolder (layer B.Cu) (tedit 5D1E2DCA)
    (at 129.54 92.71 270)
    (attr smd)
    (fp_text reference R1 (at 2.54 0) (layer B.SilkS))
    (fp_text value 1k (at 0 -1.65 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 6 "Net-(D1-Pad1)"))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 2 +VISO))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RF_Switch_Controller:R_0805_HandSolder (layer B.Cu) (tedit 5D1E2DCA)
    (at 132.08 92.71 270)
    (attr smd)
    (fp_text reference R2 (at 2.54 0) (layer B.SilkS))
    (fp_text value 1k (at 0 -1.65 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 8 "Net-(D2-Pad1)"))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 2 +VISO))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RF_Switch_Controller:R_0805_HandSolder (layer B.Cu) (tedit 5D1E2DCA)
    (at 134.62 92.71 270)
    (attr smd)
    (fp_text reference R3 (at 2.54 0) (layer B.SilkS))
    (fp_text value 1k (at 0 -1.65 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 5 GNDISO))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 9 "Net-(D3-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RF_Switch_Controller:R_0805_HandSolder (layer F.Cu) (tedit 5D1E2DCA)
    (at 139.7 125.095 180)
    (attr smd)
    (fp_text reference R4 (at -3.175 0 180) (layer F.SilkS))
    (fp_text value 30.9k (at 0 1.65 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 +VISO))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 21 /VSEL))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RF_Switch_Controller:R_0805_HandSolder (layer F.Cu) (tedit 5D1E2DCA)
    (at 139.7 123.19)
    (attr smd)
    (fp_text reference R5 (at 3.175 0) (layer F.SilkS))
    (fp_text value 10k (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 5 GNDISO))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 21 /VSEL))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RF_Switch_Controller:TestPoint_1mm (layer F.Cu) (tedit 5D1E31FB)
    (at 90.805 92.71)
    (fp_text reference TP1 (at 0 2.5) (layer F.SilkS))
    (fp_text value +5V (at 0 -2.8) (layer F.Fab))
    (fp_text user %R (at 0.7 2.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 +5V))
  )
  (module RF_Switch_Controller:TestPoint_1mm (layer F.Cu) (tedit 5D1E31FB)
    (at 97.155 92.71)
    (fp_text reference TP2 (at 0 2.5) (layer F.SilkS))
    (fp_text value GND (at 0 -2.8) (layer F.Fab))
    (fp_text user %R (at 0.7 2.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 +VISO))
  )
  (module RF_Switch_Controller:TestPoint_1mm (layer F.Cu) (tedit 5D1E31FB)
    (at 117.475 92.71)
    (fp_text reference TP3 (at 0 2.5) (layer F.SilkS))
    (fp_text value Test_Point (at 0 -2.8) (layer F.Fab))
    (fp_text user %R (at 0.7 2.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 15 /CTRL_A_TTL))
  )
  (module RF_Switch_Controller:TestPoint_1mm (layer F.Cu) (tedit 5D1E31FB)
    (at 111.125 92.71)
    (fp_text reference TP4 (at 0 2.5) (layer F.SilkS))
    (fp_text value Test_Point (at 0 -2.8) (layer F.Fab))
    (fp_text user %R (at 0.7 2.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 18 /CTRL_B_TTL))
  )
  (module RF_Switch_Controller:TestPoint_1mm (layer F.Cu) (tedit 5D1E31FB)
    (at 157.48 106.68)
    (fp_text reference TP5 (at 0 2.54) (layer F.SilkS))
    (fp_text value Test_Point (at 0 -2.8) (layer F.Fab))
    (fp_text user %R (at 0.7 2.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 11 /CTRL_A))
  )
  (module RF_Switch_Controller:TestPoint_1mm (layer F.Cu) (tedit 5D1E31FB)
    (at 157.48 136.525)
    (fp_text reference TP6 (at 0 2.54) (layer F.SilkS))
    (fp_text value Test_Point (at 0 -2.8) (layer F.Fab))
    (fp_text user %R (at 0.7 2.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 12 /CTRL_B))
  )
  (module RF_Switch_Controller:C_0805_HandSolder (layer B.Cu) (tedit 5D1E325B)
    (at 133.35 118.364 90)
    (attr smd)
    (fp_text reference C7 (at 0 1.905 180) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.65 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 3 "Net-(C4-Pad2)"))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 2 +VISO))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RF_Switch_Controller:Arduino_Due (layer F.Cu) (tedit 5D2351E1)
    (at 53.34 152.4)
    (fp_text reference U1 (at 15.875 0) (layer F.SilkS))
    (fp_text value Arduino_Due (at 49.53 -26.67) (layer F.Fab))
    (fp_text user %R (at 46.228 -24.892 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 27.94 -53.34 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(U1-Pad1)"))
    (pad 2 thru_hole oval (at 30.48 -53.34 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(U1-Pad2)"))
    (pad 3 thru_hole oval (at 33.02 -53.34 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(U1-Pad3)"))
    (pad 4 thru_hole oval (at 35.56 -53.34 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(U1-Pad4)"))
    (pad 5 thru_hole oval (at 38.1 -53.34 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 6 thru_hole oval (at 40.64 -53.34 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 +VISO))
    (pad 7 thru_hole oval (at 43.18 -53.34 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 +VISO))
    (pad 8 thru_hole oval (at 45.72 -53.34 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(U1-Pad8)"))
    (pad 16 thru_hole oval (at 68.58 -53.34 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /CTRL_A_TTL_INO))
    (pad 11 thru_hole oval (at 55.88 -53.34 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(U1-Pad11)"))
    (pad 13 thru_hole oval (at 60.96 -53.34 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(U1-Pad13)"))
    (pad 9 thru_hole rect (at 50.8 -53.34 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(U1-Pad9)"))
    (pad 10 thru_hole oval (at 53.34 -53.34 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(U1-Pad10)"))
    (pad 15 thru_hole oval (at 66.04 -53.34 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /CTRL_B_TTL_INO))
    (pad 21 thru_hole oval (at 83.82 -53.34 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(U1-Pad21)"))
    (pad 17 thru_hole rect (at 73.66 -53.34 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(U1-Pad17)"))
    (pad 18 thru_hole oval (at 76.2 -53.34 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(D1-Pad2)"))
    (pad 29 thru_hole oval (at 76.2 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "Net-(U1-Pad29)"))
    (pad 27 thru_hole oval (at 81.28 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 "Net-(U1-Pad27)"))
    (pad 30 thru_hole oval (at 73.66 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 "Net-(U1-Pad30)"))
    (pad 28 thru_hole oval (at 78.74 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 "Net-(U1-Pad28)"))
    (pad 32 thru_hole rect (at 68.58 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 "Net-(U1-Pad32)"))
    (pad 31 thru_hole oval (at 71.12 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 "Net-(U1-Pad31)"))
    (pad 33 thru_hole oval (at 63.5 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 "Net-(U1-Pad33)"))
    (pad 37 thru_hole oval (at 53.34 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 "Net-(U1-Pad37)"))
    (pad 35 thru_hole oval (at 58.42 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 "Net-(U1-Pad35)"))
    (pad 38 thru_hole oval (at 50.8 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 "Net-(U1-Pad38)"))
    (pad 36 thru_hole oval (at 55.88 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 95 "Net-(U1-Pad36)"))
    (pad 40 thru_hole rect (at 45.72 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 "Net-(U1-Pad40)"))
    (pad 39 thru_hole oval (at 48.26 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 50 "Net-(U1-Pad39)"))
    (pad 34 thru_hole oval (at 60.96 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 51 "Net-(U1-Pad34)"))
    (pad 43 thru_hole oval (at 36.576 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 52 "Net-(U1-Pad43)"))
    (pad 47 thru_hole oval (at 26.416 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 +VISO))
    (pad 45 thru_hole oval (at 31.496 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 53 "Net-(U1-Pad45)"))
    (pad 48 thru_hole oval (at 23.876 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 54 "Net-(U1-Pad48)"))
    (pad 46 thru_hole oval (at 28.956 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 55 "Net-(U1-Pad46)"))
    (pad 50 thru_hole rect (at 18.796 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 56 "Net-(U1-Pad50)"))
    (pad 49 thru_hole oval (at 21.336 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 57 "Net-(U1-Pad49)"))
    (pad 41 thru_hole oval (at 41.656 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 58 "Net-(U1-Pad41)"))
    (pad 44 thru_hole oval (at 34.036 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 59 "Net-(U1-Pad44)"))
    (pad 42 thru_hole oval (at 39.116 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 60 "Net-(U1-Pad42)"))
    (pad 65 thru_hole oval (at 93.98 -7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 62 "Net-(U1-Pad65)"))
    (pad 64 thru_hole oval (at 93.98 -10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 64 "Net-(U1-Pad64)"))
    (pad 68 thru_hole rect (at 93.98 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 67 thru_hole oval (at 93.98 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /CLK_IN))
    (pad 72 thru_hole oval (at 96.52 -7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 66 "Net-(U1-Pad72)"))
    (pad 73 thru_hole oval (at 96.52 -10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 68 "Net-(U1-Pad73)"))
    (pad 69 thru_hole oval (at 96.52 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 53 thru_hole oval (at 93.98 -38.1) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 70 "Net-(U1-Pad53)"))
    (pad 58 thru_hole oval (at 93.98 -25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 72 "Net-(U1-Pad58)"))
    (pad 59 thru_hole oval (at 93.98 -22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 74 "Net-(U1-Pad59)"))
    (pad 54 thru_hole oval (at 93.98 -35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 75 "Net-(U1-Pad54)"))
    (pad 84 thru_hole oval (at 96.52 -38.1) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 76 "Net-(U1-Pad84)"))
    (pad 80 thru_hole oval (at 96.52 -27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 77 "Net-(U1-Pad80)"))
    (pad 79 thru_hole oval (at 96.52 -25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 79 "Net-(U1-Pad79)"))
    (pad 78 thru_hole oval (at 96.52 -22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 81 "Net-(U1-Pad78)"))
    (pad 83 thru_hole oval (at 96.52 -35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 82 "Net-(U1-Pad83)"))
    (pad 77 thru_hole oval (at 96.52 -20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 83 "Net-(U1-Pad77)"))
    (pad 60 thru_hole oval (at 93.98 -20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 84 "Net-(U1-Pad60)"))
    (pad 51 thru_hole oval (at 93.98 -43.18) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 +VISO))
    (pad 57 thru_hole oval (at 93.98 -27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 85 "Net-(U1-Pad57)"))
    (pad 52 thru_hole oval (at 93.98 -40.64) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 86 "Net-(U1-Pad52)"))
    (pad 86 thru_hole oval (at 96.52 -43.18) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 +VISO))
    (pad 85 thru_hole oval (at 96.52 -40.64) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 87 "Net-(U1-Pad85)"))
    (pad 26 thru_hole oval (at 83.82 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 "Net-(U1-Pad26)"))
    (pad 25 thru_hole oval (at 86.36 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 "Net-(U1-Pad25)"))
    (pad 22 thru_hole oval (at 86.36 -53.34 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(U1-Pad22)"))
    (pad 23 thru_hole oval (at 88.9 -53.34 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(U1-Pad23)"))
    (pad 24 thru_hole oval (at 91.44 -53.34 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(U1-Pad24)"))
    (pad 81 thru_hole oval (at 96.52 -30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 80 "Net-(U1-Pad81)"))
    (pad 55 thru_hole oval (at 93.98 -33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 71 "Net-(U1-Pad55)"))
    (pad 56 thru_hole oval (at 93.98 -30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 73 "Net-(U1-Pad56)"))
    (pad 82 thru_hole oval (at 96.52 -33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 78 "Net-(U1-Pad82)"))
    (pad 76 thru_hole oval (at 96.52 -17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 65 "Net-(U1-Pad76)"))
    (pad 61 thru_hole oval (at 93.98 -17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 61 "Net-(U1-Pad61)"))
    (pad 71 thru_hole oval (at 96.52 -5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 67 "Net-(U1-Pad71)"))
    (pad 66 thru_hole oval (at 93.98 -5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 63 "Net-(U1-Pad66)"))
    (pad 70 thru_hole oval (at 96.52 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 69 "Net-(U1-Pad70)"))
    (pad 19 thru_hole oval (at 78.74 -53.34 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(U1-Pad19)"))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 99.06 149.86)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:SMA_Molex_73251-1153_EdgeMount_Horizontal (layer F.Cu) (tedit 5D1E302E)
    (at 162.56 99.695 180)
    (descr "Molex SMA RF Connectors, Edge Mount, (http://www.molex.com/pdm_docs/sd/732511150_sd.pdf)")
    (tags "sma edge")
    (attr smd)
    (fp_text reference J1 (at -1.5 7 180) (layer F.SilkS))
    (fp_text value Conn_Coaxial (at -1.72 -7.11 180) (layer F.Fab))
    (fp_text user %R (at -1.5 7 180) (layer F.Fab))
    (pad 1 smd rect (at -1.72 0 180) (size 5.08 2.29) (layers F.Cu F.Paste F.Mask)
      (net 11 /CTRL_A))
    (pad 2 smd rect (at -1.72 -4.38 180) (size 5.08 2.42) (layers F.Cu F.Paste F.Mask)
      (net 2 +VISO))
    (pad 2 smd rect (at -1.72 4.38 180) (size 5.08 2.42) (layers F.Cu F.Paste F.Mask)
      (net 2 +VISO))
    (pad 2 smd rect (at -1.72 -4.38 180) (size 5.08 2.42) (layers B.Cu B.Paste B.Mask)
      (net 2 +VISO))
    (pad 2 smd rect (at -1.72 4.38 180) (size 5.08 2.42) (layers B.Cu B.Paste B.Mask)
      (net 2 +VISO))
    (pad 2 thru_hole circle (at 1.72 -4.38 180) (size 0.97 0.97) (drill 0.46) (layers *.Cu)
      (net 2 +VISO))
    (pad 2 thru_hole circle (at 1.72 4.38 180) (size 0.97 0.97) (drill 0.46) (layers *.Cu)
      (net 2 +VISO))
    (pad 2 smd rect (at 1.27 -4.38 180) (size 0.95 0.46) (layers F.Cu)
      (net 2 +VISO))
    (pad 2 smd rect (at 1.27 4.38 180) (size 0.95 0.46) (layers F.Cu)
      (net 2 +VISO))
    (pad 2 smd rect (at 1.27 -4.38 180) (size 0.95 0.46) (layers B.Cu)
      (net 2 +VISO))
    (pad 2 smd rect (at 1.27 4.38 180) (size 0.95 0.46) (layers B.Cu)
      (net 2 +VISO))
    (model ${KISYS3DMOD}/Connector_Coaxial.3dshapes/SMA_Molex_73251-1153_EdgeMount_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RF_Switch_Controller:SMA_Molex_73251-1153_EdgeMount_Horizontal (layer F.Cu) (tedit 5D1E302E)
    (at 162.56 114.3 180)
    (descr "Molex SMA RF Connectors, Edge Mount, (http://www.molex.com/pdm_docs/sd/732511150_sd.pdf)")
    (tags "sma edge")
    (attr smd)
    (fp_text reference J2 (at -1.5 7 180) (layer F.SilkS))
    (fp_text value Conn_Coaxial (at -1.72 -7.11 180) (layer F.Fab))
    (fp_text user %R (at -1.5 7 180) (layer F.Fab))
    (pad 2 smd rect (at 1.27 4.38 180) (size 0.95 0.46) (layers B.Cu)
      (net 2 +VISO))
    (pad 2 smd rect (at 1.27 -4.38 180) (size 0.95 0.46) (layers B.Cu)
      (net 2 +VISO))
    (pad 2 smd rect (at 1.27 4.38 180) (size 0.95 0.46) (layers F.Cu)
      (net 2 +VISO))
    (pad 2 smd rect (at 1.27 -4.38 180) (size 0.95 0.46) (layers F.Cu)
      (net 2 +VISO))
    (pad 2 thru_hole circle (at 1.72 4.38 180) (size 0.97 0.97) (drill 0.46) (layers *.Cu)
      (net 2 +VISO))
    (pad 2 thru_hole circle (at 1.72 -4.38 180) (size 0.97 0.97) (drill 0.46) (layers *.Cu)
      (net 2 +VISO))
    (pad 2 smd rect (at -1.72 4.38 180) (size 5.08 2.42) (layers B.Cu B.Paste B.Mask)
      (net 2 +VISO))
    (pad 2 smd rect (at -1.72 -4.38 180) (size 5.08 2.42) (layers B.Cu B.Paste B.Mask)
      (net 2 +VISO))
    (pad 2 smd rect (at -1.72 4.38 180) (size 5.08 2.42) (layers F.Cu F.Paste F.Mask)
      (net 2 +VISO))
    (pad 2 smd rect (at -1.72 -4.38 180) (size 5.08 2.42) (layers F.Cu F.Paste F.Mask)
      (net 2 +VISO))
    (pad 1 smd rect (at -1.72 0 180) (size 5.08 2.29) (layers F.Cu F.Paste F.Mask)
      (net 11 /CTRL_A))
    (model ${KISYS3DMOD}/Connector_Coaxial.3dshapes/SMA_Molex_73251-1153_EdgeMount_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RF_Switch_Controller:SMA_Molex_73251-1153_EdgeMount_Horizontal (layer F.Cu) (tedit 5D1E302E)
    (at 162.56 128.905 180)
    (descr "Molex SMA RF Connectors, Edge Mount, (http://www.molex.com/pdm_docs/sd/732511150_sd.pdf)")
    (tags "sma edge")
    (attr smd)
    (fp_text reference J3 (at -1.5 7 180) (layer F.SilkS))
    (fp_text value Conn_Coaxial (at -1.72 -7.11 180) (layer F.Fab))
    (fp_text user %R (at -1.5 7 180) (layer F.Fab))
    (pad 2 smd rect (at 1.27 4.38 180) (size 0.95 0.46) (layers B.Cu)
      (net 2 +VISO))
    (pad 2 smd rect (at 1.27 -4.38 180) (size 0.95 0.46) (layers B.Cu)
      (net 2 +VISO))
    (pad 2 smd rect (at 1.27 4.38 180) (size 0.95 0.46) (layers F.Cu)
      (net 2 +VISO))
    (pad 2 smd rect (at 1.27 -4.38 180) (size 0.95 0.46) (layers F.Cu)
      (net 2 +VISO))
    (pad 2 thru_hole circle (at 1.72 4.38 180) (size 0.97 0.97) (drill 0.46) (layers *.Cu)
      (net 2 +VISO))
    (pad 2 thru_hole circle (at 1.72 -4.38 180) (size 0.97 0.97) (drill 0.46) (layers *.Cu)
      (net 2 +VISO))
    (pad 2 smd rect (at -1.72 4.38 180) (size 5.08 2.42) (layers B.Cu B.Paste B.Mask)
      (net 2 +VISO))
    (pad 2 smd rect (at -1.72 -4.38 180) (size 5.08 2.42) (layers B.Cu B.Paste B.Mask)
      (net 2 +VISO))
    (pad 2 smd rect (at -1.72 4.38 180) (size 5.08 2.42) (layers F.Cu F.Paste F.Mask)
      (net 2 +VISO))
    (pad 2 smd rect (at -1.72 -4.38 180) (size 5.08 2.42) (layers F.Cu F.Paste F.Mask)
      (net 2 +VISO))
    (pad 1 smd rect (at -1.72 0 180) (size 5.08 2.29) (layers F.Cu F.Paste F.Mask)
      (net 12 /CTRL_B))
    (model ${KISYS3DMOD}/Connector_Coaxial.3dshapes/SMA_Molex_73251-1153_EdgeMount_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RF_Switch_Controller:SMA_Molex_73251-1153_EdgeMount_Horizontal (layer F.Cu) (tedit 5D1E302E)
    (at 162.56 143.51 180)
    (descr "Molex SMA RF Connectors, Edge Mount, (http://www.molex.com/pdm_docs/sd/732511150_sd.pdf)")
    (tags "sma edge")
    (attr smd)
    (fp_text reference J4 (at -1.5 7 180) (layer F.SilkS))
    (fp_text value Conn_Coaxial (at -1.72 -7.11 180) (layer F.Fab))
    (fp_text user %R (at -1.5 7 180) (layer F.Fab))
    (pad 1 smd rect (at -1.72 0 180) (size 5.08 2.29) (layers F.Cu F.Paste F.Mask)
      (net 12 /CTRL_B))
    (pad 2 smd rect (at -1.72 -4.38 180) (size 5.08 2.42) (layers F.Cu F.Paste F.Mask)
      (net 2 +VISO))
    (pad 2 smd rect (at -1.72 4.38 180) (size 5.08 2.42) (layers F.Cu F.Paste F.Mask)
      (net 2 +VISO))
    (pad 2 smd rect (at -1.72 -4.38 180) (size 5.08 2.42) (layers B.Cu B.Paste B.Mask)
      (net 2 +VISO))
    (pad 2 smd rect (at -1.72 4.38 180) (size 5.08 2.42) (layers B.Cu B.Paste B.Mask)
      (net 2 +VISO))
    (pad 2 thru_hole circle (at 1.72 -4.38 180) (size 0.97 0.97) (drill 0.46) (layers *.Cu)
      (net 2 +VISO))
    (pad 2 thru_hole circle (at 1.72 4.38 180) (size 0.97 0.97) (drill 0.46) (layers *.Cu)
      (net 2 +VISO))
    (pad 2 smd rect (at 1.27 -4.38 180) (size 0.95 0.46) (layers F.Cu)
      (net 2 +VISO))
    (pad 2 smd rect (at 1.27 4.38 180) (size 0.95 0.46) (layers F.Cu)
      (net 2 +VISO))
    (pad 2 smd rect (at 1.27 -4.38 180) (size 0.95 0.46) (layers B.Cu)
      (net 2 +VISO))
    (pad 2 smd rect (at 1.27 4.38 180) (size 0.95 0.46) (layers B.Cu)
      (net 2 +VISO))
    (model ${KISYS3DMOD}/Connector_Coaxial.3dshapes/SMA_Molex_73251-1153_EdgeMount_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RF_Switch_Controller:PinSocket_1x03_P2.54mm (layer B.Cu) (tedit 5D1E2D80)
    (at 122.555 141.732 270)
    (fp_text reference J5 (at 0 -8.001) (layer B.SilkS))
    (fp_text value Interboard_Conn (at 0 -7.85 270) (layer B.Fab))
    (fp_text user %R (at 0 -2.54 180) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /CTRL_B_TTL_FPGA))
    (pad 2 thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 96 "Net-(J5-Pad2)"))
    (pad 3 thru_hole oval (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 +VISO))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "RF Switch Controller\nrev -\nJuly 2019" (at 144.78 93.98) (layer F.SilkS))
  (gr_line (start 51.435 142.24) (end 86.36 142.24) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 86.36 101.6) (end 51.435 101.6) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 86.36 101.6) (end 86.36 142.24) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 51.435 101.6) (end 51.435 88.9) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 51.435 154.94) (end 51.435 142.24) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 65.405 154.94) (end 51.435 154.94) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 167.005 88.9) (end 167.005 90.17) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 167.005 153.67) (end 167.005 154.94) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 51.435 88.9) (end 65.405 88.9) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 167.005 154.94) (end 65.405 154.94) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 167.005 90.17) (end 167.005 153.67) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 65.405 88.9) (end 167.005 88.9) (layer Edge.Cuts) (width 0.15))
  (gr_text - (at 270.51 193.04) (layer Cmts.User))
  (gr_text "July 2019" (at 213.36 193.04) (layer Cmts.User))
  (gr_text "RF Switch Controller" (at 199.39 189.23) (layer Cmts.User))
  (gr_text RF_Switch_Controller.kicad_pcb (at 199.39 185.42) (layer Cmts.User))
  (gr_text "Vlad Smarandache\nRamshaw Group" (at 196.85 173.99) (layer Cmts.User))
  (zone (net 1) (net_name +5V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 51.435 88.9) (xy 167.005 88.9) (xy 167.005 154.94) (xy 51.435 154.94) (xy 51.435 142.24)
        (xy 86.36 142.24) (xy 86.36 101.6) (xy 51.435 101.6)
      )
    )
  )
  (zone (net 2) (net_name +VISO) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 51.435 88.9) (xy 167.005 88.9) (xy 167.005 154.94) (xy 51.435 154.94) (xy 51.435 142.24)
        (xy 86.36 142.24) (xy 86.36 101.6) (xy 51.435 101.6)
      )
    )
  )
)
