(kicad_pcb (version 20170123) (host pcbnew "(2017-05-31 revision c0bb8a30c)-makepkg")
  (general
    (links 78)
    (no_connects 0)
    (area -3.263095 -2.4685 93.263095 24.9895)
    (thickness 1.6)
    (drawings 68)
    (tracks 161)
    (zones 0)
    (modules 47)
    (nets 21)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.4)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.3 5.6)
    (pad_drill 0)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_ffffffff)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 GND)
  (net 3 "Net-(C2-Pad1)")
  (net 4 "Net-(C3-Pad1)")
  (net 5 "Net-(C4-Pad1)")
  (net 6 "Net-(C5-Pad1)")
  (net 7 "Net-(C6-Pad1)")
  (net 8 VCC)
  (net 9 Button_3)
  (net 10 Button_2)
  (net 11 Button_1)
  (net 12 Button_4)
  (net 13 Button_5)
  (net 14 Button_6)
  (net 15 Output_1)
  (net 16 Output_2)
  (net 17 Output_3)
  (net 18 Output_4)
  (net 19 Output_5)
  (net 20 Output_6)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.4)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net Button_1)
    (add_net Button_2)
    (add_net Button_3)
    (add_net Button_4)
    (add_net Button_5)
    (add_net Button_6)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C6-Pad1)")
    (add_net Output_1)
    (add_net Output_2)
    (add_net Output_3)
    (add_net Output_4)
    (add_net Output_5)
    (add_net Output_6)
    (add_net VCC)
  )
  (module .pretty:VIA-0.6mm (layer F.Cu) (tedit 5A2AEFC3)
    (at 88.75 12.5)
    (zone_connect 2)
    (fp_text reference REF** (at 0 1.397) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module .pretty:VIA-0.6mm (layer F.Cu) (tedit 5A2AEFC3)
    (at 1.25 12.5)
    (zone_connect 2)
    (fp_text reference REF** (at 0 1.397) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module .pretty:VIA-0.6mm (layer F.Cu) (tedit 5A2AEFC3)
    (at 83.125 1.25)
    (zone_connect 2)
    (fp_text reference REF** (at 0 1.397) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module .pretty:VIA-0.6mm (layer F.Cu) (tedit 5A2AEFC3)
    (at 76.875 1.25)
    (zone_connect 2)
    (fp_text reference REF** (at 0 1.397) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module .pretty:VIA-0.6mm (layer F.Cu) (tedit 5A2AEFC3)
    (at 54.375 1.25)
    (zone_connect 2)
    (fp_text reference REF** (at 0 1.397) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module .pretty:VIA-0.6mm (layer F.Cu) (tedit 5A2AEFC3)
    (at 11.875 1.25)
    (zone_connect 2)
    (fp_text reference REF** (at 0 1.397) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module .pretty:VIA-0.6mm (layer F.Cu) (tedit 5A2AEFC3)
    (at 33.125 1.25)
    (zone_connect 2)
    (fp_text reference REF** (at 0 1.397) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module .pretty:VIA-0.6mm (layer F.Cu) (tedit 5A2AEFC3)
    (at 47.5 14.375)
    (zone_connect 2)
    (fp_text reference REF** (at 0 1.397) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module .pretty:VIA-0.6mm (layer F.Cu) (tedit 5A2AEFC3)
    (at 53.125 14.375)
    (zone_connect 2)
    (fp_text reference REF** (at 0 1.397) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module .pretty:VIA-0.6mm (layer F.Cu) (tedit 5A2AEFC3)
    (at 67.5 20.625)
    (zone_connect 2)
    (fp_text reference REF** (at 0 1.397) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module .pretty:VIA-0.6mm (layer F.Cu) (tedit 5A2AEFC3)
    (at 1.25 22.5)
    (zone_connect 2)
    (fp_text reference REF** (at 0 1.397) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module .pretty:VIA-0.6mm (layer F.Cu) (tedit 5A2AEFC3)
    (at 28.75 22.5)
    (zone_connect 2)
    (fp_text reference REF** (at 0 1.397) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module .pretty:VIA-0.6mm (layer F.Cu) (tedit 5A2AEFC3)
    (at 58.125 22.5)
    (zone_connect 2)
    (fp_text reference REF** (at 0 1.397) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module .pretty:VIA-0.6mm (layer F.Cu) (tedit 5A2AEFC3)
    (at 72.5 22.5)
    (zone_connect 2)
    (fp_text reference REF** (at 0 1.397) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module .pretty:VIA-0.6mm (layer F.Cu) (tedit 5A2AEFC3)
    (at 88.75 22.5)
    (zone_connect 2)
    (fp_text reference REF** (at 0 1.397) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module .pretty:VIA-0.6mm (layer F.Cu) (tedit 5A2AEFC3)
    (at 88.75 1.25)
    (zone_connect 2)
    (fp_text reference REF** (at 0 1.397) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module .pretty:VIA-0.6mm (layer F.Cu) (tedit 5A2AEFC3)
    (at 66.875 1.25)
    (zone_connect 2)
    (fp_text reference REF** (at 0 1.397) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module .pretty:VIA-0.6mm (layer F.Cu) (tedit 5A2AEFC3)
    (at 45.625 1.25)
    (zone_connect 2)
    (fp_text reference REF** (at 0 1.397) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module .pretty:VIA-0.6mm (layer F.Cu) (tedit 5A2AEFC3)
    (at 24.375 1.25)
    (zone_connect 2)
    (fp_text reference REF** (at 0 1.397) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module .pretty:VIA-0.6mm (layer F.Cu) (tedit 5A2AEFC3)
    (at 1.25 1.25)
    (zone_connect 2)
    (fp_text reference REF** (at 0 1.397) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module .pretty:1pin (layer B.Cu) (tedit 565CC809)
    (at 86.36 19.05)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 3.048) (layer B.SilkS) hide)
    (fp_text value 1pin (at 0 -2.794) (layer B.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 2.921 2.921) (drill 2.921) (layers *.Cu *.Mask))
  )
  (module .pretty:1pin (layer B.Cu) (tedit 565CC809)
    (at 3.81 19.05)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 3.048) (layer B.SilkS) hide)
    (fp_text value 1pin (at 0 -2.794) (layer B.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 2.921 2.921) (drill 2.921) (layers *.Cu *.Mask))
  )
  (module .pretty:1pin (layer B.Cu) (tedit 565CC809)
    (at 3.81 6.35)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 3.048) (layer B.SilkS) hide)
    (fp_text value 1pin (at 0 -2.794) (layer B.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 2.921 2.921) (drill 2.921) (layers *.Cu *.Mask))
  )
  (module .pretty:1pin (layer B.Cu) (tedit 565CC809)
    (at 86.36 6.35)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 3.048) (layer B.SilkS) hide)
    (fp_text value 1pin (at 0 -2.794) (layer B.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 2.921 2.921) (drill 2.921) (layers *.Cu *.Mask))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5A2EED83)
    (at 14.375 15 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at -2.5 0 90) (layer F.SilkS) hide)
    (fp_text value 0.1uF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5A2EED8D)
    (at 19.375 15 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 0 -1.9 90) (layer F.SilkS) hide)
    (fp_text value 0.1uF (at 0 1.9 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5A2EED96)
    (at 24.375 15 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at 0 -1.9 90) (layer F.SilkS) hide)
    (fp_text value 0.1uF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5A2EED9F)
    (at 35.625 15 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at 0 -1.9 180) (layer F.SilkS) hide)
    (fp_text value 0.1uF (at 0 1.9 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C4-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5A2EEDA9)
    (at 40.625 15 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C5 (at 0 -1.9 90) (layer F.SilkS) hide)
    (fp_text value 0.1uF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5A2EEDB2)
    (at 45.625 15 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C6 (at 0 -1.9 90) (layer F.SilkS) hide)
    (fp_text value 0.1uF (at 0 1.9 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C6-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module .pretty:1814676 (layer F.Cu) (tedit 5A2AF06E)
    (at 18.125 6.25)
    (fp_text reference J2 (at 0 -6.223) (layer F.SilkS) hide)
    (fp_text value CONN_01X06 (at 0 -7.747) (layer F.Fab) hide)
    (pad 1 smd rect (at -6.25 3.85) (size 1.4 3.4) (layers F.Cu F.Paste F.Mask)
      (net 11 Button_1))
    (pad 2 smd rect (at -3.75 3.85) (size 1.4 3.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -1.25 3.85) (size 1.4 3.4) (layers F.Cu F.Paste F.Mask)
      (net 10 Button_2))
    (pad 4 smd rect (at 1.25 3.85) (size 1.4 3.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at 3.75 3.85) (size 1.4 3.4) (layers F.Cu F.Paste F.Mask)
      (net 9 Button_3))
    (pad 6 smd rect (at 6.25 3.85) (size 1.4 3.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at 8.85 -2.75) (size 2.3 5.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at -8.85 -2.75) (size 2.3 5.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model "C:/Program Files/KiCad/3D lib/Junes.3dshapes/1814676_00.step"
      (at (xyz -0.3031496062992126 0.2519685039370079 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 90))
    )
  )
  (module .pretty:1814676 (layer F.Cu) (tedit 5A2AF078)
    (at 39.375 6.25)
    (fp_text reference J3 (at 0 -6.223) (layer F.SilkS) hide)
    (fp_text value CONN_01X06 (at 0 -7.747) (layer F.Fab) hide)
    (pad 7 smd rect (at -8.85 -2.75) (size 2.3 5.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at 8.85 -2.75) (size 2.3 5.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at 6.25 3.85) (size 1.4 3.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at 3.75 3.85) (size 1.4 3.4) (layers F.Cu F.Paste F.Mask)
      (net 14 Button_6))
    (pad 4 smd rect (at 1.25 3.85) (size 1.4 3.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -1.25 3.85) (size 1.4 3.4) (layers F.Cu F.Paste F.Mask)
      (net 13 Button_5))
    (pad 2 smd rect (at -3.75 3.85) (size 1.4 3.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -6.25 3.85) (size 1.4 3.4) (layers F.Cu F.Paste F.Mask)
      (net 12 Button_4))
    (model "C:/Program Files/KiCad/3D lib/Junes.3dshapes/1814676_00.step"
      (at (xyz -0.3031496062992126 0.2519685039370079 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 90))
    )
  )
  (module .pretty:1814676 (layer F.Cu) (tedit 5A2AF080)
    (at 60.625 6.236)
    (fp_text reference J4 (at 0 -6.223) (layer F.SilkS) hide)
    (fp_text value CONN_01X06 (at 0 -7.747) (layer F.Fab) hide)
    (pad 7 smd rect (at -8.85 -2.75) (size 2.3 5.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at 8.85 -2.75) (size 2.3 5.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at 6.25 3.85) (size 1.4 3.4) (layers F.Cu F.Paste F.Mask)
      (net 15 Output_1))
    (pad 5 smd rect (at 3.75 3.85) (size 1.4 3.4) (layers F.Cu F.Paste F.Mask)
      (net 16 Output_2))
    (pad 4 smd rect (at 1.25 3.85) (size 1.4 3.4) (layers F.Cu F.Paste F.Mask)
      (net 17 Output_3))
    (pad 3 smd rect (at -1.25 3.85) (size 1.4 3.4) (layers F.Cu F.Paste F.Mask)
      (net 18 Output_4))
    (pad 2 smd rect (at -3.75 3.85) (size 1.4 3.4) (layers F.Cu F.Paste F.Mask)
      (net 19 Output_5))
    (pad 1 smd rect (at -6.25 3.85) (size 1.4 3.4) (layers F.Cu F.Paste F.Mask)
      (net 20 Output_6))
    (model "C:/Program Files/KiCad/3D lib/Junes.3dshapes/1814676_00.step"
      (at (xyz -0.3031496062992126 0.2519685039370079 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 90))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5A2EED85)
    (at 11.875 18.75 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0 1.875 270) (layer F.SilkS) hide)
    (fp_text value 10K (at 0 2.1 270) (layer F.Fab))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 VCC))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 11 Button_1))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5A2EED91)
    (at 16.875 18.75 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 0 -2.1 270) (layer F.SilkS) hide)
    (fp_text value 10K (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 10 Button_2))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 VCC))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5A2EED99)
    (at 21.875 18.75 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 0 -2.1 270) (layer F.SilkS) hide)
    (fp_text value 10K (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 9 Button_3))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 VCC))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5A2EEDA5)
    (at 33.125 18.75 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 0 -2.1 270) (layer F.SilkS) hide)
    (fp_text value 10K (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 12 Button_4))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 VCC))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5A2EEDAB)
    (at 38.125 18.75 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at 0 -2.1 270) (layer F.SilkS) hide)
    (fp_text value 10K (at 0 2.1 270) (layer F.Fab))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 VCC))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 13 Button_5))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5A2EEDB5)
    (at 43.125 18.75 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R6 (at 0 -2.1 270) (layer F.SilkS) hide)
    (fp_text value 10K (at 0 2.1 270) (layer F.Fab))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 VCC))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 14 Button_6))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5A2EED88)
    (at 11.875 15 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R7 (at 0 -2.1 90) (layer F.SilkS) hide)
    (fp_text value 10K (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 11 Button_1))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5A2EED7F)
    (at 16.875 15 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R8 (at 0 -2.1 90) (layer F.SilkS) hide)
    (fp_text value 10K (at 0 2.1 90) (layer F.Fab))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 10 Button_2))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5A2EED93)
    (at 21.875 15 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R9 (at 0 -2.1 90) (layer F.SilkS) hide)
    (fp_text value 10K (at 0 2.1 90) (layer F.Fab))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 9 Button_3))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5A2EED9C)
    (at 33.125 15 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R10 (at 0 -2.1 90) (layer F.SilkS) hide)
    (fp_text value 10K (at 0 2.1 90) (layer F.Fab))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 12 Button_4))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C4-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5A2EEDA3)
    (at 38.125 15 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R11 (at 0 -2.1 90) (layer F.SilkS) hide)
    (fp_text value 10K (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 13 Button_5))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5A2EEDAE)
    (at 43.125 15 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R12 (at 0 -2.1 90) (layer F.SilkS) hide)
    (fp_text value 10K (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C6-Pad1)"))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 14 Button_6))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SOIC-14_N (layer F.Cu) (tedit 0)
    (at 60.625 17.5 90)
    (descr "Module CMS SOJ 14 pins Large")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference U1 (at 0 -1.27 90) (layer F.SilkS))
    (fp_text value 74HC14 (at 0 1.27 90) (layer F.Fab))
    (pad 1 smd rect (at -3.81 3.302 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at -2.54 3.302 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 15 Output_1))
    (pad 3 smd rect (at -1.27 3.302 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 4 smd rect (at 0 3.302 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 16 Output_2))
    (pad 5 smd rect (at 1.27 3.302 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 6 smd rect (at 2.54 3.302 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 17 Output_3))
    (pad 7 smd rect (at 3.81 3.302 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 8 smd rect (at 3.81 -3.048 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 18 Output_4))
    (pad 9 smd rect (at 2.54 -3.048 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C4-Pad1)"))
    (pad 11 smd rect (at 0 -3.048 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C5-Pad1)"))
    (pad 12 smd rect (at -1.27 -3.048 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 20 Output_6))
    (pad 13 smd rect (at -2.54 -3.048 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C6-Pad1)"))
    (pad 14 smd rect (at -3.81 -3.048 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 8 VCC))
    (pad 10 smd rect (at 1.27 -3.048 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 19 Output_5))
    (model SMD_Packages.3dshapes/SOIC-14_N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.4 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module .pretty:1814634 (layer F.Cu) (tedit 5A2AF088)
    (at 76.875 6.25)
    (fp_text reference J1 (at 0 -6.223) (layer F.SilkS) hide)
    (fp_text value CONN_01X02 (at 0 -7.747) (layer F.Fab) hide)
    (pad 7 smd rect (at -3.85 -2.75) (size 2.3 5.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at 3.85 -2.75) (size 2.3 5.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.25 3.85) (size 1.4 3.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.25 3.85) (size 1.4 3.4) (layers F.Cu F.Paste F.Mask)
      (net 8 VCC))
    (model "C:/Program Files/KiCad/3D lib/Junes.3dshapes/1814634_00.stp"
      (at (xyz -0.1082677165354331 0.2559055118110236 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 90))
    )
  )
  (gr_text "6 CHANNEL DE-BOUNCER" (at 45 20.625 180) (layer B.SilkS))
  (gr_text 1 (at 66.975 5.08 180) (layer B.SilkS))
  (gr_text 2 (at 64.435 5.08 180) (layer B.SilkS))
  (gr_text 3 (at 61.895 5.08 180) (layer B.SilkS))
  (gr_text 4 (at 59.355 5.08 180) (layer B.SilkS))
  (gr_text 5 (at 56.815 5.08 180) (layer B.SilkS))
  (gr_text 6 (at 54.275 5.08 180) (layer B.SilkS))
  (gr_text GND (at 24.475 5.08 270) (layer B.SilkS))
  (gr_text 3 (at 21.935 5.08 180) (layer B.SilkS))
  (gr_text GND (at 19.395 5.08 270) (layer B.SilkS))
  (gr_text 2 (at 16.855 5.08 180) (layer B.SilkS))
  (gr_text GND (at 14.315 5.08 270) (layer B.SilkS))
  (gr_text 1 (at 11.775 5.08 180) (layer B.SilkS))
  (gr_text GND (at 45.725 5.08 270) (layer B.SilkS))
  (gr_text 6 (at 43.185 5.08 180) (layer B.SilkS))
  (gr_text GND (at 40.645 5.08 270) (layer B.SilkS))
  (gr_text 5 (at 38.105 5.08 180) (layer B.SilkS))
  (gr_text GND (at 35.565 5.08 270) (layer B.SilkS))
  (gr_text 4 (at 33.025 5.08 180) (layer B.SilkS))
  (gr_text GND (at 78.232 5.08 90) (layer B.SilkS))
  (gr_text 3.3-5V (at 75.692 5.08 90) (layer B.SilkS))
  (gr_text INPUT (at 18.125 11.43 180) (layer B.SilkS))
  (gr_text INPUT (at 39.375 11.43 180) (layer B.SilkS))
  (gr_text OUTPUT (at 60.625 11.43 180) (layer B.SilkS))
  (gr_text POWER (at 76.875 11.43 180) (layer B.SilkS))
  (gr_line (start 0 23.75) (end 0 0) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 90 23.75) (end 0 23.75) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 90 0) (end 90 23.75) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 0 0) (end 90 0) (layer Edge.Cuts) (width 0.2))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 0 0) (xy 90 0) (xy 90 23.75) (xy 0 23.75)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 0 0) (xy 90 0) (xy 90 23.75) (xy 0 23.75)
      )
    )
  )
)
