(kicad_pcb (version 20171130) (host pcbnew "(5.1.0)-1")
  (general
    (thickness 1.6)
    (drawings 138)
    (tracks 1442)
    (zones 0)
    (modules 152)
    (nets 177)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (1 Route2 signal hide)
    (2 Route15 signal hide)
    (31 B.Cu signal hide)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user hide)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.27178)
    (user_trace_width 0.27178)
    (user_trace_width 0.2794)
    (user_trace_width 0.508)
    (user_trace_width 0.6096)
    (user_trace_width 1.27)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (user_via 0.5842 0.381)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.15)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_fffffff9)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer false)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin true)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers/"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 3.3V)
  (net 3 I_BATT)
  (net 4 ENAB_BURN4)
  (net 5 ENAB_BURN3)
  (net 6 ENAB_BURN2)
  (net 7 ENAB_BURN1)
  (net 8 ENAB_GPS)
  (net 9 SWCLK)
  (net 10 SWDIO)
  (net 11 ~RESET)
  (net 12 VSOLAR)
  (net 13 L1_PROG)
  (net 14 VBATT)
  (net 15 USB_D+)
  (net 16 USB_D-)
  (net 17 GPS_PWR_IN)
  (net 18 BURN_RELAY_B)
  (net 19 BURN_RELAY_A)
  (net 20 ENAB_BURN5)
  (net 21 "Net-(C8-Pad1)")
  (net 22 "Net-(U3-Pad13)")
  (net 23 "Net-(U3-Pad12)")
  (net 24 "Net-(U3-Pad11)")
  (net 25 "Net-(U3-Pad10)")
  (net 26 "Net-(U3-Pad9)")
  (net 27 "Net-(U1-Pad5)")
  (net 28 "Net-(R15-Pad1)")
  (net 29 "Net-(R13-Pad1)")
  (net 30 "Net-(R10-Pad1)")
  (net 31 /Power/VREG_IN)
  (net 32 "Net-(C22-Pad1)")
  (net 33 "Net-(C25-Pad1)")
  (net 34 "Net-(C26-Pad1)")
  (net 35 /Connectors/VBATT_IN)
  (net 36 "Net-(J1-PadDT)")
  (net 37 "Net-(J1-PadSW)")
  (net 38 "Net-(J1-Pad8)")
  (net 39 "Net-(J1-Pad1)")
  (net 40 "Net-(U14-Pad19)")
  (net 41 "Net-(U14-Pad16)")
  (net 42 "Net-(U14-Pad15)")
  (net 43 "Net-(U14-Pad14)")
  (net 44 "Net-(U14-Pad17)")
  (net 45 "Net-(U14-Pad18)")
  (net 46 "Net-(U14-Pad1)")
  (net 47 "Net-(U14-Pad3)")
  (net 48 "Net-(U14-Pad6)")
  (net 49 "Net-(U14-Pad5)")
  (net 50 "Net-(U14-Pad4)")
  (net 51 "Net-(U14-Pad2)")
  (net 52 "Net-(U14-Pad7)")
  (net 53 "Net-(U14-Pad9)")
  (net 54 "/RF and GPS/RF_IN")
  (net 55 "/Burn Wires/VBURN_A_IN")
  (net 56 "/Burn Wires/VBURN1")
  (net 57 "/Burn Wires/VBURN2")
  (net 58 "/Burn Wires/VBURN_B_IN")
  (net 59 "/Burn Wires/VBURN3")
  (net 60 "/Burn Wires/VBURN4")
  (net 61 "Net-(Q5-Pad1)")
  (net 62 "Net-(Q8-Pad1)")
  (net 63 "Net-(Q7-Pad1)")
  (net 64 "Net-(Q6-Pad1)")
  (net 65 "/Burn Wires/VBURN5")
  (net 66 "Net-(D4-PadA)")
  (net 67 /Avionics/XTAL1)
  (net 68 /Avionics/XTAL2)
  (net 69 DAC0)
  (net 70 "Net-(Q5-Pad3)")
  (net 71 "Net-(Q6-Pad3)")
  (net 72 "Net-(Q7-Pad3)")
  (net 73 "Net-(Q8-Pad3)")
  (net 74 /Avionics/BATTERY)
  (net 75 MISO)
  (net 76 SCK)
  (net 77 MOSI)
  (net 78 FLASH_CS)
  (net 79 FLASH_SCK)
  (net 80 FLASH_IO3)
  (net 81 FLASH_IO2)
  (net 82 FLASH_MISO)
  (net 83 FLASH_MOSI)
  (net 84 xSDCS)
  (net 85 "Net-(J5-Pad1)")
  (net 86 "Net-(J6-Pad1)")
  (net 87 "Net-(J7-Pad1)")
  (net 88 "Net-(C9-Pad1)")
  (net 89 "Net-(C12-Pad2)")
  (net 90 "Net-(C21-Pad1)")
  (net 91 "Net-(C27-Pad1)")
  (net 92 "Net-(D1-Pad1)")
  (net 93 "Net-(D3-Pad2)")
  (net 94 "Net-(D5-PadA)")
  (net 95 "Net-(J3-Pad4)")
  (net 96 "Net-(J4-Pad2)")
  (net 97 "Net-(JP5-Pad1)")
  (net 98 "Net-(JP8-Pad3)")
  (net 99 "Net-(JP9-Pad3)")
  (net 100 "Net-(JP10-Pad3)")
  (net 101 "Net-(L1-Pad2)")
  (net 102 "Net-(Q1-Pad1)")
  (net 103 "Net-(Q1-Pad3)")
  (net 104 "Net-(Q4-Pad1)")
  (net 105 "Net-(Q4-Pad3)")
  (net 106 "Net-(R5-Pad2)")
  (net 107 "Net-(R6-Pad2)")
  (net 108 "Net-(R11-Pad1)")
  (net 109 "Net-(R16-Pad1)")
  (net 110 "Net-(R16-Pad2)")
  (net 111 "Net-(R18-Pad1)")
  (net 112 "Net-(U9-Pad17)")
  (net 113 "Net-(U9-Pad18)")
  (net 114 "Net-(U9-Pad19)")
  (net 115 "Net-(U9-Pad20)")
  (net 116 "Net-(U9-Pad21)")
  (net 117 "Net-(U9-Pad22)")
  (net 118 "Net-(U9-Pad23)")
  (net 119 "Net-(U9-Pad2)")
  (net 120 "Net-(U10-Pad17)")
  (net 121 "Net-(U10-Pad18)")
  (net 122 "Net-(U10-Pad19)")
  (net 123 "Net-(U10-Pad20)")
  (net 124 "Net-(U10-Pad21)")
  (net 125 "Net-(U10-Pad22)")
  (net 126 "Net-(U10-Pad23)")
  (net 127 "Net-(U10-Pad2)")
  (net 128 "Net-(U11-Pad17)")
  (net 129 "Net-(U11-Pad18)")
  (net 130 "Net-(U11-Pad19)")
  (net 131 "Net-(U11-Pad20)")
  (net 132 "Net-(U11-Pad21)")
  (net 133 "Net-(U11-Pad22)")
  (net 134 "Net-(U11-Pad23)")
  (net 135 "Net-(U11-Pad2)")
  (net 136 "Net-(U12-Pad17)")
  (net 137 "Net-(U12-Pad18)")
  (net 138 "Net-(U12-Pad19)")
  (net 139 "Net-(U12-Pad20)")
  (net 140 "Net-(U12-Pad21)")
  (net 141 "Net-(U12-Pad22)")
  (net 142 "Net-(U12-Pad23)")
  (net 143 "Net-(U12-Pad2)")
  (net 144 "Net-(C21-Pad2)")
  (net 145 "Net-(C23-Pad1)")
  (net 146 "Net-(C25-Pad2)")
  (net 147 "Net-(L3-Pad1)")
  (net 148 "Net-(R42-Pad2)")
  (net 149 WDT_WDI)
  (net 150 ~CHRG)
  (net 151 RF_IO2)
  (net 152 /Avionics/SDA)
  (net 153 /Avionics/SCL)
  (net 154 RX)
  (net 155 TX)
  (net 156 PB15)
  (net 157 PB14)
  (net 158 PA16)
  (net 159 PB17)
  (net 160 PA22)
  (net 161 PA20)
  (net 162 PB22)
  (net 163 PB23)
  (net 164 PA18)
  (net 165 PA19)
  (net 166 PB16)
  (net 167 "Net-(R24-Pad1)")
  (net 168 "Net-(R46-Pad2)")
  (net 169 "Net-(J11-Pad1)")
  (net 170 RF_IO1)
  (net 171 "Net-(U23-Pad4)")
  (net 172 "Net-(U23-Pad3)")
  (net 173 CS_RF)
  (net 174 RF_RST)
  (net 175 RF_IO5)
  (net 176 RF_IO0)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.27178)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (diff_pair_width 0.27178)
    (diff_pair_gap 0.27178)
    (add_net /Avionics/BATTERY)
    (add_net /Avionics/SCL)
    (add_net /Avionics/SDA)
    (add_net /Avionics/XTAL1)
    (add_net /Avionics/XTAL2)
    (add_net "/Burn Wires/VBURN1")
    (add_net "/Burn Wires/VBURN2")
    (add_net "/Burn Wires/VBURN3")
    (add_net "/Burn Wires/VBURN4")
    (add_net "/Burn Wires/VBURN5")
    (add_net "/Burn Wires/VBURN_A_IN")
    (add_net "/Burn Wires/VBURN_B_IN")
    (add_net /Connectors/VBATT_IN)
    (add_net /Power/VREG_IN)
    (add_net "/RF and GPS/RF_IN")
    (add_net 3.3V)
    (add_net BURN_RELAY_A)
    (add_net BURN_RELAY_B)
    (add_net CS_RF)
    (add_net DAC0)
    (add_net ENAB_BURN1)
    (add_net ENAB_BURN2)
    (add_net ENAB_BURN3)
    (add_net ENAB_BURN4)
    (add_net ENAB_BURN5)
    (add_net ENAB_GPS)
    (add_net FLASH_CS)
    (add_net FLASH_IO2)
    (add_net FLASH_IO3)
    (add_net FLASH_MISO)
    (add_net FLASH_MOSI)
    (add_net FLASH_SCK)
    (add_net GND)
    (add_net GPS_PWR_IN)
    (add_net I_BATT)
    (add_net L1_PROG)
    (add_net MISO)
    (add_net MOSI)
    (add_net "Net-(C12-Pad2)")
    (add_net "Net-(C21-Pad1)")
    (add_net "Net-(C21-Pad2)")
    (add_net "Net-(C22-Pad1)")
    (add_net "Net-(C23-Pad1)")
    (add_net "Net-(C25-Pad1)")
    (add_net "Net-(C25-Pad2)")
    (add_net "Net-(C26-Pad1)")
    (add_net "Net-(C27-Pad1)")
    (add_net "Net-(C8-Pad1)")
    (add_net "Net-(C9-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-PadA)")
    (add_net "Net-(D5-PadA)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J1-PadDT)")
    (add_net "Net-(J1-PadSW)")
    (add_net "Net-(J11-Pad1)")
    (add_net "Net-(J3-Pad4)")
    (add_net "Net-(J4-Pad2)")
    (add_net "Net-(J5-Pad1)")
    (add_net "Net-(J6-Pad1)")
    (add_net "Net-(J7-Pad1)")
    (add_net "Net-(JP10-Pad3)")
    (add_net "Net-(JP5-Pad1)")
    (add_net "Net-(JP8-Pad3)")
    (add_net "Net-(JP9-Pad3)")
    (add_net "Net-(L1-Pad2)")
    (add_net "Net-(L3-Pad1)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(Q1-Pad3)")
    (add_net "Net-(Q4-Pad1)")
    (add_net "Net-(Q4-Pad3)")
    (add_net "Net-(Q5-Pad1)")
    (add_net "Net-(Q5-Pad3)")
    (add_net "Net-(Q6-Pad1)")
    (add_net "Net-(Q6-Pad3)")
    (add_net "Net-(Q7-Pad1)")
    (add_net "Net-(Q7-Pad3)")
    (add_net "Net-(Q8-Pad1)")
    (add_net "Net-(Q8-Pad3)")
    (add_net "Net-(R10-Pad1)")
    (add_net "Net-(R11-Pad1)")
    (add_net "Net-(R13-Pad1)")
    (add_net "Net-(R15-Pad1)")
    (add_net "Net-(R16-Pad1)")
    (add_net "Net-(R16-Pad2)")
    (add_net "Net-(R18-Pad1)")
    (add_net "Net-(R24-Pad1)")
    (add_net "Net-(R42-Pad2)")
    (add_net "Net-(R46-Pad2)")
    (add_net "Net-(R5-Pad2)")
    (add_net "Net-(R6-Pad2)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U10-Pad17)")
    (add_net "Net-(U10-Pad18)")
    (add_net "Net-(U10-Pad19)")
    (add_net "Net-(U10-Pad2)")
    (add_net "Net-(U10-Pad20)")
    (add_net "Net-(U10-Pad21)")
    (add_net "Net-(U10-Pad22)")
    (add_net "Net-(U10-Pad23)")
    (add_net "Net-(U11-Pad17)")
    (add_net "Net-(U11-Pad18)")
    (add_net "Net-(U11-Pad19)")
    (add_net "Net-(U11-Pad2)")
    (add_net "Net-(U11-Pad20)")
    (add_net "Net-(U11-Pad21)")
    (add_net "Net-(U11-Pad22)")
    (add_net "Net-(U11-Pad23)")
    (add_net "Net-(U12-Pad17)")
    (add_net "Net-(U12-Pad18)")
    (add_net "Net-(U12-Pad19)")
    (add_net "Net-(U12-Pad2)")
    (add_net "Net-(U12-Pad20)")
    (add_net "Net-(U12-Pad21)")
    (add_net "Net-(U12-Pad22)")
    (add_net "Net-(U12-Pad23)")
    (add_net "Net-(U14-Pad1)")
    (add_net "Net-(U14-Pad14)")
    (add_net "Net-(U14-Pad15)")
    (add_net "Net-(U14-Pad16)")
    (add_net "Net-(U14-Pad17)")
    (add_net "Net-(U14-Pad18)")
    (add_net "Net-(U14-Pad19)")
    (add_net "Net-(U14-Pad2)")
    (add_net "Net-(U14-Pad3)")
    (add_net "Net-(U14-Pad4)")
    (add_net "Net-(U14-Pad5)")
    (add_net "Net-(U14-Pad6)")
    (add_net "Net-(U14-Pad7)")
    (add_net "Net-(U14-Pad9)")
    (add_net "Net-(U23-Pad3)")
    (add_net "Net-(U23-Pad4)")
    (add_net "Net-(U3-Pad10)")
    (add_net "Net-(U3-Pad11)")
    (add_net "Net-(U3-Pad12)")
    (add_net "Net-(U3-Pad13)")
    (add_net "Net-(U3-Pad9)")
    (add_net "Net-(U9-Pad17)")
    (add_net "Net-(U9-Pad18)")
    (add_net "Net-(U9-Pad19)")
    (add_net "Net-(U9-Pad2)")
    (add_net "Net-(U9-Pad20)")
    (add_net "Net-(U9-Pad21)")
    (add_net "Net-(U9-Pad22)")
    (add_net "Net-(U9-Pad23)")
    (add_net PA16)
    (add_net PA18)
    (add_net PA19)
    (add_net PA20)
    (add_net PA22)
    (add_net PB14)
    (add_net PB15)
    (add_net PB16)
    (add_net PB17)
    (add_net PB22)
    (add_net PB23)
    (add_net RF_IO0)
    (add_net RF_IO1)
    (add_net RF_IO2)
    (add_net RF_IO5)
    (add_net RF_RST)
    (add_net RX)
    (add_net SCK)
    (add_net SWCLK)
    (add_net SWDIO)
    (add_net TX)
    (add_net USB_D+)
    (add_net USB_D-)
    (add_net VBATT)
    (add_net VSOLAR)
    (add_net WDT_WDI)
    (add_net xSDCS)
    (add_net ~CHRG)
    (add_net ~RESET)
  )
  (module custom-footprints:XTB28_MEZ (layer F.Cu) (tedit 5D2D1541)
    (at 144.52346 64.7573 180)
    (fp_text reference U12 (at 3.302 -27.178 180) (layer F.SilkS) hide)
    (fp_text value XTB-40 (at 0 0 180) (layer F.SilkS) hide)
    (pad 10 smd rect (at 2.54 0 90) (size 2.286 1.9812) (layers F.Cu F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 11 smd rect (at 5.08 0 90) (size 2.286 1.9812) (layers F.Cu F.Mask)
      (net 2 3.3V) (solder_mask_margin 0.0635))
    (pad 12 smd rect (at 7.62 0 90) (size 2.286 1.9812) (layers F.Cu F.Mask)
      (solder_mask_margin 0.0635))
    (pad 13 smd rect (at 10.16 0 90) (size 2.286 1.9812) (layers F.Cu F.Mask)
      (solder_mask_margin 0.0635))
    (pad 14 smd rect (at 12.7 0 90) (size 2.286 1.9812) (layers F.Cu F.Mask)
      (solder_mask_margin 0.0635))
    (pad 15 smd rect (at 14.986 -2.54 180) (size 2.286 1.9812) (layers F.Cu F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 16 smd rect (at 14.986 -5.08 180) (size 2.286 1.9812) (layers F.Cu F.Mask)
      (net 2 3.3V) (solder_mask_margin 0.0635))
    (pad 17 smd rect (at 14.986 -7.62 180) (size 2.286 1.9812) (layers F.Cu F.Mask)
      (net 136 "Net-(U12-Pad17)") (solder_mask_margin 0.0635))
    (pad 18 smd rect (at 14.986 -10.16 180) (size 2.286 1.9812) (layers F.Cu F.Mask)
      (net 137 "Net-(U12-Pad18)") (solder_mask_margin 0.0635))
    (pad 19 smd rect (at 14.986 -12.7 180) (size 2.286 1.9812) (layers F.Cu F.Mask)
      (net 138 "Net-(U12-Pad19)") (solder_mask_margin 0.0635))
    (pad 20 smd rect (at 14.986 -15.24 180) (size 2.286 1.9812) (layers F.Cu F.Mask)
      (net 139 "Net-(U12-Pad20)") (solder_mask_margin 0.0635))
    (pad 21 smd rect (at 14.986 -17.78 180) (size 2.286 1.9812) (layers F.Cu F.Mask)
      (net 140 "Net-(U12-Pad21)") (solder_mask_margin 0.0635))
    (pad 22 smd rect (at 14.986 -20.32 180) (size 2.286 1.9812) (layers F.Cu F.Mask)
      (net 141 "Net-(U12-Pad22)") (solder_mask_margin 0.0635))
    (pad 23 smd rect (at 14.986 -22.86 180) (size 2.286 1.9812) (layers F.Cu F.Mask)
      (net 142 "Net-(U12-Pad23)") (solder_mask_margin 0.0635))
    (pad 1 smd rect (at 0.254 -22.86 180) (size 2.286 1.9812) (layers F.Cu F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 2 smd rect (at 0.254 -20.32 180) (size 2.286 1.9812) (layers F.Cu F.Mask)
      (net 143 "Net-(U12-Pad2)") (solder_mask_margin 0.0635))
    (pad 3 smd rect (at 0.254 -17.78 180) (size 2.286 1.9812) (layers F.Cu F.Mask)
      (net 166 PB16) (solder_mask_margin 0.0635))
    (pad 4 smd rect (at 0.254 -15.24 180) (size 2.286 1.9812) (layers F.Cu F.Mask)
      (net 77 MOSI) (solder_mask_margin 0.0635))
    (pad 5 smd rect (at 0.254 -12.7 180) (size 2.286 1.9812) (layers F.Cu F.Mask)
      (net 76 SCK) (solder_mask_margin 0.0635))
    (pad 6 smd rect (at 0.254 -10.16 180) (size 2.286 1.9812) (layers F.Cu F.Mask)
      (net 75 MISO) (solder_mask_margin 0.0635))
    (pad 7 smd rect (at 0.254 -7.62 180) (size 2.286 1.9812) (layers F.Cu F.Mask)
      (net 165 PA19) (solder_mask_margin 0.0635))
    (pad 8 smd rect (at 0.254 -5.08 180) (size 2.286 1.9812) (layers F.Cu F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 9 smd rect (at 0.254 -2.54 180) (size 2.286 1.9812) (layers F.Cu F.Mask)
      (net 2 3.3V) (solder_mask_margin 0.0635))
  )
  (module custom-footprints:XTB28_MEZ (layer B.Cu) (tedit 5D2D1541)
    (at 129.25946 64.7573)
    (fp_text reference U11 (at 3.302 27.178) (layer B.SilkS) hide)
    (fp_text value XTB-40 (at 0 0) (layer B.SilkS) hide)
    (pad 10 smd rect (at 2.54 0 90) (size 2.286 1.9812) (layers B.Cu B.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 11 smd rect (at 5.08 0 90) (size 2.286 1.9812) (layers B.Cu B.Mask)
      (net 2 3.3V) (solder_mask_margin 0.0635))
    (pad 12 smd rect (at 7.62 0 90) (size 2.286 1.9812) (layers B.Cu B.Mask)
      (solder_mask_margin 0.0635))
    (pad 13 smd rect (at 10.16 0 90) (size 2.286 1.9812) (layers B.Cu B.Mask)
      (solder_mask_margin 0.0635))
    (pad 14 smd rect (at 12.7 0 90) (size 2.286 1.9812) (layers B.Cu B.Mask)
      (solder_mask_margin 0.0635))
    (pad 15 smd rect (at 14.986 2.54) (size 2.286 1.9812) (layers B.Cu B.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 16 smd rect (at 14.986 5.08) (size 2.286 1.9812) (layers B.Cu B.Mask)
      (net 2 3.3V) (solder_mask_margin 0.0635))
    (pad 17 smd rect (at 14.986 7.62) (size 2.286 1.9812) (layers B.Cu B.Mask)
      (net 128 "Net-(U11-Pad17)") (solder_mask_margin 0.0635))
    (pad 18 smd rect (at 14.986 10.16) (size 2.286 1.9812) (layers B.Cu B.Mask)
      (net 129 "Net-(U11-Pad18)") (solder_mask_margin 0.0635))
    (pad 19 smd rect (at 14.986 12.7) (size 2.286 1.9812) (layers B.Cu B.Mask)
      (net 130 "Net-(U11-Pad19)") (solder_mask_margin 0.0635))
    (pad 20 smd rect (at 14.986 15.24) (size 2.286 1.9812) (layers B.Cu B.Mask)
      (net 131 "Net-(U11-Pad20)") (solder_mask_margin 0.0635))
    (pad 21 smd rect (at 14.986 17.78) (size 2.286 1.9812) (layers B.Cu B.Mask)
      (net 132 "Net-(U11-Pad21)") (solder_mask_margin 0.0635))
    (pad 22 smd rect (at 14.986 20.32) (size 2.286 1.9812) (layers B.Cu B.Mask)
      (net 133 "Net-(U11-Pad22)") (solder_mask_margin 0.0635))
    (pad 23 smd rect (at 14.986 22.86) (size 2.286 1.9812) (layers B.Cu B.Mask)
      (net 134 "Net-(U11-Pad23)") (solder_mask_margin 0.0635))
    (pad 1 smd rect (at 0.254 22.86) (size 2.286 1.9812) (layers B.Cu B.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 2 smd rect (at 0.254 20.32) (size 2.286 1.9812) (layers B.Cu B.Mask)
      (net 135 "Net-(U11-Pad2)") (solder_mask_margin 0.0635))
    (pad 3 smd rect (at 0.254 17.78) (size 2.286 1.9812) (layers B.Cu B.Mask)
      (net 162 PB22) (solder_mask_margin 0.0635))
    (pad 4 smd rect (at 0.254 15.24) (size 2.286 1.9812) (layers B.Cu B.Mask)
      (net 77 MOSI) (solder_mask_margin 0.0635))
    (pad 5 smd rect (at 0.254 12.7) (size 2.286 1.9812) (layers B.Cu B.Mask)
      (net 76 SCK) (solder_mask_margin 0.0635))
    (pad 6 smd rect (at 0.254 10.16) (size 2.286 1.9812) (layers B.Cu B.Mask)
      (net 75 MISO) (solder_mask_margin 0.0635))
    (pad 7 smd rect (at 0.254 7.62) (size 2.286 1.9812) (layers B.Cu B.Mask)
      (net 160 PA22) (solder_mask_margin 0.0635))
    (pad 8 smd rect (at 0.254 5.08) (size 2.286 1.9812) (layers B.Cu B.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 9 smd rect (at 0.254 2.54) (size 2.286 1.9812) (layers B.Cu B.Mask)
      (net 2 3.3V) (solder_mask_margin 0.0635))
  )
  (module custom-footprints:XTB28_MEZ (layer B.Cu) (tedit 5D2D1541)
    (at 108.96346 64.7573)
    (fp_text reference U9 (at 3.302 27.178) (layer B.SilkS) hide)
    (fp_text value XTB-40 (at 0 0) (layer B.SilkS) hide)
    (pad 10 smd rect (at 2.54 0 90) (size 2.286 1.9812) (layers B.Cu B.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 11 smd rect (at 5.08 0 90) (size 2.286 1.9812) (layers B.Cu B.Mask)
      (net 2 3.3V) (solder_mask_margin 0.0635))
    (pad 12 smd rect (at 7.62 0 90) (size 2.286 1.9812) (layers B.Cu B.Mask)
      (solder_mask_margin 0.0635))
    (pad 13 smd rect (at 10.16 0 90) (size 2.286 1.9812) (layers B.Cu B.Mask)
      (solder_mask_margin 0.0635))
    (pad 14 smd rect (at 12.7 0 90) (size 2.286 1.9812) (layers B.Cu B.Mask)
      (solder_mask_margin 0.0635))
    (pad 15 smd rect (at 14.986 2.54) (size 2.286 1.9812) (layers B.Cu B.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 16 smd rect (at 14.986 5.08) (size 2.286 1.9812) (layers B.Cu B.Mask)
      (net 2 3.3V) (solder_mask_margin 0.0635))
    (pad 17 smd rect (at 14.986 7.62) (size 2.286 1.9812) (layers B.Cu B.Mask)
      (net 112 "Net-(U9-Pad17)") (solder_mask_margin 0.0635))
    (pad 18 smd rect (at 14.986 10.16) (size 2.286 1.9812) (layers B.Cu B.Mask)
      (net 113 "Net-(U9-Pad18)") (solder_mask_margin 0.0635))
    (pad 19 smd rect (at 14.986 12.7) (size 2.286 1.9812) (layers B.Cu B.Mask)
      (net 114 "Net-(U9-Pad19)") (solder_mask_margin 0.0635))
    (pad 20 smd rect (at 14.986 15.24) (size 2.286 1.9812) (layers B.Cu B.Mask)
      (net 115 "Net-(U9-Pad20)") (solder_mask_margin 0.0635))
    (pad 21 smd rect (at 14.986 17.78) (size 2.286 1.9812) (layers B.Cu B.Mask)
      (net 116 "Net-(U9-Pad21)") (solder_mask_margin 0.0635))
    (pad 22 smd rect (at 14.986 20.32) (size 2.286 1.9812) (layers B.Cu B.Mask)
      (net 117 "Net-(U9-Pad22)") (solder_mask_margin 0.0635))
    (pad 23 smd rect (at 14.986 22.86) (size 2.286 1.9812) (layers B.Cu B.Mask)
      (net 118 "Net-(U9-Pad23)") (solder_mask_margin 0.0635))
    (pad 1 smd rect (at 0.254 22.86) (size 2.286 1.9812) (layers B.Cu B.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 2 smd rect (at 0.254 20.32) (size 2.286 1.9812) (layers B.Cu B.Mask)
      (net 119 "Net-(U9-Pad2)") (solder_mask_margin 0.0635))
    (pad 3 smd rect (at 0.254 17.78) (size 2.286 1.9812) (layers B.Cu B.Mask)
      (net 163 PB23) (solder_mask_margin 0.0635))
    (pad 4 smd rect (at 0.254 15.24) (size 2.286 1.9812) (layers B.Cu B.Mask)
      (net 77 MOSI) (solder_mask_margin 0.0635))
    (pad 5 smd rect (at 0.254 12.7) (size 2.286 1.9812) (layers B.Cu B.Mask)
      (net 76 SCK) (solder_mask_margin 0.0635))
    (pad 6 smd rect (at 0.254 10.16) (size 2.286 1.9812) (layers B.Cu B.Mask)
      (net 75 MISO) (solder_mask_margin 0.0635))
    (pad 7 smd rect (at 0.254 7.62) (size 2.286 1.9812) (layers B.Cu B.Mask)
      (net 161 PA20) (solder_mask_margin 0.0635))
    (pad 8 smd rect (at 0.254 5.08) (size 2.286 1.9812) (layers B.Cu B.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 9 smd rect (at 0.254 2.54) (size 2.286 1.9812) (layers B.Cu B.Mask)
      (net 2 3.3V) (solder_mask_margin 0.0635))
  )
  (module custom-footprints:XTB28_MEZ (layer F.Cu) (tedit 5D2D1541)
    (at 124.20346 64.7573 180)
    (fp_text reference U10 (at 3.302 -27.178 180) (layer F.SilkS) hide)
    (fp_text value XTB-40 (at 0 0 180) (layer F.SilkS) hide)
    (pad 10 smd rect (at 2.54 0 90) (size 2.286 1.9812) (layers F.Cu F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 11 smd rect (at 5.08 0 90) (size 2.286 1.9812) (layers F.Cu F.Mask)
      (net 2 3.3V) (solder_mask_margin 0.0635))
    (pad 12 smd rect (at 7.62 0 90) (size 2.286 1.9812) (layers F.Cu F.Mask)
      (solder_mask_margin 0.0635))
    (pad 13 smd rect (at 10.16 0 90) (size 2.286 1.9812) (layers F.Cu F.Mask)
      (solder_mask_margin 0.0635))
    (pad 14 smd rect (at 12.7 0 90) (size 2.286 1.9812) (layers F.Cu F.Mask)
      (solder_mask_margin 0.0635))
    (pad 15 smd rect (at 14.986 -2.54 180) (size 2.286 1.9812) (layers F.Cu F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 16 smd rect (at 14.986 -5.08 180) (size 2.286 1.9812) (layers F.Cu F.Mask)
      (net 2 3.3V) (solder_mask_margin 0.0635))
    (pad 17 smd rect (at 14.986 -7.62 180) (size 2.286 1.9812) (layers F.Cu F.Mask)
      (net 120 "Net-(U10-Pad17)") (solder_mask_margin 0.0635))
    (pad 18 smd rect (at 14.986 -10.16 180) (size 2.286 1.9812) (layers F.Cu F.Mask)
      (net 121 "Net-(U10-Pad18)") (solder_mask_margin 0.0635))
    (pad 19 smd rect (at 14.986 -12.7 180) (size 2.286 1.9812) (layers F.Cu F.Mask)
      (net 122 "Net-(U10-Pad19)") (solder_mask_margin 0.0635))
    (pad 20 smd rect (at 14.986 -15.24 180) (size 2.286 1.9812) (layers F.Cu F.Mask)
      (net 123 "Net-(U10-Pad20)") (solder_mask_margin 0.0635))
    (pad 21 smd rect (at 14.986 -17.78 180) (size 2.286 1.9812) (layers F.Cu F.Mask)
      (net 124 "Net-(U10-Pad21)") (solder_mask_margin 0.0635))
    (pad 22 smd rect (at 14.986 -20.32 180) (size 2.286 1.9812) (layers F.Cu F.Mask)
      (net 125 "Net-(U10-Pad22)") (solder_mask_margin 0.0635))
    (pad 23 smd rect (at 14.986 -22.86 180) (size 2.286 1.9812) (layers F.Cu F.Mask)
      (net 126 "Net-(U10-Pad23)") (solder_mask_margin 0.0635))
    (pad 1 smd rect (at 0.254 -22.86 180) (size 2.286 1.9812) (layers F.Cu F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 2 smd rect (at 0.254 -20.32 180) (size 2.286 1.9812) (layers F.Cu F.Mask)
      (net 127 "Net-(U10-Pad2)") (solder_mask_margin 0.0635))
    (pad 3 smd rect (at 0.254 -17.78 180) (size 2.286 1.9812) (layers F.Cu F.Mask)
      (net 159 PB17) (solder_mask_margin 0.0635))
    (pad 4 smd rect (at 0.254 -15.24 180) (size 2.286 1.9812) (layers F.Cu F.Mask)
      (net 77 MOSI) (solder_mask_margin 0.0635))
    (pad 5 smd rect (at 0.254 -12.7 180) (size 2.286 1.9812) (layers F.Cu F.Mask)
      (net 76 SCK) (solder_mask_margin 0.0635))
    (pad 6 smd rect (at 0.254 -10.16 180) (size 2.286 1.9812) (layers F.Cu F.Mask)
      (net 75 MISO) (solder_mask_margin 0.0635))
    (pad 7 smd rect (at 0.254 -7.62 180) (size 2.286 1.9812) (layers F.Cu F.Mask)
      (net 164 PA18) (solder_mask_margin 0.0635))
    (pad 8 smd rect (at 0.254 -5.08 180) (size 2.286 1.9812) (layers F.Cu F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 9 smd rect (at 0.254 -2.54 180) (size 2.286 1.9812) (layers F.Cu F.Mask)
      (net 2 3.3V) (solder_mask_margin 0.0635))
  )
  (module LOGO (layer B.Cu) (tedit 0)
    (at 153.162 120.396 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 5D2D02B8)
    (at 116.586 139.954 270)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J11 (at 0 -2.33 270) (layer F.SilkS) hide)
    (fp_text value Conn_01x02 (at 0 4.87 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 2.54 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 169 "Net-(J11-Pad1)") (solder_mask_margin 0.0635))
  )
  (module custom-footprints:RFM98PW (layer F.Cu) (tedit 5D2CFC05)
    (at 121.1291 120.444096 270)
    (fp_text reference U23 (at 1.016 -2.667 270) (layer F.SilkS) hide)
    (fp_text value RFM98PW (at 4.191 2.286 270) (layer F.SilkS) hide)
    (fp_text user RADIO (at 3.13182 -0.84582 270) (layer F.SilkS))
    (pad 8 smd rect (at 16.9 -6.5 270) (size 2 1.3) (layers F.Cu F.Paste F.Mask)
      (net 151 RF_IO2) (solder_mask_margin 0.0635))
    (pad 7 smd rect (at 16.9 -4.5 270) (size 2 1.3) (layers F.Cu F.Paste F.Mask)
      (net 170 RF_IO1) (solder_mask_margin 0.0635))
    (pad 6 smd rect (at 16.9 -2.5 270) (size 2 1.3) (layers F.Cu F.Paste F.Mask)
      (net 176 RF_IO0) (solder_mask_margin 0.0635))
    (pad 5 smd rect (at 16.9 -0.5 270) (size 2 1.3) (layers F.Cu F.Paste F.Mask)
      (net 169 "Net-(J11-Pad1)") (solder_mask_margin 0.0635))
    (pad 4 smd rect (at 16.9 1.5 270) (size 2 1.3) (layers F.Cu F.Paste F.Mask)
      (net 171 "Net-(U23-Pad4)") (solder_mask_margin 0.0635))
    (pad 3 smd rect (at 16.9 3.5 270) (size 2 1.3) (layers F.Cu F.Paste F.Mask)
      (net 172 "Net-(U23-Pad3)") (solder_mask_margin 0.0635))
    (pad 2 smd rect (at 16.9 5.5 270) (size 2 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at 16.9 7.5 270) (size 2 1.3) (layers F.Cu F.Paste F.Mask)
      (net 87 "Net-(J7-Pad1)") (solder_mask_margin 0.0635))
    (pad 9 smd rect (at -15.9 -6.5 270) (size 2 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 3.3V) (solder_mask_margin 0.0635))
    (pad 10 smd rect (at -15.9 -4.5 270) (size 2 1.3) (layers F.Cu F.Paste F.Mask)
      (net 75 MISO) (solder_mask_margin 0.0635))
    (pad 11 smd rect (at -15.9 -2.5 270) (size 2 1.3) (layers F.Cu F.Paste F.Mask)
      (net 77 MOSI) (solder_mask_margin 0.0635))
    (pad 12 smd rect (at -15.9 -0.5 270) (size 2 1.3) (layers F.Cu F.Paste F.Mask)
      (net 76 SCK) (solder_mask_margin 0.0635))
    (pad 13 smd rect (at -15.9 1.5 270) (size 2 1.3) (layers F.Cu F.Paste F.Mask)
      (net 173 CS_RF) (solder_mask_margin 0.0635))
    (pad 14 smd rect (at -15.9 3.5 270) (size 2 1.3) (layers F.Cu F.Paste F.Mask)
      (net 174 RF_RST) (solder_mask_margin 0.0635))
    (pad 15 smd rect (at -15.9 5.5 270) (size 2 1.3) (layers F.Cu F.Paste F.Mask)
      (net 175 RF_IO5) (solder_mask_margin 0.0635))
    (pad 16 smd rect (at -15.9 7.5 270) (size 2 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 120.523 142.113 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R48 (at -3.175 0 90) (layer F.SilkS))
    (fp_text value 0 (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 169 "Net-(J11-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 3.3V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LOGO (layer F.Cu) (tedit 0)
    (at 148.59 127.127)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 133.35 122.555 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R47 (at 0 1.43 270) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.43 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 167 "Net-(R24-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 168 "Net-(R46-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 133.35 120.9802 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R46 (at 0 1.43 270) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.43 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 168 "Net-(R46-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 5D2CDB8C)
    (at 149.098 114.173 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J10 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x03 (at 0 7.41 90) (layer F.Fab))
    (fp_text user %R (at 0 2.54 180) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 157 PB14))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 156 PB15))
    (pad 1 thru_hole oval (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 69 DAC0))
  )
  (module LED_SMD:LED_0603_1608Metric (layer F.Cu) (tedit 5D2CD6B2)
    (at 139.319 56.6165 270)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D1 (at 3.0735 0.127 270) (layer F.SilkS))
    (fp_text value "GREEN LED" (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 92 "Net-(D1-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_3.2mm_M3_DIN965_Pad locked (layer F.Cu) (tedit 56D1B4CB)
    (at 180.8861 57.5691)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (attr virtual)
    (fp_text reference H4 (at 0 -3.8) (layer F.SilkS) hide)
    (fp_text value MountingHole_Pad (at 0 3.8) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 3.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module MountingHole:MountingHole_3.2mm_M3_DIN965_Pad locked (layer F.Cu) (tedit 56D1B4CB)
    (at 183.4261 143.2941)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (attr virtual)
    (fp_text reference H3 (at 0 -3.8) (layer F.SilkS) hide)
    (fp_text value MountingHole_Pad (at 0 3.8) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 3.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module MountingHole:MountingHole_3.2mm_M3_DIN965_Pad locked (layer F.Cu) (tedit 56D1B4CB)
    (at 103.4261 143.2941)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (attr virtual)
    (fp_text reference H2 (at 0 -3.8) (layer F.SilkS) hide)
    (fp_text value MountingHole_Pad (at 0 3.8) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 3.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module MountingHole:MountingHole_3.2mm_M3_ISO7380_Pad locked (layer F.Cu) (tedit 5D2CD479)
    (at 107.2261 57.5691)
    (descr "Mounting Hole 3.2mm, M3, ISO7380")
    (tags "mounting hole 3.2mm m3 iso7380")
    (attr virtual)
    (fp_text reference H1 (at 0 -3.85) (layer F.SilkS) hide)
    (fp_text value MountingHole_Pad (at 0 3.85) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 3.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x09_P2.54mm_Vertical (layer F.Cu) (tedit 5D2CD2C0)
    (at 115.697 91.948 90)
    (descr "Through hole straight pin header, 1x09, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x09 2.54mm single row")
    (fp_text reference J8 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x09 (at 0 22.65 90) (layer F.Fab))
    (fp_text user %R (at 0 10.16 180) (layer F.Fab))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 160 PA22))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 161 PA20))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 162 PB22))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 163 PB23))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 75 MISO))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 77 MOSI))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 76 SCK))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole oval (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 3.3V))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical (layer F.Cu) (tedit 5D2CD2A9)
    (at 146.558 91.948 90)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (fp_text reference J9 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x05 (at 0 12.49 90) (layer F.Fab))
    (fp_text user %R (at 0 5.08 180) (layer F.Fab))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 158 PA16))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 164 PA18))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 165 PA19))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 166 PB16))
    (pad 1 thru_hole oval (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 159 PB17))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical (layer F.Cu) (tedit 5D2CCCAA)
    (at 132.3848 105.8164)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (fp_text reference J2 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value Conn_01x05 (at 0 12.49) (layer F.Fab))
    (fp_text user %R (at 0 5.08 90) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 3.3V))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 SWDIO))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 SWCLK))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 ~RESET))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module ATSAMD51J20A-AU:QFP50P1200X1200X120-64N (layer F.Cu) (tedit 0)
    (at 146.05 104.521 90)
    (attr smd)
    (fp_text reference U2 (at 5.969 5.588 180) (layer F.SilkS))
    (fp_text value ATSAMD51J20A-AU (at -4.7226 7.35076 90) (layer F.SilkS) hide)
    (pad 64 smd rect (at -3.75 -5.67 270) (size 0.28 1.47) (layers F.Cu F.Paste F.Mask)
      (net 154 RX))
    (pad 63 smd rect (at -3.25 -5.67 270) (size 0.28 1.47) (layers F.Cu F.Paste F.Mask)
      (net 155 TX))
    (pad 62 smd rect (at -2.75 -5.67 270) (size 0.28 1.47) (layers F.Cu F.Paste F.Mask)
      (net 8 ENAB_GPS))
    (pad 61 smd rect (at -2.25 -5.67 270) (size 0.28 1.47) (layers F.Cu F.Paste F.Mask)
      (net 174 RF_RST))
    (pad 60 smd rect (at -1.75 -5.67 270) (size 0.28 1.47) (layers F.Cu F.Paste F.Mask)
      (net 7 ENAB_BURN1))
    (pad 59 smd rect (at -1.25 -5.67 270) (size 0.28 1.47) (layers F.Cu F.Paste F.Mask)
      (net 173 CS_RF))
    (pad 58 smd rect (at -0.75 -5.67 270) (size 0.28 1.47) (layers F.Cu F.Paste F.Mask)
      (net 10 SWDIO))
    (pad 57 smd rect (at -0.25 -5.67 270) (size 0.28 1.47) (layers F.Cu F.Paste F.Mask)
      (net 9 SWCLK))
    (pad 56 smd rect (at 0.25 -5.67 270) (size 0.28 1.47) (layers F.Cu F.Paste F.Mask)
      (net 2 3.3V))
    (pad 55 smd rect (at 0.75 -5.67 270) (size 0.28 1.47) (layers F.Cu F.Paste F.Mask)
      (net 101 "Net-(L1-Pad2)"))
    (pad 54 smd rect (at 1.25 -5.67 270) (size 0.28 1.47) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 53 smd rect (at 1.75 -5.67 270) (size 0.28 1.47) (layers F.Cu F.Paste F.Mask)
      (net 89 "Net-(C12-Pad2)"))
    (pad 52 smd rect (at 2.25 -5.67 270) (size 0.28 1.47) (layers F.Cu F.Paste F.Mask)
      (net 11 ~RESET))
    (pad 51 smd rect (at 2.75 -5.67 270) (size 0.28 1.47) (layers F.Cu F.Paste F.Mask)
      (net 84 xSDCS))
    (pad 50 smd rect (at 3.25 -5.67 270) (size 0.28 1.47) (layers F.Cu F.Paste F.Mask)
      (net 163 PB23))
    (pad 49 smd rect (at 3.75 -5.67 270) (size 0.28 1.47) (layers F.Cu F.Paste F.Mask)
      (net 162 PB22))
    (pad 48 smd rect (at 5.67 -3.75 180) (size 0.28 1.47) (layers F.Cu F.Paste F.Mask)
      (net 2 3.3V))
    (pad 47 smd rect (at 5.67 -3.25 180) (size 0.28 1.47) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 46 smd rect (at 5.67 -2.75 180) (size 0.28 1.47) (layers F.Cu F.Paste F.Mask)
      (net 15 USB_D+))
    (pad 45 smd rect (at 5.67 -2.25 180) (size 0.28 1.47) (layers F.Cu F.Paste F.Mask)
      (net 16 USB_D-))
    (pad 44 smd rect (at 5.67 -1.75 180) (size 0.28 1.47) (layers F.Cu F.Paste F.Mask)
      (net 149 WDT_WDI))
    (pad 43 smd rect (at 5.67 -1.25 180) (size 0.28 1.47) (layers F.Cu F.Paste F.Mask)
      (net 160 PA22))
    (pad 42 smd rect (at 5.67 -0.75 180) (size 0.28 1.47) (layers F.Cu F.Paste F.Mask)
      (net 106 "Net-(R5-Pad2)"))
    (pad 41 smd rect (at 5.67 -0.25 180) (size 0.28 1.47) (layers F.Cu F.Paste F.Mask)
      (net 161 PA20))
    (pad 40 smd rect (at 5.67 0.25 180) (size 0.28 1.47) (layers F.Cu F.Paste F.Mask)
      (net 159 PB17))
    (pad 39 smd rect (at 5.67 0.75 180) (size 0.28 1.47) (layers F.Cu F.Paste F.Mask)
      (net 166 PB16))
    (pad 38 smd rect (at 5.67 1.25 180) (size 0.28 1.47) (layers F.Cu F.Paste F.Mask)
      (net 165 PA19))
    (pad 37 smd rect (at 5.67 1.75 180) (size 0.28 1.47) (layers F.Cu F.Paste F.Mask)
      (net 164 PA18))
    (pad 36 smd rect (at 5.67 2.25 180) (size 0.28 1.47) (layers F.Cu F.Paste F.Mask)
      (net 19 BURN_RELAY_A))
    (pad 35 smd rect (at 5.67 2.75 180) (size 0.28 1.47) (layers F.Cu F.Paste F.Mask)
      (net 158 PA16))
    (pad 34 smd rect (at 5.67 3.25 180) (size 0.28 1.47) (layers F.Cu F.Paste F.Mask)
      (net 2 3.3V))
    (pad 33 smd rect (at 5.67 3.75 180) (size 0.28 1.47) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 32 smd rect (at 3.75 5.67 270) (size 0.28 1.47) (layers F.Cu F.Paste F.Mask)
      (net 6 ENAB_BURN2))
    (pad 31 smd rect (at 3.25 5.67 270) (size 0.28 1.47) (layers F.Cu F.Paste F.Mask)
      (net 75 MISO))
    (pad 30 smd rect (at 2.75 5.67 270) (size 0.28 1.47) (layers F.Cu F.Paste F.Mask)
      (net 76 SCK))
    (pad 29 smd rect (at 2.25 5.67 270) (size 0.28 1.47) (layers F.Cu F.Paste F.Mask)
      (net 77 MOSI))
    (pad 28 smd rect (at 1.75 5.67 270) (size 0.28 1.47) (layers F.Cu F.Paste F.Mask)
      (net 156 PB15))
    (pad 27 smd rect (at 1.25 5.67 270) (size 0.28 1.47) (layers F.Cu F.Paste F.Mask)
      (net 157 PB14))
    (pad 26 smd rect (at 0.75 5.67 270) (size 0.28 1.47) (layers F.Cu F.Paste F.Mask)
      (net 153 /Avionics/SCL))
    (pad 25 smd rect (at 0.25 5.67 270) (size 0.28 1.47) (layers F.Cu F.Paste F.Mask)
      (net 152 /Avionics/SDA))
    (pad 24 smd rect (at -0.25 5.67 270) (size 0.28 1.47) (layers F.Cu F.Paste F.Mask)
      (net 78 FLASH_CS))
    (pad 23 smd rect (at -0.75 5.67 270) (size 0.28 1.47) (layers F.Cu F.Paste F.Mask)
      (net 79 FLASH_SCK))
    (pad 22 smd rect (at -1.25 5.67 270) (size 0.28 1.47) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 21 smd rect (at -1.75 5.67 270) (size 0.28 1.47) (layers F.Cu F.Paste F.Mask)
      (net 2 3.3V))
    (pad 20 smd rect (at -2.25 5.67 270) (size 0.28 1.47) (layers F.Cu F.Paste F.Mask)
      (net 80 FLASH_IO3))
    (pad 19 smd rect (at -2.75 5.67 270) (size 0.28 1.47) (layers F.Cu F.Paste F.Mask)
      (net 81 FLASH_IO2))
    (pad 18 smd rect (at -3.25 5.67 270) (size 0.28 1.47) (layers F.Cu F.Paste F.Mask)
      (net 82 FLASH_MISO))
    (pad 17 smd rect (at -3.75 5.67 270) (size 0.28 1.47) (layers F.Cu F.Paste F.Mask)
      (net 83 FLASH_MOSI))
    (pad 16 smd rect (at -5.67 3.75 180) (size 0.28 1.47) (layers F.Cu F.Paste F.Mask)
      (net 107 "Net-(R6-Pad2)"))
    (pad 15 smd rect (at -5.67 3.25 180) (size 0.28 1.47) (layers F.Cu F.Paste F.Mask)
      (net 74 /Avionics/BATTERY))
    (pad 14 smd rect (at -5.67 2.75 180) (size 0.28 1.47) (layers F.Cu F.Paste F.Mask)
      (net 18 BURN_RELAY_B))
    (pad 13 smd rect (at -5.67 2.25 180) (size 0.28 1.47) (layers F.Cu F.Paste F.Mask)
      (net 3 I_BATT))
    (pad 12 smd rect (at -5.67 1.75 180) (size 0.28 1.47) (layers F.Cu F.Paste F.Mask)
      (net 4 ENAB_BURN4))
    (pad 11 smd rect (at -5.67 1.25 180) (size 0.28 1.47) (layers F.Cu F.Paste F.Mask)
      (net 150 ~CHRG))
    (pad 10 smd rect (at -5.67 0.75 180) (size 0.28 1.47) (layers F.Cu F.Paste F.Mask)
      (net 5 ENAB_BURN3))
    (pad 9 smd rect (at -5.67 0.25 180) (size 0.28 1.47) (layers F.Cu F.Paste F.Mask)
      (net 170 RF_IO1))
    (pad 8 smd rect (at -5.67 -0.25 180) (size 0.28 1.47) (layers F.Cu F.Paste F.Mask)
      (net 2 3.3V))
    (pad 7 smd rect (at -5.67 -0.75 180) (size 0.28 1.47) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -5.67 -1.25 180) (size 0.28 1.47) (layers F.Cu F.Paste F.Mask)
      (net 176 RF_IO0))
    (pad 5 smd rect (at -5.67 -1.75 180) (size 0.28 1.47) (layers F.Cu F.Paste F.Mask)
      (net 20 ENAB_BURN5))
    (pad 4 smd rect (at -5.67 -2.25 180) (size 0.28 1.47) (layers F.Cu F.Paste F.Mask)
      (net 2 3.3V))
    (pad 3 smd rect (at -5.67 -2.75 180) (size 0.28 1.47) (layers F.Cu F.Paste F.Mask)
      (net 69 DAC0))
    (pad 2 smd rect (at -5.67 -3.25 180) (size 0.28 1.47) (layers F.Cu F.Paste F.Mask)
      (net 68 /Avionics/XTAL2))
    (pad 1 smd rect (at -5.67 -3.75 180) (size 0.28 1.47) (layers F.Cu F.Paste F.Mask)
      (net 67 /Avionics/XTAL1))
    (model ${KISYS3DMOD}/Package_QFP.3dshapes/HTQFP-64-1EP_10x10mm_P0.5mm_EP8x8mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SO-8_3.9x4.9mm_P1.27mm (layer B.Cu) (tedit 5C509AD1)
    (at 136.906 96.012)
    (descr "SO, 8 Pin (https://www.nxp.com/docs/en/data-sheet/PCF8523.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SO SO")
    (attr smd)
    (fp_text reference U1 (at 1.651 -3.556) (layer B.SilkS))
    (fp_text value MAX706RS-T (at 0 -3.4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 8 smd roundrect (at 2.575 1.905) (size 1.75 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 11 ~RESET))
    (pad 7 smd roundrect (at 2.575 0.635) (size 1.75 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 11 ~RESET))
    (pad 6 smd roundrect (at 2.575 -0.635) (size 1.75 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 149 WDT_WDI))
    (pad 5 smd roundrect (at 2.575 -1.905) (size 1.75 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 27 "Net-(U1-Pad5)"))
    (pad 4 smd roundrect (at -2.575 -1.905) (size 1.75 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 3 smd roundrect (at -2.575 -0.635) (size 1.75 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at -2.575 0.635) (size 1.75 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 148 "Net-(R42-Pad2)"))
    (pad 1 smd roundrect (at -2.575 1.905) (size 1.75 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 148 "Net-(R42-Pad2)"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/TI_SO-PowerPAD-8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-footprints:QFN-16-PAD (layer F.Cu) (tedit 0)
    (at 171.0161 100.296496 180)
    (fp_text reference U6 (at -0.9419 -3.081504) (layer F.SilkS))
    (fp_text value LTC4121 (at 0 0 180) (layer F.SilkS) hide)
    (pad P$16 smd rect (at -0.75 -1.3) (size 0.25 0.7) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(R10-Pad1)") (solder_mask_margin 0.0635))
    (pad P$15 smd rect (at -0.25 -1.3) (size 0.25 0.7) (layers F.Cu F.Paste F.Mask)
      (net 111 "Net-(R18-Pad1)") (solder_mask_margin 0.0635))
    (pad P$14 smd rect (at 0.25 -1.3) (size 0.25 0.7) (layers F.Cu F.Paste F.Mask)
      (net 150 ~CHRG) (solder_mask_margin 0.0635))
    (pad P$13 smd rect (at 0.75 -1.3) (size 0.25 0.7) (layers F.Cu F.Paste F.Mask)
      (net 13 L1_PROG) (solder_mask_margin 0.0635))
    (pad P$12 smd rect (at 1.3 -0.75 90) (size 0.25 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad P$11 smd rect (at 1.3 -0.25 90) (size 0.25 0.7) (layers F.Cu F.Paste F.Mask)
      (net 109 "Net-(R16-Pad1)") (solder_mask_margin 0.0635))
    (pad P$9 smd rect (at 1.3 0.75 90) (size 0.25 0.7) (layers F.Cu F.Paste F.Mask)
      (net 14 VBATT) (solder_mask_margin 0.0635))
    (pad P$10 smd rect (at 1.3 0.25 90) (size 0.25 0.7) (layers F.Cu F.Paste F.Mask)
      (net 110 "Net-(R16-Pad2)") (solder_mask_margin 0.0635))
    (pad P$8 smd rect (at 0.75 1.3 180) (size 0.25 0.7) (layers F.Cu F.Paste F.Mask)
      (net 147 "Net-(L3-Pad1)") (solder_mask_margin 0.0635))
    (pad P$7 smd rect (at 0.25 1.3 180) (size 0.25 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad P$6 smd rect (at -0.25 1.3 180) (size 0.25 0.7) (layers F.Cu F.Paste F.Mask)
      (net 108 "Net-(R11-Pad1)") (solder_mask_margin 0.0635))
    (pad P$5 smd rect (at -0.75 1.3 180) (size 0.25 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad P$4 smd rect (at -1.3 0.75 270) (size 0.25 0.7) (layers F.Cu F.Paste F.Mask)
      (net 146 "Net-(C25-Pad2)") (solder_mask_margin 0.0635))
    (pad P$3 smd rect (at -1.3 0.25 270) (size 0.25 0.7) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(C22-Pad1)") (solder_mask_margin 0.0635))
    (pad P$1 smd rect (at -1.3 -0.75 270) (size 0.25 0.7) (layers F.Cu F.Paste F.Mask)
      (net 145 "Net-(C23-Pad1)") (solder_mask_margin 0.0635))
    (pad P$2 smd rect (at -1.3 -0.25 270) (size 0.25 0.7) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(C25-Pad1)") (solder_mask_margin 0.0635))
    (pad P$17 smd rect (at 0 0 90) (size 1.45 1.45) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-16-1EP_3x3mm_P0.5mm_EP1.8x1.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 155.321 100.584)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R45 (at 2.794 0.094) (layer F.SilkS))
    (fp_text value 10K (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 153 /Avionics/SCL))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 3.3V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 155.321 102.489)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R44 (at 2.794 0.094) (layer F.SilkS))
    (fp_text value 10K (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 152 /Avionics/SDA))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 3.3V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 131.9276 99.568 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R43 (at 3.175 -0.0254 270) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.43 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 148 "Net-(R42-Pad2)"))
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 131.9276 97.9932 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R42 (at -3.6322 -0.0254 270) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.43 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 148 "Net-(R42-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 3.3V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 133.35 126.619 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R24 (at 0 -1.524 270) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.43 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 167 "Net-(R24-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 17 GPS_PWR_IN))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_1812_4532Metric (layer F.Cu) (tedit 5B301BBE)
    (at 154.94 87.63 270)
    (descr "Inductor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.nikhef.nl/pub/departments/mt/projects/detectorR_D/dtddice/ERJ2G.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L2 (at -0.127 2.54 270) (layer F.SilkS))
    (fp_text value 3.3uH (at 0 2.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 2.1375 0 270) (size 1.125 3.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.222222)
      (net 2 3.3V))
    (pad 1 smd roundrect (at -2.1375 0 270) (size 1.125 3.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.222222)
      (net 90 "Net-(C21-Pad1)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_1812_4532Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_1812_4532Metric (layer F.Cu) (tedit 5B301BBE)
    (at 171.196 96.012)
    (descr "Inductor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.nikhef.nl/pub/departments/mt/projects/detectorR_D/dtddice/ERJ2G.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L3 (at 0 -2.65) (layer F.SilkS))
    (fp_text value 56uH (at 0 2.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 2.1375 0) (size 1.125 3.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.222222)
      (net 146 "Net-(C25-Pad2)"))
    (pad 1 smd roundrect (at -2.1375 0) (size 1.125 3.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.222222)
      (net 147 "Net-(L3-Pad1)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_1812_4532Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 163.195 105.458096 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C30 (at 2.794 0 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 3.3V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 154.8892 135.636 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R36 (at 2.286 -1.8542 90) (layer F.SilkS))
    (fp_text value 4.7k (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 62 "Net-(Q8-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 ENAB_BURN5))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mainboard:MOLEX-1X3_LOCK (layer F.Cu) (tedit 0)
    (at 170.9341 143.884096)
    (fp_text reference JP14 (at 0 0) (layer F.SilkS) hide)
    (fp_text value M03POLAR_LOCK (at 0 0) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 -0.127) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 2 thru_hole circle (at 2.54 0.127) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 VSOLAR) (solder_mask_margin 0.0635))
    (pad 3 thru_hole circle (at 5.08 -0.127) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 60 "/Burn Wires/VBURN4") (solder_mask_margin 0.0635))
    (model ${KISYS3DMOD}/Connector.3dshapes/FanPinHeader_1x03_P2.54mm_Vertical.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mainboard:PWP14_2P31X2P46-L (layer F.Cu) (tedit 0)
    (at 156.8161 80.058096 270)
    (fp_text reference U5 (at -4.112096 -1.0449) (layer F.SilkS))
    (fp_text value TPS54226PWPRPWP14_2P31X2P46-L (at 0 0 270) (layer F.SilkS) hide)
    (fp_text user >Name (at -1.976118 3.8862 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.7686 -1.950034 270) (size 1.6002 0.3048) (layers F.Cu F.Paste F.Mask)
      (net 2 3.3V) (solder_mask_margin 0.0635))
    (pad 2 smd rect (at -2.7686 -1.300021 270) (size 1.6002 0.3048) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(R13-Pad1)") (solder_mask_margin 0.0635))
    (pad 3 smd rect (at -2.7686 -0.650012 270) (size 1.6002 0.3048) (layers F.Cu F.Paste F.Mask)
      (net 91 "Net-(C27-Pad1)") (solder_mask_margin 0.0635))
    (pad 4 smd rect (at -2.7686 0 270) (size 1.6002 0.3048) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(C26-Pad1)") (solder_mask_margin 0.0635))
    (pad 5 smd rect (at -2.7686 0.650012 270) (size 1.6002 0.3048) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 6 smd rect (at -2.7686 1.300021 270) (size 1.6002 0.3048) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(R15-Pad1)") (solder_mask_margin 0.0635))
    (pad 7 smd rect (at -2.7686 1.950034 270) (size 1.6002 0.3048) (layers F.Cu F.Paste F.Mask)
      (net 14 VBATT) (solder_mask_margin 0.0635))
    (pad 8 smd rect (at 2.7686 1.950034 270) (size 1.6002 0.3048) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 9 smd rect (at 2.7686 1.300021 270) (size 1.6002 0.3048) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 10 smd rect (at 2.7686 0.650012 270) (size 1.6002 0.3048) (layers F.Cu F.Paste F.Mask)
      (net 90 "Net-(C21-Pad1)") (solder_mask_margin 0.0635))
    (pad 11 smd rect (at 2.7686 0 270) (size 1.6002 0.3048) (layers F.Cu F.Paste F.Mask)
      (net 90 "Net-(C21-Pad1)") (solder_mask_margin 0.0635))
    (pad 12 smd rect (at 2.7686 -0.650012 270) (size 1.6002 0.3048) (layers F.Cu F.Paste F.Mask)
      (net 144 "Net-(C21-Pad2)") (solder_mask_margin 0.0635))
    (pad 13 smd rect (at 2.7686 -1.300021 270) (size 1.6002 0.3048) (layers F.Cu F.Paste F.Mask)
      (net 31 /Power/VREG_IN) (solder_mask_margin 0.0635))
    (pad 14 smd rect (at 2.7686 -1.950034 270) (size 1.6002 0.3048) (layers F.Cu F.Paste F.Mask)
      (net 31 /Power/VREG_IN) (solder_mask_margin 0.0635))
    (pad 15 smd rect (at 0 0 270) (size 2.31 2.46) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SSOP-14_5.3x6.2mm_P0.65mm.step
      (at (xyz 0 0 0))
      (scale (xyz 0.8 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 145.6055 109.982 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C10 (at 2.9845 0 180) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.43 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 3.3V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 155.321 98.552)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at 2.413 0.094) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 74 /Avionics/BATTERY))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-footprints:NDS8434 (layer F.Cu) (tedit 5CECB0CF)
    (at 123.825 143.891 180)
    (descr "<b>Small Outline Package</b> Fits JEDEC packages (narrow SOIC-8)")
    (attr smd)
    (fp_text reference U20 (at -0.127 4.572 180) (layer F.SilkS))
    (fp_text value NDS8434 (at -0.254493 0.432628 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.905 2.6162 180) (size 0.6096 2.2098) (layers F.Cu F.Paste F.Mask)
      (net 58 "/Burn Wires/VBURN_B_IN"))
    (pad 2 smd rect (at -0.635 2.6162 180) (size 0.6096 2.2098) (layers F.Cu F.Paste F.Mask)
      (net 58 "/Burn Wires/VBURN_B_IN"))
    (pad 3 smd rect (at 0.635 2.6162 180) (size 0.6096 2.2098) (layers F.Cu F.Paste F.Mask)
      (net 58 "/Burn Wires/VBURN_B_IN"))
    (pad 4 smd rect (at 1.905 2.6162 180) (size 0.6096 2.2098) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(Q6-Pad3)"))
    (pad 5 smd rect (at 1.905 -2.6162 180) (size 0.6096 2.2098) (layers F.Cu F.Paste F.Mask)
      (net 59 "/Burn Wires/VBURN3"))
    (pad 6 smd rect (at 0.635 -2.6162 180) (size 0.6096 2.2098) (layers F.Cu F.Paste F.Mask)
      (net 59 "/Burn Wires/VBURN3"))
    (pad 7 smd rect (at -0.635 -2.6162 180) (size 0.6096 2.2098) (layers F.Cu F.Paste F.Mask)
      (net 59 "/Burn Wires/VBURN3"))
    (pad 8 smd rect (at -1.905 -2.6162 180) (size 0.6096 2.2098) (layers F.Cu F.Paste F.Mask)
      (net 59 "/Burn Wires/VBURN3"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/HTSOP-8-1EP_3.9x4.9mm_P1.27mm_EP2.4x3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module custom-footprints:D_SOD-123 (layer F.Cu) (tedit 5D21238C)
    (at 149.606 62.357 90)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D3 (at 0 -2 90) (layer F.SilkS))
    (fp_text value MBR120 (at 0 2.1 90) (layer F.Fab))
    (fp_text user %R (at 0 -2 90) (layer F.Fab))
    (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 93 "Net-(D3-Pad2)"))
    (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 35 /Connectors/VBATT_IN))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Coaxial:SMA_Amphenol_901-144_Vertical (layer F.Cu) (tedit 5B2F4C32)
    (at 104.7461 135.684096)
    (descr https://www.amphenolrf.com/downloads/dl/file/id/7023/product/3103/901_144_customer_drawing.pdf)
    (tags "SMA THT Female Jack Vertical")
    (fp_text reference J7 (at 0 -4.75) (layer F.SilkS))
    (fp_text value Conn_Coaxial (at 0 5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.05 2.05) (drill 1.5) (layers *.Cu *.Mask)
      (net 87 "Net-(J7-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 2.54) (size 2.25 2.25) (drill 1.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.54 -2.54) (size 2.25 2.25) (drill 1.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at -2.54 -2.54) (size 2.25 2.25) (drill 1.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at -2.54 2.54) (size 2.25 2.25) (drill 1.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_Coaxial.3dshapes/SMA_Amphenol_901-144_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Coaxial:SMA_Amphenol_901-144_Vertical (layer F.Cu) (tedit 5B2F4C32)
    (at 104.7461 112.824096)
    (descr https://www.amphenolrf.com/downloads/dl/file/id/7023/product/3103/901_144_customer_drawing.pdf)
    (tags "SMA THT Female Jack Vertical")
    (fp_text reference J6 (at 0 -4.75) (layer F.SilkS))
    (fp_text value Conn_Coaxial (at 0 5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.05 2.05) (drill 1.5) (layers *.Cu *.Mask)
      (net 86 "Net-(J6-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 2.54) (size 2.25 2.25) (drill 1.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.54 -2.54) (size 2.25 2.25) (drill 1.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at -2.54 -2.54) (size 2.25 2.25) (drill 1.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at -2.54 2.54) (size 2.25 2.25) (drill 1.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_Coaxial.3dshapes/SMA_Amphenol_901-144_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Coaxial:SMA_Amphenol_901-144_Vertical (layer F.Cu) (tedit 5B2F4C32)
    (at 104.7461 124.254096)
    (descr https://www.amphenolrf.com/downloads/dl/file/id/7023/product/3103/901_144_customer_drawing.pdf)
    (tags "SMA THT Female Jack Vertical")
    (fp_text reference J5 (at 0 -4.75) (layer F.SilkS))
    (fp_text value Conn_Coaxial (at 0 5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.05 2.05) (drill 1.5) (layers *.Cu *.Mask)
      (net 85 "Net-(J5-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 2.54) (size 2.25 2.25) (drill 1.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.54 -2.54) (size 2.25 2.25) (drill 1.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at -2.54 -2.54) (size 2.25 2.25) (drill 1.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at -2.54 2.54) (size 2.25 2.25) (drill 1.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_Coaxial.3dshapes/SMA_Amphenol_901-144_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystal:Crystal_SMD_3215-2Pin_3.2x1.5mm (layer F.Cu) (tedit 5A0FD1B2)
    (at 142.494 113.284 180)
    (descr "SMD Crystal FC-135 https://support.epson.biz/td/api/doc_check.php?dl=brief_FC-135R_en.pdf")
    (tags "SMD SMT Crystal")
    (attr smd)
    (fp_text reference Y1 (at 0 1.524 180) (layer F.SilkS))
    (fp_text value 32.768kHz (at 0 2 180) (layer F.Fab))
    (fp_text user %R (at 0 -2 180) (layer F.Fab))
    (pad 1 smd rect (at 1.25 0 180) (size 1 1.8) (layers F.Cu F.Paste F.Mask)
      (net 67 /Avionics/XTAL1))
    (pad 2 smd rect (at -1.25 0 180) (size 1 1.8) (layers F.Cu F.Paste F.Mask)
      (net 68 /Avionics/XTAL2))
    (model ${KISYS3DMOD}/Crystal.3dshapes/Crystal_SMD_Abracon_ABM8G-4Pin_3.2x2.5mm.step
      (at (xyz 0 0 0))
      (scale (xyz 0.9 0.7 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 140.97 56.642 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R5 (at 3.048 0.127 270) (layer F.SilkS))
    (fp_text value 2.2K (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 92 "Net-(D1-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 106 "Net-(R5-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 136.398 109.601 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at -2.286 0) (layer F.SilkS))
    (fp_text value 10K (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 3.3V))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 SWCLK))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 136.906 100.33)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at -2.794 0) (layer F.SilkS))
    (fp_text value 10K (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 3.3V))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 ~RESET))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 155.321 98.552 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 0 1.43 180) (layer B.SilkS))
    (fp_text value 316K (at 0 -1.43 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 14 VBATT))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 74 /Avionics/BATTERY))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 155.321 100.584 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at 0 -1.524 180) (layer B.SilkS))
    (fp_text value 110K (at 0 -1.43 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 74 /Avionics/BATTERY))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 149.098 105.029 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C16 (at 0.127 -1.397 90) (layer B.SilkS))
    (fp_text value 10uF (at 0 -1.43 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 3.3V))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 136.906 104.14 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C14 (at 3.302 0.127 180) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 89 "Net-(C12-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 149.733 98.933)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C15 (at -2.794 0) (layer B.SilkS))
    (fp_text value 1uF (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 3.3V))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 136.906 102.616)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C12 (at -3.302 0.127) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 89 "Net-(C12-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 142.367 96.647)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C13 (at 2.921 0) (layer B.SilkS))
    (fp_text value 1uF (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 3.3V))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 151.892 105.029 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C11 (at -2.794 0 90) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.43 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 3.3V))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 136.906 100.33)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C4 (at -2.413 0) (layer B.SilkS))
    (fp_text value 1uF (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 11 ~RESET))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 144.526 115.189)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at 0.762 -1.524 90) (layer F.SilkS))
    (fp_text value 22pF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 68 /Avionics/XTAL2))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 140.462 115.189 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at 0.635 1.524 270) (layer F.SilkS))
    (fp_text value 22pF (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 67 /Avionics/XTAL1))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-footprints:NDS8434 (layer F.Cu) (tedit 5CECB0CF)
    (at 161.6964 138.2268 270)
    (descr "<b>Small Outline Package</b> Fits JEDEC packages (narrow SOIC-8)")
    (attr smd)
    (fp_text reference U22 (at -0.457406 -0.203291 270) (layer F.SilkS))
    (fp_text value NDS8434 (at -0.254493 0.432628 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.905 2.6162 270) (size 0.6096 2.2098) (layers F.Cu F.Paste F.Mask)
      (net 58 "/Burn Wires/VBURN_B_IN"))
    (pad 2 smd rect (at -0.635 2.6162 270) (size 0.6096 2.2098) (layers F.Cu F.Paste F.Mask)
      (net 58 "/Burn Wires/VBURN_B_IN"))
    (pad 3 smd rect (at 0.635 2.6162 270) (size 0.6096 2.2098) (layers F.Cu F.Paste F.Mask)
      (net 58 "/Burn Wires/VBURN_B_IN"))
    (pad 4 smd rect (at 1.905 2.6162 270) (size 0.6096 2.2098) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(Q8-Pad3)"))
    (pad 5 smd rect (at 1.905 -2.6162 270) (size 0.6096 2.2098) (layers F.Cu F.Paste F.Mask)
      (net 65 "/Burn Wires/VBURN5"))
    (pad 6 smd rect (at 0.635 -2.6162 270) (size 0.6096 2.2098) (layers F.Cu F.Paste F.Mask)
      (net 65 "/Burn Wires/VBURN5"))
    (pad 7 smd rect (at -0.635 -2.6162 270) (size 0.6096 2.2098) (layers F.Cu F.Paste F.Mask)
      (net 65 "/Burn Wires/VBURN5"))
    (pad 8 smd rect (at -1.905 -2.6162 270) (size 0.6096 2.2098) (layers F.Cu F.Paste F.Mask)
      (net 65 "/Burn Wires/VBURN5"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/HTSOP-8-1EP_3.9x4.9mm_P1.27mm_EP2.4x3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module custom-footprints:NDS8434 (layer F.Cu) (tedit 5CECB0CF)
    (at 173.8884 138.2268 270)
    (descr "<b>Small Outline Package</b> Fits JEDEC packages (narrow SOIC-8)")
    (attr smd)
    (fp_text reference U21 (at -0.0508 -5.3086 90) (layer F.SilkS))
    (fp_text value NDS8434 (at -0.254493 0.432628 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.905 2.6162 270) (size 0.6096 2.2098) (layers F.Cu F.Paste F.Mask)
      (net 58 "/Burn Wires/VBURN_B_IN"))
    (pad 2 smd rect (at -0.635 2.6162 270) (size 0.6096 2.2098) (layers F.Cu F.Paste F.Mask)
      (net 58 "/Burn Wires/VBURN_B_IN"))
    (pad 3 smd rect (at 0.635 2.6162 270) (size 0.6096 2.2098) (layers F.Cu F.Paste F.Mask)
      (net 58 "/Burn Wires/VBURN_B_IN"))
    (pad 4 smd rect (at 1.905 2.6162 270) (size 0.6096 2.2098) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(Q7-Pad3)"))
    (pad 5 smd rect (at 1.905 -2.6162 270) (size 0.6096 2.2098) (layers F.Cu F.Paste F.Mask)
      (net 60 "/Burn Wires/VBURN4"))
    (pad 6 smd rect (at 0.635 -2.6162 270) (size 0.6096 2.2098) (layers F.Cu F.Paste F.Mask)
      (net 60 "/Burn Wires/VBURN4"))
    (pad 7 smd rect (at -0.635 -2.6162 270) (size 0.6096 2.2098) (layers F.Cu F.Paste F.Mask)
      (net 60 "/Burn Wires/VBURN4"))
    (pad 8 smd rect (at -1.905 -2.6162 270) (size 0.6096 2.2098) (layers F.Cu F.Paste F.Mask)
      (net 60 "/Burn Wires/VBURN4"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/HTSOP-8-1EP_3.9x4.9mm_P1.27mm_EP2.4x3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module custom-footprints:NDS8434 (layer F.Cu) (tedit 5CECB0CF)
    (at 183.515 92.329 180)
    (descr "<b>Small Outline Package</b> Fits JEDEC packages (narrow SOIC-8)")
    (attr smd)
    (fp_text reference U19 (at -3.302 0 270) (layer F.SilkS))
    (fp_text value NDS8434 (at -0.254493 0.432628 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.905 2.6162 180) (size 0.6096 2.2098) (layers F.Cu F.Paste F.Mask)
      (net 55 "/Burn Wires/VBURN_A_IN"))
    (pad 2 smd rect (at -0.635 2.6162 180) (size 0.6096 2.2098) (layers F.Cu F.Paste F.Mask)
      (net 55 "/Burn Wires/VBURN_A_IN"))
    (pad 3 smd rect (at 0.635 2.6162 180) (size 0.6096 2.2098) (layers F.Cu F.Paste F.Mask)
      (net 55 "/Burn Wires/VBURN_A_IN"))
    (pad 4 smd rect (at 1.905 2.6162 180) (size 0.6096 2.2098) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(Q5-Pad3)"))
    (pad 5 smd rect (at 1.905 -2.6162 180) (size 0.6096 2.2098) (layers F.Cu F.Paste F.Mask)
      (net 57 "/Burn Wires/VBURN2"))
    (pad 6 smd rect (at 0.635 -2.6162 180) (size 0.6096 2.2098) (layers F.Cu F.Paste F.Mask)
      (net 57 "/Burn Wires/VBURN2"))
    (pad 7 smd rect (at -0.635 -2.6162 180) (size 0.6096 2.2098) (layers F.Cu F.Paste F.Mask)
      (net 57 "/Burn Wires/VBURN2"))
    (pad 8 smd rect (at -1.905 -2.6162 180) (size 0.6096 2.2098) (layers F.Cu F.Paste F.Mask)
      (net 57 "/Burn Wires/VBURN2"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/HTSOP-8-1EP_3.9x4.9mm_P1.27mm_EP2.4x3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module custom-footprints:NDS8434 (layer F.Cu) (tedit 5CECB0CF)
    (at 104.902 96.52 90)
    (descr "<b>Small Outline Package</b> Fits JEDEC packages (narrow SOIC-8)")
    (attr smd)
    (fp_text reference U18 (at -3.175 -0.381 180) (layer F.SilkS))
    (fp_text value NDS8434 (at -0.254493 0.432628 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.905 2.6162 90) (size 0.6096 2.2098) (layers F.Cu F.Paste F.Mask)
      (net 55 "/Burn Wires/VBURN_A_IN"))
    (pad 2 smd rect (at -0.635 2.6162 90) (size 0.6096 2.2098) (layers F.Cu F.Paste F.Mask)
      (net 55 "/Burn Wires/VBURN_A_IN"))
    (pad 3 smd rect (at 0.635 2.6162 90) (size 0.6096 2.2098) (layers F.Cu F.Paste F.Mask)
      (net 55 "/Burn Wires/VBURN_A_IN"))
    (pad 4 smd rect (at 1.905 2.6162 90) (size 0.6096 2.2098) (layers F.Cu F.Paste F.Mask)
      (net 105 "Net-(Q4-Pad3)"))
    (pad 5 smd rect (at 1.905 -2.6162 90) (size 0.6096 2.2098) (layers F.Cu F.Paste F.Mask)
      (net 56 "/Burn Wires/VBURN1"))
    (pad 6 smd rect (at 0.635 -2.6162 90) (size 0.6096 2.2098) (layers F.Cu F.Paste F.Mask)
      (net 56 "/Burn Wires/VBURN1"))
    (pad 7 smd rect (at -0.635 -2.6162 90) (size 0.6096 2.2098) (layers F.Cu F.Paste F.Mask)
      (net 56 "/Burn Wires/VBURN1"))
    (pad 8 smd rect (at -1.905 -2.6162 90) (size 0.6096 2.2098) (layers F.Cu F.Paste F.Mask)
      (net 56 "/Burn Wires/VBURN1"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/HTSOP-8-1EP_3.9x4.9mm_P1.27mm_EP2.4x3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module custom-footprints:NDS8434 (layer B.Cu) (tedit 5CECB0CF)
    (at 134.112 132.08 180)
    (descr "<b>Small Outline Package</b> Fits JEDEC packages (narrow SOIC-8)")
    (attr smd)
    (fp_text reference U7 (at -3.429 0.127 270) (layer B.SilkS))
    (fp_text value NDS8434 (at -0.254493 -0.432628 180) (layer B.SilkS) hide)
    (pad 1 smd rect (at -1.905 -2.6162 180) (size 0.6096 2.2098) (layers B.Cu B.Paste B.Mask)
      (net 2 3.3V))
    (pad 2 smd rect (at -0.635 -2.6162 180) (size 0.6096 2.2098) (layers B.Cu B.Paste B.Mask)
      (net 2 3.3V))
    (pad 3 smd rect (at 0.635 -2.6162 180) (size 0.6096 2.2098) (layers B.Cu B.Paste B.Mask)
      (net 2 3.3V))
    (pad 4 smd rect (at 1.905 -2.6162 180) (size 0.6096 2.2098) (layers B.Cu B.Paste B.Mask)
      (net 103 "Net-(Q1-Pad3)"))
    (pad 5 smd rect (at 1.905 2.6162 180) (size 0.6096 2.2098) (layers B.Cu B.Paste B.Mask)
      (net 17 GPS_PWR_IN))
    (pad 6 smd rect (at 0.635 2.6162 180) (size 0.6096 2.2098) (layers B.Cu B.Paste B.Mask)
      (net 17 GPS_PWR_IN))
    (pad 7 smd rect (at -0.635 2.6162 180) (size 0.6096 2.2098) (layers B.Cu B.Paste B.Mask)
      (net 17 GPS_PWR_IN))
    (pad 8 smd rect (at -1.905 2.6162 180) (size 0.6096 2.2098) (layers B.Cu B.Paste B.Mask)
      (net 17 GPS_PWR_IN))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/HTSOP-8-1EP_3.9x4.9mm_P1.27mm_EP2.4x3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module "Adafruit Feather M4 Express:BTN_KMR2_4.6X2.8" (layer F.Cu) (tedit 0)
    (at 129.159 99.568 180)
    (fp_text reference SW1 (at -2.032 -1.778 180) (layer F.SilkS) hide)
    (fp_text value "KMR231NG LFS" (at -2.032 2.159 180) (layer F.Fab) hide)
    (pad A smd rect (at 2.05 -0.8 180) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 ~RESET) (solder_mask_margin 0.0508))
    (pad B smd rect (at 2.05 0.8 180) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0508))
    (pad B' smd rect (at -2.05 0.8 180) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0508))
    (pad A' smd rect (at -2.05 -0.8 180) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 ~RESET) (solder_mask_margin 0.0508))
    (model ${CUSTOM_FOOTPRINT_DIR}/3d/KMR221GLF.STEP
      (offset (xyz 0 0 1.397))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Inductor_SMD:L_0806_2016Metric (layer B.Cu) (tedit 5BD4D8AF)
    (at 137.668 102.87 270)
    (descr "Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L1 (at 0.762 1.65 270) (layer B.SilkS))
    (fp_text value 10uH (at 0.762 -1.65 270) (layer B.Fab))
    (fp_text user %R (at 0.762 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 1.5 0 270) (size 0.5 1.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 101 "Net-(L1-Pad2)"))
    (pad 1 smd roundrect (at 0 0 270) (size 0.5 1.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 89 "Net-(C12-Pad2)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 142.113 93.98 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R7 (at -2.54 -0.127 270) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.43 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 149 WDT_WDI))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 167.59 101.603568 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R16 (at -0.098032 -1.2454 90) (layer B.SilkS))
    (fp_text value 845K (at 0 -1.43 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 109 "Net-(R16-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 110 "Net-(R16-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 167.590962 98.522971 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R19 (at 0.206829 1.246362 270) (layer B.SilkS))
    (fp_text value 2.1M (at 0 -1.43 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 14 VBATT))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 110 "Net-(R16-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 164.208481 76.154975 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R25 (at -2.733019 -0.172025 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 BURN_RELAY_A))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 172.004459 111.047575 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R26 (at 0.013925 1.443459 270) (layer F.SilkS))
    (fp_text value 10k (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 BURN_RELAY_B))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 155.7528 133.1976)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R31 (at 2.8702 0.0254 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 ENAB_BURN5))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_2512_6332Metric (layer F.Cu) (tedit 5B301BBD)
    (at 164.0551 87.170096)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R8 (at 0.2829 2.491904) (layer F.SilkS))
    (fp_text value 0.025 (at 0 2.62) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -2.9 0) (size 1.35 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.185185)
      (net 31 /Power/VREG_IN))
    (pad 2 smd roundrect (at 2.9 0) (size 1.35 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.185185)
      (net 14 VBATT))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 107.569 100.33 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R37 (at -3.048 0 180) (layer F.SilkS))
    (fp_text value 100k (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 105 "Net-(Q4-Pad3)"))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 55 "/Burn Wires/VBURN_A_IN"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 178.816 91.567)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R38 (at -2.9499 -0.078904) (layer F.SilkS))
    (fp_text value 100k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 55 "/Burn Wires/VBURN_A_IN"))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 70 "Net-(Q5-Pad3)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 127.80615 140.843 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R39 (at -0.381 1.09885 90) (layer F.SilkS))
    (fp_text value 100k (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 71 "Net-(Q6-Pad3)"))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 58 "/Burn Wires/VBURN_B_IN"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 168.6052 135.9408 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R40 (at 1.1938 3.0988) (layer F.SilkS))
    (fp_text value 100k (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 72 "Net-(Q7-Pad3)"))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 58 "/Burn Wires/VBURN_B_IN"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 175.3581 88.948096 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R33 (at 0 1.2411 270) (layer F.SilkS))
    (fp_text value 4.7k (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 ENAB_BURN2))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 61 "Net-(Q5-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 129.822104 140.8395 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R34 (at -0.3845 1.114896 90) (layer F.SilkS))
    (fp_text value 4.7k (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 64 "Net-(Q6-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 ENAB_BURN3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 166.878 135.89 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R35 (at 1.27 -2.794 180) (layer F.SilkS))
    (fp_text value 4.7k (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 63 "Net-(Q7-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 ENAB_BURN4))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 104.5535 101.834096 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R32 (at -3.067904 0.031 90) (layer F.SilkS))
    (fp_text value 4.7k (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 104 "Net-(Q4-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 ENAB_BURN1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 102.1151 101.834096 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R27 (at 3.067904 -0.0564 270) (layer F.SilkS))
    (fp_text value 10k (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 ENAB_BURN1))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 172.6911 88.948096 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R28 (at 0.048096 -1.3681 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 ENAB_BURN2))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 131.854104 140.8395 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R29 (at 0.3845 -1.241896 270) (layer F.SilkS))
    (fp_text value 10k (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 ENAB_BURN3))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 167.64 133.5024)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R30 (at 2.921 -0.0254) (layer F.SilkS))
    (fp_text value 10k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 ENAB_BURN4))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 129.921 135.128 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R23 (at 3.048 -0.127 270) (layer B.SilkS))
    (fp_text value 3.3K (at 0 -1.43 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 3.3V))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 103 "Net-(Q1-Pad3)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 122.6531 136.954096)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R22 (at -3.1461 0.078904) (layer B.SilkS))
    (fp_text value 4.7K (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 8 ENAB_GPS))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 102 "Net-(Q1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 122.6531 134.795096)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R21 (at -3.1461 -0.048096) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 8 ENAB_GPS))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 151.638 74.470096 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R15 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value 100K (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 "Net-(R15-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 91 "Net-(C27-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 167.6111 105.458096 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R20 (at -2.794 0.0289 90) (layer F.SilkS))
    (fp_text value 6.04K (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 L1_PROG))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 171.6751 105.458096 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R18 (at 2.794 -0.033 270) (layer F.SilkS))
    (fp_text value 100k (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 111 "Net-(R18-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 3.3V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 156.2827 70.329896)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R14 (at -3.0572 -0.035396) (layer F.SilkS))
    (fp_text value 22.1k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 "Net-(R13-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 169.6431 105.458096 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R17 (at 2.794 -0.033 270) (layer F.SilkS))
    (fp_text value 100k (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 150 ~CHRG))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 3.3V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 159.7371 70.329896)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R13 (at 0 1.552104) (layer F.SilkS))
    (fp_text value 73.2K (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 "Net-(R13-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 3.3V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 177.5171 93.402496 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R12 (at -0.0289 -1.212504 180) (layer F.SilkS))
    (fp_text value 43K (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 108 "Net-(R11-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 177.5171 95.806096)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R11 (at 0.0289 1.221904) (layer F.SilkS))
    (fp_text value 330K (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 108 "Net-(R11-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 "Net-(C22-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 177.2631 105.966096)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R10 (at 0.0289 1.475904) (layer F.SilkS))
    (fp_text value 40.9K (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 "Net-(R10-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 "Net-(C22-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 173.7071 105.458096 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R9 (at 2.370667 -0.033 270) (layer F.SilkS))
    (fp_text value 100K (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 "Net-(R10-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 156.5656 135.636 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R41 (at 1.016 3.2004) (layer F.SilkS))
    (fp_text value 100k (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 73 "Net-(Q8-Pad3)"))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 58 "/Burn Wires/VBURN_B_IN"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 165.5791 105.458096 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R6 (at 2.370667 0.0346 270) (layer F.SilkS))
    (fp_text value 10k (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 L1_PROG))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 107 "Net-(R6-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1210_3225Metric (layer F.Cu) (tedit 5B301BBE)
    (at 161.7691 81.836096 90)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C19 (at -2.872904 -0.0981 180) (layer F.SilkS))
    (fp_text value 220UF (at 0 2.28 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0 90) (size 1.25 2.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 31 /Power/VREG_IN))
    (pad 2 smd roundrect (at 1.4 0 90) (size 1.25 2.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1210_3225Metric (layer F.Cu) (tedit 5B301BBE)
    (at 165.481 81.836096 90)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C20 (at -2.872904 0.0635 180) (layer F.SilkS))
    (fp_text value 220UF (at 0 2.28 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0 90) (size 1.25 2.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 31 /Power/VREG_IN))
    (pad 2 smd roundrect (at 1.4 0 90) (size 1.25 2.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 164.1313 78.330896 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C29 (at -2.8102 -0.028104 180) (layer F.SilkS))
    (fp_text value 2.2uF (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 35 /Connectors/VBATT_IN))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 155.2921 72.184096 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C27 (at 2.794 0.1575 180) (layer F.SilkS))
    (fp_text value 1.0uF (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 91 "Net-(C27-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 155.2921 73.962096 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C26 (at -0.0289 -1.348904 180) (layer F.SilkS))
    (fp_text value 3.3nF (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 34 "Net-(C26-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 166.303834 100.378096 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C28 (at 0 -1.43 270) (layer F.SilkS))
    (fp_text value 22uF (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 VBATT))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 160.147 94.361 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C24 (at 0 -1.397 270) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 3.3V))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 157.8321 87.170096 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C21 (at 0.048096 1.4259 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 90 "Net-(C21-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 144 "Net-(C21-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 175.9931 101.081296)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C25 (at 2.667 0.094) (layer F.SilkS))
    (fp_text value 22nF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 "Net-(C25-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 146 "Net-(C25-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 175.9931 102.937696)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C23 (at 2.667 0.094) (layer F.SilkS))
    (fp_text value 2.2uF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 145 "Net-(C23-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 175.9931 99.097896)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C22 (at 2.667 0.094) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 "Net-(C22-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 150.2121 88.313096)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C18 (at -2.8575 0.094) (layer F.SilkS))
    (fp_text value 22uF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 3.3V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 150.2121 86.154096)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C17 (at -2.8575 0.094) (layer F.SilkS))
    (fp_text value 22uF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 3.3V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 160.1181 97.457096 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C9 (at -0.078904 1.0449 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 88 "Net-(C9-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 162.2771 97.457096 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C8 (at -0.078904 2.0609 270) (layer F.SilkS))
    (fp_text value 10nF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 "Net-(C8-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 160.1181 97.457096 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C7 (at 2.588096 0.0289 90) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.43 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 3.3V))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 155.2921 96.669696 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C6 (at -2.4419 -0.167804 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 3.3V))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 162.2771 97.457096 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C5 (at 2.588096 0.0289 90) (layer B.SilkS))
    (fp_text value 10uF (at 0 -1.43 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 3.3V))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mainboard:PWRDI-123 (layer F.Cu) (tedit 0)
    (at 182.118 106.474096)
    (fp_text reference D2 (at -0.8601 2.555404) (layer F.SilkS))
    (fp_text value DFLS130L (at 0 0) (layer F.SilkS) hide)
    (pad C smd rect (at -1.1 0) (size 2.2 1.4) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(C22-Pad1)") (solder_mask_margin 0.0635))
    (pad A smd rect (at 1.45 0) (size 0.9 1.4) (layers F.Cu F.Paste F.Mask)
      (net 12 VSOLAR) (solder_mask_margin 0.0635))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123.wrl
      (offset (xyz -0.127 0 0))
      (scale (xyz 0.9 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mainboard:MOLEX-1X3_LOCK (layer F.Cu) (tedit 0)
    (at 102.6731 87.233596 270)
    (fp_text reference JP11 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value M03POLAR_LOCK (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 -0.127 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 2 thru_hole circle (at 2.54 0.127 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 VSOLAR) (solder_mask_margin 0.0635))
    (pad 3 thru_hole circle (at 5.08 -0.127 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 56 "/Burn Wires/VBURN1") (solder_mask_margin 0.0635))
    (model ${KISYS3DMOD}/Connector.3dshapes/FanPinHeader_1x03_P2.54mm_Vertical.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mainboard:MOLEX-1X3_LOCK (layer F.Cu) (tedit 0)
    (at 184.3961 102.981596 90)
    (fp_text reference JP12 (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value M03POLAR_LOCK (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 -0.127 90) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 2 thru_hole circle (at 2.54 0.127 90) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 VSOLAR) (solder_mask_margin 0.0635))
    (pad 3 thru_hole circle (at 5.08 -0.127 90) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 57 "/Burn Wires/VBURN2") (solder_mask_margin 0.0635))
    (model ${KISYS3DMOD}/Connector.3dshapes/FanPinHeader_1x03_P2.54mm_Vertical.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mainboard:MOLEX-1X3_LOCK (layer F.Cu) (tedit 0)
    (at 112.649 144.272)
    (fp_text reference JP13 (at 0 0) (layer F.SilkS) hide)
    (fp_text value M03POLAR_LOCK (at 0 0) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 -0.127) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 2 thru_hole circle (at 2.54 0.127) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 VSOLAR) (solder_mask_margin 0.0635))
    (pad 3 thru_hole circle (at 5.08 -0.127) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 59 "/Burn Wires/VBURN3") (solder_mask_margin 0.0635))
    (model ${KISYS3DMOD}/Connector.3dshapes/FanPinHeader_1x03_P2.54mm_Vertical.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mainboard:MOLEX-1X3_LOCK (layer B.Cu) (tedit 0)
    (at 162.6041 56.584096)
    (fp_text reference JP10 (at 0 0) (layer B.SilkS) hide)
    (fp_text value M03POLAR_LOCK (at 0 0) (layer B.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0.127) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 2 thru_hole circle (at 2.54 -0.127) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 VSOLAR) (solder_mask_margin 0.0635))
    (pad 3 thru_hole circle (at 5.08 0.127) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 100 "Net-(JP10-Pad3)") (solder_mask_margin 0.0635))
    (model ${KISYS3DMOD}/Connector.3dshapes/FanPinHeader_1x03_P2.54mm_Vertical.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mainboard:MOLEX-1X3_LOCK (layer F.Cu) (tedit 0)
    (at 135.407265 143.884096)
    (fp_text reference JP8 (at 0 0) (layer F.SilkS) hide)
    (fp_text value M03POLAR_LOCK (at 0 0) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 -0.127) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 2 thru_hole circle (at 2.54 0.127) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 VSOLAR) (solder_mask_margin 0.0635))
    (pad 3 thru_hole circle (at 5.08 -0.127) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 98 "Net-(JP8-Pad3)") (solder_mask_margin 0.0635))
    (model ${KISYS3DMOD}/Connector.3dshapes/FanPinHeader_1x03_P2.54mm_Vertical.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mainboard:MOLEX-1X3_LOCK (layer F.Cu) (tedit 0)
    (at 123.6056 56.584096 180)
    (fp_text reference JP9 (at 0 0 180) (layer F.SilkS) hide)
    (fp_text value M03POLAR_LOCK (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 -0.127 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 2 thru_hole circle (at 2.54 0.127 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 VSOLAR) (solder_mask_margin 0.0635))
    (pad 3 thru_hole circle (at 5.08 -0.127 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 99 "Net-(JP9-Pad3)") (solder_mask_margin 0.0635))
    (model ${KISYS3DMOD}/Connector.3dshapes/FanPinHeader_1x03_P2.54mm_Vertical.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mainboard:SCREWTERMINAL-3.5MM-2_LOCK (layer F.Cu) (tedit 0)
    (at 177.4061 77.994096 90)
    (fp_text reference JP2 (at -1.27 -1.778 90) (layer F.SilkS))
    (fp_text value M023.5MM_LOCK (at -1.27 -1.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at -0.1778 0 90) (size 2.032 2.032) (drill 1.2) (layers *.Cu *.Mask)
      (net 35 /Connectors/VBATT_IN) (solder_mask_margin 0.0635))
    (pad 2 thru_hole circle (at 3.6778 0 90) (size 2.032 2.032) (drill 1.2) (layers *.Cu *.Mask)
      (net 96 "Net-(J4-Pad2)") (solder_mask_margin 0.0635))
    (model ${KISYS3DMOD}/TerminalBlock_Altech.3dshapes/Altech_AK300_1x02_P5.00mm_45-Degree.step
      (at (xyz 0 0 0))
      (scale (xyz 0.7 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mainboard:SCREWTERMINAL-3.5MM-2_LOCK (layer F.Cu) (tedit 0)
    (at 177.4061 84.994096 90)
    (fp_text reference JP3 (at -1.27 -1.778 90) (layer F.SilkS))
    (fp_text value M023.5MM_LOCK (at -1.27 -1.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at -0.1778 0 90) (size 2.032 2.032) (drill 1.2) (layers *.Cu *.Mask)
      (net 35 /Connectors/VBATT_IN) (solder_mask_margin 0.0635))
    (pad 2 thru_hole circle (at 3.6778 0 90) (size 2.032 2.032) (drill 1.2) (layers *.Cu *.Mask)
      (net 96 "Net-(J4-Pad2)") (solder_mask_margin 0.0635))
    (model ${KISYS3DMOD}/TerminalBlock_Altech.3dshapes/Altech_AK300_1x02_P5.00mm_45-Degree.step
      (at (xyz 0 0 0))
      (scale (xyz 0.7 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mainboard:SCREWTERMINAL-3.5MM-2_LOCK (layer B.Cu) (tedit 0)
    (at 170.2661 77.994096 90)
    (fp_text reference JP5 (at -1.27 2.54 90) (layer B.SilkS) hide)
    (fp_text value M023.5MM_LOCK (at -1.27 1.27 90) (layer B.Fab))
    (pad 1 thru_hole rect (at -0.1778 0 90) (size 2.032 2.032) (drill 1.2) (layers *.Cu *.Mask)
      (net 97 "Net-(JP5-Pad1)") (solder_mask_margin 0.0635))
    (pad 2 thru_hole circle (at 3.6778 0 90) (size 2.032 2.032) (drill 1.2) (layers *.Cu *.Mask)
      (net 35 /Connectors/VBATT_IN) (solder_mask_margin 0.0635))
    (model ${KISYS3DMOD}/TerminalBlock_Altech.3dshapes/Altech_AK300_1x02_P5.00mm_45-Degree.step
      (at (xyz 0 0 0))
      (scale (xyz 0.7 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mainboard:SCREWTERMINAL-3.5MM-2_LOCK (layer B.Cu) (tedit 0)
    (at 170.2661 84.994096 90)
    (fp_text reference JP6 (at -1.27 2.54 90) (layer B.SilkS) hide)
    (fp_text value M023.5MM_LOCK (at -1.27 1.27 90) (layer B.Fab))
    (pad 1 thru_hole rect (at -0.1778 0 90) (size 2.032 2.032) (drill 1.2) (layers *.Cu *.Mask)
      (net 14 VBATT) (solder_mask_margin 0.0635))
    (pad 2 thru_hole circle (at 3.6778 0 90) (size 2.032 2.032) (drill 1.2) (layers *.Cu *.Mask)
      (net 97 "Net-(JP5-Pad1)") (solder_mask_margin 0.0635))
    (model ${KISYS3DMOD}/TerminalBlock_Altech.3dshapes/Altech_AK300_1x02_P5.00mm_45-Degree.step
      (at (xyz 0 0 0))
      (scale (xyz 0.7 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mainboard:SCREWTERMINAL-3.5MM-2_LOCK (layer F.Cu) (tedit 0)
    (at 177.4061 70.984096 90)
    (fp_text reference JP4 (at -1.27 -1.778 90) (layer F.SilkS))
    (fp_text value M023.5MM_LOCK (at -1.27 -1.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at -0.1778 0 90) (size 2.032 2.032) (drill 1.2) (layers *.Cu *.Mask)
      (net 96 "Net-(J4-Pad2)") (solder_mask_margin 0.0635))
    (pad 2 thru_hole circle (at 3.6778 0 90) (size 2.032 2.032) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (model ${KISYS3DMOD}/TerminalBlock_Altech.3dshapes/Altech_AK300_1x02_P5.00mm_45-Degree.step
      (at (xyz 0 0 0))
      (scale (xyz 0.7 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mainboard:S1216_24PIN_PACKAGE (layer B.Cu) (tedit 0)
    (at 123.220562 123.652543 180)
    (fp_text reference U14 (at 0 0) (layer B.SilkS) hide)
    (fp_text value S1216V8 (at 0 0 180) (layer B.SilkS) hide)
    (fp_text user >Name (at -2.54 -10.16 180) (layer B.SilkS) hide)
    (pad 8 smd rect (at 5.85 1.98 90) (size 0.8128 1.6256) (layers B.Cu B.Paste B.Mask)
      (net 168 "Net-(R46-Pad2)") (solder_mask_margin 0.0635))
    (pad 11 smd rect (at 5.85 5.28 90) (size 0.8128 1.6256) (layers B.Cu B.Paste B.Mask)
      (net 54 "/RF and GPS/RF_IN") (solder_mask_margin 0.0635))
    (pad 10 smd rect (at 5.85 4.18 90) (size 0.8128 1.6256) (layers B.Cu B.Paste B.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 9 smd rect (at 5.85 3.08 90) (size 0.8128 1.6256) (layers B.Cu B.Paste B.Mask)
      (net 53 "Net-(U14-Pad9)") (solder_mask_margin 0.0635))
    (pad 7 smd rect (at 5.85 -1.02 90) (size 0.8128 1.6256) (layers B.Cu B.Paste B.Mask)
      (net 52 "Net-(U14-Pad7)") (solder_mask_margin 0.0635))
    (pad 2 smd rect (at 5.85 -6.52 90) (size 0.8128 1.6256) (layers B.Cu B.Paste B.Mask)
      (net 51 "Net-(U14-Pad2)") (solder_mask_margin 0.0635))
    (pad 4 smd rect (at 5.85 -4.32 90) (size 0.8128 1.6256) (layers B.Cu B.Paste B.Mask)
      (net 50 "Net-(U14-Pad4)") (solder_mask_margin 0.0635))
    (pad 5 smd rect (at 5.85 -3.22 90) (size 0.8128 1.6256) (layers B.Cu B.Paste B.Mask)
      (net 49 "Net-(U14-Pad5)") (solder_mask_margin 0.0635))
    (pad 6 smd rect (at 5.85 -2.12 90) (size 0.8128 1.6256) (layers B.Cu B.Paste B.Mask)
      (net 48 "Net-(U14-Pad6)") (solder_mask_margin 0.0635))
    (pad 12 smd rect (at 5.85 6.38 90) (size 0.8128 1.6256) (layers B.Cu B.Paste B.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 3 smd rect (at 5.85 -5.42 90) (size 0.8128 1.6256) (layers B.Cu B.Paste B.Mask)
      (net 47 "Net-(U14-Pad3)") (solder_mask_margin 0.0635))
    (pad 1 smd rect (at 5.85 -7.62 90) (size 0.8128 1.6256) (layers B.Cu B.Paste B.Mask)
      (net 46 "Net-(U14-Pad1)") (solder_mask_margin 0.0635))
    (pad 24 smd rect (at -6.35 -7.62 90) (size 0.8128 1.6256) (layers B.Cu B.Paste B.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 20 smd rect (at -6.35 -3.22 90) (size 0.8128 1.6256) (layers B.Cu B.Paste B.Mask)
      (net 154 RX) (solder_mask_margin 0.0635))
    (pad 21 smd rect (at -6.35 -4.32 90) (size 0.8128 1.6256) (layers B.Cu B.Paste B.Mask)
      (net 155 TX) (solder_mask_margin 0.0635))
    (pad 22 smd rect (at -6.35 -5.42 90) (size 0.8128 1.6256) (layers B.Cu B.Paste B.Mask)
      (net 17 GPS_PWR_IN) (solder_mask_margin 0.0635))
    (pad 23 smd rect (at -6.35 -6.52 90) (size 0.8128 1.6256) (layers B.Cu B.Paste B.Mask)
      (net 17 GPS_PWR_IN) (solder_mask_margin 0.0635))
    (pad 18 smd rect (at -6.35 -1.02 90) (size 0.8128 1.6256) (layers B.Cu B.Paste B.Mask)
      (net 45 "Net-(U14-Pad18)") (solder_mask_margin 0.0635))
    (pad 17 smd rect (at -6.35 1.98 90) (size 0.8128 1.6256) (layers B.Cu B.Paste B.Mask)
      (net 44 "Net-(U14-Pad17)") (solder_mask_margin 0.0635))
    (pad 13 smd rect (at -6.35 6.38 90) (size 0.8128 1.6256) (layers B.Cu B.Paste B.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 14 smd rect (at -6.35 5.28 90) (size 0.8128 1.6256) (layers B.Cu B.Paste B.Mask)
      (net 43 "Net-(U14-Pad14)") (solder_mask_margin 0.0635))
    (pad 15 smd rect (at -6.35 4.18 90) (size 0.8128 1.6256) (layers B.Cu B.Paste B.Mask)
      (net 42 "Net-(U14-Pad15)") (solder_mask_margin 0.0635))
    (pad 16 smd rect (at -6.35 3.08 90) (size 0.8128 1.6256) (layers B.Cu B.Paste B.Mask)
      (net 41 "Net-(U14-Pad16)") (solder_mask_margin 0.0635))
    (pad 19 smd rect (at -6.35 -2.12 90) (size 0.8128 1.6256) (layers B.Cu B.Paste B.Mask)
      (net 40 "Net-(U14-Pad19)") (solder_mask_margin 0.0635))
  )
  (module mainboard:QFN32-5X5MM (layer B.Cu) (tedit 0)
    (at 112.161878 118.60415 180)
    (descr "<h3>32-pin QFN 5.0 x 5.0 mm, 0.5mm pitch</h3>\n<p>Used by ESP8266</p>\n<p><a href=\"http://espressif.com/sites/default/files/documentation/0a-esp8266_datasheet_en_v4.4.pdf\">Datasheet</a></p>")
    (fp_text reference U13 (at -1.376122 4.05015) (layer B.SilkS))
    (fp_text value EP2W+ (at 0 -3.048) (layer B.Fab))
    (pad 1 smd rect (at -2.5 1.75 180) (size 0.762 0.3048) (layers B.Cu B.Paste B.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 2 smd rect (at -2.5 1.25 180) (size 0.762 0.3048) (layers B.Cu B.Paste B.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 3 smd rect (at -2.5 0.75 180) (size 0.762 0.3048) (layers B.Cu B.Paste B.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 4 smd rect (at -2.5 0.25 180) (size 0.762 0.3048) (layers B.Cu B.Paste B.Mask)
      (net 54 "/RF and GPS/RF_IN") (solder_mask_margin 0.0635))
    (pad 5 smd rect (at -2.5 -0.25 180) (size 0.762 0.3048) (layers B.Cu B.Paste B.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 6 smd rect (at -2.5 -0.75 180) (size 0.762 0.3048) (layers B.Cu B.Paste B.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 7 smd rect (at -2.5 -1.25 180) (size 0.762 0.3048) (layers B.Cu B.Paste B.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 8 smd rect (at -2.5 -1.75 180) (size 0.762 0.3048) (layers B.Cu B.Paste B.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 9 smd rect (at -1.75 -2.5 90) (size 0.762 0.3048) (layers B.Cu B.Paste B.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 10 smd rect (at -1.25 -2.5 90) (size 0.762 0.3048) (layers B.Cu B.Paste B.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 11 smd rect (at -0.75 -2.5 90) (size 0.762 0.3048) (layers B.Cu B.Paste B.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 12 smd rect (at -0.25 -2.5 90) (size 0.762 0.3048) (layers B.Cu B.Paste B.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 13 smd rect (at 0.25 -2.5 90) (size 0.762 0.3048) (layers B.Cu B.Paste B.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 14 smd rect (at 0.75 -2.5 90) (size 0.762 0.3048) (layers B.Cu B.Paste B.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 15 smd rect (at 1.25 -2.5 90) (size 0.762 0.3048) (layers B.Cu B.Paste B.Mask)
      (net 85 "Net-(J5-Pad1)") (solder_mask_margin 0.0635))
    (pad 16 smd rect (at 1.75 -2.5 90) (size 0.762 0.3048) (layers B.Cu B.Paste B.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 17 smd rect (at 2.5 -1.75) (size 0.762 0.3048) (layers B.Cu B.Paste B.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 18 smd rect (at 2.5 -1.25) (size 0.762 0.3048) (layers B.Cu B.Paste B.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 19 smd rect (at 2.5 -0.75) (size 0.762 0.3048) (layers B.Cu B.Paste B.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 20 smd rect (at 2.5 -0.25) (size 0.762 0.3048) (layers B.Cu B.Paste B.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 21 smd rect (at 2.5 0.25) (size 0.762 0.3048) (layers B.Cu B.Paste B.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 22 smd rect (at 2.5 0.75) (size 0.762 0.3048) (layers B.Cu B.Paste B.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 23 smd rect (at 2.5 1.25) (size 0.762 0.3048) (layers B.Cu B.Paste B.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 24 smd rect (at 2.5 1.75) (size 0.762 0.3048) (layers B.Cu B.Paste B.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 25 smd rect (at 1.75 2.5 270) (size 0.762 0.3048) (layers B.Cu B.Paste B.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 26 smd rect (at 1.25 2.5 270) (size 0.762 0.3048) (layers B.Cu B.Paste B.Mask)
      (net 86 "Net-(J6-Pad1)") (solder_mask_margin 0.0635))
    (pad 27 smd rect (at 0.75 2.5 270) (size 0.762 0.3048) (layers B.Cu B.Paste B.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 28 smd rect (at 0.25 2.5 270) (size 0.762 0.3048) (layers B.Cu B.Paste B.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 29 smd rect (at -0.25 2.5 270) (size 0.762 0.3048) (layers B.Cu B.Paste B.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 30 smd rect (at -0.75 2.5 270) (size 0.762 0.3048) (layers B.Cu B.Paste B.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 31 smd rect (at -1.25 2.5 270) (size 0.762 0.3048) (layers B.Cu B.Paste B.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 32 smd rect (at -1.75 2.5 270) (size 0.762 0.3048) (layers B.Cu B.Paste B.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad EP smd rect (at 0 0 180) (size 2.794 2.794) (layers B.Cu B.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mainboard:LGA24-8X4 (layer F.Cu) (tedit 0)
    (at 161.3881 101.648096)
    (descr "<h3>24-pin LGA 8x4 pins</h3>\n<p>Footprint: 3.5 x 3mm</p>\n<p>Used by:\n<ul><li>LSM9DS1</li></ul></p>\n<p><em>Unproven</em></p>")
    (fp_text reference U3 (at 0 0) (layer F.SilkS) hide)
    (fp_text value LSM9DS1 (at 0 0) (layer F.SilkS) hide)
    (fp_text user >Name (at -1.778 -1.778) (layer F.SilkS) hide)
    (fp_text user >Value (at -1.778 1.778) (layer F.Fab))
    (fp_text user X (at 0.603 -0.557) (layer F.Fab))
    (fp_text user Y (at -0.571 0.647) (layer F.Fab))
    (fp_text user Z (at 0.354 -0.063) (layer F.Fab))
    (pad 1 smd rect (at -1.505 -1.225 90) (size 0.45 0.27) (layers F.Cu F.Paste F.Mask)
      (net 2 3.3V) (solder_mask_margin 0.0635))
    (pad 2 smd rect (at -1.475 -0.645 180) (size 0.45 0.27) (layers F.Cu F.Paste F.Mask)
      (net 153 /Avionics/SCL) (solder_mask_margin 0.0635))
    (pad 3 smd rect (at -1.475 -0.215 180) (size 0.45 0.27) (layers F.Cu F.Paste F.Mask)
      (net 2 3.3V) (solder_mask_margin 0.0635))
    (pad 4 smd rect (at -1.475 0.215 180) (size 0.45 0.27) (layers F.Cu F.Paste F.Mask)
      (net 152 /Avionics/SDA) (solder_mask_margin 0.0635))
    (pad 5 smd rect (at -1.475 0.645 180) (size 0.45 0.27) (layers F.Cu F.Paste F.Mask)
      (net 2 3.3V) (solder_mask_margin 0.0635))
    (pad 6 smd rect (at -1.505 1.225 270) (size 0.45 0.27) (layers F.Cu F.Paste F.Mask)
      (net 2 3.3V) (solder_mask_margin 0.0635))
    (pad 7 smd rect (at -1.075 1.225 270) (size 0.45 0.27) (layers F.Cu F.Paste F.Mask)
      (net 2 3.3V) (solder_mask_margin 0.0635))
    (pad 8 smd rect (at -0.645 1.225 270) (size 0.45 0.27) (layers F.Cu F.Paste F.Mask)
      (net 2 3.3V) (solder_mask_margin 0.0635))
    (pad 9 smd rect (at -0.215 1.225 270) (size 0.45 0.27) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(U3-Pad9)") (solder_mask_margin 0.0635))
    (pad 10 smd rect (at 0.215 1.225 270) (size 0.45 0.27) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(U3-Pad10)") (solder_mask_margin 0.0635))
    (pad 11 smd rect (at 0.645 1.225 270) (size 0.45 0.27) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(U3-Pad11)") (solder_mask_margin 0.0635))
    (pad 12 smd rect (at 1.075 1.225 270) (size 0.45 0.27) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(U3-Pad12)") (solder_mask_margin 0.0635))
    (pad 13 smd rect (at 1.505 1.225 270) (size 0.45 0.27) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(U3-Pad13)") (solder_mask_margin 0.0635))
    (pad 14 smd rect (at 1.475 0.645) (size 0.45 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 15 smd rect (at 1.475 0.215) (size 0.45 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 16 smd rect (at 1.475 -0.215) (size 0.45 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 17 smd rect (at 1.475 -0.645) (size 0.45 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 18 smd rect (at 1.505 -1.225 90) (size 0.45 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 19 smd rect (at 1.075 -1.225 90) (size 0.45 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 20 smd rect (at 0.645 -1.225 90) (size 0.45 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 21 smd rect (at 0.215 -1.225 90) (size 0.45 0.27) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(C8-Pad1)") (solder_mask_margin 0.0635))
    (pad 22 smd rect (at -0.215 -1.225 90) (size 0.45 0.27) (layers F.Cu F.Paste F.Mask)
      (net 2 3.3V) (solder_mask_margin 0.0635))
    (pad 23 smd rect (at -0.645 -1.225 90) (size 0.45 0.27) (layers F.Cu F.Paste F.Mask)
      (net 2 3.3V) (solder_mask_margin 0.0635))
    (pad 24 smd rect (at -1.075 -1.225 90) (size 0.45 0.27) (layers F.Cu F.Paste F.Mask)
      (net 88 "Net-(C9-Pad1)") (solder_mask_margin 0.0635))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-24-1EP_4x5mm_P0.5mm_EP2.65x3.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.8 0.5 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mainboard:21-0057F (layer F.Cu) (tedit 0)
    (at 161.3881 91.107096)
    (fp_text reference U4 (at 2.1879 0.586904) (layer F.SilkS))
    (fp_text value MAX4372TEUK+T (at 0 0) (layer F.SilkS) hide)
    (fp_text user * (at -2.032 -1.3716) (layer F.SilkS) hide)
    (fp_text user * (at -1.1938 -0.4064) (layer F.Fab))
    (fp_text user >Name (at -3.2766 0.635) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.1938 -0.95) (size 1.3208 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 2 smd rect (at -1.1938 0) (size 1.3208 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 3 I_BATT) (solder_mask_margin 0.0635))
    (pad 3 smd rect (at -1.1938 0.95) (size 1.3208 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 2 3.3V) (solder_mask_margin 0.0635))
    (pad 4 smd rect (at 1.1938 0.95) (size 1.3208 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 14 VBATT) (solder_mask_margin 0.0635))
    (pad 5 smd rect (at 1.1938 -0.95) (size 1.3208 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 31 /Power/VREG_IN) (solder_mask_margin 0.0635))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mainboard:MOLEX_503182-1852 (layer B.Cu) (tedit 0)
    (at 123.063 101.473 270)
    (fp_text reference J1 (at -8.027259 -6.773 180) (layer B.SilkS) hide)
    (fp_text value 503182-1852 (at 9.285231 -6.775709) (layer B.Fab))
    (pad 1 smd rect (at -2.9 6.355 270) (size 0.8 1.24) (layers B.Cu B.Paste B.Mask)
      (net 39 "Net-(J1-Pad1)") (solder_mask_margin 0.0635))
    (pad 2 smd rect (at -1.8 6.355 270) (size 0.8 1.24) (layers B.Cu B.Paste B.Mask)
      (net 84 xSDCS) (solder_mask_margin 0.0635))
    (pad 3 smd rect (at -0.7 6.355 270) (size 0.8 1.24) (layers B.Cu B.Paste B.Mask)
      (net 77 MOSI) (solder_mask_margin 0.0635))
    (pad 4 smd rect (at 0.4 6.355 270) (size 0.8 1.24) (layers B.Cu B.Paste B.Mask)
      (net 2 3.3V) (solder_mask_margin 0.0635))
    (pad 5 smd rect (at 1.5 6.355 270) (size 0.8 1.24) (layers B.Cu B.Paste B.Mask)
      (net 76 SCK) (solder_mask_margin 0.0635))
    (pad 6 smd rect (at 2.6 6.355 270) (size 0.8 1.24) (layers B.Cu B.Paste B.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 7 smd rect (at 3.7 6.355 270) (size 0.8 1.24) (layers B.Cu B.Paste B.Mask)
      (net 75 MISO) (solder_mask_margin 0.0635))
    (pad 8 smd rect (at 4.8 6.355 270) (size 0.8 1.24) (layers B.Cu B.Paste B.Mask)
      (net 38 "Net-(J1-Pad8)") (solder_mask_margin 0.0635))
    (pad P1 smd rect (at -7.245 5.725 270) (size 0.95 2.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad P2 smd rect (at 7.145 5.875 270) (size 1.15 2.2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad SW smd rect (at 6.74 3.725 270) (size 1.16 1.25) (layers B.Cu B.Paste B.Mask)
      (net 37 "Net-(J1-PadSW)") (solder_mask_margin 0.0635))
    (pad DT smd rect (at 6.74 -5.275 270) (size 1.16 1.2) (layers B.Cu B.Paste B.Mask)
      (net 36 "Net-(J1-PadDT)") (solder_mask_margin 0.0635))
    (pad P3 smd rect (at -7.145 -5.605 270) (size 1.15 2.2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad P4 smd rect (at -2.84 -6.4 270) (size 1.5 1.15) (layers B.Cu B.Paste B.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad P5 smd rect (at 4.94 -6.4 270) (size 1.5 1.15) (layers B.Cu B.Paste B.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (model ${CUSTOM_FOOTPRINT_DIR}/3d/5031821852.STEP
      (offset (xyz 0 -6.756400000000001 1.5748))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module mainboard:FRAMATOME_10118194-0001LF (layer F.Cu) (tedit 0)
    (at 147.4181 55.039096 180)
    (fp_text reference J3 (at -4.5077 0.90154 90) (layer F.SilkS) hide)
    (fp_text value 10118194-0001LF (at 5.90914 -0.100153 90) (layer F.Fab))
    (fp_text user "PCB Edge" (at 4.261981 1.504231 180) (layer F.Fab))
    (pad 1 smd rect (at -1.3 -2.675) (size 0.45 1.35) (layers F.Cu F.Paste F.Mask)
      (net 93 "Net-(D3-Pad2)") (solder_mask_margin 0.0635))
    (pad 2 smd rect (at -0.65 -2.675) (size 0.45 1.35) (layers F.Cu F.Paste F.Mask)
      (net 16 USB_D-) (solder_mask_margin 0.0635))
    (pad 3 smd rect (at 0 -2.675) (size 0.45 1.35) (layers F.Cu F.Paste F.Mask)
      (net 15 USB_D+) (solder_mask_margin 0.0635))
    (pad 4 smd rect (at 0.65 -2.675) (size 0.45 1.35) (layers F.Cu F.Paste F.Mask)
      (net 95 "Net-(J3-Pad4)") (solder_mask_margin 0.0635))
    (pad 5 smd rect (at 1.3 -2.675) (size 0.45 1.35) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad P$6 thru_hole circle (at -2.5 -2.7 180) (size 1.35 1.35) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0635))
    (pad P$7 thru_hole circle (at 2.5 -2.7 180) (size 1.35 1.35) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0635))
    (pad P$8 thru_hole circle (at -3.5 0 180) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0635))
    (pad P$9 thru_hole circle (at 3.5 0 180) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0635))
    (pad P$10 smd rect (at -1 0 180) (size 1.5 1.55) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.0635))
    (pad P$11 smd rect (at 1 0 180) (size 1.5 1.55) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.0635))
    (pad P$12 smd rect (at -3.05 0 180) (size 1.5 1.55) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.0635))
    (pad P$13 smd rect (at 3.05 0 180) (size 1.5 1.55) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.0635))
    (model ${CUSTOM_FOOTPRINT_DIR}/3d/10118194.STEP
      (offset (xyz 0 3.048 -0.4318))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module mainboard:DCJ0303 (layer F.Cu) (tedit 0)
    (at 147.9261 137.970096)
    (descr "<b>DC POWER JACK</b> Pad shape changed to LONG 2007.07.26<p>\nSource: DCJ0303.pdf")
    (fp_text reference J4 (at 2.36 -5.55) (layer F.SilkS) hide)
    (fp_text value DCJ0303 (at 0 0) (layer F.SilkS) hide)
    (fp_line (start 5.2 -0.85) (end 4.2 -0.85) (layer Edge.Cuts) (width 0.05))
    (fp_line (start 4.2 -0.85) (end 4.2 0.85) (layer Edge.Cuts) (width 0.05))
    (fp_line (start 4.2 0.85) (end 5.2 0.85) (layer Edge.Cuts) (width 0.05))
    (fp_line (start 5.2 0.85) (end 5.2 -0.85) (layer Edge.Cuts) (width 0.05))
    (fp_line (start 0.85 3.5) (end -0.85 3.5) (layer Edge.Cuts) (width 0.05))
    (fp_line (start -0.85 3.5) (end -0.85 2.5) (layer Edge.Cuts) (width 0.05))
    (fp_line (start -0.85 2.5) (end 0.85 2.5) (layer Edge.Cuts) (width 0.05))
    (fp_line (start 0.85 2.5) (end 0.85 3.5) (layer Edge.Cuts) (width 0.05))
    (fp_line (start 0.85 -2.5) (end -0.85 -2.5) (layer Edge.Cuts) (width 0.05))
    (fp_line (start -0.85 -2.5) (end -0.85 -3.5) (layer Edge.Cuts) (width 0.05))
    (fp_line (start -0.85 -3.5) (end 0.85 -3.5) (layer Edge.Cuts) (width 0.05))
    (fp_line (start 0.85 -3.5) (end 0.85 -2.5) (layer Edge.Cuts) (width 0.05))
    (pad 1 thru_hole oval (at 0 -3 180) (size 4 2) (drill 1) (layers *.Cu *.Mask)
      (net 14 VBATT) (solder_mask_margin 0.0635))
    (pad 3 thru_hole oval (at 0 3 180) (size 4 2) (drill 1) (layers *.Cu *.Mask)
      (net 96 "Net-(J4-Pad2)") (solder_mask_margin 0.0635))
    (pad 2 thru_hole oval (at 4.7 0 90) (size 4 2) (drill 1) (layers *.Cu *.Mask)
      (net 96 "Net-(J4-Pad2)") (solder_mask_margin 0.0635))
    (model ${CUSTOM_FOOTPRINT_DIR}/3d/BARREL.STEP
      (offset (xyz -0 -2.8448 0.1524))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 180))
    )
  )
  (module mainboard:SOT-23 (layer B.Cu) (tedit 0)
    (at 126.7171 135.938096 90)
    (fp_text reference Q1 (at 2.207096 0.7909) (layer B.SilkS))
    (fp_text value IRLML2803 (at 0 0 90) (layer B.SilkS) hide)
    (fp_text user >Name (at -2.042212 1.906909 90) (layer B.SilkS) hide)
    (pad 1 smd rect (at -0.9525 -1.0033 90) (size 0.5588 1.3208) (layers B.Cu B.Paste B.Mask)
      (net 102 "Net-(Q1-Pad1)") (solder_mask_margin 0.0635))
    (pad 2 smd rect (at 0.9525 -1.0033 90) (size 0.5588 1.3208) (layers B.Cu B.Paste B.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 3 smd rect (at 0 0.8763 90) (size 0.5588 1.3208) (layers B.Cu B.Paste B.Mask)
      (net 103 "Net-(Q1-Pad3)") (solder_mask_margin 0.0635))
  )
  (module mainboard:SOT-23 (layer F.Cu) (tedit 0)
    (at 107.842904 103.5121 270)
    (fp_text reference Q4 (at -0.7691 -1.123096) (layer F.SilkS))
    (fp_text value IRLML2803 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text user >Name (at -2.042212 -1.906909 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 1.0033 270) (size 0.5588 1.3208) (layers F.Cu F.Paste F.Mask)
      (net 104 "Net-(Q4-Pad1)") (solder_mask_margin 0.0635))
    (pad 2 smd rect (at 0.9525 1.0033 270) (size 0.5588 1.3208) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 3 smd rect (at 0 -0.8763 270) (size 0.5588 1.3208) (layers F.Cu F.Paste F.Mask)
      (net 105 "Net-(Q4-Pad3)") (solder_mask_margin 0.0635))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module mainboard:SOT-23 (layer F.Cu) (tedit 0)
    (at 178.7871 88.948096 270)
    (fp_text reference Q5 (at -0.937096 -1.0449) (layer F.SilkS))
    (fp_text value IRLML2803 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text user >Name (at -2.042212 -1.906909 270) (layer F.SilkS) hide)
    (pad 3 smd rect (at 0 -0.8763 270) (size 0.5588 1.3208) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(Q5-Pad3)") (solder_mask_margin 0.0635))
    (pad 2 smd rect (at 0.9525 1.0033 270) (size 0.5588 1.3208) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.9525 1.0033 270) (size 0.5588 1.3208) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(Q5-Pad1)") (solder_mask_margin 0.0635))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module mainboard:SOT-23 (layer F.Cu) (tedit 0)
    (at 128.905 144.526 180)
    (fp_text reference Q6 (at -1.905 -0.381) (layer F.SilkS))
    (fp_text value IRLML2803 (at 0 0 180) (layer F.SilkS) hide)
    (fp_text user >Name (at -2.042212 -1.906909 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 1.0033 180) (size 0.5588 1.3208) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(Q6-Pad1)") (solder_mask_margin 0.0635))
    (pad 2 smd rect (at 0.9525 1.0033 180) (size 0.5588 1.3208) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 3 smd rect (at 0 -0.8763 180) (size 0.5588 1.3208) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(Q6-Pad3)") (solder_mask_margin 0.0635))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module mainboard:SOT-23 (layer F.Cu) (tedit 0)
    (at 167.894 139.2428 270)
    (fp_text reference Q7 (at 3.2512 1.143) (layer F.SilkS))
    (fp_text value IRLML2803 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text user >Name (at -2.042212 -1.906909 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 1.0033 270) (size 0.5588 1.3208) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(Q7-Pad1)") (solder_mask_margin 0.0635))
    (pad 2 smd rect (at 0.9525 1.0033 270) (size 0.5588 1.3208) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 3 smd rect (at 0 -0.8763 270) (size 0.5588 1.3208) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(Q7-Pad3)") (solder_mask_margin 0.0635))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module mainboard:RELAY5-PE_CO (layer F.Cu) (tedit 0)
    (at 170.7861 59.865096 90)
    (fp_text reference U16 (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value PE014006 (at 0 0 90) (layer F.SilkS) hide)
    (fp_text user * (at -8.2042 -19.7358 90) (layer F.SilkS) hide)
    (fp_text user >Name (at -7.0866 -7.9756 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -7.62 -17.1958 90) (size 2.0066 2.0066) (drill 1.2954) (layers *.Cu *.Mask)
      (net 14 VBATT) (solder_mask_margin 0.0635))
    (pad 11 thru_hole circle (at -7.62 -7.0358 90) (size 2.0066 2.0066) (drill 1.2954) (layers *.Cu *.Mask)
      (net 55 "/Burn Wires/VBURN_A_IN") (solder_mask_margin 0.0635))
    (pad 14 thru_hole circle (at -7.62 0.5842 90) (size 2.0066 2.0066) (drill 1.2954) (layers *.Cu *.Mask)
      (net 14 VBATT) (solder_mask_margin 0.0635))
    (pad 12 thru_hole circle (at 0 0.5842 270) (size 2.0066 2.0066) (drill 1.2954) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 5 thru_hole circle (at 0 -17.1958 90) (size 2.0066 2.0066) (drill 1.2954) (layers *.Cu *.Mask)
      (net 66 "Net-(D4-PadA)") (solder_mask_margin 0.0635))
    (model ${KISYS3DMOD}/Relay_THT.3dshapes/Relay_SPDT_Schrack-RT1-FormC_RM5mm.step
      (offset (xyz -6.680200000000001 16.764 0))
      (scale (xyz 0.68 0.8 0.6))
      (rotate (xyz 0 0 90))
    )
  )
  (module mainboard:RELAY5-PE_CO locked (layer F.Cu) (tedit 0)
    (at 183.6131 132.001096)
    (fp_text reference U17 (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value PE014006 (at 0 0) (layer F.SilkS) hide)
    (fp_text user * (at -8.2042 -19.7358) (layer F.SilkS))
    (fp_text user >Name (at -7.0866 -7.9756) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -7.62 -17.1958) (size 2.0066 2.0066) (drill 1.2954) (layers *.Cu *.Mask)
      (net 14 VBATT) (solder_mask_margin 0.0635))
    (pad 11 thru_hole circle (at -7.62 -7.0358) (size 2.0066 2.0066) (drill 1.2954) (layers *.Cu *.Mask)
      (net 58 "/Burn Wires/VBURN_B_IN") (solder_mask_margin 0.0635))
    (pad 14 thru_hole circle (at -7.62 0.5842) (size 2.0066 2.0066) (drill 1.2954) (layers *.Cu *.Mask)
      (net 14 VBATT) (solder_mask_margin 0.0635))
    (pad 12 thru_hole circle (at 0 0.5842 180) (size 2.0066 2.0066) (drill 1.2954) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 5 thru_hole circle (at 0 -17.1958) (size 2.0066 2.0066) (drill 1.2954) (layers *.Cu *.Mask)
      (net 94 "Net-(D5-PadA)") (solder_mask_margin 0.0635))
    (model ${KISYS3DMOD}/Relay_THT.3dshapes/Relay_SPDT_Schrack-RT1-FormC_RM5mm.step
      (offset (xyz -6.680200000000001 16.764 -0))
      (scale (xyz 0.68 0.8 0.6))
      (rotate (xyz 0 0 90))
    )
  )
  (module mainboard:SOT-23 (layer F.Cu) (tedit 0)
    (at 155.7528 138.938 270)
    (fp_text reference Q8 (at 3.556 1.4478) (layer F.SilkS))
    (fp_text value IRLML2803 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text user >Name (at -2.042212 -1.906909 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 1.0033 270) (size 0.5588 1.3208) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(Q8-Pad1)") (solder_mask_margin 0.0635))
    (pad 2 smd rect (at 0.9525 1.0033 270) (size 0.5588 1.3208) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 3 smd rect (at 0 -0.8763 270) (size 0.5588 1.3208) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(Q8-Pad3)") (solder_mask_margin 0.0635))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module mainboard:MOLEX-1X3_LOCK (layer F.Cu) (tedit 0)
    (at 157.7501 143.884096)
    (fp_text reference JP15 (at 0 0) (layer F.SilkS) hide)
    (fp_text value M03POLAR_LOCK (at 0 0) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 -0.127) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 2 thru_hole circle (at 2.54 0.127) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 VSOLAR) (solder_mask_margin 0.0635))
    (pad 3 thru_hole circle (at 5.08 -0.127) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 65 "/Burn Wires/VBURN5") (solder_mask_margin 0.0635))
    (model ${KISYS3DMOD}/Connector.3dshapes/FanPinHeader_1x03_P2.54mm_Vertical.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mainboard:SON127P600X500X90-9N (layer F.Cu) (tedit 0)
    (at 157.861 106.426)
    (descr "<b>DFN Small Flag Package</b><br>\n")
    (fp_text reference U8 (at -0.889 3.683) (layer F.SilkS))
    (fp_text value MR25H40MDF (at 0 3.81) (layer F.Fab))
    (pad 1 smd rect (at -2.85 -1.905) (size 1.05 0.45) (layers F.Cu F.Paste F.Mask)
      (net 78 FLASH_CS) (solder_mask_margin 0.0635))
    (pad 2 smd rect (at -2.85 -0.635) (size 1.05 0.45) (layers F.Cu F.Paste F.Mask)
      (net 82 FLASH_MISO) (solder_mask_margin 0.0635))
    (pad 3 smd rect (at -2.85 0.635) (size 1.05 0.45) (layers F.Cu F.Paste F.Mask)
      (net 81 FLASH_IO2) (solder_mask_margin 0.0635))
    (pad 4 smd rect (at -2.85 1.905) (size 1.05 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 5 smd rect (at 2.85 1.905) (size 1.05 0.45) (layers F.Cu F.Paste F.Mask)
      (net 83 FLASH_MOSI) (solder_mask_margin 0.0635))
    (pad 6 smd rect (at 2.85 0.635) (size 1.05 0.45) (layers F.Cu F.Paste F.Mask)
      (net 79 FLASH_SCK) (solder_mask_margin 0.0635))
    (pad 7 smd rect (at 2.85 -0.635) (size 1.05 0.45) (layers F.Cu F.Paste F.Mask)
      (net 80 FLASH_IO3) (solder_mask_margin 0.0635))
    (pad 8 smd rect (at 2.85 -1.905) (size 1.05 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 3.3V) (solder_mask_margin 0.0635))
    (pad 9 smd rect (at 0 0 90) (size 2.1 2.1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/DFN-8-1EP_6x5mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mainboard:SOT23 (layer F.Cu) (tedit 0)
    (at 165.227 73.555696 90)
    (descr <b>SOT-23</b>)
    (fp_text reference Q2 (at -0.421804 -4.3399 180) (layer F.SilkS))
    (fp_text value 2N5088 (at -1.905 3.175 90) (layer F.Fab))
    (pad 3 smd rect (at 0 -1.1 90) (size 1 1.4) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(D4-PadA)") (solder_mask_margin 0.0635))
    (pad 2 smd rect (at 0.95 1.1 90) (size 1 1.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.95 1.1 90) (size 1 1.4) (layers F.Cu F.Paste F.Mask)
      (net 19 BURN_RELAY_A) (solder_mask_margin 0.0635))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module mainboard:SOT23 (layer F.Cu) (tedit 0)
    (at 175.7645 110.969896 270)
    (descr <b>SOT-23</b>)
    (fp_text reference Q3 (at -2.003896 -2.1625 180) (layer F.SilkS))
    (fp_text value 2N5088 (at -1.905 3.175 90) (layer F.Fab))
    (pad 3 smd rect (at 0 -1.1 270) (size 1 1.4) (layers F.Cu F.Paste F.Mask)
      (net 94 "Net-(D5-PadA)") (solder_mask_margin 0.0635))
    (pad 2 smd rect (at 0.95 1.1 270) (size 1 1.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.95 1.1 270) (size 1 1.4) (layers F.Cu F.Paste F.Mask)
      (net 18 BURN_RELAY_B) (solder_mask_margin 0.0635))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module mainboard:PWRDI-123 (layer F.Cu) (tedit 0)
    (at 164.7155 70.431496)
    (fp_text reference D4 (at 2.48 0.498004) (layer F.SilkS))
    (fp_text value SBR2A40P1Q-7 (at 0 0) (layer F.SilkS) hide)
    (pad C smd rect (at -1.1 0) (size 2.2 1.4) (layers F.Cu F.Paste F.Mask)
      (net 14 VBATT) (solder_mask_margin 0.0635))
    (pad A smd rect (at 1.45 0) (size 0.9 1.4) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(D4-PadA)") (solder_mask_margin 0.0635))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mainboard:PWRDI-123 (layer F.Cu) (tedit 0)
    (at 179.7269 110.868296 90)
    (fp_text reference D5 (at -0.955204 2.8356 90) (layer F.SilkS))
    (fp_text value SBR2A40P1Q-7 (at 0 0 90) (layer F.SilkS) hide)
    (pad C smd rect (at -1.1 0 90) (size 2.2 1.4) (layers F.Cu F.Paste F.Mask)
      (net 14 VBATT) (solder_mask_margin 0.0635))
    (pad A smd rect (at 1.45 0 90) (size 0.9 1.4) (layers F.Cu F.Paste F.Mask)
      (net 94 "Net-(D5-PadA)") (solder_mask_margin 0.0635))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123.wrl
      (offset (xyz -0.1778 0 0))
      (scale (xyz 0.9 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LOGO (layer F.Cu) (tedit 0)
    (at 150.622 123.698)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module LOGO (layer B.Cu) (tedit 0)
    (at 162.179 127.127 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module LOGO (layer F.Cu) (tedit 0)
    (at 157.48 120.396)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module LOGO (layer F.Cu) (tedit 0)
    (at 157.48 120.396)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (gr_text "Rail\nSwitch" (at 186.055 65.3034 90) (layer B.SilkS))
  (gr_text Batteries (at 186.055 74.4982 90) (layer B.SilkS))
  (gr_text + (at 183.6674 78.867) (layer B.SilkS))
  (gr_text - (at 183.2102 80.0862 90) (layer B.SilkS))
  (gr_text + (at 183.6166 85.8774) (layer B.SilkS))
  (gr_text - (at 183.261 73.152 90) (layer B.SilkS))
  (gr_text RFM98PW (at 123.063 119.888 90) (layer F.SilkS))
  (gr_text "RADIO\nVCC" (at 117.729 140.97) (layer F.SilkS))
  (gr_text GND (at 112.649 140.462) (layer F.SilkS))
  (gr_text GND (at 111.125 143.51 90) (layer F.SilkS))
  (gr_text rexlab.stanford.edu (at 147.447 130.937) (layer F.SilkS))
  (gr_text rexlab.stanford.edu (at 163.322 130.937) (layer B.SilkS))
  (gr_text HOLLIDAY (at 147.447 55.04942 180) (layer B.Mask))
  (gr_text GPS (at 122.809 126.619 90) (layer B.SilkS))
  (gr_text WDT (at 132.461 93.091 90) (layer B.SilkS))
  (gr_text ON/OFF (at 131.191 96.139 90) (layer B.SilkS))
  (dimension 95.885 (width 0.15) (layer Dwgs.User)
    (gr_text "3.7750 in" (at 195.483 100.4316 270) (layer Dwgs.User))
    (feature1 (pts (xy 186.5061 148.3741) (xy 194.769421 148.3741)))
    (feature2 (pts (xy 186.5061 52.4891) (xy 194.769421 52.4891)))
    (crossbar (pts (xy 194.183 52.4891) (xy 194.183 148.3741)))
    (arrow1a (pts (xy 194.183 148.3741) (xy 193.596579 147.247596)))
    (arrow1b (pts (xy 194.183 148.3741) (xy 194.769421 147.247596)))
    (arrow2a (pts (xy 194.183 52.4891) (xy 193.596579 53.615604)))
    (arrow2b (pts (xy 194.183 52.4891) (xy 194.769421 53.615604)))
  )
  (dimension 90.17 (width 0.15) (layer Dwgs.User)
    (gr_text "3.5500 in" (at 143.4211 45.563) (layer Dwgs.User))
    (feature1 (pts (xy 188.5061 54.4891) (xy 188.5061 46.276579)))
    (feature2 (pts (xy 98.3361 54.4891) (xy 98.3361 46.276579)))
    (crossbar (pts (xy 98.3361 46.863) (xy 188.5061 46.863)))
    (arrow1a (pts (xy 188.5061 46.863) (xy 187.379596 47.449421)))
    (arrow1b (pts (xy 188.5061 46.863) (xy 187.379596 46.276579)))
    (arrow2a (pts (xy 98.3361 46.863) (xy 99.462604 47.449421)))
    (arrow2b (pts (xy 98.3361 46.863) (xy 99.462604 46.276579)))
  )
  (gr_text LED (at 139.827 52.705 90) (layer F.SilkS))
  (gr_text PA16 (at 157.48 93.98 45) (layer F.SilkS))
  (gr_text PA18 (at 154.93025 93.98 45) (layer F.SilkS))
  (gr_text PA19 (at 152.3805 93.98 45) (layer F.SilkS))
  (gr_text PB16 (at 149.86975 93.98 45) (layer F.SilkS))
  (gr_text PB17 (at 147.32 93.98 45) (layer F.SilkS))
  (gr_text PA22 (at 136.779 94.147 45) (layer F.SilkS))
  (gr_text PA20 (at 134.241375 94.147 45) (layer F.SilkS))
  (gr_text PB22 (at 131.74275 94.147 45) (layer F.SilkS))
  (gr_text PB23 (at 129.205125 94.147 45) (layer F.SilkS))
  (gr_text GND (at 118.820625 94.147 45) (layer F.SilkS))
  (gr_text 3V3 (at 116.205 94.147 45) (layer F.SilkS))
  (gr_text PB14 (at 157.226 111.252 45) (layer F.SilkS))
  (gr_text PB15 (at 154.559 111.125 45) (layer F.SilkS))
  (gr_text DAC0 (at 152.019 111.252 45) (layer F.SilkS))
  (gr_text GND (at 183.642 104.394 180) (layer F.SilkS))
  (gr_text GND (at 169.418 143.129 90) (layer F.SilkS))
  (gr_text GND (at 156.21 143.129 90) (layer F.SilkS))
  (gr_text GND (at 133.858 143.256 90) (layer F.SilkS))
  (gr_text GND (at 112.649 143.129 90) (layer F.SilkS))
  (gr_text GND (at 103.378 85.725) (layer F.SilkS))
  (gr_text MISO (at 126.5895 94.147 45) (layer F.SilkS))
  (gr_text MOSI (at 124.051875 94.147 45) (layer F.SilkS))
  (gr_text SCK (at 121.33225 94.147 45) (layer F.SilkS))
  (gr_text ~RESET (at 125.73 97.663 90) (layer F.SilkS))
  (gr_text ~RESET (at 137.758473 113.919) (layer F.SilkS))
  (gr_text "Passive grid = 10mils\nIC grid = 50 mils\nFanout grid = 2mil RFM, " (at 210.2577 69.034496) (layer Cmts.User))
  (gr_text "PAYLOAD 1 " (at 115.951 77.724 90) (layer F.SilkS))
  (gr_line (start 98.3361 54.4891) (end 98.3361 146.3741) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 100.3361 146.3741) (end 98.3361 146.3741) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 100.3361 148.3741) (end 186.5061 148.3741) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 186.5061 146.3741) (end 186.5061 148.3741) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 188.5061 146.3741) (end 188.5061 54.4891) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 186.5061 54.4891) (end 188.5061 54.4891) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 186.5061 52.4891) (end 154.2761 52.499096) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 154.2761 52.499096) (end 153.0061 53.388096) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 153.0061 53.388096) (end 142.2111 53.388096) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 142.2111 53.388096) (end 140.931103 52.4891) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 140.931103 52.4891) (end 100.3361 52.4891) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 100.3361 54.4891) (end 100.3361 52.4891) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_text "Passive grid = 10mils\nIC grid = 50 mils\nFanout grid = 2mil RFM, " (at -68.6343 67.637496) (layer Cmts.User))
  (gr_text Batteries (at 186.055 85.4202 90) (layer F.SilkS))
  (gr_text "Rail\nSwitch" (at 186.0261 71.803096 90) (layer F.SilkS))
  (gr_text JTAG (at 131.699 117.602 90) (layer F.SilkS))
  (gr_text GPS2 (at 98.7771 121.714096 90) (layer F.SilkS))
  (gr_text + (at 181.4033 85.874696) (layer F.SilkS))
  (gr_text - (at 183.2102 82.3214 90) (layer F.SilkS))
  (gr_text + (at 181.4541 78.872765) (layer F.SilkS))
  (gr_text - (at 183.261 75.3845 90) (layer F.SilkS))
  (gr_text SWDIO (at 137.550435 108.712) (layer F.SilkS))
  (gr_text GPS1 (at 98.7771 110.411096 90) (layer F.SilkS))
  (gr_text "GPS ~RST" (at 131.318 124.587 90) (layer B.SilkS))
  (gr_text RADIO (at 99.7931 134.033096 -90) (layer B.SilkS))
  (gr_text SWCLK (at 137.753635 111.379) (layer F.SilkS))
  (gr_text 3V3 (at 136.398 106.299) (layer F.SilkS))
  (gr_text VBATT (at 168.402 87.63 90) (layer F.SilkS))
  (gr_text VSOLAR (at 104.0857 68.323296) (layer F.SilkS))
  (gr_text Footswitch (at 161.7691 85.646096 -90) (layer B.SilkS))
  (gr_text 1 (at 164.3091 84.122096 -90) (layer B.SilkS))
  (gr_text 2 (at 164.3091 78.026096 -90) (layer B.SilkS))
  (gr_text "4.5V\nTO\n18V" (at 152.527 147.701) (layer F.SilkS))
  (gr_text SOLAR (at 135.636 147.955) (layer F.SilkS))
  (gr_text "DEPOLY 2" (at 156.718 147.940987) (layer F.SilkS))
  (gr_text "DEPOLY 3" (at 169.926 147.955) (layer F.SilkS))
  (gr_text "DEPOLY 1" (at 111.633 148.082) (layer F.SilkS))
  (gr_text "ANTENNA 1" (at 188.174775 104.648 90) (layer F.SilkS))
  (gr_text "ANTENNA 2" (at 98.775325 85.8266 270) (layer F.SilkS))
  (gr_text SOLAR (at 162.687 52.832 -180) (layer B.SilkS))
  (gr_text SOLAR (at 123.237243 52.770325 180) (layer F.SilkS))
  (gr_text C+M (at 173.48235 63.870359 90) (layer F.SilkS))
  (gr_text GND (at 136.618618 116.507096) (layer F.SilkS))
  (gr_text VSOL (at 182.7241 100.124096 90) (layer F.SilkS))
  (gr_text GND (at 182.7241 102.664096 90) (layer F.SilkS))
  (gr_text VSOL (at 182.8511 101.521096 -90) (layer B.SilkS))
  (gr_text GND (at 182.8511 103.807096 -90) (layer B.SilkS))
  (gr_text VBURN (at 182.7241 97.076096 90) (layer F.SilkS))
  (gr_text VBURN (at 182.8511 98.981096 -90) (layer B.SilkS))
  (gr_text VSOL (at 104.2381 89.154 90) (layer F.SilkS))
  (gr_text GND (at 104.2035 86.6775 90) (layer F.SilkS))
  (gr_text VSOL (at 104.3651 89.075096 -90) (layer B.SilkS))
  (gr_text GND (at 104.3651 86.789096 -90) (layer B.SilkS))
  (gr_text VBURN (at 104.267 91.567 90) (layer F.SilkS))
  (gr_text VBURN (at 104.3651 91.615096 -90) (layer B.SilkS))
  (gr_text VSOL (at 120.269 58.595096 180) (layer F.SilkS))
  (gr_text GND (at 125.095 57.404 270) (layer F.SilkS))
  (gr_text VSOL (at 121.8911 58.595096 -180) (layer B.SilkS))
  (gr_text GND (at 124.1771 58.595096 -180) (layer B.SilkS))
  (gr_text VSOL (at 173.8341 141.983296) (layer F.SilkS))
  (gr_text GND (at 171.2941 141.983296) (layer F.SilkS))
  (gr_text VSOL (at 172.6911 142.161096) (layer B.SilkS))
  (gr_text GND (at 170.4051 142.161096) (layer B.SilkS))
  (gr_text VBURN (at 176.8821 141.983296) (layer F.SilkS))
  (gr_text VBURN (at 175.2311 142.161096) (layer B.SilkS))
  (gr_text VSOL (at 160.6261 142.034096) (layer F.SilkS))
  (gr_text GND (at 158.0861 142.034096) (layer F.SilkS))
  (gr_text VSOL (at 159.4831 142.161096) (layer B.SilkS))
  (gr_text GND (at 157.1971 142.161096) (layer B.SilkS))
  (gr_text VBURN (at 163.6741 142.034096) (layer F.SilkS))
  (gr_text VBURN (at 162.0231 142.161096) (layer B.SilkS))
  (gr_text VSOL (at 138.2741 142.034096) (layer F.SilkS))
  (gr_text GND (at 135.7341 142.034096) (layer F.SilkS))
  (gr_text VSOL (at 137.1311 142.161096) (layer B.SilkS))
  (gr_text GND (at 134.8451 142.161096) (layer B.SilkS))
  (gr_text VSOL (at 115.5411 142.288096) (layer F.SilkS))
  (gr_text GND (at 113.0011 142.288096) (layer F.SilkS))
  (gr_text VSOL (at 114.3981 142.415096) (layer B.SilkS))
  (gr_text GND (at 112.1121 142.415096) (layer B.SilkS))
  (gr_text VBURN (at 118.5891 142.288096) (layer F.SilkS))
  (gr_text VBURN (at 116.9381 142.415096) (layer B.SilkS))
  (gr_text VSOL (at 164.4361 54.404096 180) (layer F.SilkS))
  (gr_text GND (at 162.1501 54.404096 180) (layer F.SilkS))
  (gr_text VSOL (at 165.8331 58.595096) (layer B.SilkS))
  (gr_text GND (at 160.655 57.277 90) (layer B.SilkS))
  (gr_text "PAYLOAD 2" (at 135.89 78.359 90) (layer F.SilkS))
  (gr_text "PAYLOAD 3" (at 117.475 71.882 -90) (layer B.SilkS))
  (gr_text "PAYLOAD 4" (at 137.541 71.755 -90) (layer B.SilkS))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (priority 4)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.1524) (thermal_bridge_width 0.3302))
    (polygon
      (pts
        (xy 100.3361 52.4891) (xy 140.931103 52.4891) (xy 142.2111 53.388096) (xy 153.0061 53.388096) (xy 154.2761 52.499096)
        (xy 186.5061 52.4891) (xy 186.818969 52.513723) (xy 187.124134 52.586987) (xy 187.414081 52.707087) (xy 187.681671 52.871066)
        (xy 187.920314 53.074886) (xy 188.124134 53.313529) (xy 188.288113 53.581119) (xy 188.408213 53.871066) (xy 188.5061 54.4891)
        (xy 188.5061 146.3741) (xy 188.481477 146.686969) (xy 188.408213 146.992134) (xy 188.288113 147.282081) (xy 188.124134 147.549671)
        (xy 187.920314 147.788314) (xy 187.681671 147.992134) (xy 187.414081 148.156113) (xy 187.124134 148.276213) (xy 186.5061 148.3741)
        (xy 100.3361 148.3741) (xy 100.023231 148.349477) (xy 99.718066 148.276213) (xy 99.428119 148.156113) (xy 99.160529 147.992134)
        (xy 98.921886 147.788314) (xy 98.718066 147.549671) (xy 98.554087 147.282081) (xy 98.433987 146.992134) (xy 98.3361 146.3741)
        (xy 98.3361 54.4891) (xy 98.360723 54.176231) (xy 98.433987 53.871066) (xy 98.554087 53.581119) (xy 98.718066 53.313529)
        (xy 98.921886 53.074886) (xy 99.160529 52.871066) (xy 99.428119 52.707087) (xy 99.718066 52.586987)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (priority 6)
    (connect_pads yes (clearance 0.000001))
    (min_thickness 0.4064)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 160.3721 100.886096) (xy 160.3721 102.410096) (xy 162.4041 102.410096) (xy 162.4041 100.886096)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (priority 6)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.1524) (thermal_bridge_width 0.3302))
    (polygon
      (pts
        (xy 107.2861 112.824096) (xy 130.556 112.824096) (xy 130.556 144.574096) (xy 109.8261 144.574096) (xy 109.8261 129.334096)
        (xy 107.2861 129.334096)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (priority 6)
    (connect_pads yes (clearance 0.000001))
    (min_thickness 0.271781)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 115.4141 121.714096) (xy 115.4141 115.364096) (xy 109.0641 115.364096) (xy 108.9371 115.491096) (xy 108.9371 121.714096)
      )
    )
  )
  (zone (net 56) (net_name "/Burn Wires/VBURN1") (layer F.Cu) (hatch edge 0.508)
    (priority 6)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.1524) (thermal_bridge_width 0.3302))
    (polygon
      (pts
        (xy 100.711 91.059) (xy 104.14 91.059) (xy 104.14 98.806) (xy 100.711 98.806)
      )
    )
  )
  (zone (net 59) (net_name "/Burn Wires/VBURN3") (layer F.Cu) (hatch edge 0.508)
    (priority 6)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.1524) (thermal_bridge_width 0.3302))
    (polygon
      (pts
        (xy 120.142 144.145) (xy 118.745 143.002) (xy 117.6655 143.002) (xy 117.602 143.637) (xy 116.713 143.637)
        (xy 116.713 146.812) (xy 126.238 146.812) (xy 126.238 144.145)
      )
    )
  )
  (zone (net 31) (net_name /Power/VREG_IN) (layer F.Cu) (hatch edge 0.508)
    (priority 6)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.1524) (thermal_bridge_width 0.3302))
    (polygon
      (pts
        (xy 157.8321 81.915) (xy 157.8321 86.995) (xy 158.877 86.995) (xy 158.877 90.424) (xy 161.036 90.424)
        (xy 161.036 91.186) (xy 164.465 91.186) (xy 164.465 81.915)
      )
    )
  )
  (zone (net 60) (net_name "/Burn Wires/VBURN4") (layer F.Cu) (hatch edge 0.508)
    (priority 7)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.1524) (thermal_bridge_width 0.381))
    (polygon
      (pts
        (xy 175.006 143.891) (xy 174.5615 142.875) (xy 174.5996 135.4836) (xy 178.0032 135.4836) (xy 177.927 143.891)
      )
    )
  )
  (zone (net 14) (net_name VBATT) (layer F.Cu) (hatch edge 0.508)
    (priority 8)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.1524) (thermal_bridge_width 0.3302) (smoothing fillet) (radius 0.254))
    (polygon
      (pts
        (xy 173.736 93.218) (xy 168.529 93.218) (xy 168.529 99.108096) (xy 170.2781 99.108096) (xy 170.2781 102.410096)
        (xy 165.735 102.362) (xy 165.735 92.885096) (xy 161.036 92.885096) (xy 161.036 91.361096) (xy 164.4361 91.361096)
        (xy 164.465 83.185) (xy 173.736 83.185)
      )
    )
  )
  (zone (net 30) (net_name "Net-(R10-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 6)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.1524) (thermal_bridge_width 0.3302))
    (polygon
      (pts
        (xy 171.704 104.267) (xy 171.45 104.267) (xy 171.45 101.394096) (xy 172.212 101.394096) (xy 173.863 103.172096)
        (xy 177.3901 103.378) (xy 177.3901 108.506096) (xy 171.6751 108.506096)
      )
    )
  )
  (zone (net 146) (net_name "Net-(C25-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (priority 5)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.1524) (thermal_bridge_width 0.3302))
    (polygon
      (pts
        (xy 171.323 93.218) (xy 171.323 99.489096) (xy 173.0721 99.489096) (xy 173.1991 99.616096) (xy 173.5801 99.616096)
        (xy 173.5801 96.822096) (xy 177.1361 96.822096) (xy 177.1361 91.919896) (xy 173.5801 91.919896) (xy 173.5801 93.218)
      )
    )
  )
  (zone (net 147) (net_name "Net-(L3-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 4)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.1524) (thermal_bridge_width 0.3302))
    (polygon
      (pts
        (xy 171.2941 97.584096) (xy 171.2941 93.218) (xy 168.5001 93.218) (xy 168.5001 99.108096) (xy 169.5161 99.108096)
        (xy 171.323 99.06)
      )
    )
  )
  (zone (net 32) (net_name "Net-(C22-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.1524) (thermal_bridge_width 0.3302))
    (polygon
      (pts
        (xy 177.165 103.378) (xy 173.736 103.124) (xy 172.466 101.6) (xy 173.3261 96.822096) (xy 177.165 96.822096)
        (xy 177.165 90.805) (xy 181.483 90.805) (xy 181.5811 108.506096) (xy 177.419 108.458)
      )
    )
  )
  (zone (net 97) (net_name "Net-(JP5-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 8)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.1524) (thermal_bridge_width 0.3302))
    (polygon
      (pts
        (xy 173.355 76.756096) (xy 168.529 76.756096) (xy 168.529 83.058) (xy 173.355 83.058)
      )
    )
  )
  (zone (net 90) (net_name "Net-(C21-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 4)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.1524) (thermal_bridge_width 0.3302) (smoothing fillet) (radius 0.254))
    (polygon
      (pts
        (xy 156.0541 82.090096) (xy 157.353 82.090096) (xy 157.353 86.995) (xy 158.75 86.995) (xy 158.75 89.281)
        (xy 152.7521 89.281) (xy 152.7521 84.582) (xy 156.0541 84.582)
      )
    )
  )
  (zone (net 29) (net_name "Net-(R13-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 6)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.1524) (thermal_bridge_width 0.3302))
    (polygon
      (pts
        (xy 159.8641 69.212296) (xy 159.8641 72.438096) (xy 158.75 73.533) (xy 158.75 76.581) (xy 157.48 76.581)
        (xy 157.48 73.533) (xy 156.21 72.263) (xy 156.5621 71.422096) (xy 156.5621 69.212296)
      )
    )
  )
  (zone (net 96) (net_name "Net-(J4-Pad2)") (layer Route15) (hatch edge 0.508)
    (priority 6)
    (connect_pads yes (clearance 0.000001))
    (min_thickness 0.2794)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 176.2471 79.931096) (xy 176.2471 82.725096) (xy 181.991 82.725096) (xy 181.991 69.898096) (xy 176.1201 69.898096)
        (xy 176.1201 72.565096) (xy 176.1201 76.2) (xy 179.1681 76.2) (xy 179.1681 79.804096) (xy 179.1681 79.931096)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (priority 3)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.1524) (thermal_bridge_width 0.3302) (smoothing fillet) (radius 0.254))
    (polygon
      (pts
        (xy 148.082 66.087406) (xy 163.576 66.167) (xy 164.592 67.183) (xy 164.592 81.915) (xy 156.083 81.915)
        (xy 156.083 84.455) (xy 150.114 84.455) (xy 150.114 88.439406) (xy 148.082 88.439406) (xy 148.082 78.533406)
        (xy 148.082 69.008406)
      )
    )
  )
  (zone (net 12) (net_name VSOLAR) (layer F.Cu) (hatch edge 0.508)
    (priority 3)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.1524) (thermal_bridge_width 0.3302))
    (polygon
      (pts
        (xy 159.004 148.336) (xy 188.595 148.336) (xy 188.595 52.451) (xy 98.298 52.451) (xy 98.3234 91.059)
        (xy 100.965 91.059) (xy 105.918 91.059) (xy 105.918 65.659) (xy 110.109 61.595) (xy 143.764 61.595)
        (xy 146.177 64.008) (xy 181.229 64.008) (xy 181.229 108.204) (xy 175.133 108.204) (xy 175.133 141.351)
        (xy 159.004 141.351)
      )
    )
  )
  (zone (net 35) (net_name /Connectors/VBATT_IN) (layer F.Cu) (hatch edge 0.508)
    (priority 5)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.1524) (thermal_bridge_width 0.3302))
    (polygon
      (pts
        (xy 145.669 63.246) (xy 180.721 63.246) (xy 181.991 64.516) (xy 181.991 88.9) (xy 180.213 88.9)
        (xy 177.8635 91.7448) (xy 173.736 91.7448) (xy 173.736 83.312) (xy 163.83 83.312) (xy 163.83 77.216)
        (xy 164.592 77.216) (xy 164.592 67.183) (xy 163.576 66.167) (xy 155.956 66.167) (xy 148.463 66.167)
      )
    )
  )
  (zone (net 55) (net_name "/Burn Wires/VBURN_A_IN") (layer F.Cu) (hatch edge 0.508)
    (priority 4)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.1524) (thermal_bridge_width 0.3302))
    (polygon
      (pts
        (xy 108.585 95.631) (xy 108.585 98.806) (xy 104.267 98.806) (xy 104.267 95.631)
      )
    )
  )
  (zone (net 58) (net_name "/Burn Wires/VBURN_B_IN") (layer F.Cu) (hatch edge 0.508)
    (priority 4)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.1524) (thermal_bridge_width 0.3302))
    (polygon
      (pts
        (xy 128.1684 139.7) (xy 128.1684 142.0876) (xy 122.428 142.0876) (xy 122.428 139.7)
      )
    )
  )
  (zone (net 55) (net_name "/Burn Wires/VBURN_A_IN") (layer F.Cu) (hatch edge 0.508)
    (priority 7)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.1524) (thermal_bridge_width 0.3302))
    (polygon
      (pts
        (xy 185.674 88.9) (xy 185.674 92.075) (xy 179.197 92.075) (xy 179.197 88.9)
      )
    )
  )
  (zone (net 57) (net_name "/Burn Wires/VBURN2") (layer F.Cu) (hatch edge 0.508)
    (priority 7)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.1524) (thermal_bridge_width 0.3302))
    (polygon
      (pts
        (xy 185.674 92.202) (xy 185.674 98.933) (xy 181.229 98.933) (xy 181.229 92.202)
      )
    )
  )
  (zone (net 58) (net_name "/Burn Wires/VBURN_B_IN") (layer F.Cu) (hatch edge 0.508)
    (priority 7)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.1524) (thermal_bridge_width 0.381))
    (polygon
      (pts
        (xy 169.6974 139.6873) (xy 169.6974 134.6073) (xy 172.8724 134.6073) (xy 172.8724 139.6873)
      )
    )
  )
  (zone (net 65) (net_name "/Burn Wires/VBURN5") (layer F.Cu) (hatch edge 0.508)
    (priority 7)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.1524) (thermal_bridge_width 0.381))
    (polygon
      (pts
        (xy 161.798 143.754261) (xy 161.8488 135.636) (xy 165.735 135.636) (xy 165.735 143.7132)
      )
    )
  )
  (zone (net 58) (net_name "/Burn Wires/VBURN_B_IN") (layer F.Cu) (hatch edge 0.508)
    (priority 7)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.1524) (thermal_bridge_width 0.381))
    (polygon
      (pts
        (xy 157.6324 139.67477) (xy 157.6324 134.493) (xy 160.6804 134.493) (xy 160.6804 139.67477)
      )
    )
  )
  (zone (net 17) (net_name GPS_PWR_IN) (layer B.Cu) (hatch edge 0.508)
    (priority 7)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.1524) (thermal_bridge_width 0.3302))
    (polygon
      (pts
        (xy 128.651 128.27) (xy 136.525 128.27) (xy 136.525 130.937) (xy 128.651 130.937)
      )
    )
  )
  (zone (net 2) (net_name 3.3V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.1524) (thermal_bridge_width 0.3302))
    (polygon
      (pts
        (xy 186.5061 148.3741) (xy 100.3361 148.3741) (xy 100.023231 148.349477) (xy 99.718066 148.276213) (xy 99.428119 148.156113)
        (xy 99.160529 147.992134) (xy 98.921886 147.788314) (xy 98.718066 147.549671) (xy 98.554087 147.282081) (xy 98.433987 146.992134)
        (xy 98.3361 146.3741) (xy 98.3361 54.4891) (xy 98.360723 54.176231) (xy 98.433987 53.871066) (xy 98.554087 53.581119)
        (xy 98.718066 53.313529) (xy 98.921886 53.074886) (xy 99.160529 52.871066) (xy 99.428119 52.707087) (xy 99.718066 52.586987)
        (xy 100.3361 52.4891) (xy 140.931103 52.4891) (xy 142.2111 53.388096) (xy 153.0061 53.388096) (xy 154.2761 52.499096)
        (xy 186.5061 52.4891) (xy 186.818969 52.513723) (xy 187.124134 52.586987) (xy 187.414081 52.707087) (xy 187.681671 52.871066)
        (xy 187.920314 53.074886) (xy 188.124134 53.313529) (xy 188.288113 53.581119) (xy 188.408213 53.871066) (xy 188.5061 54.4891)
        (xy 188.5061 146.3741) (xy 188.481477 146.686969) (xy 188.408213 146.992134) (xy 188.288113 147.282081) (xy 188.124134 147.549671)
        (xy 187.920314 147.788314) (xy 187.681671 147.992134) (xy 187.414081 148.156113) (xy 187.124134 148.276213)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer Route2) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.1524) (thermal_bridge_width 0.3556))
    (polygon
      (pts
        (xy 98.298 52.451) (xy 188.595 52.451) (xy 188.595 148.336) (xy 98.298 148.336)
      )
    )
  )
)
