(kicad_pcb (version 4) (host pcbnew 4.0.4-stable)
  (general
    (links 18)
    (no_connects 0)
    (area 77.872999 74.872999 122.127001 125.127001)
    (thickness 1.6)
    (drawings 17)
    (tracks 97)
    (zones 0)
    (modules 15)
    (nets 9)
  )
  (page USLetter)
  (title_block
    (title "OSH Park Badge")
    (company www.MakersBox.us)
    (comment 1 "K. Olsen")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.4064)
    (user_trace_width 0.254)
    (user_trace_width 0.3048)
    (user_trace_width 0.4064)
    (user_trace_width 0.6096)
    (user_trace_width 2.032)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.254)
    (edge_width 0.254)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (user_via 1 0.5)
    (uvia_size 0.762)
    (uvia_drill 0.508)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 17.78 17.78)
    (pad_drill 0)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (grid_origin 210.82 95.25)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerbers/))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +BATT)
  (net 3 "Net-(CON1-Pad1)")
  (net 4 "Net-(CON1-Pad3)")
  (net 5 "Net-(CON1-Pad4)")
  (net 6 "Net-(CON1-Pad5)")
  (net 7 "Net-(D1-Pad1)")
  (net 8 "Net-(IC1-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net +BATT)
    (add_net GND)
    (add_net "Net-(CON1-Pad1)")
    (add_net "Net-(CON1-Pad3)")
    (add_net "Net-(CON1-Pad4)")
    (add_net "Net-(CON1-Pad5)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(IC1-Pad2)")
  )
  (module Connect:1pin (layer B.Cu) (tedit 59A338E8)
    (at 99.82 83.75)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 3.5 1) (layer B.SilkS) hide)
    (fp_text value 1pin (at 3 -0.5) (layer B.Fab))
    (pad 1 smd rect (at 0 0) (size 20 5) (layers B.Cu B.Paste B.Mask))
  )
  (module LEDs:LED-1206 (layer F.Cu) (tedit 59A241A3)
    (at 99.82 100.25 180)
    (descr "LED 1206 smd package")
    (tags "LED1206 SMD")
    (attr smd)
    (fp_text reference D1 (at 0 -2 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 2 180) (layer F.Fab))
    (pad 2 smd rect (at 1.905 0) (size 2 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(CON1-Pad4)"))
    (pad 1 smd rect (at -1.905 0) (size 2 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D1-Pad1)"))
    (model LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIJ-8_5.3x5.3mm_Pitch1.27mm (layer B.Cu) (tedit 58D85853)
    (at 99.82 95.25)
    (descr "8-Lead Plastic Small Outline (SM) - Medium, 5.28 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference ATTINY (at 1.651 0 270) (layer B.SilkS))
    (fp_text value ATTINY (at 0 -3.68) (layer B.Fab))
    (pad 1 smd rect (at -3.65 1.905) (size 1.7 0.65) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(CON1-Pad5)"))
    (pad 2 smd rect (at -3.65 0.635) (size 1.7 0.65) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(IC1-Pad2)"))
    (pad 3 smd rect (at -3.65 -0.635) (size 1.7 0.65) (layers B.Cu B.Paste B.Mask))
    (pad 4 smd rect (at -3.65 -1.905) (size 1.7 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 3.65 -1.905) (size 1.7 0.65) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(CON1-Pad4)"))
    (pad 6 smd rect (at 3.65 -0.635) (size 1.7 0.65) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(CON1-Pad1)"))
    (pad 7 smd rect (at 3.65 0.635) (size 1.7 0.65) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(CON1-Pad3)"))
    (pad 8 smd rect (at 3.65 1.905) (size 1.7 0.65) (layers B.Cu B.Paste B.Mask)
      (net 2 +BATT))
    (model Housings_SOIC.3dshapes/SOIJ-8_5.3x5.3mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module myFootPrints:BATT_CR2032_SMD (layer B.Cu) (tedit 598FCE2F)
    (at 99.82 110.25 180)
    (tags battery)
    (fp_text reference BT1 (at 0 -5.08 180) (layer B.SilkS) hide)
    (fp_text value Battery (at 0 2.54 180) (layer B.SilkS) hide)
    (pad 2 smd circle (at -0.18 0.25 180) (size 17.78 17.78) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -11.43 0 180) (size 2.54 5.08) (layers B.Cu B.Paste B.Mask)
      (net 2 +BATT))
    (pad 1 smd rect (at 11.43 0 180) (size 2.54 5.08) (layers B.Cu B.Paste B.Mask)
      (net 2 +BATT))
  )
  (module Pin_Headers:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 598FCE21)
    (at 99.82 83.25)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at -0.6 -0.5) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 0.9) (layer F.Fab))
    (pad "" thru_hole circle (at 0.18 -0.25) (size 3 3) (drill 2) (layers *.Cu *.Mask))
  )
  (module myFootPrints:AVR-ISP-6 (layer B.Cu) (tedit 5860A6AE)
    (at 110.82 93.25 180)
    (descr "6-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "dil dip 2.54 300")
    (fp_text reference CON1 (at 0 2.54 180) (layer B.SilkS) hide)
    (fp_text value AVR-ISP-6 (at 0 3.72 180) (layer B.Fab) hide)
    (pad 1 smd oval (at 0 0 180) (size 1.6 1.6) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(CON1-Pad1)"))
    (pad 2 smd rect (at 2.54 0 180) (size 1.6 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 +BATT))
    (pad 3 smd oval (at 0 -2.54 180) (size 1.6 1.6) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(CON1-Pad3)"))
    (pad 4 smd oval (at 2.54 -2.54 180) (size 1.6 1.6) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(CON1-Pad4)"))
    (pad 5 smd oval (at 0 -5.08 180) (size 1.6 1.6) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(CON1-Pad5)"))
    (pad 6 smd oval (at 2.54 -5.08 180) (size 1.6 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 58C47DA8)
    (at 85.82 100.25)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C1 (at 0 0) (layer F.SilkS))
    (fp_text value "0.1 uF" (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 +BATT))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58C47DAE)
    (at 113.82 100.25)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R1 (at 0 0) (layer F.SilkS))
    (fp_text value 330 (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_SMD:SW_SPST_EVQP0 (layer F.Cu) (tedit 5993BC6B)
    (at 99.82 118.25)
    (descr "Light Touch Switch")
    (attr smd)
    (fp_text reference SW1 (at 0 -2) (layer F.SilkS))
    (fp_text value SW_PUSH (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at 3.4 -2) (size 3.2 1) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(IC1-Pad2)"))
    (pad 1 smd rect (at -3.4 -2) (size 3.2 1) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(IC1-Pad2)"))
    (pad 2 smd rect (at -3.4 2) (size 3.2 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 3.4 2) (size 3.2 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Buttons_Switches_SMD.3dshapes/SW_SPST_EVQQ2_03W.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module myFootPrints:OSHPark (layer F.Cu) (tedit 0)
    (at 99.82 90.25)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module myFootPrints:OSHParkPurple (layer F.Cu) (tedit 0)
    (at 99.82 97.25)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module myFootPrints:OSHWA2 (layer F.Cu) (tedit 0)
    (at 110.82 108.25)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module myFootPrints:OSHWA (layer F.Cu) (tedit 0)
    (at 90.32 107.25)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module myFootPrints:MB225rev (layer F.Cu) (tedit 0)
    (at 115.82 92.25 90)
    (fp_text reference VAL (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value MB225rev (at 0 0 90) (layer F.SilkS) hide)
  )
  (module myFootPrints:MadeInOregonRev25 (layer F.Cu) (tedit 0)
    (at 90.82 95.25 90)
    (fp_text reference VAL (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value MadeInOregonRev25 (at 0 0 90) (layer F.SilkS) hide)
  )
  (gr_text + (at 108.32 91.5) (layer B.SilkS))
  (gr_text ISP (at 106.32 93.25 90) (layer B.SilkS))
  (gr_text "Designed by\nwww.MakersBox.us" (at 116.82 96.25 90) (layer B.SilkS))
  (gr_text www.OSHPark.com (at 84.82 99.25 90) (layer B.SilkS))
  (dimension 44 (width 0.3) (layer Dwgs.User)
    (gr_text "44.000 mm" (at 99.82 130.6) (layer Dwgs.User))
    (feature1 (pts (xy 121.82 114.25) (xy 121.82 131.95)))
    (feature2 (pts (xy 77.82 114.25) (xy 77.82 131.95)))
    (crossbar (pts (xy 77.82 129.25) (xy 121.82 129.25)))
    (arrow1a (pts (xy 121.82 129.25) (xy 120.693496 129.836421)))
    (arrow1b (pts (xy 121.82 129.25) (xy 120.693496 128.663579)))
    (arrow2a (pts (xy 77.82 129.25) (xy 78.946504 129.836421)))
    (arrow2b (pts (xy 77.82 129.25) (xy 78.946504 128.663579)))
  )
  (dimension 50 (width 0.3) (layer Dwgs.User)
    (gr_text "50.000 mm" (at 68.47 100.25 270) (layer Dwgs.User))
    (feature1 (pts (xy 97.82 125.25) (xy 67.12 125.25)))
    (feature2 (pts (xy 97.82 75.25) (xy 67.12 75.25)))
    (crossbar (pts (xy 69.82 75.25) (xy 69.82 125.25)))
    (arrow1a (pts (xy 69.82 125.25) (xy 69.233579 124.123496)))
    (arrow1b (pts (xy 69.82 125.25) (xy 70.406421 124.123496)))
    (arrow2a (pts (xy 69.82 75.25) (xy 69.233579 76.376504)))
    (arrow2b (pts (xy 69.82 75.25) (xy 70.406421 76.376504)))
  )
  (gr_text 2017 (at 90.57 114.75) (layer F.Mask))
  (gr_text 2017 (at 90.57 114.75) (layer F.Cu))
  (gr_text CR2032 (at 99.82 121.25) (layer B.SilkS))
  (gr_text "http://www.mathopenref.com/coordpolycalc.html\nx100 y100 6 sides 25 radius 30 deg starting angle" (at 97.82 143.25) (layer Dwgs.User))
  (gr_line (start 122 113) (end 122 88) (angle 90) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 100 125) (end 122 113) (angle 90) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 78 113) (end 100 125) (angle 90) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 78 87) (end 78 113) (angle 90) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 122 88) (end 100 75) (angle 90) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 100 75) (end 78 87) (angle 90) (layer Edge.Cuts) (width 0.254))
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 99.82 77.25) (xy 119.82 89.25) (xy 119.82 112.25) (xy 99.82 122.25) (xy 79.82 112.25)
        (xy 79.82 88.25)
      )
    )
  )
)
