(kicad_pcb (version 20171130) (host pcbnew "(5.1.9)-1")
  (general
    (thickness 1.6)
    (drawings 1565)
    (tracks 10)
    (zones 0)
    (modules 7)
    (nets 8)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 1.83)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad4)")
  (net 2 "Net-(J1-Pad3)")
  (net 3 "Net-(J1-Pad2)")
  (net 4 "Net-(J1-Pad1)")
  (net 5 "Net-(TP4-Pad1)")
  (net 6 "Net-(TP5-Pad1)")
  (net 7 "Net-(TP6-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(TP4-Pad1)")
    (add_net "Net-(TP5-Pad1)")
    (add_net "Net-(TP6-Pad1)")
  )
  (module Footprint:SMTP (layer F.Cu) (tedit 60745503)
    (at 161.29 140.97)
    (fp_text reference TP6 (at 0 -2.6) (layer F.SilkS))
    (fp_text value TestPoint_Small (at 0 2.4) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.9 1.9) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(TP6-Pad1)"))
  )
  (module Footprint:SMTP (layer F.Cu) (tedit 60745503)
    (at 161.29 137.16)
    (fp_text reference TP5 (at 0 -2.6) (layer F.SilkS))
    (fp_text value TestPoint_Small (at 0 2.4) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.9 1.9) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(TP5-Pad1)"))
  )
  (module Footprint:SMTP (layer F.Cu) (tedit 60745503)
    (at 161.29 131.445)
    (fp_text reference TP4 (at 0 -2.6) (layer F.SilkS))
    (fp_text value TestPoint_Small (at 0 2.4) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.9 1.9) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(TP4-Pad1)"))
  )
  (module Footprint:SMTP (layer F.Cu) (tedit 60745503)
    (at 155.575 131.445)
    (fp_text reference TP3 (at 0 -2.6) (layer F.SilkS))
    (fp_text value TestPoint_Small (at 0 2.4) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.9 1.9) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad3)"))
  )
  (module Footprint:SMTP (layer F.Cu) (tedit 60745503)
    (at 149.86 131.445)
    (fp_text reference TP2 (at 0 -2.6) (layer F.SilkS))
    (fp_text value TestPoint_Small (at 0 2.4) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.9 1.9) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J1-Pad2)"))
  )
  (module Footprint:SMTP (layer F.Cu) (tedit 60745503)
    (at 144.145 131.445)
    (fp_text reference TP1 (at 0 -2.6) (layer F.SilkS))
    (fp_text value TestPoint_Small (at 0 2.4) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.9 1.9) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J1-Pad1)"))
  )
  (module Connector_Molex:Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 5EA53D3B)
    (at 149.225 142.875)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-04A example for new part number: 22-27-2041, 4 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 vertical")
    (fp_text reference J1 (at 3.81 -4.12) (layer F.SilkS))
    (fp_text value Conn_01x04_Male (at 3.81 4.08) (layer F.Fab))
    (fp_text user %R (at 3.81 -2.22) (layer F.Fab))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.74 2.19) (drill 1.19) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad4)"))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.74 2.19) (drill 1.19) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad3)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.74 2.19) (drill 1.19) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad2)"))
    (pad 1 thru_hole roundrect (at 0 0) (size 1.74 2.19) (drill 1.19) (layers *.Cu *.Mask) (roundrect_rratio 0.143678)
      (net 4 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 128.16566 144.862975) (end 178.147108 144.862975) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 123.946384 139.605175) (end 123.946384 141.351302) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 135.376384 128.810175) (end 135.376384 129.267375) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 136.882999 129.690772) (end 137.678753 128.386779) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 124.184447 141.926039) (end 126.62932 144.370912) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 126.486384 131.509048) (end 126.486384 137.979575) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 129.42332 128.235439) (end 126.724447 130.934312) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 180.639184 137.979575) (end 179.826384 137.979575) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 127.293141 145.421775) (end 127.7294 144.735975) (angle -32.5) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 125.673584 137.979575) (end 125.673584 138.792375) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 127.204057 143.796175) (end 126.62932 144.370912) (angle -45) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 134.563584 128.810175) (end 135.376384 128.810175) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 167.9402 128.810175) (end 168.634015 128.386779) (angle -58.6) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 179.108711 143.796175) (end 179.108711 144.608975) (angle -45) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 181.553584 141.351302) (end 182.12832 141.926039) (angle -45) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 128.16566 144.050175) (end 127.7294 144.735975) (angle -32.5) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 138.372568 128.810175) (end 138.372568 127.997375) (angle -58.6) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 171.749184 128.810175) (end 171.749184 127.997375) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 124.759184 139.605175) (end 124.759184 138.792375) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 176.314711 128.810175) (end 176.889447 128.235439) (angle -45) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 124.759184 141.351302) (end 123.946384 141.351302) (angle -45) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 181.553584 139.605175) (end 182.366384 139.605175) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 178.147108 144.050175) (end 178.147108 144.862975) (angle -32.5) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 179.019626 145.421775) (end 179.019626 144.608975) (angle -32.5) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 170.123584 129.267375) (end 169.429769 129.690772) (angle -148.6) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 179.013584 131.509048) (end 179.826384 131.509048) (angle -45) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 127.299184 131.509048) (end 126.724447 130.934312) (angle -45) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 129.998057 128.810175) (end 129.998057 127.997375) (angle -45) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 136.189184 129.267375) (end 135.376384 129.267375) (angle -148.6) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 134.563584 127.997375) (end 129.998057 127.997375) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 176.314711 127.997375) (end 171.749184 127.997375) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 167.9402 127.997375) (end 138.372568 127.997375) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 170.936384 128.810175) (end 170.936384 129.267375) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 169.429769 129.690772) (end 168.634015 128.386779) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 179.683447 144.370912) (end 182.12832 141.926039) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 179.58832 130.934312) (end 176.889447 128.235439) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 179.826384 137.979575) (end 179.826384 131.509048) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 182.366384 141.351302) (end 182.366384 139.605175) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 125.673584 138.792375) (end 124.759184 138.792375) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 181.553584 138.792375) (end 180.639184 138.792375) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 127.293141 144.608975) (end 127.204057 144.608975) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 179.019626 144.608975) (end 179.108711 144.608975) (layer Edge.Cuts) (width 0.05))
)
