(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 14)
    (no_connects 0)
    (area 129.518999 82.845 144.801001 101.786)
    (thickness 1.6)
    (drawings 20)
    (tracks 55)
    (zones 0)
    (modules 9)
    (nets 11)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user hide)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFEFFBF)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(D1-Pad1)")
  (net 2 Tele_ctrl)
  (net 3 S_pwr)
  (net 4 Ign_24V)
  (net 5 +24V)
  (net 6 "Net-(P1-Pad5)")
  (net 7 Earth)
  (net 8 "Net-(Q1-Pad3)")
  (net 9 "Net-(Q2-Pad1)")
  (net 10 "Net-(Q1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +24V)
    (add_net Earth)
    (add_net Ign_24V)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(P1-Pad5)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(Q1-Pad3)")
    (add_net "Net-(Q2-Pad1)")
    (add_net S_pwr)
    (add_net Tele_ctrl)
  )
  (module Diodes_SMD:D_SOD-323_HandSoldering (layer F.Cu) (tedit 5B7B1FA2)
    (at 136.398 98.171 180)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D1 (at 2.921 1.905 180) (layer F.SilkS))
    (fp_text value D (at 0.1 1.9 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.85 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 1.25 0 180) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 2 Tele_ctrl))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module FootPrints:DT0X_6P (layer F.Cu) (tedit 5B7B0384)
    (at 137.16 93.98)
    (fp_text reference P1 (at 0.508 0.762 90) (layer B.SilkS) hide)
    (fp_text value CONN_01X06 (at 0 -10.16 180) (layer F.Fab))
    (fp_text user 6 (at 1.905 -4.572) (layer B.SilkS))
    (fp_text user 5 (at 1.905 0) (layer B.SilkS))
    (fp_text user 4 (at 1.905 4.318) (layer B.SilkS))
    (fp_text user 3 (at -2.159 4.318) (layer B.SilkS))
    (fp_text user 2 (at -2.032 0) (layer B.SilkS))
    (fp_text user 1 (at -2.032 -4.572) (layer B.SilkS))
    (pad 5 thru_hole circle (at 4.572 0) (size 3.048 3.048) (drill 1.524) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(P1-Pad5)"))
    (pad 2 thru_hole circle (at -4.5466 0) (size 3.048 3.048) (drill 1.524) (layers *.Cu *.Mask F.SilkS)
      (net 2 Tele_ctrl))
    (pad 1 thru_hole circle (at -4.5466 -4.445) (size 3.048 3.048) (drill 1.524) (layers *.Cu *.Mask F.SilkS)
      (net 5 +24V))
    (pad 3 thru_hole circle (at -4.5466 4.445) (size 3.048 3.048) (drill 1.524) (layers *.Cu *.Mask F.SilkS)
      (net 4 Ign_24V))
    (pad 4 thru_hole circle (at 4.572 4.445) (size 3.048 3.048) (drill 1.524) (layers *.Cu *.Mask F.SilkS)
      (net 3 S_pwr))
    (pad 6 thru_hole circle (at 4.572 -4.445) (size 3.048 3.048) (drill 1.524) (layers *.Cu *.Mask F.SilkS)
      (net 7 Earth))
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5B7B1FAC)
    (at 139.319 92.71 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 0.889 1.651 180) (layer F.SilkS))
    (fp_text value 2.2K (at 0 1.55 90) (layer F.Fab))
    (fp_text user %R (at 1.27 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(Q2-Pad1)"))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(Q1-Pad3)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SOD-323_HandSoldering (layer F.Cu) (tedit 5B7B1FC2)
    (at 136.398 100.076 180)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D2 (at 2.921 -0.508 180) (layer F.SilkS))
    (fp_text value D (at 0.1 1.9 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.85 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 3 S_pwr))
    (pad 2 smd rect (at 1.25 0 180) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 4 Ign_24V))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5B7B1FCC)
    (at 139.192 98.298 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 2.413 -0.381 360) (layer F.SilkS))
    (fp_text value 2.2K (at 0 1.55 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5B7B1FB6)
    (at 139.319 88.773 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at -1.397 -1.651 360) (layer F.SilkS))
    (fp_text value 10K (at 0 1.55 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 Earth))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(Q1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5B7B1FB1)
    (at 136.525 92.964)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at -3.048 -1.016) (layer F.SilkS))
    (fp_text value 2.2K (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 +24V))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(Q2-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23_Handsoldering (layer F.Cu) (tedit 5BA3EED7)
    (at 136.525 89.535 270)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at -2.19964 2.83972 360) (layer F.SilkS))
    (fp_text value 2N3904 (at 0 2.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 360) (layer F.Fab))
    (pad 1 smd rect (at -1.5 -0.95 270) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at -1.5 0.95 270) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 7 Earth))
    (pad 3 smd rect (at 1.5 0 270) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(Q1-Pad3)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes\SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23_Handsoldering (layer F.Cu) (tedit 5BA3EEBD)
    (at 137.541 95.41764)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q2 (at 3.62204 0.74168) (layer F.SilkS))
    (fp_text value FDN338P (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.5 -0.95) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(Q2-Pad1)"))
    (pad 2 smd rect (at -1.5 0.95) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 5 +24V))
    (pad 3 smd rect (at 1.5 0) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 3 S_pwr))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes\SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 144.526 89.408) (end 141.732 86.614) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 144.526 98.552) (end 144.526 89.408) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 141.732 101.346) (end 144.526 98.552) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 132.588 101.346) (end 141.732 101.346) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 129.794 98.552) (end 132.588 101.346) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 129.794 89.408) (end 129.794 98.552) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 132.588 86.614) (end 129.794 89.408) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 141.732 86.614) (end 132.588 86.614) (angle 90) (layer Edge.Cuts) (width 0.15))
)
