<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.1.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="13" y2="0" width="0" layer="20"/>
<wire x1="13" y1="0" x2="13" y2="68" width="0" layer="20"/>
<wire x1="13" y1="68" x2="0" y2="68" width="0" layer="20"/>
<wire x1="0" y1="68" x2="0" y2="0" width="0" layer="20"/>
<hole x="6.5" y="63" drill="3.5"/>
<hole x="6.5" y="8" drill="3.5"/>
<text>+</text>
<text>-</text>
<text>1</text>
<text>2</text>
<text>3</text>
<text>-</text>
<text>3</text>
<text>2</text>
<text>1</text>
<text>+</text>
<text>May
2020</text>
</plain>
<libraries>
<library name="SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TACTILE-PTH">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="dp_devices">
<description>Dangerous Prototypes Standard PCB sizes
http://dangerousprototypes.com</description>
<packages>
<package name="M1X5">
</package>
</packages>
</library>
<library name="1Nicks">
<description>Nick's Custom Library</description>
<packages>
<package name="R0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="CHIPLED_1206">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_LY N971.pdf</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="S1" library="SparkFun" package="TACTILE-PTH" value="SWITCH-MOMENTARY-2PTH">
<attribute name="NAME"/>
</element>
<element name="S2" library="SparkFun" package="TACTILE-PTH" value="SWITCH-MOMENTARY-2PTH">
<attribute name="NAME"/>
</element>
<element name="S3" library="SparkFun" package="TACTILE-PTH" value="SWITCH-MOMENTARY-2PTH">
<attribute name="NAME"/>
</element>
<element name="J1" library="dp_devices" package="M1X5" value="CON_HEADER_1X05-PTH">
<attribute name="NAME"/>
</element>
<element name="R1" library="1Nicks" package="R0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="1Nicks" package="CHIPLED_1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED2" library="1Nicks" package="CHIPLED_1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED3" library="1Nicks" package="CHIPLED_1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="1Nicks" package="R0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED4" library="1Nicks" package="CHIPLED_1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED5" library="1Nicks" package="CHIPLED_1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED6" library="1Nicks" package="CHIPLED_1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="1Nicks" package="R0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="S3" pad="3"/>
<contactref element="S2" pad="3"/>
<contactref element="S1" pad="3"/>
<contactref element="J1" pad="1"/>
<contactref element="LED1" pad="C"/>
<contactref element="LED4" pad="C"/>
<contactref element="LED2" pad="C"/>
<contactref element="LED5" pad="C"/>
<contactref element="LED3" pad="C"/>
<contactref element="LED6" pad="C"/>
</signal>
<signal name="N$2">
<contactref element="S3" pad="1"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="S2" pad="1"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="N$4">
<contactref element="S1" pad="1"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="VCC">
<contactref element="J1" pad="5"/>
<contactref element="R1" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="LED1" pad="A"/>
<contactref element="R1" pad="2"/>
<contactref element="LED4" pad="A"/>
</signal>
<signal name="N$5">
<contactref element="LED6" pad="A"/>
<contactref element="LED3" pad="A"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="LED5" pad="A"/>
<contactref element="LED2" pad="A"/>
<contactref element="R2" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
