<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="26.6" y2="0" width="0" layer="20"/>
<wire x1="26.6" y1="0" x2="26.7" y2="34.8" width="0" layer="20"/>
<wire x1="26.7" y1="34.8" x2="0" y2="34.8" width="0" layer="20"/>
<wire x1="0" y1="34.8" x2="0" y2="0" width="0" layer="20"/>
<text>VCC</text>
<text>GND</text>
<text>OE</text>
<text>OUT</text>
<text>Green Shoe Garage</text>
<text>rev 1.0       3OCT15</text>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="1X2-3.5MM">
</package>
<package name="1X03-CLEANBIG">
</package>
</packages>
</library>
<library name="TSL230R">
<packages>
<package name="DIP8">
<description>&lt;B&gt;Dual In Line&lt;/B&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="adafruit" package="1X2-3.5MM" value="1X2-3.5MM"/>
<element name="J2" library="adafruit" package="1X2-3.5MM" value="1X2-3.5MM"/>
<element name="LIGHT1" library="TSL230R" package="DIP8" value="TSL230RDIP8"/>
<element name="S0" library="adafruit" package="1X03-CLEANBIG" value=""/>
<element name="S1" library="adafruit" package="1X03-CLEANBIG" value=""/>
<element name="S2" library="adafruit" package="1X03-CLEANBIG" value=""/>
<element name="S3" library="adafruit" package="1X03-CLEANBIG" value=""/>
</elements>
<signals>
<signal name="VCC">
<contactref element="J1" pad="1"/>
<contactref element="S0" pad="3"/>
<contactref element="S1" pad="3"/>
<contactref element="S3" pad="1"/>
<contactref element="S2" pad="1"/>
<contactref element="LIGHT1" pad="5"/>
</signal>
<signal name="GND">
<contactref element="J1" pad="2"/>
<contactref element="S0" pad="1"/>
<contactref element="S1" pad="1"/>
<contactref element="S3" pad="3"/>
<contactref element="S2" pad="3"/>
<contactref element="LIGHT1" pad="4"/>
</signal>
<signal name="OUT">
<contactref element="J2" pad="1"/>
<contactref element="LIGHT1" pad="6"/>
</signal>
<signal name="OE">
<contactref element="J2" pad="2"/>
<contactref element="LIGHT1" pad="3"/>
</signal>
<signal name="N$1">
<contactref element="S0" pad="2"/>
<contactref element="LIGHT1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="S1" pad="2"/>
<contactref element="LIGHT1" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="S3" pad="2"/>
<contactref element="LIGHT1" pad="8"/>
</signal>
<signal name="N$4">
<contactref element="LIGHT1" pad="7"/>
<contactref element="S2" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
