<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="-0.635" y1="52.705" x2="45.39" y2="52.705" width="0" layer="20"/>
<wire x1="45.39" y1="52.705" x2="45.39" y2="80" width="0" layer="20"/>
<wire x1="45.39" y1="80" x2="-0.635" y2="80" width="0" layer="20"/>
<wire x1="-0.635" y1="80" x2="-0.635" y2="52.705" width="0" layer="20"/>
<text>5V</text>
<text>GND</text>
<text>Data</text>
<text>Latch</text>
<text>Clk</text>
<text>5V</text>
<text>GND</text>
</plain>
<libraries>
<library name="Daniel">
<packages>
<package name="BREADBOARD_POT">
</package>
<package name="16DIP">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="TO92-EBC-OVAL">
<description>&lt;b&gt;TO-92&lt;/b&gt;&lt;p&gt;
grid 5.08 mm</description>
</package>
<package name="1X05-3.5MM">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.5">
<description>1/2W Resistor, 0.5" wide&lt;p&gt;

Yageo CFR series &lt;a href="http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf"&gt;http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf&lt;/a&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Displays">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of display devices- LED displays, LCD displays, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LCD-16X2_NOHOLES">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$3" library="Daniel" package="BREADBOARD_POT" value="10K"/>
<element name="U2" library="Daniel" package="16DIP" value=""/>
<element name="LCD_NPN" library="adafruit" package="TO92-EBC-OVAL" value="2N2222">
<attribute name="VALUE"/>
</element>
<element name="R10" library="SparkFun-Resistors" package="AXIAL-0.5" value="4.7K">
<attribute name="VALUE"/>
</element>
<element name="R11" library="SparkFun-Resistors" package="AXIAL-0.5" value="47K">
<attribute name="VALUE"/>
</element>
<element name="J1" library="adafruit" package="1X05-3.5MM" value="1X5"/>
<element name="U1" library="SparkFun-Displays" package="LCD-16X2_NOHOLES" value="LCD-16X2NOHOLES"/>
</elements>
<signals>
<signal name="GND">
<contactref element="U$3" pad="3"/>
<contactref element="U2" pad="13"/>
<contactref element="U2" pad="8"/>
<contactref element="LCD_NPN" pad="E"/>
<contactref element="R11" pad="P$1"/>
<contactref element="J1" pad="5"/>
<contactref element="U1" pad="1"/>
<contactref element="U1" pad="5"/>
</signal>
<signal name="5V">
<contactref element="U2" pad="16"/>
<contactref element="U2" pad="10"/>
<contactref element="J1" pad="1"/>
<contactref element="U$3" pad="1"/>
<contactref element="U1" pad="2"/>
<contactref element="U1" pad="15"/>
</signal>
<signal name="DATA">
<contactref element="U2" pad="14"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="CLOCK">
<contactref element="U2" pad="11"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="LATCH">
<contactref element="U2" pad="12"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="CONTRAST">
<contactref element="U$3" pad="2"/>
<contactref element="U1" pad="3"/>
</signal>
<signal name="RS">
<contactref element="U2" pad="7"/>
<contactref element="U1" pad="4"/>
</signal>
<signal name="NC">
<contactref element="U2" pad="6"/>
</signal>
<signal name="BACKLIGHT">
<contactref element="U2" pad="5"/>
<contactref element="R10" pad="P$2"/>
</signal>
<signal name="LCD4">
<contactref element="U2" pad="4"/>
<contactref element="U1" pad="11"/>
</signal>
<signal name="LCD5">
<contactref element="U2" pad="3"/>
<contactref element="U1" pad="12"/>
</signal>
<signal name="LCD6">
<contactref element="U2" pad="2"/>
<contactref element="U1" pad="13"/>
</signal>
<signal name="LCD7">
<contactref element="U2" pad="1"/>
<contactref element="U1" pad="14"/>
</signal>
<signal name="E">
<contactref element="U2" pad="15"/>
<contactref element="U1" pad="6"/>
</signal>
<signal name="SER_OUT">
<contactref element="U2" pad="9"/>
</signal>
<signal name="N$28">
<contactref element="LCD_NPN" pad="B"/>
<contactref element="R10" pad="P$1"/>
<contactref element="R11" pad="P$2"/>
</signal>
<signal name="BACKLIGHT-">
<contactref element="LCD_NPN" pad="C"/>
<contactref element="U1" pad="16"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
